# ACS Group-of-Prefixed-URLs Configuration Mode Commands

The ACS Group-of-Prefixed-URLs Configuration Mode is used to create and configure groups of prefixed URLs.

IMPORTANT:

This configuration mode is customer specific. For more information, contact your Cisco account representative.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
prefixed-url

This command allows you to add or remove URLs from the current group of prefixed URLs.

IMPORTANT:

A maximum of 10 URLs can be added per group.
Platform:

ASR 5000

ASR 5500
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] prefixed-url url

no

If added previously, removes the specified URL from the current group of prefixed URLs.
url

Specifies the URL to add/remove.

url must be an alphanumeric string of 1 through 63 characters.
Usage:

Use this command to add or remove URLs to be filtered from the group of prefixed URLs.
Example:
The following command adds the URL http://abc.net to the current group of prefixed URLs:

    prefixed-url http://abc.net