# show cpu table

Table 1. show cpu table Command Output Descriptions

Field | Description
--- | ---
CPU | Displays the number of the CPU in the format slot_number/cpu_number.
State | Indicates the CPU state as one of the following: Actve: The CPU is active and available for session processing.Sndby: The CPU is on standby.
Load | Indicates the CPU load for the following time intervals: Now: Current load5min: Load within the last 5 minutes15min: Load within the last 15 minutes
CPU-Usage | Indicates the CPU usage as a percentage for the following time intervals: Now: Current usage5min: Usage within the last 5 minutes15min: Usage within the last 15 minutes
Memory | Indicates the memory usage for the following time intervals: Now: Current usage5min: Usage within the last 5 minutes15min: Usage within the last 15 minutes In addition, the total memory available on the CPU is displayed. The PSC has two CPUs, the main CPU (CPU 0) contains 16 GB of memory. The second CPU is contained within the card’s NPU and provides an additional 512 MB of memory.The PSC2 has two CPUs, the main CPU (CPU 0) contains 32 GB of memory.