# ACS Host Pool Configuration Mode Commands

The ACS Host Pool Configuration Mode is used to define a pool of host addresses within the ACS Configuration Mode. The host pool facilitates to create rules to handle the packets coming from or going to a group of hosts within an access policy.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
ip

This command allows you to add/remove an individual or a range of host IPv4/IPv6 address(es) from the current host pool.
Platform:

ASR 5000

ASR 5500
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] ip { ipv4/ipv6_address | ipv4/ipv6_address/maskbit | range start_ipv4/ipv6_address to end_ipv4/ipv6_address }

no

If added previously, removes the specified IPv4/IPv6 address(es) from the current host pool.
ipv4/ipv6_address

Specifies an IPv4/IPv6 address to add to the current host pool.

ipv4/ipv6_address must be an IPv4/IPv6 address.
ipv4/ipv6_address/maskbit

Specifies an IPv4/IPv6 address/mask bits combination to add to the current host pool.

ipv4/ipv6_address must be an IPv4/IPv6 address.

maskbit must be the number of bits in the subnet mask, and must be a numeric value.
range start_ipv4/ipv6_address to end_ipv4/ipv6_address

Specifies a range of IPv4/IPv6 addresses to add to the current host pool.

start_ipv4/ipv6_address specifies the starting IPv4/IPv6 address of the range, and must be less than end_ipv4/v6_address.

end_ipv4/v6_address specifies the ending IPv4/IPv6 address of the range, and must be greater than start_ipv4/ipv6_address.
Usage:

Use this command to add an individual or a range of IPv4/IPv6 addresses to a host pool. Up to 10 sets of IPv4/IPv6 addresses can be configured in each host pool.
Example:
The following command adds all IPv4 addresses from 10.2.3.4 through 10.4.5.6 to the current host pool:

    ip range 10.2.3.4 to 10.4.5.6