# show pgw

This chapter describes the output of the show pgw command.
show pgw-service all

Displays configuration information for all P-GW services configured on the system.
Table 1. show pgw-service all Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the P-GW service configured and running on the system.
Service-ID | The system-generated identification number associated with the P-GW service name.
Context | The context name where the P-GW service is configured.
Accounting Context | The context name where the accounting configuration and/or interface(s) are configured.
Accounting gtpp group | Displays all the configured GTPP server groups associated with this service for accounting.
Status | Indicates whether the P-GW service is started or not.
Restart Counter | Specifies the restart counter.
EGTP Service | The eGTP service name configured for use by this service.
LMA Service | The LMA service name configured for use by this service.
GGSN Service | The GGSN service name associated with this service.
Session-Delete-Delay Timer | Indicates whether there is a delay in terminating a session.
Session-Delete-Delay Timeout | Specifies the time (msecs) to retain a session before terminating it.
PLMN ID List | The Public Land Mobile Network identifier list associated with this P-GW service. A PLMN contains a Mobile Country Code (MCC) and Mobile Network Code (MNC). Up to five PLMN IDs can be configured for each P-GW service.
Newcall Policy | The newcall policy configured for this P-GW service. Specifies whether the P-GW will accept or reject requests for a static IP address if the address is already in use by another session
dns-client Context Name | The context where the DNS client is configured and used by this service.
gx-li context | Refer to the Lawful Intercept Configuration Guide.
gx-li transport | Refer to the Lawful Intercept Configuration Guide.
QCI-QOS Mapping Table Name | The QoS Class Index to QoS mapping table configured for use with this service.
Authorize | Enables/disables subscriber session authorization with HSS over S6b Diameter interface.
S6b IPv6 Reporting | Specifies whether IPv6 address reporting through AAR towards the S6b interface is enabled or disabled.
Duplicate Subscriber Addr Request | Specifies whether the P-GW will accept or reject requests for a static IP address if the address is already in use by another session.
Fqdn-name | The name of Fully Qualified Domain Name (FQDN) which is used for authorization over S6b interface between P-GW and 3GPP AAA/HSS.
SAEGW service | Specifies whether P-GW service is part of SAEGW service.

show pgw-service statistics all
Table 2. show pgw-service statistics all Command Output Descriptions

Field | Description
--- | ---
PGW Node Level Statistics
VPN Name | The name of the context in which the P-GW service is configured.
Total Active UE | The total number of active subscribers.
Total bearers active
Default bearers | The total number of active default bearers using the P-GW node.
Non-Emergency | The total number of active default non-emergency bearers using the P-GW node.
Emergency | The total number of active default emergency bearers using the P-GW node.
Dedicated bearers | The total number of active dedicated bearers using the P-GW node.
UE-initiated | The total number of active UE-initiated dedicated bearers using the P-GW node.
Network-initiated | The total number of active network-initiated dedicated bearers using the P-GW node.
Non-Emergency | The total number of active non-emergency dedicated bearers using the P-GW node.
Emergency | The total number of active emergency dedicated bearers using the P-GW node.
Total bearers setup
Default bearers | The total number of default bearers set up using the P-GW node.
Non-Emergency | The total number of default non-emergency bearers set up using the P-GW node.
Emergency | The total number of default emergency bearers set up using the P-GW node.
Dedicated bearers | The total number of dedicated bearers set up using the P-GW node.
UE-initiated | The total number of UE-initiated dedicated bearers set up using the P-GW node.
Network-initiated | The total number of network-initiated dedicated bearers set up using the P-GW node.
Non-Emergency | The total number of non-emergency dedicated bearers set up using the P-GW node.
Emergency | The total number of emergency dedicated bearers set up using the P-GW node.
Total bearers released
Default bearers | The total number of default bearers released using the P-GW node.
Network init release | The total number of default bearers released due to an network-initiated release using the P-GW node.
MME init release | The total number of default bearers released due to an MME-initiated release using the P-GW node.
Dedicated bearers | The total number of dedicated bearers released using the P-GW node.
Network init release | The total number of dedicated bearers released due to an network-initiated release using the P-GW node.
MME Initiated release | The total number of dedicated bearers released due to an MME-initiated release using the P-GW node.
Default bearer release | The total number of dedicated bearers released due to a default bearer release using the P-GW node.
Total bearers release failure
Default bearers | The total number of default bearer release failures using the P-GW node.
Dedicated bearers | The total number of dedicated bearer release failures using the P-GW node.
Total bearers rejected
Default bearers | The total number of default bearers rejected using the P-GW node.
Dedicated bearers | The total number of dedicated bearers rejected using the P-GW node.
UE-req reject | The total number of UE-requested bearers rejected using the P-GW node.
Network-req reject | The total number of network-requested bearers rejected using the P-GW node.
Total Emergency default bearer rejected | The total number of emergency default bearer rejected using the P-GW node.
Total Emergency dedicated bearers rejected | The total number of emergency dedicated bearer rejected using the P-GW node.
Total bearers modified
UE-initiated mod | The total number of UE-initiated bearers modified using the P-GW node.
Network-initiated mod | The total number of network-initiated bearers modified using the P-GW node.
Total bearers modification failure
UE-initiated mod fail | The total number of UE-initiated bearer modification failures using the P-GW node.
Network-initiated mod fail | The total number of network-initiated bearer modification failures using the P-GW node.
Subscriber session statistics
Total bearers active
Default bearers | The total number of active default bearers using the P-GW service(s) on this system.
Dedicated bearers | The total number of active dedicated bearers using the P-GW service(s) on this system. This counter increments for both network and UE-initiated dedicated bearers.
Total bearers setup
Default bearers | The total number of default bearers setup using the P-GW service(s) on this system.
Dedicated bearers | The total number of dedicated bearers setup using the P-GW service(s) on this system. This counter increments for both network and UE-initiated dedicated bearer setup.
Total bearers released
Default bearers | The total number of default bearers released using the P-GW service(s) on this system.
Network initiated release
Admin disconnect | The total number of default bearers released due to an administrative disconnect using the P-GW service(s) on this system.
GTP-U error ind | The total number of default bearers released due to a GTP-U error indication using the P-GW service(s) on this system.
SGW Path failure | The total number of default bearers released due to an S-GW path failure using the P-GW service(s) on this system.
MME Initiated release | The total number of default bearers released due to an MME initiated release using the P-GW service(s) on this system.
Dedicated bearers | The total number of dedicated bearers released using the P-GW service(s) on this system.
Network initiated release
Admin disconnect | The total number of dedicated bearers released due to an administrative disconnect using the P-GW service(s) on this system.
GTP-U error ind | The total number of dedicated bearers released due to a GTP-U error indication using the P-GW service(s) on this system.
MME initiated release | The total number of dedicated bearers released due to an MME initiated release using the P-GW service(s) on this system.
Default bearer release | The total number of dedicated bearers released due to a default bearer release using the P-GW service(s) on this system.
Total bearers release failure
Default bearers | The total number of default bearer release failures using the P-GW service(s) on this system.
Dedicated bearers | The total number of dedicated bearer release failures using the P-GW service(s) on this system.
Total bearers rejected:
Default bearers | The total number of default bearers rejected using the P-GW service(s) on this system.
No Resource | The total number of default bearers rejected due to a no resource condition using the P-GW service(s) on this system.
Missing or unknown APN | The total number of default bearers rejected due to a missing or unknown APN using the P-GW service(s) on this system.
APN selection-Mode mismatch | The total number of default bearers rejected due to an APN selection mode mismatch using the P-GW service(s) on this system.
Pref PDN-Type not supported | The total number of default bearers rejected due to a preferred PDN type not supported condition using the P-GW service(s) on this system.
APN restr violation | The total number of default bearers rejected due to an APN restriction violation using the P-GW service(s) on this system.
Subs auth failed | The total number of default bearers rejected due to a subscriber authentication failure using the P-GW service(s) on this system.
Subs static addr not allowed | The total number of default bearers rejected due to a disallowed subscriber static IP address using the P-GW service(s) on this system.
Subs static addr not alloc | The total number of default bearers rejected due to an unallocated subscriber static IP address using the P-GW service(s) on this system.
Dynamic addr not alloc | The total number of default bearers rejected due to an unallocated dynamic IP address using the P-GW service(s) on this system.
Subs static addr not present | The total number of default bearers rejected due to a missing subscriber static IP address using the P-GW service(s) on this system.
Dedicated bearers | The total number of dedicated bearers rejected using the P-GW service(s) on this system.
UE-req reject | The total number of UE-requested dedicated bearers rejected using the P-GW service(s) on this system.
Network-req reject | The total number of network-requested dedicated bearers rejected using the P-GW service(s) on this system.
Total bearers modified
UE-initiated modification | The total number of UE-initiated bearers modified using the P-GW service(s) on this system.
QOS modification | The total number of UE-initiated bearers with a QoS modification using the P-GW service(s) on this system.
TFT modification | The total number of UE-initiated bearers with a TFT modification using the P-GW service(s) on this system.
Network-initiated modification | The total number of network-initiated bearers modified using the P-GW service(s) on this system.
QOS modification | The total number of network-initiated bearers with a QoS modification using the P-GW service(s) on this system.
TFT modification | The total number of network-initiated bearers with a TFT modification using the P-GW service(s) on this system.
Total bearers modification failure
UE-initiated mod failed | The total number of UE-initiated bearer modification failures using the P-GW service(s) on this system.
QOS mod fail | The total number of UE-initiated bearer modification failures due to QoS modification failures using the P-GW service(s) on this system.
Semantic err in TFT oper | The total number of UE-initiated bearer modification failures due to semantic errors in a TFT operation using the P-GW service(s) on this system.
Syntact err in TFT oper | The total number of UE-initiated bearer modification failures due to syntactic errors in a TFT operation using the P-GW service(s) on this system.
Semantic err in pkt filter | The total number of UE-initiated bearer modification failures due to semantic errors in a packet filter using the P-GW service(s) on this system.
Syntact err in pkt filter | The total number of UE-initiated bearer modification failures due to syntactic errors in a packet filter using the P-GW service(s) on this system.
Network-initiated mod failed | The total number of network-initiated bearer modification failures using the P-GW service(s) on this system.
QOS mod fail | The total number of network-initiated bearer modification failures due to QoS modification failures using the P-GW service(s) on this system.
Semantic err in TFT oper | The total number of network-initiated bearer modification failures due to semantic errors in a TFT operation using the P-GW service(s) on this system.
Syntact err in TFT oper | The total number of network-initiated bearer modification failures due to syntactic errors in a TFT operation using the P-GW service(s) on this system.
Semantic err in pkt filter | The total number of network-initiated bearer modification failures due to semantic errors in a packet filter using the P-GW service(s) on this system.
Syntact err in pkt filter | The total number of network-initiated bearer modification failures due to syntactic errors in a packet filter using the P-GW service(s) on this system.
Total PDN-Type stats
PDN-Type IPv4 sessions | The total number of PDN-type IPv4 sessions using the P-GW service(s) on this system.
Active | The total number of active PDN-type IPv4 sessions using the P-GW service(s) on this system.
Setup | The total number of setup PDN-type IPv4 sessions using the P-GW service(s) on this system.
Released | The total number of released PDN-type IPv4 sessions using the P-GW service(s) on this system.
PDN-Type IPv6 sessions | The total number of PDN-type IPv6 sessions using the P-GW service(s) on this system.
Active | The total number of active PDN-type IPv6 sessions using the P-GW service(s) on this system.
Setup | The total number of setup PDN-type IPv6 sessions using the P-GW service(s) on this system.
Released | The total number of released PDN-type IPv6 sessions using the P-GW service(s) on this system.
PDN-Type IPv4v6 sessions | The total number of PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
Active | The total number of active PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
Setup | The total number of setup PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
Released | The total number of released PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
IP address allocation statistics
Total IPv4 addrs allocated | The total number of IPv4 addresses allocated using the P-GW service(s) on this system.
Local pool add assign | The total number of local IP pool IPv4 addresses allocated using the P-GW service(s) on this system.
Static addr assign | The total number of static IPv4 addresses allocated using the P-GW service(s) on this system.
Radius provided addr assign | The total number of RADIUS-provided IPv4 addresses allocated using the P-GW service(s) on this system.
Total IPv6 addrs allocated | The total number of IPv6 addresses allocated using the P-GW service(s) on this system.
Stateless auto config | The total number of stateless address auto configuration IPv6 addresses allocated using the P-GW service(s) on this system.
Local pool add assign | The total number of local IP pool IPv6 addresses allocated using the P-GW service(s) on this system.
Static addr assign | The total number of static IPv6 addresses allocated using the P-GW service(s) on this system.
Radius provided addr assign | The total number of RADIUS-provided IPv6 addresses allocated using the P-GW service(s) on this system.
SGi tunneling statistics
Total IPv4 tunnel sessions | The total number of IPv4 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
IP-in-IP tun sessn active | The total number of active IP-in-IP tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
IP-in-IP tun sessions setup | The total number of setup IP-in-IP tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
IP-in-IP tun sessions released | The total number of released IP-in-IP tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
GRE-tun sessions active | The total number of active GRE tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
GRE-tun sessions setup | The total number of setup GRE tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
GRE-tun session release | The total number of released GRE tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
Total IPv6 tunneled sessions | The total number of IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
6to4 tun sessions active | The total number of active IPv4-in-IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
6to4 tun session setup | The total number of setup IPv4-in-IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
6to4 tun sessions released | The total number of released IPv4-in-IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
Subscriber PLMN Statistics
Home subscribers sessions | The total number of home subscriber sessions using the P-GW service(s) on this system.
Sessions active | The total number of active home subscriber sessions using the P-GW service(s) on this system.
Sessions setup | The total number of setup home subscriber sessions using the P-GW service(s) on this system.
Sessions released | The total number of released home subscriber sessions using the P-GW service(s) on this system.
Roaming subscribers sessions | The total number of roaming subscriber sessions using the P-GW service(s) on this system.
Sessions active | The total number of active roaming subscriber sessions using the P-GW service(s) on this system.
Sessions setup | The total number of setup roaming subscriber sessions using the P-GW service(s) on this system.
Sessions released | The total number of released roaming subscriber sessions using the P-GW service(s) on this system.
Visiting subscribers sessions | The total number of visiting subscriber sessions using the P-GW service(s) on this system.
Sessions active | The total number of active visiting subscriber sessions using the P-GW service(s) on this system.
Sessions setup | The total number of setup visiting subscriber sessions using the P-GW service(s) on this system.
Sessions released | The total number of released visiting subscriber sessions using the P-GW service(s) on this system.
Subscriber QoS Statistics
Total bearers active
QCI 1 - 9 | The total number of active bearers with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of active bearers with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of active bearers with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total bearers setup
QCI 1 - 9 | The total number of setup bearers with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of setup bearers with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of setup bearers with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total bearers released
QCI 1 - 9 | The total number of released bearers with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of released bearers with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of released bearers with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Subscriber Data Statistics
Total Uplink packets forwarded
QCI 1 - 9 | The total number of uplink packets forwarded with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of uplink packets forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of uplink packets forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Uplink bytes forwarded
QCI 1 - 9 | The total number of uplink bytes forwarded with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of uplink bytes forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of uplink bytes forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Downlink packets forwarded
QCI 1 - 9 | The total number of downlink packets forwarded with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of downlink packets forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of downlink packets forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Downlink bytes forwarded
QCI 1 - 9 | The total number of downlink bytes forwarded with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of downlink bytes forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of downlink bytes forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Uplink packets dropped
QCI 1 - 9 | The total number of uplink packets dropped with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of uplink packets dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of uplink packets dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Uplink bytes dropped
QCI 1 - 9 | The total number of uplink bytes dropped with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of uplink bytes dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of uplink bytes dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Downlink packets dropped
QCI 1 - 9 | The total number of downlink packets dropped with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of downlink packets dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of downlink packets dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.
Total Downlink bytes dropped
QCI 1 - 9 | The total number of downlink bytes dropped with a QoS Class Index using the P-GW service(s) on this system.
Non-Std QCI (Non-GBR) | The total number of downlink bytes dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
Non-Std QCI (GBR) | The total number of downlink bytes dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.