# Sample ADC Configuration

This appendix contains a sample Application Detection and Control (ADC) configuration within an ECS service that includes the examples from the procedures in Application Detection and Control Configuration chapter.

    configure

       license
    key "\

    VER=1|C1M=SanDiskSDCFJ-4096|C1S=116919K2106K0235|DOI=1217844147|DOE=12\

    33741747|ISS=1|NUM=26914|CMT=bngnc18,_chassis1,_|LSP=100000|LS0|LSF=100000|SIG=MCwCFFABNedEgGb8fAw8u0lvwxbWbJEBAhQvpG9YREYRFDDElzNUBuZv3kbHQw"

       system
    hostname host_name

       autoconfirm

       crash
    enable encrypted url 057285fc2112177777b5e7a716356c3e332f12f89

       card
    1

          mode
    active psc

          exit

       card
    4

          mode
    active psc

          exit

       card
    16

          mode
    active psc

          exit

       require
    active-charging

       context
    local

          interface
    spio1

             ip
    address 1.2.3.4 255.255.255.0

             exit

          server
    ftpd

             exit

          ssh
    key 0d94d7812a224fd97a58d9c6dab47bd7b318e705d1ee91d45254ef1286be8ef5cc271cf3d05656652014d69a568d099664ed2354369ce6481772a2dbf0f37ad20dc1e2b765d8c9f041759c0e1e8a9e53e3975b1724329d1a2012bf0221cc132014a1224cdfc45ca7
    len 461

          ssh
    key 75f41778bab0a173ee6e4e79c102638966c38eb5490fe46be064007e6951792a6abaf2733c4f4972318eb3b77f85d8925d4aae335dedfa0619f03cdfb3f35fef82cfa97eb1b2517654aad83afc2c7c5c08d76e2e4e9d8edaddd280f7963c227ff8f122ecefb9d8e0
    len 457 type v2-dsa

          server
    sshd

             subsystem
    sftp

             exit

          server
    telnetd

             exit

          subscriber
    default

             exit

          administrator
    admin encrypted password abc123def456ghi ftp

          aaa
    group default

             exit

          gtpp
    group default

             exit

          ip
    route 0.0.0.0 0.0.0.0 1.2.3.4 spio1

             exit

         exit

       port
    ethernet 24/1

          no
    shutdown

          bind
    interface spio1 local

          exit

       ntp

          enable

          server
    10.6.1.1

          exit

       snmp
    engine-id local 87e55bf69c4c479d

      active-charging
    service service_1

          p2p-detection
    protocol all

          ruledef
    ch_ares

             p2p
    protocol = ares

             exit

          ruledef
    ch_bittorrent

             p2p
    protocol = bittorrent

             exit

           ruledef
    ch_blackberry

             p2p
    protocol = blackberry

             exit

          ruledef
    ch_edonkey

             p2p
    protocol = edonkey

             exit

           ruledef
    ch_facebook

             p2p
    protocol = facebook

             exit

          ruledef
    ch_gmail

             p2p
    protocol = gmail

             exit

          ruledef
    ch_gtalk

             p2p
    protocol = gtalk

             exit

          ruledef
    ch_mypeople

             p2p
    protocol = mypeople

             exit

          ruledef
    ch_skype

             p2p
    protocol = skype

             exit

          ruledef
    ch_yahoo

             p2p
    protocol = yahoo

             exit

          ruledef
    ch_audio_gtalk

             p2p
    protocol = gtalk

             p2p
    traffic-type = audio

             rule-application
    charging

             exit

          ruledef
    ch_audio_skype

             p2p
    protocol = skype

             p2p
    traffic-type = audio

             rule-application
    charging

             exit

          ruledef
    ch_audio_yahoo

             p2p
    protocol = yahoo

             p2p
    traffic-type = audio

             rule-application
    charging

             exit

          ruledef
    ch_audio

             p2p
    traffic-type = audio

             rule-application
    charging

             exit

          ruledef
    ch_video_gtalk

             p2p
    protocol = gtalk

             p2p
    traffic-type = video

             rule-application
    charging

             exit

          ruledef
    ch_video_yahoo

             p2p
    protocol = yahoo

             p2p
    traffic-type = video

             rule-application
    charging

             exit

          ruledef
    ch_unclassified_gtalk

             p2p
    protocol = gtalk

             p2p
    traffic-type = unclassified

             rule-application
    charging

             exit

          ruledef
    ch_unclassified_skype

             p2p
    protocol = skype

             p2p
    traffic-type = unclassified

             rule-application
    charging

             exit

          ruledef
    ch_unclassified_yahoo

             p2p
    protocol = yahoo

             p2p
    traffic-type = unclassified

             rule-application
    charging

             exit

          ruledef
    rt_dns-tcp

             tcp
    either-port = 53

             rule-application
    routing

             exit

          ruledef
    rt_dns-udp

             udp
    either-port = 53

             rule-application
    routing

             exit

          ruledef
    rt_ftp-control

             tcp
    either-port = 21

             rule-application
    routing

             exit

          ruledef
    rt_ftp-data

             tcp
    either-port = 20

             rule-application
    routing

             exit

          ruledef
    rt_http

             tcp
    either-port = 80

             rule-application
    routing

             exit

          ruledef
    rt_https

             tcp
    either-port = 443

             rule-application
    routing

             exit

          ruledef
    rt_imap

             tcp
    either-port = 143

             rule-application
    routing

             exit

          ruledef
    rt_mms-wapcl-ct

             wsp
    content type = application/vnd.wap.mms-message

             rule-application
    routing

             exit

          ruledef
    rt_mms_http_ct

             http
    content type = application/vnd.wap.mms-message

             rule-application
    routing

             exit

          ruledef
    rt_mms_http_url

             http
    url ends-with .mms

             rule-application
    routing

             exit

          ruledef
    rt_mms_wapcl-url

             wsp
    url ends-with .mms

             rule-application
    routing

             exit

          ruledef
    rt_pop3

             tcp
    either-port = 110

             rule-application
    routing

             exit

          ruledef
    rt_rtsp

             tcp
    either-port = 554

             rule-application
    routing

             exit

          ruledef
    rt_rtsp-8556

             tcp
    either-port = 8556

             rule-application
    routing

             exit

          ruledef
    rt_sdp

             sip
    content type = application/sdp

             rule-application
    routing

             exit

          ruledef
    rt_sip

             udp
    either-port = 5060

             rule-application
    routing

             exit

          ruledef
    rt_smtp

             tcp
    either-port = 25

             rule-application
    routing

             exit

          ruledef
    rt_wap2.0

             tcp
    either-port = 8080

             rule-application
    routing

             exit

          ruledef
    rt_wsp-connection-less

             udp
    either-port = 9200

             rule-application
    routing

             exit

          ruledef
    rt_wsp-connection-oriented

             udp
    either-port = 9201

             ip
    protocol = 51

             ip
    protocol = 50

             ip
    protocol = 47

             ip
    downlink = TRUE

             ip
    uplink = TRUE

             ip
    any-match = TRUE

             tcp
    any-match = TRUE

             udp
    dst-port = 5000

             rule-application
    routing

             exit

          charging-action
    ca_BWC

             flow
    limit-for-bandwidth direction downlink peak-data-rate 4000 peak-burst-size
    1024 violate-action discard committed-data-rate 3200 committed-burst-size
    512 exceed-action discard

             exit

          charging-action
    ca_nothing

             content-id
    1

             exit

          charging-action
    ca_terminate

             flow
    action terminate-flow

             exit

          rulebase
    base_1

             action
    priority 504 ruledef ch_ares charging-action ca_nothing

             action
    priority 507 ruledef ch_bittorrent charging-action ca_nothing

             action
    priority 508 ruledef ch_blackberry charging-action ca_nothing

             action
    priority 515 ruledef ch_edonkey charging-action ca_nothing

             action
    priority 516 ruledef ch_facebook charging-action ca_nothing

             action
    priority 526 ruledef ch_gmail charging-action ca_nothing

             action
    priority 528 ruledef ch_gtalk charging-action ca_nothing

             action
    priority 629 ruledef ch_mypeople charging-action ca_nothing

             action
    priority 578 ruledef ch_skype charging-action ca_nothing

             action
    priority 614 ruledef ch_yahoo charging-action ca_nothing

             action
    priority 618 ruledef ch_audio_gtalk charging-action
    ca_nothing

             action
    priority 620 ruledef ch_audio_skype charging-action
    ca_nothing

             action
    priority 621 ruledef ch_audio_yahoo charging-action
    ca_nothing

             action
    priority 623 ruledef ch_video_gtalk charging-action
    ca_nothing

             action
    priority 624 ruledef ch_video_msn charging-action
    ca_nothing

             action
    priority 626 ruledef ch_video_yahoo charging-action
    ca_nothing

             p2p
    dynamic-flow-detection

             exit

          rulebase
    default

             exit

          exit

       context
    isp

          ip
    access-list list_1

             redirect
    css service service_1 ip any any

             exit

          ip
    pool pool1 9.8.7.6 255.255.255.0 static

          interface
    inet

             ip
    address 8.7.6.5 255.255.255.0

             exit

          subscriber
    default

             exit

          aaa
    group default

             exit

          gtpp
    group default

             exit

          ip
    route 0.0.0.0 0.0.0.0 7.6.5.4 inet

             exit

          exit

       context
    ggsn

          interface
    ggsn-ingress

             ip
    address 6.5.4.3 255.255.255.0

             exit

          subscriber
    default

             exit

          apn
    radius.com

             selection-mode
    sent-by-ms

             accounting-mode
    none

             ip
    access-group list_1 in

             ip
    access-group list_1 out

             ip
    source-violation ignore

             ip
    context-name isp

             active-charging
    rulebase base_1

             exit

          aaa
    group default

             exit

          gtpp
    group default

             exit

          ggsn-service
    ggsn

             retransmission-timeout
    1

             max-retransmission
    1

             gtpu
    udp-checksum insert

             plmn
    unlisted-sgsn home

             bind
    address 5.4.3.2

             exit

          exit

       port
    ethernet 17/1

          medium
    speed 1000 duplex full

          no
    shutdown

          bind
    interface ggsn-ingress ggsn

          exit

       port
    ethernet 20/1

          medium
    speed 1000 duplex full

          no
    shutdown

          bind
    interface inet isp

          exit

       task
    facility sessmgr start aggressive

       task
    facility acsmgr start aggressive

       end