# show hss-peer-service

This chapter includes the show hss-peer-service command output tables.

show hss-peer-service name <name>

Table 1. show hss-peer-service name <name> Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the HSS peer service configured and running on the system.
Context | The name of the VPN context in which HSS peer service configured and running on the system.
Status | Indicates whether the HSS peer service is started or not.
Diameter hss-endpoint | The Diameter endpoint name configured in the HSS peer service configuration mode for the S6a HSS interface.
Diameter eir-endpoint | The Diameter endpoint name configured in the HSS peer service configuration mode for the S13 EIR interface.
Diameter hss-dictionary | The name of Diameter dictionary configured for messaging which is to be used for HSS peer service sessions.
Request timeout | The timeout duration in seconds set for heartbeat checking of Diameter requests with the HSS server.
Request Auth-vectors | The number of authentication vectors the MME requests in an Authentication-Information-Request (AIR) message to the HSS for each UE requiring authentication.
Notify-Req-Msg | Displays if the MME is configured to send Notify-Request-Messages to the HSS. Possible values are Enable and Disable.
Failure-Handling | This group shows the configuration/settings of failure handling actions on various type of Diameter messages for different type of failure.
Message Type | The type of Diameter messages configured for failure handling on specific type of failure or error. The following types of Diameter messages can be configured for failure handling: Authentication-Information-Request Check-Identity-Request Notify-Request Purge-UE-Request Update-Location-Request
Failure Type | The type of message failures to trigger the failure handing actions on specific Diameter messages. The following types of failure can be handled for different types of diameter messages: Diameter Result Code (3000 to 9999) single or a range of code. Request Timeout
Action | The type of action to be taken of a type of failure for specific type of Diameter messages. The following types of action can be configured for different types of diameter message failures: Continue Retry-and-terminate Terminate

show hss-peer-service session full

Table 2. show hss-peer-service session full Command Output Descriptions

Field | Description
--- | ---
HSS
Peer | The HSS peer name.
Mode | The mode of the session.
Callid | The EPS subscriber’s call identity in 8 digit hex number of the connected call to an HSS peer service session.
NAI | The network access identifier (NAI) of MME-HSS session on the HSS peer service.
MDN | The mobile directory number (MDN) of the MME-HSS session on the HSS peer service.
Service Name | The name of HSS peer service for which statistics are displayed.
State | The status of MME-HSS session on the HSS peer service.
Pending Requests | The status of pending request between the MME and the HSS over the S6a interface during this MME-HSS session on the HSS peer service.
API Requests
Open | The number of api sessions opened.
Close | The number of api sessions closed.
Update Locations | The number of ULR messages initiated by the MME or SGSN application.
Purge UE | The number of Purge Request messages initiated by the MME or SGSN application.
Authenticate | The number of AIR messages initiated by the MME or SGSN application.
Notify | The number of Notify Request messages initiated by the MME or SGSN application.
Identity Check | The number of MICR messages initiated by the MME or SGSN application.
Recoveries | The number of api session recoveries initiated.
Micro Checkpoint | Not used.
Full Checkpoint | Note used.
User Data Query | The number of user data requests sent by the MME or SGSN application.
API Successes
Open | The number of api sessions opened successfully.
Close | The number of api sessions closed successfully.
Update Locations | The number of ULR messages successfully sent by the MME or SGSN application.
Purge UE | The number of Purge Request messages successfully sent by the MME or SGSN application.
Authenticate | The number of AIR messages successfully sent by the MME or SGSN application.
Notify | The number of Notify Request messages successfully sent by the MME or SGSN application.
Identity Check | The number of MICR messages successfully sent by the MME or SGSN application.
Recoveries | The number of api sessions recovered successfully.
Micro Checkpoint | Not used.
Full Checkpoint | Not used.
User Data Query | Not used.
API Errors
Open | The number of api sessions which encountered an error when opened.
Close | The number of api sessions which encountered an error when closed.
Update Locations | The number of ULR messages that failed to be sent by the MME or SGSN application.
Purge UE | The number of Purge Request messages that failed to be sent by the MME or SGSN application.
Authenticate | The number of AIR messages that failed to be sent by the MME or SGSN application.
Notify | The number of Notify Request messages that failed to be sent by the MME or SGSN application.
Identity Check | The number of MICR messages that failed to be sent by the MME or SGSN application.
Recoveries | The number of api sessions that failed recovering.
Micro Checkpoint | Not used.
Full Checkpoint | Not used.
User Data Query | The number of user data request that couldn not be processed.
Server Requests
Update Locations | The number of ULR messages created at the session level.
Purge UE | The number of Purge Request messages created at the session level.
Authenticate | The number of AIR messages created at the session level.
Notify | The number of Notify Request messages created at the session level.
Identity Check | The number of MICR messages created at the session level.
User Data Req | Not used.
Server Successes
Update Locations | The number of ULR messages successfully sent.
Purge UE | The number of Purge Request messages successfully sent.
Authenticate | The number of AIR messages successfully sent.
Notify | The number of Notify Request messages successfully sent.
Identity Check | The number of MICR messages successfully sent.
User Data Req | Not used.
Server Errors
Update Locations | The number of ULR messages which could not be sent. The peer is unavailable, down, or the session could not be opened.
Purge UE | The number of Purge Request messages which could not be sent. The peer is unavailable, down, or the session could not be opened.
Authenticate | The number of AIR messages which could not be sent. The peer is unavailable, down, or the session could not be opened.
Notify | The number of Notify Request messages which could not be sent. The peer is unavailable, down, or the session could not be opened.
Identity Check | The number of MICR messages which could not be sent. The peer is unavailable, down, or the session could not be opened.
User Data Req | Not used.

show hss-peer-service statistics all

Table 3. show hss-peer-service statistics all Command Output Descriptions

Field | Description
--- | ---
HSS Statistics for all services
Session Stats
Total Current Sessions | The total number of sessions currently accessing the HSS peer service.
Session Failovers | The total number of session failovers occurring on the SS peer service.
Total Starts | The total number os sessions started on the HSS peer service.
Total Session Updates | The total number of sessions updated on the HSS peer service.
Total Terminated | The total number of sessions that were terminated on the HSS peer service.
Message Stats
UL Request | The total number of Update Location Request messages sent by the HSS peer service to the HSS.
UL Answer | The total number of Update Location Answer messages received by the HSS peer service from the HSS.
ULR Retries | The total number of Update Location Request Retry messages sent by the HSS peer service to the HSS.
ULA Timeouts | The total number of Update Location Answer Timeout messages received by the HSS peer service from the HSS.
ULA Dropped | The total number of Update Location Answer Dropped messages received by the HSS peer service from the HSS.
PU Request | The total number of Purge UE Request messages sent by the HSS peer service to the HSS.
PU Answer | The total number of Purge UE Answer messages received by the HSS peer service from the HSS.
PUR Retries | The total number of Purge UE Request Retry messages sent by the HSS peer service to the HSS.
PUA Timeouts | The total number of Purge UE Answer Timeout messages received by the HSS peer service from the HSS.
PUA Dropped | The total number of Purge UE Answer Dropped messages received by the HSS peer service from the HSS.
AI Request | The total number of Authentication Information Request messages sent by the HSS peer service to the HSS.
AI Answer | The total number of Authentication Information Answer messages received by the HSS peer service from the HSS.
AIR Retries | The total number of Authentication Information Request Retry messages sent by the HSS peer service to the HSS.
AIA Timeouts | The total number of Authentication Information Answer Timeout messages received by the HSS peer service from the HSS.
AIA Dropped | The total number of Authentication Information Answer Dropped messages received by the HSS peer service from the HSS.
CL Request | The total number of Cancel Location Request messages sent by the HSS peer service to the HSS.
CL Answer | The total number of Cancel Location Answer messages received by the HSS peer service from the HSS.
CLR Retries | The total number of Cancel Location Request Retry messages sent by the HSS peer service to the HSS.
CLA Timeouts | The total number of Cancel Location Answer Timeout messages received by the HSS peer service from the HSS.
CLA Dropped | The total number of Cancel Location Answer Dropped messages received by the HSS peer service from the HSS.
ISD Request | The total number of Insert Subscriber Data Request messages received by the HSS peer service from the HSS.
ISD Answer | The total number of Insert Subscriber Data Answer messages sent by the HSS peer service to the HSS.
ISDR Retries | The total number of Insert Subscriber Data Request Retry messages received by the HSS peer service from the HSS.
ISDA Timeouts | The total number of Insert Subscriber Data Answer Timeout messages sent by the HSS peer service to the HSS.
ISDA Dropped | The total number of Insert Subscriber Data Answer Dropped messages sent by the HSS peer service to the HSS.
DSD Request | The total number of Delete Subscriber Data Request messages received by the HSS peer service from the HSS.
DSD Answer | The total number of Delete Subscriber Data Answer messages sent by the HSS peer service to the HSS.
DSDR Retries | The total number of Delete Subscriber Data Request Retry messages received by the HSS peer service from the HSS.
DSDA Timeouts | The total number of Delete Subscriber Data Answer Timeout messages sent by the HSS peer service to the HSS.
DSDA Dropped | The total number of Delete Subscriber Data Answer Dropped messages sent by the HSS peer service to the HSS.
R Request | The total number of Reset Request messages received by the HSS peer service from the HSS.
R Answer | The total number of Reset Answer messages sent by the HSS peer service to the HSS.
RR Retries | The total number of Reset Request Retry messages received by the HSS peer service from the HSS.
RA Timeouts | The total number of Reset Answer Timeout messages sent by the HSS peer service to the HSS.
RA Dropped | The total number of Reset Answer Dropped messages sent by the HSS peer service to the HSS.
N Request | The total number of Notify Request messages sent by the HSS peer service to the HSS.
N Answer | The total number of Notify Answer messages received by the HSS peer service from the HSS.
NR Retries | The total number of Notify Request Retry messages sent by the HSS peer service to the HSS.
NA Timeouts | The total number of Notify Answer Timeout messages received by the HSS peer service from the HSS.
NA Dropped | The total number of Notify Answer Dropped messages received by the HSS peer service from the HSS.
MIC Request | The total number of Mobile Identity Check Request messages sent by the HSS peer service to the HSS.
MIC Answer | The total number of Mobile Identity Check Answer messages received by the HSS peer service from the HSS.
MICR Retries | The total number of Mobile Identity Check Request Retry messages sent by the HSS peer service to the HSS.
MICA Timeouts | The total number of Mobile Identity Check Answer Timeout messages received by the HSS peer service from the HSS.
MICA Dropped | The total number of Mobile Identity Check Answer Dropped messages received by the HSS peer service to the HSS.
Message Error Stats
Unable To Comply | The total number of Update Location Answer messages containing the result code “Unable To Comply” received by the HSS peer service from the HSS.
Auth Data Unavailable | The total number of Update Location Answer messages containing the result code “Auth Data Unavailable” received by the HSS peer service from the HSS.
User Unknown | The total number of Update Location Answer messages containing the result code “User Unknown” received by the HSS peer service from the HSS.
Equipment Unknown | The total number of Update Location Answer messages containing the result code “Equipment Unknown” received by the HSS peer service from the HSS.
Unknown EPS Subscription | The total number of Update Location Answer messages containing the result code “Unknown EPS Subscription” received by the HSS peer service from the HSS.
RAT Not Allowed | The total number of Update Location Answer messages containing the result code “RAT Not Allowed” received by the HSS peer service from the HSS.
Authorization Rejected | The total number of Update Location Answer messages containing the result code “Authorization Rejected” received by the HSS peer service from the HSS.
Roaming Not Allowed | The total number of Update Location Answer messages containing the result code “Roaming Not Allowed” received by the HSS peer service from the HSS.
Other Errors | The total number of Update Location Answer messages containing the result code “Other Errors” received by the HSS peer service from the HSS.