# show nw-reachability server all

Table 1. show nw-reachability server Command Output Descriptions

Field | Description
--- | ---
Server | The name that was configured for this server in the current context.
remote-addr | The IP address to which ping packets are sent in order to determine network reachability.
local-addr | The IP address that is used as the source address of ping packets sent to the reachability server.
state | The state of the network reachability server. Either Up or Down. Up: The server is responding to ping packets. Down: The server is not responding to ping packets.
Total Network Reachability Servers: | The total number of network reachability servers that are configured in the current context.
Up: | The number of network reachability servers that are responding.