# show apn-profile

This chapter describes the output of the show apn-profile command.

show apn-profile full name

Table 1. show apn-profile full name Command Output Descriptions

Field | Description
--- | ---
APN Profile Name | Indicates the name of the Access Point Name (APN) profile.
Resolution Priority | Indicates the address-resolution-mode configured for this APN Profile. Possible values are dns-fallback and local.
Charging Characteristics Prefer Local | Indicates whether the APN profile prefers the charging characteristics settings from the APN profile instead of the charging characteristics received from the HLR.
Charging Characteristics Behavior | Indicates the behavior bit in charging characteristics provided by the APN profile when the HLR does not provide a value.
Charging Characteristics Profile-Index | Indicates the charging characteristics profile index specified by the APN profile, such as 4 for prepaid billing or 8 for normal billing.
3gpp qos to dscp Uplink mapping This group displays 3GPP QoS to Differentiated Services Code Point (DSCP) uplink mapping information.
conversational | Indicates the DSCP configured for conversational type of traffic.
streaming | Indicates the DSCP configured for streaming type of traffic.
interactive (TP 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1.
interactive (TP 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2.
interactive (TP 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3.
3gpp qos to dscp Uplink mapping based on Allocation Priority This group displays 3GPP QoS to Differentiated Services Code Point (DSCP) uplink mapping information based on allocation priority.
interactive (TP 1, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 1.
interactive (TP 1, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 2.
interactive (TP 1, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 3.
interactive (TP 2, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 1.
interactive (TP 2, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 2.
interactive (TP 2, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 3.
interactive (TP 3, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 1.
interactive (TP 3, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 2.
interactive (TP 3, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 3.
3gpp qos to Downlink mapping This group displays 3GPP QoS to Differentiated Services Code Point (DSCP) downlink mapping information.
conversational | Indicates the DSCP configured for conversational type of traffic.
streaming | Indicates the DSCP configured for streaming type of traffic.
interactive (TP 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1.
interactive (TP 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2.
interactive (TP 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3.
3gpp qos to dscp Downlink mapping based on Allocation Priority This group displays 3GPP QoS to Differentiated Services Code Point (DSCP) downlink mapping information based on allocation priority.
interactive (TP 1, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 1.
interactive (TP 1, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 2.
interactive (TP 1, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 3.
interactive (TP 2, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 1.
interactive (TP 2, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 2.
interactive (TP 2, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 3.
interactive (TP 3, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 1.
interactive (TP 3, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 2.
interactive (TP 3, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 3.
IP Source Validation | Indicates whether check for IP source validation violations is enabled.
Direct Tunnel | Indicates if the SGSN allows direct tunneling if the direct tunneling is supported by destination node.
Service Restriction for Access Type > UMTS | Indicates if the SGSN is configured to restrict the PDP context activation from Universal Mobile Telecommunications Systems (3G) network access.
Inactivity Idle timeout in seconds | Indicates the PDP inactivity timeout value in seconds.
Inactivity Idle timeout action | Indicates the action to be taken when the PDP inactivity timeout value is reached.
Inactivity Idle timeout action condition | Indicates the condition that warrants a PDP detach when PDP inactivity timeout value is reached.
Allocation OR Retention Priority | Indicates the QoS Allocation/Retention Priority.
Traffic Policing
Traffic Policing Uplink | Indicates if traffic policing is configured for uplink traffic.
Traffic Policing Downlink | Indicates if traffic policing is configured for downlink traffic.
Idle Mode ACL (SGW)
IPv4 ACL | Indicates the configuration of access control lists (ACLs) that define rules to apply to downlink data destined for UEs in an idle mode - IPv4.
IPv6 ACL | Indicates the configuration of access control lists (ACLs) that define rules to apply to downlink data destined for UEs in an idle mode - IPv6.
DNS Extension with MSISDN | Indicates whether the SGSN is configured to append an offset group of digits from the MSISDN to the APN string that is being sent in the DNS query.
DNS Extension with LAC-RAC | Indicates whether the SGSN is configured to append geographical information to the APN string that is being sent in the DNS query.
DNS Extension with RNC-ID | Indicates whether the SGSN is configured to include the ID of the calling RNC in the APN string that is being sent in the DNS query.
DNS Extension with Charging Characteristics | Indicates whether the SGSN is configured to include the profile index value of the charging characteristics in the APN string that is being sent in the DNS query.
SNAPTR DNS Query for APN Resolution | Indicates whether the SGSN is configured to send Straightforward Name Authority Pointer (SNAPTR) type DNS query for APN resolution.
P-GW
IP-Address | Indicates the IP address of the P-GW supporting APNs associated with this APN profile.
S5-S8-Protocol | Indicates the S5-S8 protocol configured for the this P-GW.
Weight | Indicates the weight assigned to this P-GW for load balancing purposes.
QOS APN-AMBR
MAX uplink | Indicates the aggregate maximum bit rate (AMBR) for uplink (subscriber to network) traffic.
MAX downlink | Indicates the aggregate maximum bit rate (AMBR) for downlink (network to subscriber) traffic.
QOS Default BRR MBR
QCI | Indicates the QoS Class Identifier (QCI) for the default bearer.
ARP | Indicates the QoS address retention priority (ARP) value for the default bearer.
Preemption-Capability | Indicates the configuration of the QoS preemption capability flag for the default bearer.
Preemption-Vulnerability | Indicates the configuration of the QoS vulnerability capability flag for the default bearer.