# show lte-policy

This chapter describes the output of the show apn-remap-table command.

show lte-policy congestion-action-profile name

Table 1. show lte-policy congestion-action-profile name Command Output Descriptions

Field | Description
--- | ---
handovers | Indicates the action the MME is configured to take for handovers when a congestion control threshold is reached. Possible actions are none (ignore), reject, drop.
combined-attaches | Indicates the action the MME is configured to take for combined Attach requests when a congestion control threshold is reached. Possible actions are none (ignore), reject, drop.
ps-attaches | Indicates the action the MME is configured to take for packet switched Attach requests when a congestion control threshold is reached. Possible actions are none (ignore), reject, drop.
addn-pdn-connects | Indicates the action the MME is configured to take for additional PDN context connections when a congestion control threshold is reached. Possible actions are none (ignore), reject, drop.
addn-brr-requests | Indicates the action the MME is configured to take for additional bearer requests when a congestion control threshold is reached. Possible actions are none (ignore), reject, drop.
service-request | Indicates that the Default APN should be used if the DNS query fails.
tau-request | Indicates the dummy APN to be used when the default APN is not present in the subscription.
s1-setups time to wait | Indicates whether to use the APN from the first subscription record when the configured default APN is not available.
exclude-emergency-events | Indicates whether the MME is configured to exclude emergency calls when a congestion control threshold is reached. This setting is disabled when ‘no exclude-emergency-events’ is displayed.
exclude-voice-events | Indicates whether the MME is configured to exclude voice calls when a congestion control threshold is reached. This setting is disabled when ‘no exclude-voice-events’ is displayed.

show lte-policy ho-restrict-list name

Table 2. show lte-policy ho-restrict-list name Command Output Descriptions

Field | Description
--- | ---
forbidden tracking areas | Lists the PLMN IDs which are part of the handover restriction list.
forbidden location areas | Lists the PLMN IDs which are part of the handover restriction list.

show lte-policy lte-emergency-profile name

Table 3. show lte-policy lte-emergency-profile name Command Output Descriptions

Field | Description
--- | ---
ue-validation-level | Indicates the type of UE that can use the emergency bearer service through this profile.
apn | Indicates the name and PDN type of the access point name (APN) used for emergency PDN connections.
qos | Indicates the quality of service (QoS) settings for this emergency bearer service.
ambr | Indicates the maximum aggregated uplink and downlink bitrate values for this profile.
FQDN PGW | Indicates the Fully Qualified Domain Name of the P-GW to be used for emergency bearer services through this profile.
STATIC PGW | Indicates the static IP address, protocol, and weight of the P-GW to be used for emergency bearer services through this profile.

show lte-policy paging-map name

Table 4. show lte-policy paging-map name Command Output Descriptions

Field | Description
--- | ---
Paging Map n
Precedence | Indicates the order in which the MME checks the entries for this paging-map.
Traffic Type | Indicates the traffic type (either CS or PS) that is specified for this paging-map.
Paging profile | Indicates the paging-profile to be used for this traffic type.

show lte-policy paging-profile name

Table 5. show lte-policy paging-profile name Command Output Descriptions

Field | Description
--- | ---
Paging Profile n
Paging Stage n: Lists all Paging Stages configured for this Paging Profile.
Paging Action | Indicates how the paging request should be formed. Possible options are: all-enb-all-tai all-enb-last-tai last-n-enb-last-tai
Match Criteria | Indicates the criteria for selecting a given paging stage. Possible options are: ue-contact-time all
T3413-Timeout | Indicates the time interval in seconds between paging requests.
Max Paging Retries | Indicates the number of paging requests to be sent out during this paging stage.

show lte-policy tai-mgmt-db name

Table 6. show lte-policy tai-mgmt-db name Command Output Descriptions

Field | Description
--- | ---
TAI Management DB n
Time Zone | Indicates the time zone settings to be used for the UE timezone in S11 and NAS messages.
Short Network Name | Indicates the short network name to be used in the Short network name IE in the EMM Information message sent by the MME.
Long Network Name | Indicates the full (long) network name to be used in the Long network name IE in the EMM Information message sent by the MME.
TAI Management Object | Lists all Tracking Area Identifier objects configured in this TAI Management Database.