# show asnpc-service

This chapter includes the show asnpc-service command output tables.
show asnpc-service all
Table 1. show asnpc-service all Command Output Descriptions

Field | Description
--- | ---
Service name | The ASN GW service name.
Context | The context in which the service is configured.
Anchor PC ID | The anchor paging controller identifier.
Bind | The bind status.
Max Subscribers | The maximum number of subscribers.
IP address | IP address of ASN GW server where this service is located.
UDP Port | The UDP port number.
Service Status | Status of this service.
Maximum number of retransmissions | The maximum number of retransmissions.
Maximum number of paging-announce retransmissions | The maximum number of paging-announce retransmissions.
Retransmission timeout | The retransmission timeout duration.
Setup timeout | The session setup timeout duration.
Active-relay timeout | Indicates the timeout duration for active relay of R4 or R6 messages.
Paging-announce timeout | Indicates the paging announce timeout duration in seconds.
Paging-announce retransmission timeout | Indicates the paging announce retransmission timeout duration in seconds.
Policy transaction-id-validation | Possible values are: ALLOW: Enforce tid validation procedure as per NWG specification, section 3.1. DISALLOW: Do not enforce tid validation procedure as per NWG specification, section 3.1.
Policy zero-function-type | Possible values are: ALLOW: If configured, function type is not considered for transaction id generation/validation. DISALLOW: If configured, function type is considered for transaction id generation/validation.
Transaction Id. Seed | If configured, initial value of tid is set to this configured value, otherwise, initial value of tid is set to a random number.
Peer ASNGW address | The list of ASN GW IP addresses with which the PCLR is permitted to interact.
Number of Paging Groups configured | The total number of paging groups configured for this service.
Paging Group | The paging group ID associated with this service.
Paging Offset | The offsets configured for the Paging Group.
Number of MSIDs | The current total number of MNs assigned/using the offset.

show asnpc-service session all
Table 2. show asnpc-service session all Command Output Descriptions

Field | Description
--- | ---
CALLID | The subscriber’s call identification number.
MSID | The subscriber’s Mobile Station Identification number.
BS/PA Address | IP address of the base-station or paging agent.
Session Type | Indicates the type of ASN PC session. Possible type of sessions are: Anchor Non-anchor
Total ASNPC Sessions | The total number of ASN PC sessions on chassis including all modes.

show asnpc-service session full
Table 3. show asnpc-service session all Command Output Descriptions

Field | Description
--- | ---
Username | The subscriber’s user name.
Callid | The subscriber’s call identification number.
MSID | The subscriber’s Mobile Station Identification number.
ASNPC Service Address | IP address of system where ASN PC service is running.
BS/PA Address | IP address of the base-station or paging agent.
BS ID | The identifier of base station. Generally it is MAC address of the BS.
Authenticator Address | IP address of the authenticator ASN GW.
DPF/ASNGW Address | IP address of the system where data path function/ASN GW service is running.
Idle-mode timeout | Indicates the total configured timeout duration in seconds for an MS to enter the idle mode from active mode.
Remaining Idle Mode Timeout | Indicates the remaining timeout duration in seconds for an MS to enter the idle mode from active mode.
Paging Information
Paging Cycle | Indicates the number of paging cycles happened in this ASN PC service session.
Paging Offset | Indicates the paging offset for paging announce.
Paging Group ID | Indicates the paging group identifier which contains the group of paging agents bounded with this paging controller session.
Paging Interval | Interval time in seconds between two paging announces.
MS Information
Idle Mode Authorization Indication | Indicates the idle mode authorization status.
SA Descriptor Information | Indicates the Security Association description information. SA descriptor is a compound attribute whose sub-attributes describe the properties of a Security Association (SA). These properties include the SA ID, the SA type, the SA service type, and the cryptographic suite employed within the SA.
SA ID | Indicates the identifier for the security association.
SA Type | Indicates the types of security association. Possible values are:
Cryptographic Suite | Indicates the cryptographic suite employed within the security association. Possible values are: 0: Primary SA 1: Static SA 3: Dynamic SA 4. Group SA 5: MBS SA
SA Service Type | Indicates the service types of the corresponding SA type. Possible values are: 0: Unicast service 1: Group multicast service 2: MBS service Note that this shall be defined only when SA type is Static SA or Dynamic SA.
SA Index | Indicates the index of security association.
Older/Newer TEK Parameters | Indicates the older or newer Traffic Encryption Key (TEK) parameters involved.
TEK TLV (in hex) | Indicates the TEK total length value in hexadecimal.
TEK Sequence Number | Indicates the TEK sequence number.
TEK Lifetime | Indicates the TEK lifetime in seconds.
PN Counter | Indicates the packet number counter in downlink direction that are used for encryption and decryption by the Base Station.
RxPN Counter | Indicates the packet number counter in uplink direction that are used for encryption and decryption by the Base Station.
Total ASNPC Sessions | The total number of ASN PC sessions on chassis including all modes.

show asnpc-service session counters verbose
Table 4. show asnpc-service session counters verbose Command Output Descriptions

Field | Description
--- | ---
Username | The subscriber’s user name.
Callid | The subscriber’s call identification number.
MSID | The subscriber’s Mobile Station Identification number.
Message Groups
R6 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R6 interface.
R6 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R6 interface.
R6 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R6 interface.
R6 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R6 interface.
R6 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R6 interface.
R6 Location Update Request Msg | Groups the statistics of the Location Update Request messages on R6 interface.
R6 Location Update Response Msg | Groups the statistics of the Location Update Response messages on R6 interface.
R6 Location Update Confirm Msg | Groups the statistics of the Location Update Confirm messages on R6 interface.
R6 Paging Announce Msg | Groups the statistics of the Paging Announce messages on R6 interface.
R4 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R4 interface.
R4 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R4 interface.
R4 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R4 interface.
R4 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R4 interface.
R4 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R4 interface.
R4 Network Exit MS State Change Request Msg | Groups the statistics of the Network Exit MS State Change Request messages on R4 interface.
R4 Network Exit MS State Change Response Msg | Groups the statistics of the Network Exit MS State Change Response messages on R4 interface.
R4 Delete MS Entry Request Msg | Groups the statistics of the Delete MS Entry Request messages on R4 interface.
R4 Delete MS Entry Response Msg | Groups the statistics of the Delete MS Entry Response messages on R4 interface.
R4 Initiate Paging Request Msg | Groups the statistics of the Initiate Paging Request messages on R4 interface.
R4 Initiate Paging Response Msg | Groups the statistics of the Initiate Paging Response messages on R4 interface.
R4 Anchor PC Ind Msg | Groups the statistics of the Anchor Paging Controller Indicator messages on R4 interface.
R4 Anchor PC Ack Msg | Groups the statistics of the Anchor Paging Controller Ack messages on R4 interface.
R4 Context Request Msg | Groups the statistics of the Context Request messages on R4 interface.
R4 Context Report Msg | Groups the statistics of the Context Report messages on R4 interface.
R6/R4 Unknown Messages | Groups the statistics of the Unknown type of messages on R6 and/or R4 interface.
Message Statistics
Total Sent | The total number of this type of message sent on specific interface.
Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
Retransmissions Sent | The total number of this type of message re-transmitted on specific interface.
Total Received | The total number of this type of message received on specific interface.
Total Accepted | The total number of this type of message accepted on specific interface.
Total Relayed | The total number of this type of message relayed on specific interface.
Total Denied | The total number of this type of message denied on specific interface.
Total Discarded | The total number of this type of message discarded on specific interface.
Badly Formed | The total number of badly formed this type of message on specific interface.
Decode Error | The total number of this type of message on specific interface with decode error.
Unspecified Error | The total number of this type of message on specific interface with unspecified error.
Paging Config Error | The total number of this type of errors messages on specified interface occurred. This error occurs when paging node id (BS id) is not configured in configured paging groups.
Missing Mandatory TLV | The total number of this type of message on specific interface with missing mandatory TLVs.
TLV Value Invalid | The total number of this type of message on specific interface with invalid TLV value.
Unknown TLV | The total number of this type of message on specific interface with unknown TLVs.
Duplicate TLV Found | The total number of this type of message on specific interface with duplicate TLVs.
No session Found | The total number of this type of message on specific interface without any session information.
Transaction Id. Error | The total number of this type of message on specific interface. with transaction id error.
Data messages
GRE R6 Receive | The total number of data message received with through GRE tunnel on R6 interface.
GRE R4 Receive | The total number of data message received through GRE tunnel on R4 interface.
Packets Received | The total number of data packets received/sent through GRE tunnel on R4/R6 interface.
Bytes Received | The total number of data bytes received/sent through GRE tunnel on R4/R6 interface.
Protocol Type Error | The total number of data message received/sent with protocol type error through GRE tunnel on R4/R6 interface.
GRE Key Absent | The total number of data message received/sent without GRE key through GRE tunnel on R4/R6 interface.
GRE Checksum Error | The total number of data message received/sent with checksum error through GRE tunnel on R4/R6 interface.
Invalid Packet Length | The total number of data message received/sent with invalid packet length through GRE tunnel on R4/R6 interface.
No Session found | The total number of data message received/sent without any session information through GRE tunnel on R4/R6 interface.
Unspecified Error | The total number of data message received/sent with unknown error through GRE tunnel on R4/R6 interface.
GRE R6 Send | The total number of data message sent through GRE tunnel on R6 interface.
GRE R4 Send | The total number of data message sent through GRE tunnel on R4 interface.
Packets Sent | The total number of data packets sent through GRE tunnel on R4/R6 interface.
Send Error | The total number of data message sent with error through GRE tunnel on R4/R6 interface.
Bytes Sent | The total number of data bytes sent through GRE tunnel on R4/R6 interface.

show asnpc-service statistics verbose
Table 5. show asnpc-service statistics verbose Command Output Descriptions

Field | Description
--- | ---
Message Groups
R6 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R6 interface.
R6 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R6 interface.
R6 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R6 interface.
R6 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R6 interface.
R6 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R6 interface.
R6 Location Update Request Msg | Groups the statistics of the Location Update Request messages on R6 interface.
R6 Location Update Response Msg | Groups the statistics of the Location Update Response messages on R6 interface.
R6 Location Update Confirm Msg | Groups the statistics of the Location Update Confirm messages on R6 interface.
R6 Paging Announce Msg | Groups the statistics of the Paging Announce messages on R6 interface.
R4 Idle Mode Entry MS State Change Request Msg | Groups the statistics of the Idle Mode Entry MS State Change Request messages on R4 interface.
R4 Idle Mode Entry MS State Change Response Msg | Groups the statistics of the Idle Mode Entry MS State Change Response messages on R4 interface.
R4 Idle Mode Entry MS State Change Ack Msg | Groups the statistics of the Idle Mode Entry MS State Change Ack messages on R4 interface.
R4 Idle Mode Exit MS State Change Request Msg | Groups the statistics of the Idle Mode Exit MS State Change Request messages on R4 interface.
R4 Idle Mode Exit MS State Change Response Msg | Groups the statistics of the Idle Mode Exit MS State Change Response messages on R4 interface.
R4 Initiate Paging Request Msg | Groups the statistics of the Initiate Paging Request messages on R4 interface.
R4 Initiate Paging Response Msg | Groups the statistics of the Initiate Paging Response messages on R4 interface.
R4 Location Update Request Msg | Groups the statistics of the Location Update Request messages on R4 interface.
R4 Location Update Response Msg | Groups the statistics of the Location Update Response messages on R4 interface.
R4 Location Update Confirm Msg | Groups the statistics of the Location Update Confirm messages on R4 interface.
R4 Network Exit MS State Change Request Msg | Groups the statistics of the Network Exit MS State Change Request messages on R4 interface.
R4 Network Exit MS State Change Response Msg | Groups the statistics of the Network Exit MS State Change Response messages on R4 interface.
R4 Delete MS Entry Request Msg | Groups the statistics of the Delete MS Entry Request messages on R4 interface.
R4 Delete MS Entry Response Msg | Groups the statistics of the Delete MS Entry Response messages on R4 interface.
R4 Anchor PC Ind Msg | Groups the statistics of the Anchor Paging Controller Indicator messages on R4 interface.
R4 Anchor PC Ack Msg | Groups the statistics of the Anchor Paging Controller Ack messages on R4 interface.
R4 PC Relocation Ind Msg | Groups the statistics of the PC Relocation Ind messages on the R4 interface.
R4 PC Relocation Ack Msg | Groups the statistics of the PC Relocation Ack messages on the R4 interface.
R4 Context Request Msg | Groups the statistics of the Context Request messages on R4 interface.
R4 Context Report Msg | Groups the statistics of the Context Report messages on R4 interface.
R4 CMAC Key Count Update Msg | Groups the statistics of the CMAC Key Count Update messages on the R4 interface.
R4 CMAC Key Count Ack Msg | Groups the statistics of the CMAC Key Count Ack messages on the R4 interface.
R6/R4 Unknown Messages | Groups the statistics of the Unknown type of messages on R6 and/or R4 interface.
Message Statistics
Total Sent | The total number of this type of message sent on specific interface.
Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
Retransmissions Sent | The total number of this type of message re-transmitted on specific interface.
Total Received | The total number of this type of message received on specific interface.
Total Accepted | The total number of this type of message accepted on specific interface.
Total Relayed | The total number of this type of message relayed on specific interface.
Total Denied | The total number of this type of message denied on specific interface.
Total Discarded | The total number of this type of message discarded on specific interface.
Badly Formed | The total number of badly formed this type of message on specific interface.
Decode Error | The total number of this type of message on specific interface with decode error.
Unspecified Error | The total number of this type of message on specific interface with unspecified error.
Missing Mandatory TLV | The total number of this type of message on specific interface with missing mandatory TLVs.
TLV Value Invalid | The total number of this type of message on specific interface with invalid TLV value.
Unknown TLV | The total number of this type of message on specific interface with unknown TLVs.
Duplicate TLV Found | The total number of this type of message on specific interface with duplicate TLVs.
No session Found | The total number of this type of message on specific interface without any session information.
Transaction Id. Error | The total number of this type of message on specific interface. with transaction id error.