# ASNGW Schema Statistics

The ASNGW schema provides operational statistics that can be used for monitoring and troubleshooting the following products: ASNGW
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables ASN-GW Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the ASN GW service. This is a key variable. | String
vpnid | The identification number of the context configured on the system that is currently facilitating the ASN GW service. This is an internal reference number. This is a key variable. | Int32
servname | The name of the ASN GW service for which the statistics are displayed. This is a key variable. | String
servid | The identification number of the ASN GW service for which the statistics are displayed. This is a key variable. | Int32
peeripaddr | IP address of the peer ASN GW. | String
r6mspreattreq-totsent | The total number of MS pre-attachment request messages sent on the R6 interface. | Int32
r6mspreattreq-retranssent | The total number of MS pre-attachment request messages re-transmitted on the R6 interface. | Int32
r6mspreattreq-totsendfail | The total number of failures occurred during transaction ID generation and R6 MS Pre-attachment request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6mspreattreq-totrec | The total number of MS pre-attachment request messages received on the R6 interface. | Int32
r6mspreattreq-totacc | The total number of MS pre-attachment request messages accepted on the R6 interface. | Int32
r6mspreattreq-totrelay | The total number of MS pre-attachment request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a MS pre-attachment request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6mspreattreq-totdenied | The total number of MS pre-attachment request messages denied on the R6 interface. | Int32
r6mspreattreq-totdiscard | The total number of MS pre-attachment request messages discarded on the R6 interface. | Int32
r6mspreattreq-badform | The total number of badly formed MS pre-attachment request messages on the R6 interface. | Int32
r6mspreattreq-decodeerr | The total number of MS pre-attachment request messages on the R6 interface with decode error. | Int32
r6mspreattreq-unspecerr | The total number of MS pre-attachment request messages on the R6 interface with unspecified error. | Int32
r6mspreattreq-missmandtlv | The total number of MS pre-attachment request messages on the R6 interface with missing mandatory TLVs. | Int32
r6mspreattreq-tlvvalinval | The total number of MS pre-attachment request messages on the R6 interface with invalid TLV value. | Int32
r6mspreattreq-unknowntlv | The total number of MS pre-attachment request messages on the R6 interface with unknown TLVs. | Int32
r6mspreattreq-duptlvfound | The total number of MS pre-attachment request messages on the R6 interface with duplicate TLVs. | Int32
r6mspreattreq-nosessfound | The total number of MS pre-attachment request messages on the R6 interface without any session information. | Int32
r6mspreattreq-adminprohib | The total number of MS pre-attachment request messages discarded or denied due to admin prohibit. Triggers: Changes every time a MS pre-attachment request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6mspreattreq-noresourcedrop | The total number of MS pre-attachment request messages discarded or denied due to resource unavailability. Triggers: Changes every time a MS pre-attachment request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6mspreattreq-transiderr | The total number of MS pre-attachment request messages on the R6 interface with transaction ID errors. | Int32
r6mspreattrsp-totsent | The total number of MS pre-attachment response messages sent on the R6 interface. | Int32
r6mspreattrsp-retranssent | The total number of MS pre-attachment response messages re-transmitted on the R6 interface. | Int32
r6mspreattrsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 MS Pre-attachment response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6mspreattrsp-totrec | The total number of MS pre-attachment response messages received on the R6 interface. | Int32
r6mspreattrsp-totacc | The total number of MS pre-attachment response messages accepted on the R6 interface. | Int32
r6mspreattrsp-totrelay | The total number of MS pre-attachment response messages denied on the R6 interface. | Int32
r6mspreattrsp-totdenied | The total number of MS pre-attachment response messages discarded on the R6 interface. | Int32
r6mspreattrsp-totdiscard | The total number of badly formed MS pre-attachment response messages on the R6 interface. | Int32
r6mspreattrsp-badform | The total number of MS pre-attachment response messages on the R6 interface with decode error. | Int32
r6mspreattrsp-decodeerr | The total number of MS pre-attachment response messages on the R6 interface with unspecified error. | Int32
r6mspreattrsp-unspecerr | The total number of MS pre-attachment response messages on the R6 interface with missing mandatory TLVs. | Int32
r6mspreattrsp-missmandtlv | The total number of MS pre-attachment response messages on the R6 interface with invalid TLV value. | Int32
r6mspreattrsp-tlvvalinval | The total number of MS pre-attachment response messages denied on the R6 interface. | Int32
r6mspreattrsp-unknowntlv | The total number of MS pre-attachment response messages on the R6 interface with unknown TLVs. | Int32
r6mspreattrsp-duptlvfound | The total number of MS pre-attachment response messages on the R6 interface with duplicate TLVs. | Int32
r6mspreattrsp-nosessfound | The total number of MS pre-attachment response messages on the R6 interface without any session information. | Int32
r6mspreattrsp-adminprohib | The total number of MS pre-attachment response messages discarded or denied due to admin prohibit. Triggers: Changes every time a MS pre-attachment response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6mspreattrsp-noresourcedrop | The total number of MS pre-attachment response messages discarded or denied due to resource unavailability. Triggers: Changes every time a MS pre-attachment response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6mspreattrsp-transiderr | The total number of MS pre-attachment response messages on the R6 interface with transaction ID errors. | Int32
r6mspreattack-totsent | The total number of MS pre-attachment acknowledgement messages sent on the R6 interface. | Int32
r6mspreattack-retranssent | The total number of MS pre-attachment acknowledgement messages re-transmitted on the R6 interface. | Int32
r6mspreattack-totsendfail | The total number of failures occurred during transaction ID generation and R6 MS Pre-attachment acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6mspreattack-totrec | The total number of MS pre-attachment acknowledgement messages received on the R6 interface. | Int32
r6mspreattack-totacc | The total number of MS pre-attachment acknowledgement messages accepted on the R6 interface. | Int32
r6mspreattack-totrelay | The total number of MS pre-attachment acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a MS pre-attachment acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6mspreattack-totdenied | The total number of MS pre-attachment acknowledgement messages denied on the R6 interface. | Int32
r6mspreattack-totdiscard | The total number of MS pre-attachment acknowledgement messages discarded on the R6 interface. | Int32
r6mspreattack-badform | The total number of badly formed MS pre-attachment acknowledgement messages on the R6 interface. | Int32
r6mspreattack-decodeerr | The total number of MS pre-attachment acknowledgement messages on the R6 interface with decode error. | Int32
r6mspreattack-unspecerr | The total number of MS pre-attachment acknowledgement messages on the R6 interface with unspecified error. | Int32
r6mspreattack-missmandtlv | The total number of MS pre-attachment acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6mspreattack-tlvvalinval | The total number of MS pre-attachment acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6mspreattack-unknowntlv | The total number of MS pre-attachment acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6mspreattack-duptlvfound | The total number of MS pre-attachment acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6mspreattack-nosessfound | The total number of MS pre-attachment acknowledgement messages on the R6 interface without any session information. | Int32
r6mspreattack-adminprohib | The total number of MS pre-attachment acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a MS pre-attachment acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6mspreattack-noresourcedrop | The total number of MS pre-attachment acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a MS pre-attachment acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6mspreattack-transiderr | The total number of MS pre-attachment acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6nwexitmsstachareq-totsent | The total number of network exit MS state change request messages sent on the R6 the interface. | Int32
r6nwexitmsstachareq-retranssent | The total number of network exit MS state change request messages re-transmitted on the R6 interface. | Int32
r6nwexitmsstachareq-totsendfail | The total number of failures occurred during transaction ID generation and R6 network exit MS state change request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6nwexitmsstachareq-totrec | The total number of network exit MS state change request messages received on the R6 interface. | Int32
r6nwexitmsstachareq-totacc | The total number of network exit MS state change request messages accepted on the R6 interface. | Int32
r6nwexitmsstachareq-totrelay | The total number of network exit MS state change request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a network exit MS state change request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6nwexitmsstachareq-totdenied | The total number of network exit MS state change request messages denied on the R6 interface. | Int32
r6nwexitmsstachareq-totdiscard | The total number of network exit MS state change request messages discarded on the R6 interface. | Int32
r6nwexitmsstachareq-badform | The total number of badly formed network exit MS state change request messages on the R6 interface. | Int32
r6nwexitmsstachareq-decodeerr | The total number of network exit MS state change request messages on the R6 interface with decode error. | Int32
r6nwexitmsstachareq-unspecerr | The total number of network exit MS state change request messages on the R6 interface with unspecified error. | Int32
r6nwexitmsstachareq-missmandtlv | The total number of network exit MS state change request messages on the R6 interface with missing mandatory TLVs. | Int32
r6nwexitmsstachareq-tlvvalinval | The total number of network exit MS state change request messages on the R6 interface with invalid TLV value. | Int32
r6nwexitmsstachareq-unknowntlv | The total number of network exit MS state change request messages on the R6 interface with unknown TLVs. | Int32
r6nwexitmsstachareq-duptlvfound | The total number of network exit MS state change request messages on the R6 interface with duplicate TLVs. | Int32
r6nwexitmsstachareq-nosessfound | The total number of network exit MS state change request messages on the R6 interface without any session information. | Int32
r6nwexitmsstachareq-adminprohib | The total number of network exit MS state change request messages on the R6 interface with transaction ID errors. | Int32
r6nwexitmsstachareq-noresourcedrop | The total number of network exit MS state change request messages discarded or denied due to resource unavailability. Triggers: Changes every time a network exit MS state change request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6nwexitmsstachareq-transiderr | The total number of network exit MS state change request messages discarded or denied due to transaction ID errors. | Int32
r6nwexitmsstacharsp-totsent | The total number of network exit MS state change response messages sent on the R6 interface. | Int32
r6nwexitmsstacharsp-retranssent | The total number of network exit MS state change response messages re-transmitted on the R6 interface. | Int32
r6nwexitmsstacharsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 network exit MS state change response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6nwexitmsstacharsp-totrec | The total number of network exit MS state change response messages received on the R6 interface. | Int32
r6nwexitmsstacharsp-totacc | The total number of network exit MS state change response messages accepted on the R6 interface. | Int32
r6nwexitmsstacharsp-totrelay | The total number of network exit MS state change response messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a network exit MS state change response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6nwexitmsstacharsp-totdenied | The total number of network exit MS state change response messages denied on the R6 interface. | Int32
r6nwexitmsstacharsp-totdiscard | The total number of network exit MS state change response messages discarded on the R6 interface. | Int32
r6nwexitmsstacharsp-badform | The total number of badly formed network exit MS state change response messages on the R6 interface. | Int32
r6nwexitmsstacharsp-decodeerr | The total number of network exit MS state change response messages on the R6 interface with decode error. | Int32
r6nwexitmsstacharsp-unspecerr | The total number of network exit MS state change response messages on the R6 interface with unspecified error. | Int32
r6nwexitmsstacharsp-missmandtlv | The total number of network exit MS state change response messages on the R6 interface with missing mandatory TLVs. | Int32
r6nwexitmsstacharsp-tlvvalinval | The total number of network exit MS state change response messages on the R6 interface with invalid TLV value. | Int32
r6nwexitmsstacharsp-unknowntlv | The total number of network exit MS state change response messages on the R6 interface with unknown TLVs. | Int32
r6nwexitmsstacharsp-duptlvfound | The total number of network exit MS state change response messages on the R6 interface with duplicate TLVs. | Int32
r6nwexitmsstacharsp-nosessfound | The total number of network exit MS state change response messages on the R6 interface without any session information. | Int32
r6nwexitmsstacharsp-adminprohib | The total number of network exit MS state change response messages discarded or denied due to admin prohibit. Triggers: Changes every time a network exit MS state change response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6nwexitmsstacharsp-noresourcedrop | The total number of network exit MS state change response messages discarded or denied due to resource unavailability. Triggers: Changes every time a network exit MS state change response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service. | Int32
r6nwexitmsstacharsp-transiderr | The total number of network exit MS state change response messages on the R6 interface with transaction ID errors. | Int32
r6contextreq-totsent | The total number of context request messages sent on the R6 interface. | Int32
r6contextreq-retranssent | The total number of context request messages re-transmitted on the R6 interface. | Int32
r6contextreq-totsendfail | The total number of failures occurred during transaction ID generation and R6 Context Request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6contextreq-totrec | The total number of context request messages received on the R6 interface. | Int32
r6contextreq-totacc | The total number of context request messages accepted on the R6 interface. | Int32
r6contextreq-totrelay | The total number of context request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a context request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6contextreq-totdenied | The total number of context request messages denied on the R6 interface. | Int32
r6contextreq-totdiscard | The total number of context request messages discarded on the R6 interface. | Int32
r6contextreq-badform | The total number of badly formed context request messages on the R6 interface. | Int32
r6contextreq-decodeerr | The total number of context request messages on the R6 interface with decode error. | Int32
r6contextreq-unspecerr | The total number of context request messages on the R6 interface with unspecified error. | Int32
r6contextreq-missmandtlv | The total number of context request messages on the R6 interface with missing mandatory TLVs. | Int32
r6contextreq-tlvvalinval | The total number of context request messages on the R6 interface with invalid TLV value. | Int32
r6contextreq-unknowntlv | The total number of context request messages on the R6 interface with unknown TLVs. | Int32
r6contextreq-duptlvfound | The total number of context request messages on the R6 interface with duplicate TLVs. | Int32
r6contextreq-nosessfound | The total number of context request messages on the R6 interface without any session information. | Int32
r6contextreq-adminprohib | The total number of context request messages discarded or denied due to admin prohibit. Triggers: Changes every time a context request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6contextreq-noresourcedrop | The total number of context request messages discarded or denied due to resource unavailability. Triggers: Changes every time a context request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service. | Int32
r6contextreq-transiderr | The total number of context request messages on the R6 interface with transaction ID errors. | Int32
r6contextrepo-totsent | The total number of context report messages sent on the R6 interface. | Int32
r6contextrepo-retranssent | The total number of context report messages re-transmitted on the R6 interface. | Int32
r6contextrepo-totsendfail | The total number of failures occurred during transaction ID generation and R6 Context Report message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6contextrepo-totrec | The total number of context report messages received on the R6 interface. | Int32
r6contextrepo-totacc | The total number of context report messages =accepted on the R6 interface. | Int32
r6contextrepo-totrelay | The total number of context report messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a context report message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6contextrepo-totdenied | The total number of context report messages denied on the R6 interface. | Int32
r6contextrepo-totdiscard | The total number of context report messages discarded on the R6 interface. | Int32
r6contextrepo-badform | The total number of badly formed context report messages on the R6 interface. | Int32
r6contextrepo-decodeerr | The total number of context report messages on the R6 interface with decode error. | Int32
r6contextrepo-unspecerr | The total number of context report messages on the R6 interface with unspecified error. | Int32
r6contextrepo-missmandtlv | The total number of context report messages on the R6 interface with missing mandatory TLVs. | Int32
r6contextrepo-tlvvalinval | The total number of context report messages on the R6 interface with invalid TLV value. | Int32
r6contextrepo-unknowntlv | The total number of context report messages on the R6 interface with unknown TLVs. | Int32
r6contextrepo-duptlvfound | The total number of context report messages on the R6 interface with duplicate TLVs. | Int32
r6contextrepo-nosessfound | The total number of context report messages on the R6 interface without any session information. | Int32
r6contextrepo-adminprohib | The total number of context report messages discarded or denied due to admin prohibit. Triggers: Changes every time a context report message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6contextrepo-noresourcedrop | The total number of context report messages discarded or denied due to resource unavailability. Triggers: Changes every time a context report message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6contextrepo-transiderr | The total number of context report messages on the R6 interface with transaction ID errors. | Int32
r6contextack-totsent | The total number of context acknowledgement messages sent on the R6 interface. | Int32
r6contextack-retranssent | The total number of context acknowledgement messages re-transmitted on the R6 interface. | Int32
r6contextack-totsendfail | The total number of failures occurred during transaction ID generation and R6 Context acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6contextack-totrec | The total number of context acknowledgement messages received on the R6 interface. | Int32
r6contextack-totacc | The total number of context acknowledgement messages accepted on the R6 interface. | Int32
r6contextack-totrelay | The total number of context acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a context acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6contextack-totdenied | The total number of context acknowledgement messages denied on the R6 interface. | Int32
r6contextack-totdiscard | The total number of context acknowledgement messages discarded on the R6 interface. | Int32
r6contextack-badform | The total number of badly formed context acknowledgement messages on the R6 interface. | Int32
r6contextack-decodeerr | The total number of context acknowledgement messages on the R6 interface with decode error. | Int32
r6contextack-unspecerr | The total number of context acknowledgement messages on the R6 interface with unspecified error. | Int32
r6contextack-missmandtlv | The total number of context acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6contextack-tlvvalinval | The total number of context acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6contextack-unknowntlv | The total number of context acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6contextack-duptlvfound | The total number of context acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6contextack-nosessfound | The total number of context acknowledgement messages on the R6 interface without any session information. | Int32
r6contextack-adminprohib | The total number of context acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a context acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6contextack-noresourcedrop | The total number of context acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a context acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6contextack-transiderr | The total number of context acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6autheaptra-totsent | The total number of authentication EAP transfer messages sent on the R6 interface. | Int32
r6autheaptra-retranssent | The total number of authentication EAP transfer messages re-transmitted on the R6 interface. | Int32
r6autheaptra-totsendfail | The total number of failures occurred during transaction ID generation and R6 EAP transfer message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6autheaptra-totrec | The total number of authentication EAP transfer messages received on the R6 interface. | Int32
r6autheaptra-totacc | The total number of authentication EAP transfer messages accepted on the R6 interface. | Int32
r6autheaptra-totrelay | The total number of authentication EAP transfer messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an authentication EAP transfer message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6autheaptra-totdenied | The total number of authentication EAP transfer messages denied on the R6 interface. | Int32
r6autheaptra-totdiscard | The total number of authentication EAP transfer messages discarded on the R6 interface. | Int32
r6autheaptra-badform | The total number of badly formed authentication EAP transfer messages on the R6 interface. | Int32
r6autheaptra-decodeerr | The total number of authentication EAP transfer messages on the R6 interface with decode error. | Int32
r6autheaptra-unspecerr | The total number of authentication EAP transfer messages on the R6 interface with unspecified error. | Int32
r6autheaptra-missmandtlv | The total number of authentication EAP transfer messages on the R6 interface with missing mandatory TLVs. | Int32
r6autheaptra-tlvvalinval | The total number of authentication EAP transfer messages on the R6 interface with invalid TLV value. | Int32
r6autheaptra-unknowntlv | The total number of authentication EAP transfer messages on the R6 interface with unknown TLVs. | Int32
r6autheaptra-duptlvfound | The total number of authentication EAP transfer messages on the R6 interface with duplicate TLVs. | Int32
r6autheaptra-nosessfound | The total number of authentication EAP transfer messages on the R6 interface without any session information. | Int32
r6autheaptra-adminprohib | The total number of authentication EAP transfer messages discarded or denied due to admin prohibit. Triggers: Changes every time an authentication EAP transfer message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6autheaptra-noresourcedrop | The total number of authentication EAP transfer messages discarded or denied due to resource unavailability. Triggers: Changes every time an authentication EAP transfer message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6autheaptra-transiderr | The total number of authentication EAP transfer messages on the R6 interface with transaction ID errors. | Int32
r6autheapsta-totrec | The total number of authentication EAP start messages sent on the R6 interface. | Int32
r6autheapsta-totacc | The total number of authentication EAP start messages accepted on the R6 interface. | Int32
r6autheapsta-totrelay | The total number of authentication EAP start messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an authentication EAP start message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6autheapsta-totdenied | The total number of authentication EAP start messages denied on the R6 interface. | Int32
r6autheapsta-totdiscard | The total number of authentication EAP start messages discarded on the R6 interface. | Int32
r6autheapsta-badform | The total number of badly formed authentication EAP start messages on the R6 interface. | Int32
r6autheapsta-decodeerr | The total number of authentication EAP start messages on the R6 interface with decode error. | Int32
r6autheapsta-unspecerr | The total number of authentication EAP start messages on the R6 interface with unspecified error. | Int32
r6autheapsta-missmandtlv | The total number of authentication EAP start messages on the R6 interface with missing mandatory TLVs. | Int32
r6autheapsta-tlvvalinval | The total number of authentication EAP start messages on the R6 interface with invalid TLV value. | Int32
r6autheapsta-unknowntlv | The total number of authentication EAP start messages on the R6 interface with unknown TLVs. | Int32
r6autheapsta-duptlvfound | The total number of authentication EAP start messages on the R6 interface with duplicate TLVs. | Int32
r6autheapsta-nosessfound | The total number of authentication EAP start messages on the R6 interface without any session information. | Int32
r6autheapsta-adminprohib | The total number of authentication EAP start messages discarded or denied due to admin prohibit. Triggers: Changes every time an authentication EAP start message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6autheapsta-noresourcedrop | The total number of authentication EAP start messages discarded or denied due to resource unavailability. Triggers: Changes every time an authentication EAP start message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6autheapsta-transiderr | The total number of authentication EAP start messages on the R6 interface with transaction ID errors. | Int32
r6msattreq-totsent | The total number of MS attachment request messages sent on the R6 interface. | Int32
r6msattreq-retranssent | The total number of MS attachment request messages re-transmitted on the R6 interface. | Int32
r6msattreq-totsendfail | The total number of failures occurred during transaction ID generation and R6 MS Attachment Request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6msattreq-totrec | The total number of MS attachment request messages received on the R6 interface. | Int32
r6msattreq-totacc | The total number of MS attachment request messages accepted on the R6 interface. | Int32
r6msattreq-totrelay | The total number of MS attachment request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an MS attachment request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6msattreq-totdenied | The total number of MS attachment request messages denied on the R6 interface. | Int32
r6msattreq-totdiscard | The total number of MS attachment request messages discarded on the R6 interface. | Int32
r6msattreq-badform | The total number of badly formed MS attachment request messages on the R6 interface. | Int32
r6msattreq-decodeerr | The total number of MS attachment request messages on the R6 interface with decode error. | Int32
r6msattreq-unspecerr | The total number of MS attachment request messages on the R6 interface with unspecified error. | Int32
r6msattreq-missmandtlv | The total number of MS attachment request messages on the R6 interface with missing mandatory TLVs. | Int32
r6msattreq-tlvvalinval | The total number of MS attachment request messages on the R6 interface with invalid TLV value. | Int32
r6msattreq-unknowntlv | The total number of MS attachment request messages on the R6 interface with unknown TLVs. | Int32
r6msattreq-duptlvfound | The total number of MS attachment request messages on the R6 interface with duplicate TLVs. | Int32
r6msattreq-nosessfound | The total number of MS attachment request messages on the R6 interface without any session information. | Int32
r6msattreq-adminprohib | The total number of MS attachment request messages discarded or denied due to admin prohibit. Triggers: Changes every time an MS attachment request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6msattreq-noresourcedrop | The total number of MS attachment request messages discarded or denied due to resource unavailability. Triggers: Changes every time an MS attachment request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6msattreq-transiderr | The total number of MS attachment request messages on the R6 interface with transaction ID errors. | Int32
r6msattrsp-totsent | The total number of MS attachment response messages sent on the R6 interface. | Int32
r6msattrsp-retranssent | The total number of MS attachment response messages re-transmitted on the R6 interface. | Int32
r6msattrsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 MS Attachment Response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6msattrsp-totrec | The total number of MS attachment response messages received on the R6 interface. | Int32
r6msattrsp-totacc | The total number of MS attachment response messages accepted on the R6 interface. | Int32
r6msattrsp-totrelay | The total number of MS attachment response messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an MS attachment response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6msattrsp-totdenied | The total number of MS attachment response messages denied on the R6 interface. | Int32
r6msattrsp-totdiscard | The total number of MS attachment response messages discarded on the R6 interface. | Int32
r6msattrsp-badform | The total number of badly formed MS attachment response messages on the R6 interface. | Int32
r6msattrsp-decodeerr | The total number of MS attachment response messages on the R6 interface with decode error. | Int32
r6msattrsp-unspecerr | The total number of MS attachment response messages on the R6 interface with unspecified error. | Int32
r6msattrsp-missmandtlv | The total number of MS attachment response messages on the R6 interface with missing mandatory TLVs. | Int32
r6msattrsp-tlvvalinval | The total number of MS attachment response messages on the R6 interface with invalid TLV value. | Int32
r6msattrsp-unknowntlv | The total number of MS attachment response messages on the R6 interface with unknown TLVs. | Int32
r6msattrsp-duptlvfound | The total number of MS attachment response messages on the R6 interface with duplicate TLVs. | Int32
r6msattrsp-nosessfound | The total number of MS attachment response messages on the R6 interface without any session information. | Int32
r6msattrsp-adminprohib | The total number of MS attachment response messages discarded or denied due to admin prohibit. Triggers: Changes every time an MS attachment response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6msattrsp-noresourcedrop | The total number of MS attachment response messages discarded or denied due to resource unavailability. Triggers: Changes every time an MS attachment response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6msattrsp-transiderr | The total number of MS attachment response messages on the R6 interface with transaction ID errors. | Int32
r6msattack-totsent | The total number of MS attachment acknowledgement messages sent on the R6 interface. | Int32
r6msattack-retranssent | The total number of MS attachment acknowledgement messages re-transmitted on the R6 interface. | Int32
r6msattack-totsendfail | The total number of failures occurred during transaction ID generation and R6 MS attachment acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6msattack-totrec | The total number of MS attachment acknowledgement messages received on the R6 interface. | Int32
r6msattack-totacc | The total number of MS attachment acknowledgement messages accepted on the R6 interface. | Int32
r6msattack-totrelay | The total number of MS attachment acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an MS attachment acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6msattack-totdenied | The total number of MS attachment acknowledgement messages denied on the R6 interface. | Int32
r6msattack-totdiscard | The total number of MS attachment acknowledgement messages discarded on the R6 interface. | Int32
r6msattack-badform | The total number of badly formed MS attachment acknowledgement messages on the R6 interface. | Int32
r6msattack-decodeerr | The total number of MS attachment acknowledgement messages on the R6 interface with decode error. | Int32
r6msattack-unspecerr | The total number of MS attachment acknowledgement messages on the R6 interface with unspecified error. | Int32
r6msattack-missmandtlv | The total number of MS attachment acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6msattack-tlvvalinval | The total number of MS attachment acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6msattack-unknowntlv | The total number of MS attachment acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6msattack-duptlvfound | The total number of MS attachment acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6msattack-nosessfound | The total number of MS attachment acknowledgement messages on the R6 interface without any session information. | Int32
r6msattack-adminprohib | The total number of MS attachment acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an MS attachment acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6msattack-noresourcedrop | The total number of MS attachment acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an MS attachment acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6msattack-transiderr | The total number of MS attachment acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6datapathpreregreq-totsent | The total number of data path pre-registration request messages sent on the R6 interface. | Int32
r6datapathpreregreq-retranssent | The total number of data path pre-registration request messages re-transmitted on the R6 interface. | Int32
r6datapathpreregreq-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path pre-registration request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathpreregreq-totrec | The total number of data path pre-registration request messages received on the R6 interface. | Int32
r6datapathpreregreq-totacc | The total number of data path pre-registration request messages accepted on the R6 interface. | Int32
r6datapathpreregreq-totrelay | The total number of data path pre-registration request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path pre-registration request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathpreregreq-totdenied | The total number of data path pre-registration request messages denied on the R6 interface. | Int32
r6datapathpreregreq-totdiscard | The total number of data path pre-registration request messages discarded on the R6 interface. | Int32
r6datapathpreregreq-badform | The total number of badly formed data path pre-registration request messages on the R6 interface. | Int32
r6datapathpreregreq-decodeerr | The total number of data path pre-registration request messages on the R6 interface with decode error. | Int32
r6datapathpreregreq-unspecerr | The total number of data path pre-registration request messages on the R6 interface with unspecified error. | Int32
r6datapathpreregreq-missmandtlv | The total number of data path pre-registration request messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathpreregreq-tlvvalinval | The total number of data path pre-registration request messages on the R6 interface with invalid TLV value. | Int32
r6datapathpreregreq-unknowntlv | The total number of data path pre-registration request messages on the R6 interface with unknown TLVs. | Int32
r6datapathpreregreq-duptlvfound | The total number of data path pre-registration request messages on the R6 interface with duplicate TLVs. | Int32
r6datapathpreregreq-nosessfound | The total number of data path pre-registration request messages on the R6 interface without any session information. | Int32
r6datapathpreregreq-adminprohib | The total number of data path pre-registration request messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path pre-registration request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathpreregreq-noresourcedrop | The total number of data path pre-registration request messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path pre-registration request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathpreregreq-transiderr | The total number of data path pre-registration request messages on the R6 interface with transaction ID errors. | Int32
r6datapathpreregrsp-totsent | The total number of data path pre-registration response messages sent on the R6 interface. | Int32
r6datapathpreregrsp-retranssent | The total number of data path pre-registration response messages re-transmitted on the R6 interface. | Int32
r6datapathpreregrsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path pre-registration response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathpreregrsp-totrec | The total number of data path pre-registration response messages received on the R6 interface. | Int32
r6datapathpreregrsp-totacc | The total number of data path pre-registration response messages accepted on the R6 interface. | Int32
r6datapathpreregrsp-totrelay | The total number of data path pre-registration response messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path pre-registration response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathpreregrsp-totdenied | The total number of data path pre-registration response messages denied on the R6 interface. | Int32
r6datapathpreregrsp-totdiscard | The total number of data path pre-registration response messages discarded on the R6 interface. | Int32
r6datapathpreregrsp-badform | The total number of badly formed data path pre-registration response messages on the R6 interface. | Int32
r6datapathpreregrsp-decodeerr | The total number of data path pre-registration response messages on the R6 interface with decode error. | Int32
r6datapathpreregrsp-unspecerr | The total number of data path pre-registration response messages on the R6 interface with unspecified error. | Int32
r6datapathpreregrsp-missmandtlv | The total number of data path pre-registration response messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathpreregrsp-tlvvalinval | The total number of data path pre-registration response messages on the R6 interface with invalid TLV value. | Int32
r6datapathpreregrsp-unknowntlv | The total number of data path pre-registration response messages on the R6 interface with unknown TLVs. | Int32
r6datapathpreregrsp-duptlvfound | The total number of data path pre-registration response messages on the R6 interface with duplicate TLVs. | Int32
r6datapathpreregrsp-nosessfound | The total number of data path pre-registration response messages on the R6 interface without any session information. | Int32
r6datapathpreregrsp-adminprohib | The total number of data path pre-registration response messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path pre-registration response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathpreregrsp-noresourcedrop | The total number of data path pre-registration response messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path pre-registration response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathpreregrsp-transiderr | The total number of data path pre-registration response messages on the R6 interface with transaction ID errors. | Int32
r6datapathpreregack-totsent | The total number of data path pre-registration acknowledgement messages sent on the R6 interface. | Int32
r6datapathpreregack-retranssent | The total number of data path pre-registration acknowledgement messages re-transmitted on the R6 interface. | Int32
r6datapathpreregack-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path pre-registration acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathpreregack-totrec | The total number of data path pre-registration acknowledgement messages received on the R6 interface. | Int32
r6datapathpreregack-totacc | The total number of data path pre-registration acknowledgement messages accepted on the R6 interface. | Int32
r6datapathpreregack-totrelay | The total number of data path pre-registration acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path pre-registration acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathpreregack-totdenied | The total number of data path pre-registration acknowledgement messages denied on the R6 interface. | Int32
r6datapathpreregack-totdiscard | The total number of data path pre-registration acknowledgement messages discarded on the R6 interface. | Int32
r6datapathpreregack-badform | The total number of badly formed data path pre-registration acknowledgement messages on the R6 interface. | Int32
r6datapathpreregack-decodeerr | The total number of data path pre-registration acknowledgement messages on the R6 interface with decode error. | Int32
r6datapathpreregack-unspecerr | The total number of data path pre-registration acknowledgement messages on the R6 interface with unspecified error. | Int32
r6datapathpreregack-missmandtlv | The total number of data path pre-registration acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathpreregack-tlvvalinval | The total number of data path pre-registration acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6datapathpreregack-unknowntlv | The total number of data path pre-registration acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6datapathpreregack-duptlvfound | The total number of data path pre-registration acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6datapathpreregack-nosessfound | The total number of data path pre-registration acknowledgement messages on the R6 interface without any session information. | Int32
r6datapathpreregack-adminprohib | The total number of data path pre-registration acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path pre-registration acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathpreregack-noresourcedrop | The total number of data path pre-registration acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path pre-registration acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathpreregack-transiderr | The total number of data path pre-registration acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6datapathregreq-totsent | The total number of data path registration request messages sent on the R6 interface. | Int32
r6datapathregreq-retranssent | The total number of data path registration request messages re-transmitted on the R6 interface. | Int32
r6datapathregreq-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path registration request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathregreq-totrec | The total number of data path registration request messages received on the R6 interface. | Int32
r6datapathregreq-totacc | The total number of data path registration request messages accepted on the R6 interface. | Int32
r6datapathregreq-totrelay | The total number of data path registration request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path registration request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathregreq-totdenied | The total number of data path registration request messages denied on the R6 interface. | Int32
r6datapathregreq-totdiscard | The total number of data path registration request messages discarded on the R6 interface. | Int32
r6datapathregreq-badform | The total number of badly formed data path registration request messages on the R6 interface. | Int32
r6datapathregreq-decodeerr | The total number of data path registration request messages on the R6 interface with decode error. | Int32
r6datapathregreq-unspecerr | The total number of data path registration request messages on the R6 interface with unspecified error. | Int32
r6datapathregreq-missmandtlv | The total number of data path registration request messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathregreq-tlvvalinval | The total number of data path registration request messages on the R6 interface with invalid TLV value. | Int32
r6datapathregreq-unknowntlv | The total number of data path registration request messages on the R6 interface with unknown TLVs. | Int32
r6datapathregreq-duptlvfound | The total number of data path registration request messages on the R6 interface with duplicate TLVs. | Int32
r6datapathregreq-nosessfound | The total number of data path registration request messages on the R6 interface without any session information. | Int32
r6datapathregreq-adminprohib | The total number of data path registration request messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path registration request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathregreq-noresourcedrop | The total number of data path registration request messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path registration request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathregreq-transiderr | The total number of data path registration request messages on the R6 interface with transaction ID errors. | Int32
r6datapathregrsp-totsent | The total number of data path registration response messages sent on the R6 interface. | Int32
r6datapathregrsp-retranssent | The total number of data path registration response messages re-transmitted on the R6 interface. | Int32
r6datapathregrsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path registration response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathregrsp-totrec | The total number of data path registration response messages received on the R6 interface. | Int32
r6datapathregrsp-totacc | The total number of data path registration response messages accepted on the R6 interface. | Int32
r6datapathregrsp-totrelay | The total number of data path registration response messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path registration response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathregrsp-totdenied | The total number of data path registration response messages denied on the R6 interface. | Int32
r6datapathregrsp-totdiscard | The total number of data path registration response messages discarded on the R6 interface. | Int32
r6datapathregrsp-badform | The total number of badly formed data path registration response messages on the R6 interface. | Int32
r6datapathregrsp-decodeerr | The total number of data path registration response messages on the R6 interface with decode error. | Int32
r6datapathregrsp-unspecerr | The total number of data path registration response messages on the R6 interface with unspecified error. | Int32
r6datapathregrsp-missmandtlv | The total number of data path registration response messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathregrsp-tlvvalinval | The total number of data path registration response messages on the R6 interface with invalid TLV value. | Int32
r6datapathregrsp-unknowntlv | The total number of data path registration response messages on the R6 interface with unknown TLVs. | Int32
r6datapathregrsp-duptlvfound | The total number of data path registration response messages on the R6 interface with duplicate TLVs. | Int32
r6datapathregrsp-nosessfound | The total number of data path registration response messages on the R6 interface without any session information. | Int32
r6datapathregrsp-adminprohib | The total number of data path registration response messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path registration response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathregrsp-noresourcedrop | The total number of data path registration response messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path registration response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathregrsp-transiderr | The total number of data path registration response messages on the R6 interface with transaction ID errors. | Int32
r6datapathregack-totsent | The total number of data path registration acknowledgement messages sent on the R6 interface. | Int32
r6datapathregack-retranssent | The total number of data path registration acknowledgement messages re-transmitted on the R6 interface. | Int32
r6datapathregack-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path registration acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathregack-totrec | The total number of data path registration acknowledgement messages received on the R6 interface. | Int32
r6datapathregack-totacc | The total number of data path registration acknowledgement messages accepted on the R6 interface. | Int32
r6datapathregack-totrelay | The total number of data path registration acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path registration acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathregack-totdenied | The total number of data path registration acknowledgement messages denied on the R6 interface. | Int32
r6datapathregack-totdiscard | The total number of data path registration acknowledgement messages discarded on the R6 interface. | Int32
r6datapathregack-badform | The total number of badly formed data path registration acknowledgement messages on the R6 interface. | Int32
r6datapathregack-decodeerr | The total number of data path registration acknowledgement messages on the R6 interface with decode error. | Int32
r6datapathregack-unspecerr | The total number of data path registration acknowledgement messages on the R6 interface with unspecified error. | Int32
r6datapathregack-missmandtlv | The total number of data path registration acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathregack-tlvvalinval | The total number of data path registration acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6datapathregack-unknowntlv | The total number of data path registration acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6datapathregack-duptlvfound | The total number of data path registration acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6datapathregack-nosessfound | The total number of data path registration acknowledgement messages on the R6 interface without any session information. | Int32
r6datapathregack-adminprohib | The total number of data path registration acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path registration acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathregack-noresourcedrop | The total number of data path registration acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path registration acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathregack-transiderr | The total number of data path registration acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6pathmodreq-totsent | The total number of data path modification request messages sent on the R6 interface. | Int32
r6pathmodreq-retranssent | The total number of retransmitted data path modification request messages sent on the R6 interface. | Int32
r6pathmodreq-totsendfail | The total number of failed data path modification request messages sent on the R6 interface. | Int32
r6pathmodreq-totrec | The total number of data path modification request messages received on the R6 interface. | Int32
r6pathmodreq-totacc | The total number of accepted data path modification request messages sent on the R6 interface. | Int32
r6pathmodreq-totrelay | The total number of data path modification request messages relayed on the R6 interface. | Int32
r6pathmodreq-totdenied | The total number of denied data path modification request messages sent on the R6 interface. | Int32
r6pathmodreq-totdiscard | The total number of discarded data path modification request messages sent on the R6 interface. | Int32
r6pathmodreq-badform | The total number of data path modification request messages with a bad format sent on the R6 interface. | Int32
r6pathmodreq-decodeerr | The total number of data path modification request messages with decode errors sent on the R6 interface. | Int32
r6pathmodreq-unspecerr | The total number of data path modification request messages with unspecified errors sent on the R6 interface. | Int32
r6pathmodreq-missmandtlv | The total number of data path modification request messages sent on the R6 interface with a missing mandatory TLV. | Int32
r6pathmodreq-tlvvalinval | The total number of data path modification request messages sent on the R6 interface with an invalid TLV. | Int32
r6pathmodreq-unknowntlv | The total number of data path modification request messages sent on the R6 interface with an unknown TLV. | Int32
r6pathmodreq-duptlvfound | The total number of data path modification request messages sent on the R6 interface found with a duplicate TLV. | Int32
r6pathmodreq-nosessfound | The total number of data path modification request messages sent on the R6 interface with no session found. | Int32
r6pathmodreq-adminprohib | The total number of data path modification request messages sent on the R6 interface with administration prohibited. | Int32
r6pathmodreq-noresourcedrop | The total number of data path modification request messages discarded or denied due to resource unavailability. | Int32
r6pathmodreq-transiderr | The total number of data path modification request messages sent on the R6 interface with transaction ID errors. | Int32
r6pathmodrsp-totsent | The total number of data path modification response messages sent on the R6 interface. | Int32
r6pathmodrsp-retranssent | The total number of retransmitted data path modification response messages sent on the R6 interface. | Int32
r6pathmodrsp-totsendfail | The total number of failed data path modification response messages sent on the R6 interface. | Int32
r6pathmodrsp-totrec | The total number of data path modification response messages received on the R6 interface. | Int32
r6pathmodrsp-totacc | The total number of accepted data path modification response messages sent on the R6 interface. | Int32
r6pathmodrsp-totrelay | The total number of data path modification response messages relayed on the R6 interface. | Int32
r6pathmodrsp-totdenied | The total number of denied data path modification response messages sent on the R6 interface. | Int32
r6pathmodrsp-totdiscard | The total number of discarded data path modification response messages sent on the R6 interface. | Int32
r6pathmodrsp-badform | The total number of data path modification response messages with a bad format sent on the R6 interface. | Int32
r6pathmodrsp-decodeerr | The total number of data path modification response messages with decode errors sent on the R6 interface. | Int32
r6pathmodrsp-unspecerr | The total number of data path modification response messages with unspecified errors sent on the R6 interface. | Int32
r6pathmodrsp-missmandtlv | The total number of data path modification response messages sent on the R6 interface with a missing mandatory TLV. | Int32
r6pathmodrsp-tlvvalinval | The total number of data path modification response messages sent on the R6 interface with an invalid TLV. | Int32
r6pathmodrsp-unknowntlv | The total number of data path modification response messages sent on the R6 interface with an unknown TLV. | Int32
r6pathmodrsp-duptlvfound | The total number of data path modification response messages sent on the R6 interface found with a duplicate TLV. | Int32
r6pathmodrsp-nosessfound | The total number of data path modification response messages sent on the R6 interface with no session found. | Int32
r6pathmodrsp-adminprohib | The total number of data path modification response messages sent on the R6 interface with administration prohibited. | Int32
r6pathmodrsp-noresourcedrop | The total number of data path modification response messages sent on the R6 interface discarded or denied due to resource unavailability. | Int32
r6pathmodrsp-transiderr | The total number of data path modification response messages sent on the R6 interface with transaction ID errors. | Int32
r6pathmodack-totsent | The total number of data path modification acknowledgement messages sent on the R6 interface. | Int32
r6pathmodack-retranssent | The total number of retransmitted data path modification acknowledgement messages sent on the R6 interface. | Int32
r6pathmodack-totsendfail | The total number of failed data path modification acknowledgement messages sent on the R6 interface. | Int32
r6pathmodack-totrec | The total number of data path modification acknowledgement messages received on the R6 interface. | Int32
r6pathmodack-totacc | The total number of data path modification acknowledgement messages received on the R6 interface. | Int32
r6pathmodack-totrelay | The total number of data path modification acknowledgement messages relayed on the R6 interface. | Int32
r6pathmodack-totdenied | The total number of denied data path modification acknowledgement messages sent on the R6 interface. | Int32
r6pathmodack-totdiscard | The total number of discarded data path modification acknowledgement messages sent on the R6 interface. | Int32
r6pathmodack-badform | The total number of data path modification acknowledgement messages with a bad format sent on the R6 interface. | Int32
r6pathmodack-decodeerr | The total number of data path modification acknowledgement messages with decode errors sent on the R6 interface. | Int32
r6pathmodack-unspecerr | The total number of data path modification acknowledgement messages with unspecified errors sent on the R6 interface. | Int32
r6pathmodack-missmandtlv | The total number of data path modification acknowledgement messages sent on the R6 interface with a missing mandatory TLV. | Int32
r6pathmodack-tlvvalinval | The total number of data path modification acknowledgement messages sent on the R6 interface with an invalid TLV. | Int32
r6pathmodack-unknowntlv | The total number of data path modification acknowledgement messages sent on the R6 interface with an unknown TLV. | Int32
r6pathmodack-duptlvfound | The total number of data path modification acknowledgement messages sent on the R6 interface found with a duplicate TLV. | Int32
r6pathmodack-nosessfound | The total number of data path modification acknowledgement messages sent on the R6 interface with no session found. | Int32
r6pathmodack-adminprohib | The total number of data path modification acknowledgement messages sent on the R6 interface with administration prohibited. | Int32
r6pathmodack-noresourcedrop | The total number of data path modification acknowledgement messages sent on the R6 discarded or denied due to resource unavailability. | Int32
r6pathmodack-transiderr | The total number of data path modification acknowledgement messages sent on the R6 interface with transaction ID errors. | Int32
r6datapathderegreq-totsent | The total number of data path de-registration request messages sent on the R6 interface. | Int32
r6datapathderegreq-retranssent | The total number of data path de-registration request messages re-transmitted on the R6 interface. | Int32
r6datapathderegreq-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path de-registration request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathderegreq-totrec | The total number of data path de-registration request messages received on the R6 interface. | Int32
r6datapathderegreq-totacc | The total number of data path de-registration request messages accepted on the R6 interface. | Int32
r6datapathderegreq-totrelay | The total number of data path de-registration request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path de-registration request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathderegreq-totdenied | The total number of data path de-registration request messages denied on the R6 interface. | Int32
r6datapathderegreq-totdiscard | The total number of data path de-registration request messages discarded on the R6 interface. | Int32
r6datapathderegreq-badform | The total number of badly formed data path de-registration request messages on the R6 interface. | Int32
r6datapathderegreq-decodeerr | The total number of data path de-registration request messages on the R6 interface with decode error. | Int32
r6datapathderegreq-unspecerr | The total number of data path de-registration request messages on the R6 interface with unspecified error. | Int32
r6datapathderegreq-missmandtlv | The total number of data path de-registration request messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathderegreq-tlvvalinval | The total number of data path de-registration request messages on the R6 interface with invalid TLV value. | Int32
r6datapathderegreq-unknowntlv | The total number of data path de-registration request messages on the R6 interface with unknown TLVs. | Int32
r6datapathderegreq-duptlvfound | The total number of data path de-registration request messages on the R6 interface with duplicate TLVs. | Int32
r6datapathderegreq-nosessfound | The total number of data path de-registration request messages on the R6 interface without any session information. | Int32
r6datapathderegreq-adminprohib | The total number of data path de-registration request messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path de-registration request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathderegreq-noresourcedrop | The total number of data path de-registration request messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path de-registration request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services.services. | Int32
r6datapathderegreq-transiderr | The total number of data path de-registration request messages on the R6 interface with transaction ID errors. | Int32
r6datapathderegrsp-totsent | The total number of data path de-registration response messages sent on the R6 interface. | Int32
r6datapathderegrsp-retranssent | The total number of data path de-registration response messages re-transmitted on the R6 interface. | Int32
r6datapathderegrsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 data path de-registration response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathderegrsp-totrec | The total number of data path de-registration response messages received on the R6 interface. | Int32
r6datapathderegrsp-totacc | The total number of data path de-registration response messages accepted on the R6 interface. | Int32
r6datapathderegrsp-totrelay | The total number of data path de-registration response messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a data path de-registration response message is relayed by the R6 interface. Availability: across all ASNGW services.services. | Int32
r6datapathderegrsp-totdenied | The total number of data path de-registration response messages denied on the R6 interface. | Int32
r6datapathderegrsp-totdiscard | The total number of data path de-registration response messages discarded on the R6 interface. | Int32
r6datapathderegrsp-badform | The total number of badly formed data path de-registration response messages on the R6 interface. | Int32
r6datapathderegrsp-decodeerr | The total number of data path de-registration response messages on the R6 interface with decode error. | Int32
r6datapathderegrsp-unspecerr | The total number of data path de-registration response messages on the R6 interface with unspecified error. | Int32
r6datapathderegrsp-missmandtlv | The total number of data path de-registration response messages on the R6 interface with missing mandatory TLVs. | Int32
r6datapathderegrsp-tlvvalinval | The total number of data path de-registration response messages on the R6 interface with invalid TLV value. | Int32
r6datapathderegrsp-unknowntlv | The total number of data path de-registration response messages on the R6 interface with unknown TLVs. | Int32
r6datapathderegrsp-duptlvfound | The total number of data path de-registration response messages on the R6 interface with duplicate TLVs. | Int32
r6datapathderegrsp-nosessfound | The total number of data path de-registration response messages on the R6 interface without any session information. | Int32
r6datapathderegrsp-adminprohib | The total number of data path de-registration response messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path de-registration response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6datapathderegrsp-noresourcedrop | The total number of data path de-registration response messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path de-registration response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6datapathderegrsp-transiderr | The total number of data path de-registration response messages on the R6 interface with transaction ID errors. | Int32
r6keychadir-totsent | The total number of key change direct messages sent on the R6 interface. | Int32
r6keychadir-retranssent | The total number of failures occurred during transaction ID generation and R6 Key change directive message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6keychadir-totsendfail | The total number of key change direct messages re-transmitted on the R6 interface. | Int32
r6keychadir-totrec | The total number of key change direct messages received on the R6 interface. | Int32
r6keychadir-totacc | The total number of key change direct messages accepted on the R6 interface. | Int32
r6keychadir-totrelay | The total number of key change directive messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a key change directive message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6keychadir-totdenied | The total number of key change direct messages denied on the R6 interface. | Int32
r6keychadir-totdiscard | The total number of key change direct messages discarded on the R6 interface. | Int32
r6keychadir-badform | The total number of badly formed key change direct messages on the R6 interface. | Int32
r6keychadir-decodeerr | The total number of key change direct messages on the R6 interface with decode error. | Int32
r6keychadir-unspecerr | The total number of key change direct messages on the R6 interface with unspecified error. | Int32
r6keychadir-missmandtlv | The total number of key change direct messages on the R6 interface with missing mandatory TLVs. | Int32
r6keychadir-tlvvalinval | The total number of key change direct messages on the R6 interface with invalid TLV value. | Int32
r6keychadir-unknowntlv | The total number of key change direct messages on the R6 interface with unknown TLVs. | Int32
r6keychadir-duptlvfound | The total number of key change direct messages on the R6 interface with duplicate TLVs. | Int32
r6keychadir-nosessfound | The total number of key change direct messages on the R6 interface without any session information. | Int32
r6keychadir-adminprohib | The total number of key change directive messages discarded or denied due to admin prohibit. Triggers: Changes every time a key change directive message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6keychadir-noresourcedrop | The total number of key change directive messages discarded or denied due to resource unavailability. Triggers: Changes every time a key change directive message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6keychadir-transiderr | The total number of key change direct messages on the R6 interface with transaction ID errors. | Int32
r6keychaack-totsent | The total number of key change acknowledgement messages sent on the R6 interface. | Int32
r6keychaack-retranssent | The total number of failures occurred during transaction ID generation and R6 Key change acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6keychaack-totsendfail | The total number of key change acknowledgement messages re-transmitted on the R6 interface. | Int32
r6keychaack-totrec | The total number of key change acknowledgement messages received on the R6 interface. | Int32
r6keychaack-totacc | The total number of key change acknowledgement messages accepted on the R6 interface. | Int32
r6keychaack-totrelay | The total number of key change acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a key change acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6keychaack-totdenied | The total number of key change acknowledgement messages denied on the R6 interface. | Int32
r6keychaack-totdiscard | The total number of key change acknowledgement messages discarded on the R6 interface. | Int32
r6keychaack-badform | The total number of badly formed key change acknowledgement messages on the R6 interface. | Int32
r6keychaack-decodeerr | The total number of key change acknowledgement messages on the R6 interface with decode error. | Int32
r6keychaack-unspecerr | The total number of key change acknowledgement messages on the R6 interface with unspecified error. | Int32
r6keychaack-missmandtlv | The total number of key change acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6keychaack-tlvvalinval | The total number of key change acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6keychaack-unknowntlv | The total number of key change acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6keychaack-duptlvfound | The total number of key change acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6keychaack-nosessfound | The total number of key change acknowledgement messages on the R6 interface without any session information. | Int32
r6keychaack-adminprohib | The total number of key change acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a key change acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6keychaack-noresourcedrop | The total number of key change acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a key change acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6keychaack-transiderr | The total number of key change acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6keychacnf-totrec | The total number of key change confirm messages received on the R6 interface. | Int32
r6keychacnf-totacc | The total number of key change confirm messages accepted on the R6 interface. | Int32
r6keychacnf-totrelay | The total number of key change confirm messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a key change confirm message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6keychacnf-totdenied | The total number of key change confirm messages denied on the R6 interface. | Int32
r6keychacnf-totdiscard | The total number of key change confirm messages discarded on the R6 interface. | Int32
r6keychacnf-badform | The total number of badly formed key change confirm messages on the R6 interface. | Int32
r6keychacnf-decodeerr | The total number of key change confirm messages on the R6 interface with decode error. | Int32
r6keychacnf-unspecerr | The total number of key change confirm messages on the R6 interface with unspecified error. | Int32
r6keychacnf-missmandtlv | The total number of key change confirm messages on the R6 interface with missing mandatory TLVs. | Int32
r6keychacnf-tlvvalinval | The total number of key change confirm messages on the R6 interface with invalid TLV value. | Int32
r6keychacnf-unknowntlv | The total number of key change confirm messages on the R6 interface with unknown TLVs. | Int32
r6keychacnf-duptlvfound | The total number of key change confirm messages on the R6 interface with duplicate TLVs. | Int32
r6keychacnf-nosessfound | The total number of key change confirm messages on the R6 interface without any session information. | Int32
r6keychacnf-adminprohib | The total number of key change confirm messages discarded or denied due to admin prohibit. Triggers: Changes every time a key change confirm message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6keychacnf-noresourcedrop | The total number of key change confirm messages discarded or denied due to resource unavailability. Triggers: Changes every time a key change confirm message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r6keychacnf-transiderr | The total number of key change confirm messages on the R6 interface with transaction ID errors. | Int32
r6cmackeycounupd-totsent | The total number of CMAC key count update messages sent on the R6 interface. | Int32
r6cmackeycounupd-retranssent | The total number of CMAC key count update messages re-transmitted on the R6 interface. | Int32
r6cmackeycounupd-totsendfail | The total number of failures occurred during transaction ID generation and R6 CMAC key count update message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6cmackeycounupd-totrec | The total number of CMAC key count update messages received on the R6 interface. | Int32
r6cmackeycounupd-totacc | The total number of CMAC key count update messages accepted on the R6 interface. | Int32
r6cmackeycounupd-totrelay | The total number of CMAC key count update messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a CMAC key count update message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6cmackeycounupd-totdenied | The total number of CMAC key count update messages denied on the R6 interface. | Int32
r6cmackeycounupd-totdiscard | The total number of CMAC key count update messages discarded on the R6 interface. | Int32
r6cmackeycounupd-badform | The total number of badly formed CMAC key count update messages on the R6 interface. | Int32
r6cmackeycounupd-decodeerr | The total number of CMAC key count update messages on the R6 interface with decode error. | Int32
r6cmackeycounupd-unspecerr | The total number of CMAC key count update messages on the R6 interface with unspecified error. | Int32
r6cmackeycounupd-missmandtlv | The total number of CMAC key count update messages on the R6 interface with missing mandatory TLVs. | Int32
r6cmackeycounupd-tlvvalinval | The total number of CMAC key count update messages on the R6 interface with invalid TLV value. | Int32
r6cmackeycounupd-unknowntlv | The total number of CMAC key count update messages on the R6 interface with unknown TLVs. | Int32
r6cmackeycounupd-duptlvfound | The total number of CMAC key count update messages on the R6 interface with duplicate TLVs. | Int32
r6cmackeycounupd-nosessfound | The total number of CMAC key count update messages on the R6 interface without any session information. | Int32
r6cmackeycounupd-adminprohib | The total number of CMAC key count update messages discarded or denied due to admin prohibit. Triggers: Changes every time a CMAC key count update message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6cmackeycounupd-noresourcedrop | The total number of CMAC key count update messages discarded or denied due to resource unavailability. Triggers: Changes every time a CMAC key count update message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6cmackeycounupd-transiderr | The total number of CMAC key count update messages on the R6 interface with transaction ID errors. | Int32
r6cmackeycounack-totsent | The total number of CMAC key count acknowledgement messages sent on the R6 interface. | Int32
r6cmackeycounack-retranssent | The total number of CMAC key count acknowledgement messages re-transmitted on the R6 interface. | Int32
r6cmackeycounack-totsendfail | The total number of failures occurred during transaction ID generation and R6 CMAC key count acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6cmackeycounack-totrec | The total number of CMAC key count acknowledgement messages received on the R6 interface. | Int32
r6cmackeycounack-totacc | The total number of CMAC key count acknowledgement messages accepted on the R6 interface. | Int32
r6cmackeycounack-totrelay | The total number of CMAC key count acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a CMAC key count acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6cmackeycounack-totdenied | The total number of CMAC key count acknowledgement messages denied on the R6 interface. | Int32
r6cmackeycounack-totdiscard | The total number of CMAC key count acknowledgement messages discarded on the R6 interface. | Int32
r6cmackeycounack-badform | The total number of badly formed CMAC key count acknowledgement messages on the R6 interface. | Int32
r6cmackeycounack-decodeerr | The total number of CMAC key count acknowledgement messages on the R6 interface with decode error. | Int32
r6cmackeycounack-unspecerr | The total number of CMAC key count acknowledgement messages on the R6 interface with unspecified error. | Int32
r6cmackeycounack-missmandtlv | The total number of CMAC key count acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6cmackeycounack-tlvvalinval | The total number of CMAC key count acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6cmackeycounack-unknowntlv | The total number of CMAC key count acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6cmackeycounack-duptlvfound | The total number of CMAC key count acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6cmackeycounack-nosessfound | The total number of CMAC key count acknowledgement messages on the R6 interface without any session information. | Int32
r6cmackeycounack-adminprohib | The total number of CMAC key count acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a CMAC key count acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6cmackeycounack-noresourcedrop | The total number of CMAC key count acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a CMAC key count acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6cmackeycounack-transiderr | The total number of CMAC key count acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6horeq-totsent | The total number of R6 handover request messages sent on the R6 interface. | Int32
r6horeq-retranssent | The total number of R6 handover request messages re-transmitted on the R6 interface. | Int32
r6horeq-totsendfail | The total number of failures occurred during transaction ID generation and R6 handover request message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6horeq-totrec | The total number of R6 handover request messages received on the R6 interface. | Int32
r6horeq-totacc | The total number of R6 handover request messages accepted on the R6 interface. | Int32
r6horeq-totrelay | The total number of R6 handover request messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an R6 handover request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6horeq-totdenied | The total number of R6 handover request messages denied on the R6 interface. | Int32
r6horeq-totdiscard | The total number of R6 handover request messages discarded on the R6 interface. | Int32
r6horeq-badform | The total number of badly formed R6 handover request messages on the R6 interface. | Int32
r6horeq-decodeerr | The total number of R6 handover request messages on the R6 interface with decode error. | Int32
r6horeq-unspecerr | The total number of R6 handover request messages on the R6 interface with unspecified error. | Int32
r6horeq-missmandtlv | The total number of R6 handover request messages on the R6 interface with missing mandatory TLVs. | Int32
r6horeq-tlvvalinval | The total number of R6 handover request messages on the R6 interface with invalid TLV value. | Int32
r6horeq-unknowntlv | The total number of R6 handover request messages on the R6 interface with unknown TLVs. | Int32
r6horeq-duptlvfound | The total number of R6 handover request messages on the R6 interface with duplicate TLVs. | Int32
r6horeq-nosessfound | The total number of R6 handover request messages on the R6 interface without any session information. | Int32
r6horeq-adminprohib | The total number of R6 handover request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 handover request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6horeq-noresourcedrop | The total number of R6 handover request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 handover request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6horeq-transiderr | The total number of R6 handover request messages on the R6 interface with transaction ID errors. | Int32
r6horsp-totsent | The total number of R6 handover response messages sent on the R6 interface. | Int32
r6horsp-retranssent | The total number of R6 handover response messages re-transmitted on the R6 interface. | Int32
r6horsp-totsendfail | The total number of failures occurred during transaction ID generation and R6 handover response message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6horsp-totrec | The total number of R6 handover response messages received on the R6 interface. | Int32
r6horsp-totacc | The total number of R6 handover response messages accepted on the R6 interface. | Int32
r6horsp-totrelay | The total number of R6 handover response messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an R6 handover response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6horsp-totdenied | The total number of R6 handover response messages denied on the R6 interface. | Int32
r6horsp-totdiscard | The total number of R6 handover response messages discarded on the R6 interface. | Int32
r6horsp-badform | The total number of badly formed R6 handover response messages on the R6 interface. | Int32
r6horsp-decodeerr | The total number of R6 handover response messages on the R6 interface with decode error. | Int32
r6horsp-unspecerr | The total number of R6 handover response messages on the R6 interface with unspecified error. | Int32
r6horsp-missmandtlv | The total number of R6 handover response messages on the R6 interface with missing mandatory TLVs. | Int32
r6horsp-tlvvalinval | The total number of R6 handover response messages on the R6 interface with invalid TLV value. | Int32
r6horsp-unknowntlv | The total number of R6 handover response messages on the R6 interface with unknown TLVs. | Int32
r6horsp-duptlvfound | The total number of R6 handover response messages on the R6 interface with duplicate TLVs. | Int32
r6horsp-nosessfound | The total number of R6 handover response messages on the R6 interface without any session information. | Int32
r6horsp-adminprohib | The total number of R6 handover response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 handover response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6horsp-noresourcedrop | The total number of R6 handover response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 handover response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6horsp-transiderr | The total number of R6 handover response messages on the R6 interface with transaction ID errors. | Int32
r6hoack-totsent | The total number of R6 handover acknowledgement messages sent on the R6 interface. | Int32
r6hoack-retranssent | The total number of R6 handover acknowledgement messages re-transmitted on the R6 interface. | Int32
r6hoack-totsendfail | The total number of failures occurred during transaction ID generation and R6 handover acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6hoack-totrec | The total number of R6 handover acknowledgement messages received on the R6 interface. | Int32
r6hoack-totacc | The total number of R6 handover acknowledgement messages accepted on the R6 interface. | Int32
r6hoack-totrelay | The total number of R6 handover acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an R6 handover acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6hoack-totdenied | The total number of R6 handover acknowledgement messages denied on the R6 interface. | Int32
r6hoack-totdiscard | The total number of R6 handover acknowledgement messages discarded on the R6 interface. | Int32
r6hoack-badform | The total number of badly formed R6 handover acknowledgement messages on the R6 interface. | Int32
r6hoack-decodeerr | The total number of R6 handover acknowledgement messages on the R6 interface with decode error. | Int32
r6hoack-unspecerr | The total number of R6 handover acknowledgement messages on the R6 interface with unspecified error. | Int32
r6hoack-missmandtlv | The total number of R6 handover acknowledgement messages on the R6 interface with missing mandatory TLVs. | Int32
r6hoack-tlvvalinval | The total number of R6 handover acknowledgement messages on the R6 interface with invalid TLV value. | Int32
r6hoack-unknowntlv | The total number of R6 handover acknowledgement messages on the R6 interface with unknown TLVs. | Int32
r6hoack-duptlvfound | The total number of R6 handover acknowledgement messages on the R6 interface with duplicate TLVs. | Int32
r6hoack-nosessfound | The total number of R6 handover acknowledgement messages on the R6 interface without any session information. | Int32
r6hoack-adminprohib | The total number of R6 handover acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 handover acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6hoack-noresourcedrop | The total number of R6 handover acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 handover acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6hoack-transiderr | The total number of R6 handover acknowledgement messages on the R6 interface with transaction ID errors. | Int32
r6hocnf-totsent | The total number of R6 handover confirm messages sent on the R6 interface. | Int32
r6hocnf-retranssent | The total number of R6 handover confirm messages re-transmitted on the R6 interface. | Int32
r6hocnf-totsendfail | The total number of failures occurred during transaction ID generation and R6 handover confirm message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6hocnf-totrec | The total number of R6 handover confirm messages received on the R6 interface. | Int32
r6hocnf-totacc | The total number of R6 handover confirm messages accepted on the R6 interface. | Int32
r6hocnf-totrelay | The total number of R6 handover confirm messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an R6 handover confirm message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6hocnf-totdenied | The total number of R6 handover confirm messages denied on the R6 interface. | Int32
r6hocnf-totdiscard | The total number of R6 handover confirm messages discarded on the R6 interface. | Int32
r6hocnf-badform | The total number of badly formed R6 handover confirm messages on the R6 interface. | Int32
r6hocnf-decodeerr | The total number of R6 handover confirm messages on the R6 interface with decode error. | Int32
r6hocnf-unspecerr | The total number of R6 handover confirm messages on the R6 interface with unspecified error. | Int32
r6hocnf-missmandtlv | The total number of R6 handover confirm messages on the R6 interface with missing mandatory TLVs. | Int32
r6hocnf-tlvvalinval | The total number of R6 handover confirm messages on the R6 interface with invalid TLV value. | Int32
r6hocnf-unknowntlv | The total number of R6 handover confirm messages on the R6 interface with unknown TLVs. | Int32
r6hocnf-duptlvfound | The total number of R6 handover confirm messages on the R6 interface with duplicate TLVs. | Int32
r6hocnf-nosessfound | The total number of R6 handover confirm messages on the R6 interface without any session information. | Int32
r6hocnf-adminprohib | The total number of R6 handover confirm messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 handover confirm message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6hocnf-noresourcedrop | The total number of R6 handover confirm messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 handover confirm message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6hocnf-transiderr | The total number of R6 handover confirm messages on the R6 interface with transaction ID errors. | Int32
r6hocmpl-totsent | The total number of R6 handover complete messages sent on the R6 interface. | Int32
r6hocmpl-retranssent | The total number of R6 handover complete messages re-transmitted on the R6 interface. | Int32
r6hocmpl-totsendfail | The total number of failures occurred during transaction ID generation and R6 handover complete message not sent for specific interface. This counter is used to count the error while sending the R6 packets. | Int32
r6hocmpl-totrec | The total number of R6 handover complete messages received on the R6 interface. | Int32
r6hocmpl-totacc | The total number of R6 handover complete messages accepted on the R6 interface. | Int32
r6hocmpl-totrelay | The total number of R6 handover complete messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an R6 handover complete message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6hocmpl-totdenied | The total number of R6 handover complete messages denied on the R6 interface. | Int32
r6hocmpl-totdiscard | The total number of R6 handover complete messages discarded on the R6 interface. | Int32
r6hocmpl-badform | The total number of badly formed R6 handover complete messages on the R6 interface. | Int32
r6hocmpl-decodeerr | The total number of R6 handover complete messages on the R6 interface with decode error. | Int32
r6hocmpl-unspecerr | The total number of R6 handover complete messages on the R6 interface with unspecified error. | Int32
r6hocmpl-missmandtlv | The total number of R6 handover complete messages on the R6 interface with missing mandatory TLVs. | Int32
r6hocmpl-tlvvalinval | The total number of R6 handover complete messages on the R6 interface with invalid TLV value. | Int32
r6hocmpl-unknowntlv | The total number of R6 handover complete messages on the R6 interface with unknown TLVs. | Int32
r6hocmpl-duptlvfound | The total number of R6 handover complete messages on the R6 interface with duplicate TLVs. | Int32
r6hocmpl-nosessfound | The total number of R6 handover complete messages on the R6 interface without any session information. | Int32
r6hocmpl-adminprohib | The total number of R6 handover complete messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 handover complete message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6hocmpl-noresourcedrop | The total number of R6 handover complete messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 handover complete message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6hocmpl-transiderr | The total number of R6 handover complete messages on the R6 interface with transaction ID errors. | Int32
r6unknown-totrec | The total number of unknown messages received on the R6 interface. | Int32
r6unknown-totacc | The total number of unknown messages accepted on the R6 interface. | Int32
r6unknown-totrelay | The total number of unknown messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an unknown message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6unknown-totdenied | The total number of unknown messages denied on the R6 interface. | Int32
r6unknown-totdiscard | The total number of unknown messages discarded on the R6 interface. | Int32
r6unknown-badform | The total number of badly formed unknown messages on the R6 interface. | Int32
r6unknown-decodeerr | The total number of unknown messages on the R6 interface with decode error. | Int32
r6unknown-unspecerr | The total number of unknown messages on the R6 interface with unspecified error. | Int32
r6unknown-missmandtlv | The total number of unknown messages on the R6 interface with missing mandatory TLVs. | Int32
r6unknown-tlvvalinval | The total number of unknown messages on the R6 interface with invalid TLV value. | Int32
r6unknown-unknowntlv | The total number of unknown messages on the R6 interface with unknown TLVs. | Int32
r6unknown-duptlvfound | The total number of unknown messages on the R6 interface with duplicate TLVs. | Int32
r6unknown-nosessfound | The total number of unknown messages on the R6 interface without any session information. | Int32
r6unknown-adminprohib | The total number of unknown messages discarded or denied due to admin prohibit. Triggers: Changes every time an unknown message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6unknown-noresourcedrop | The total number of unknown messages discarded or denied due to resource unavailability. Triggers: Changes every time an unknown message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6unknown-transiderr | The total number of unknown messages on the R6 interface with transaction ID errors. | Int32
r6datagrerec-totpackrec | The total number of data packets received through GRE tunnel R6 interface. | Int32
r6datagrerec-prottyperrror | Total number of protectd type errors received through GRE tunnel R6 interface. | Int32
r6datagrerec-totbytrec | The total number of data bytes received through GRE tunnel R6 interface. | Int32
r6datagrerec-grekeyabs | The total number of data message received without GRE key through GRE tunnel R6 interface. | Int32
r6datagrerec-grechkerr | The total number of data message received with checksum error through GRE tunnel R6 interface. | Int32
r6datagrerec-invpacklen | The total number of data message received with invalid packet length error through GRE tunnel R6 interface. | Int32
r6datagrerec-nosessfou | The total number of data message received through GRE tunnel without session information the R6 interface. | Int32
r6datagrerec-unspecerr | The total number of data message received through GRE tunnel with unspecified error R6 interface. | Int32
r6datagresend-totpacksent | Total number of data packets sent through GRE tunnel R6 interface. | Int32
r6datagresend-senderr | Total number of errors happend while sending data packets through GRE tunnel R6 interface. | Int32
r6datagresend-totbytsent | Total number of data bytes sent through GRE tunnel R6 interface. | Int32
r6datagresend-unspeerr | The total number of data message sent through GRE tunnel with unspecified error R6 interface. | Int 32
r6imexitstaind-totsent | The total number of R6 Idle Mode Exit State Indication messages sent to the base station. | Int32
r6imexitstaind-retranssent | The total number of Idle Mode Exit State Indication messages retransmitted on the R6 interface to the base station. | Int32
r6imexitstaind-totsendfail | The total number of Idle Mode Exit State Indication message failures received from the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6imexitstaind-totrec | The total number of R6 Idle Mode Exit State Indication messages received by the base station. | Int32
r6imexitstaind-totacc | The total number of R6 Idle Mode Exit State Indication messages accepted by base station. | Int32
r6imexitstaind-totrelay | The total number of R6 Idle Mode Exit State Indication messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Idle Mode Exit State Indication message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6imexitstaind-totdenied | The total number of Idle Mode Exit State Indication messages denied on the R6 interface. | Int32
r6imexitstaind-totdiscard | The total number of Idle Mode Exit State Indication messages discarded on the R6 interface. | Int32
r6imexitstaind-badform | The total number of badly formed R6 Idle Mode Exit State Indication messages sent to the base station. | Int32
r6imexitstaind-decodeerr | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with decode errors. | Int32
r6imexitstaind-unspecerr | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with unspecified errors. | Int32
r6imexitstaind-missmandtlv | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with missing mandatory TLVs. | Int32
r6imexitstaind-tlvvalinval | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with an invalid TLV. | Int32
r6imexitstaind-unknowntlv | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with an unknown TLV. | Int32
r6imexitstaind-duptlvfound | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with duplicate TLVs. | Int32
r6imexitstaind-nosessfound | The total number of R6 Idle Mode Exit State Indication messages sent to the base station without any session information. | Int32
r6imexitstaind-admprohibit | The total number of R6 Idle Mode Exit State Indication messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Idle Mode Exit State Indication message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6imexitstaind-noresourcedrop | The total number of R6 Idle Mode Exit State Indication messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Idle Mode Exit State Indication message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6imexitstaind-transiderr | The total number of R6 Idle Mode Exit State Indication messages sent to the base station with a transaction ID error. | Int32
r6imexitstaindack-totsent | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station. | Int32
r6imexitstaindack-retranssent | The total number of Idle Mode Exit State Indication Acknowledgement messages retransmitted on the R6 interface to the base station. | Int32
r6imexitstaindack-totsendfail | The total number of Idle Mode Exit State Indication Acknowledgement message failures received from the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int 32
r6imexitstaindack-totrec | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages received by the base station. | Int32
r6imexitstaindack-totacc | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages accepted by base station. |
r6imexitstaindack-totrelay | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Idle Mode Exit State Indication Acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6imexitstaindack-totdenied | The total number of Idle Mode Exit State Indication Acknowledgement messages denied on the R6 interface | Int32
r6imexitstaindack-totdiscard | The total number of Idle Mode Exit State Indication Acknowledgement messages discarded on the R6 interface. | Int32
r6imexitstaindack-badform | The total number of badly formed R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station. | Int32
r6imexitstaindack-decodeerr | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with decode errors. | Int32
r6imexitstaindack-unspecerr | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with unspecified errors. | Int32
r6imexitstaindack-missmandtlv | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with missing mandatory TLVs. | Int32
r6imexitstaindack-tlvvalinval | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with an invalid TLV. | Int32
r6imexitstaindack-unknowntlv | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with an unknown TLV. | Int32
r6imexitstaindack-duptlvfound | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with duplicate TLVs. | Int32
r6imexitstaindack-nosessfound | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station without any session information. | Int32
r6imexitstaindack-admprohibit | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Idle Mode Exit State Indication Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6imexitstaindack-noresourcedrop | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Idle Mode Exit State Indication Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6imexitstaindack-transiderr | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages sent to the base station with a transaction ID error. | Int32
r6datapathderegack-totsent | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station. | Int32
r6datapathderegack-retranssent | The total number of Data Path Deregistration Acknowledgement messages retransmitted on the R6 interface to the base station. | Int32
r6datapathderegack-totsendfail | The total number of Data Path Deregistration Acknowledgement message failures received from the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6datapathderegack-totrec | The total number of R6 Data Path Deregistration Acknowledgement messages received by the base station. | Int32
r6datapathderegack-totacc | The total number of R6 Idle Mode Exit State Indication Acknowledgement messages accepted by base station. | Int32
r6datapathderegack-totrelay | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Idle Mode Exit State Indication Acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6datapathderegack-totdenied | The total number of Data Path Deregistration Acknowledgement messages denied on the R6 interface | Int32
r6datapathderegack-totdiscard | The total number of Data Path Deregistration Acknowledgement messages discarded on the R6 interface. | Int32
r6datapathderegack-badform | The total number of badly formed R6 Data Path Deregistration Acknowledgement messages sent to the base station. | Int32
r6datapathderegack-decodeerr | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station with decode errors. | Int32
r6datapathderegack-unspecerr | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station with unspecified errors. | Int32
r6datapathderegack-missmandtlv | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station with missing mandatory TLVs. | Int32
r6datapathderegack-tlvvalinval | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station with an invalid TLV. | Int32
r6datapathderegack-unknowntlv | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station with an unknown TLV. | Int32
r6datapathderegack-duptlvfound | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station with duplicate TLVs. | Int32
r6datapathderegack-nosessfound | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station without any session information. | Int32
r6datapathderegack-admprohibit | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Idle Mode Exit State Indication Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6datapathderegack-noresourcedrop | The total number of R6 Data Path Deregistration Acknowledgement messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Idle Mode Exit State Indication Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6datapathderegack-transiderr | The total number of R6Data Path Deregistration Acknowledgement messages sent to the base station with a transaction ID error. | Int32
r4nwexitmsstachareq-totsent | The total number of network exit MS state change request messages sent on the R4 interface. | Int32
r4nwexitmsstachareq-retranssent | The total number of network exit MS state change request messages re-transmitted on the the R4 interface. | Int32
r4nwexitmsstachareq-totsendfail | The total number of failures occurred during transaction ID generation and R4 network exit MS state change request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4nwexitmsstachareq-totrec | The total number of network exit MS state change request messages received on the the R4 interface. | Int32
r4nwexitmsstachareq-totacc | The total number of network exit MS state change request messages accepted on the the R4 interface. | Int32
r4nwexitmsstachareq-totrelay | The total number of network exit MS state change request messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a network exit MS state change request message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4nwexitmsstachareq-totdenied | The total number of network exit MS state change request messages denied on the the R4 interface. | Int32
r4nwexitmsstachareq-totdiscard | The total number of network exit MS state change request messages discarded on the the R4 interface. | Int32
r4nwexitmsstachareq-badform | The total number of badly formed network exit MS state change request messages on the the R4 interface. | Int32
r4nwexitmsstachareq-decodeerr | The total number of network exit MS state change request messages on the the R4 interface with decode error. | Int32
r4nwexitmsstachareq-unspecerr | The total number of network exit MS state change request messages on the the R4 interface with unspecified error. | Int32
r4nwexitmsstachareq-missmandtlv | The total number of network exit MS state change request messages on the the R4 interface with missing mandatory TLVs. | Int32
r4nwexitmsstachareq-tlvvalinval | The total number of network exit MS state change request messages on the the R4 interface with invalid TLV value. | Int32
r4nwexitmsstachareq-unknowntlv | The total number of network exit MS state change request messages on the the R4 interface with unknown TLVs. | Int32
r4nwexitmsstachareq-duptlvfound | The total number of network exit MS state change request messages on the the R4 interface with duplicate TLVs. | Int32
r4nwexitmsstachareq-nosessfound | The total number of network exit MS state change request messages on the the R4 interface without any session information. | Int32
r4nwexitmsstachareq-adminprohib | The total number of network exit MS state change request messages discarded or denied due to admin prohibit. Triggers: Changes every time a network exit MS state change request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4nwexitmsstachareq-noresourcedrop | The total number of network exit MS state change request messages discarded or denied due to resource unavailability. Triggers: Changes every time a network exit MS state change request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4nwexitmsstachareq-transiderr | The total number of network exit MS state change request messages on the the R4 interface with transaction ID errors. | Int32
r4nwexitmsstacharsp-totsent | The total number of network exit MS state change response messages sent on the the R4 interface. | Int32
r4nwexitmsstacharsp-retranssent | The total number of network exit MS state change response messages re-transmitted on the the R4 interface. | Int32
r4nwexitmsstacharsp-totsendfail | The total number of failures occurred during transaction ID generation and R4 network exit MS state change response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4nwexitmsstacharsp-totrec | The total number of network exit MS state change response messages received on the the R4 interface. | Int32
r4nwexitmsstacharsp-totacc | The total number of network exit MS state change response messages accepted on the the R4 interface. | Int32
r4nwexitmsstacharsp-totrelay | The total number of network exit MS state change response messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a network exit MS state change response message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4nwexitmsstacharsp-totdenied | The total number of network exit MS state change response messages denied on the the R4 interface. | Int32
r4nwexitmsstacharsp-totdiscard | The total number of network exit MS state change response messages discarded on the the R4 interface. | Int32
r4nwexitmsstacharsp-badform | The total number of badly formed network exit MS state change response messages on the the R4 interface. | Int32
r4nwexitmsstacharsp-decodeerr | The total number of network exit MS state change response messages on the the R4 interface with decode error. | Int32
r4nwexitmsstacharsp-unspecerr | The total number of network exit MS state change response messages on the the R4 interface with unspecified error. | Int32
r4nwexitmsstacharsp-missmandtlv | The total number of network exit MS state change response messages on the the R4 interface with missing mandatory TLVs. | Int32
r4nwexitmsstacharsp-tlvvalinval | The total number of network exit MS state change response messages on the the R4 interface with invalid TLV value. | Int32
r4nwexitmsstacharsp-unknowntlv | The total number of network exit MS state change response messages on the the R4 interface with unknown TLVs. | Int32
r4nwexitmsstacharsp-duptlvfound | The total number of network exit MS state change response messages on the the R4 interface with duplicate TLVs. | Int32
r4nwexitmsstacharsp-nosessfound | The total number of network exit MS state change response messages on the the R4 interface without any session information. | Int32
r4nwexitmsstacharsp-adminprohib | The total number of network exit MS state change response messages discarded or denied due to admin prohibit. Triggers: Changes every time a network exit MS state change response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4nwexitmsstacharsp-noresourcedrop | The total number of network exit MS state change response messages discarded or denied due to resource unavailability. Triggers: Changes every time a network exit MS state change response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4nwexitmsstacharsp-transiderr | The total number of network exit MS state change response messages on the the R4 interface with transaction ID errors. | Int32
r4contextreq-totsent | The total number of context request messages sent on the the R4 interface. | Int32
r4contextreq-retranssent | The total number of context request messages re-transmitted on the the R4 interface. | Int32
r4contextreq-totsendfail | The total number of failures occurred during transaction ID generation and R4 Context Request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4contextreq-totrec | The total number of context request messages received on the the R4 interface. | Int32
r4contextreq-totacc | The total number of context request messages accepted on the the R4 interface. | Int32
r4contextreq-totrelay | The total number of context request messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a context request message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4contextreq-totdenied | The total number of context request messages denied on the the R4 interface. | Int32
r4contextreq-totdiscard | The total number of context request messages discarded on the the R4 interface. | Int32
r4contextreq-badform | The total number of badly formed context request messages on the the R4 interface. | Int32
r4contextreq-decodeerr | The total number of context request messages on the the R4 interface with decode error. | Int32
r4contextreq-unspecerr | The total number of context request messages on the the R4 interface with unspecified error. | Int32
r4contextreq-missmandtlv | The total number of context request messages on the the R4 interface with missing mandatory TLVs. | Int32
r4contextreq-tlvvalinval | The total number of context request messages on the the R4 interface with invalid TLV value. | Int32
r4contextreq-unknowntlv | The total number of context request messages on the the R4 interface with unknown TLVs. | Int32
r4contextreq-duptlvfound | The total number of context request messages on the the R4 interface with duplicate TLVs. | Int32
r4contextreq-nosessfound | The total number of context request messages on the the R4 interface without any session information. | Int32
r4contextreq-adminprohib | The total number of context request messages discarded or denied due to admin prohibit. Triggers: Changes every time a context request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4contextreq-noresourcedrop | The total number of context request messages discarded or denied due to resource unavailability. Triggers: Changes every time a context request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4contextreq-transiderr | The total number of context request messages on the the R4 interface with transaction ID errors. | Int32
r4contextrepo-totsent | The total number of context report messages sent on the the R4 interface. | Int32
r4contextrepo-retranssent | The total number of context report messages re-transmitted on the the R4 interface. | Int32
r4contextrepo-totsendfail | The total number of failures occurred during transaction ID generation and R4 Context Report message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4contextrepo-totrec | The total number of context report messages received on the the R4 interface. | Int32
r4contextrepo-totacc | The total number of context report messages accepted on the the R4 interface. | Int32
r4contextrepo-totrelay | The total number of context report messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a context report message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4contextrepo-totdenied | The total number of context report messages denied on the the R4 interface. | Int32
r4contextrepo-totdiscard | The total number of context report messages discarded on the the R4 interface. | Int32
r4contextrepo-badform | The total number of badly formed context report messages on the the R4 interface. | Int32
r4contextrepo-decodeerr | The total number of context report messages on the the R4 interface with decode error. | Int32
r4contextrepo-unspecerr | The total number of context report messages on the the R4 interface with unspecified error. | Int32
r4contextrepo-missmandtlv | The total number of context report messages on the the R4 interface with missing mandatory TLVs. | Int32
r4contextrepo-tlvvalinval | The total number of context report messages on the the R4 interface with invalid TLV value. | Int32
r4contextrepo-unknowntlv | The total number of context report messages on the the R4 interface with unknown TLVs. | Int32
r4contextrepo-duptlvfound | The total number of context report messages on the the R4 interface with duplicate TLVs. | Int32
r4contextrepo-nosessfound | The total number of context report messages on the the R4 interface without any session information. | Int32
r4contextrepo-adminprohib | The total number of context report messages discarded or denied due to admin prohibit. Triggers: Changes every time a context report message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4contextrepo-noresourcedrop | The total number of context report messages discarded or denied due to resource unavailability. Triggers: Changes every time a context report message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4contextrepo-transiderr | The total number of context report messages on the the R4 interface with transaction ID errors. | Int32
r4contextack-totsent | The total number of context acknowledgement messages sent on the the R4 interface. | Int32
r4contextack-retranssent | The total number of context acknowledgement messages re-transmitted on the the R4 interface. | Int32
r4contextack-totsendfail | The total number of failures occurred during transaction ID generation and R4 Context acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4contextack-totrec | The total number of context acknowledgement messages received on the the R4 interface. | Int32
r4contextack-totacc | The total number of context acknowledgement messages accepted on the the R4 interface. | Int32
r4contextack-totrelay | The total number of context acknowledgement messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a context acknowledgement message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4contextack-totdenied | The total number of context acknowledgement messages denied on the the R4 interface. | Int32
r4contextack-totdiscard | The total number of context acknowledgement messages discarded on the the R4 interface. | Int32
r4contextack-badform | The total number of badly formed context acknowledgement messages on the the R4 interface. | Int32
r4contextack-decodeerr | The total number of context acknowledgement messages on the the the R4 interface with decode error. | Int32
r4contextack-unspecerr | The total number of context acknowledgement messages on the the the R4 interface with unspecified error. | Int32
r4contextack-missmandtlv | The total number of context acknowledgement messages on the the the R4 interface with missing mandatory TLVs. | Int32
r4contextack-tlvvalinval | The total number of context acknowledgement messages on the the the R4 interface with invalid TLV value. | Int32
r4contextack-unknowntlv | The total number of context acknowledgement messages on the the the R4 interface with unknown TLVs. | Int32
r4contextack-duptlvfound | The total number of context acknowledgement messages on the the the R4 interface with duplicate TLVs. | Int32
r4contextack-nosessfound | The total number of context acknowledgement messages on the the the R4 interface without any session information. | Int32
r4contextack-adminprohib | The total number of context acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a context acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4contextack-noresourcedrop | The total number of context acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a context acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4contextack-transiderr | The total number of context acknowledgement messages on the the the R4 interface with transaction ID errors. | Int32
r4autheaptra-totsent | The total number of authentication EAP transfer messages sent on the the the R4 interface. | Int32
r4autheaptra-retranssent | The total number of authentication EAP transfer messages re-transmitted on the the the R4 interface. | Int32
r4autheaptra-totsendfail | The total number of failures that occurred during transaction ID generation and R4 EAP transfer message failure. This counter is used to count the error while sending the R4 packets. | Int32
r4autheaptra-totrec | The total number of authentication EAP transfer messages received on the the the R4 interface. | Int32
r4autheaptra-totacc | The total number of authentication EAP transfer messages accepted on the the the R4 interface. | Int32
r4autheaptra-totrelay | The total number of authentication EAP transfer messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time an authentication EAP transfer message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4autheaptra-totdenied | The total number of authentication EAP transfer messages denied on the the the R4 interface. | Int32
r4autheaptra-totdiscard | The total number of authentication EAP transfer messages discarded on the the the R4 interface. | Int32
r4autheaptra-badform | The total number of badly formed authentication EAP transfer messages on the the the R4 interface. | Int32
r4autheaptra-decodeerr | The total number of authentication EAP transfer messages on the the R4 interface with decode error. | Int32
r4autheaptra-unspecerr | The total number of authentication EAP transfer messages on the the R4 interface with unspecified error. | Int32
r4autheaptra-missmandtlv | The total number of authentication EAP transfer messages on the the R4 interface with missing mandatory TLVs. | Int32
r4autheaptra-tlvvalinval | The total number of authentication EAP transfer messages on the the R4 interface with invalid TLV value. | Int32
r4autheaptra-unknowntlv | The total number of authentication EAP transfer messages on the the R4 interface with unknown TLVs. | Int32
r4autheaptra-duptlvfound | The total number of authentication EAP transfer messages on the the R4 interface with duplicate TLVs. | Int32
r4autheaptra-nosessfound | The total number of authentication EAP transfer messages on the the R4 interface without any session information. | Int32
r4autheaptra-adminprohib | The total number of authentication EAP transfer messages on the the R4 interface discarded or denied due to admin prohibit. | Int32
r4autheaptra-noresourcedrop | The total number of authentication EAP transfer messages on the the R4 interface discarded or denied due to resource unavailability. | Int32
r4autheaptra-transiderr | The total number of authentication EAP transfer messages on the the R4 interface with transaction ID errors. | Int32
r4autheapsta-totrec | The total number of authentication EAP start messages sent on the the R4 interface. | Int32
r4autheapsta-totacc | The total number of authentication EAP start messages accepted on the the R4 interface. | Int32
r4autheapsta-totrelay | The total number of authentication EAP start messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time an authentication EAP start message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4autheapsta-totdenied | The total number of authentication EAP start messages denied on the the R4 interface. | Int32
r4autheapsta-totdiscard | The total number of authentication EAP start messages discarded on the the R4 interface. | Int32
r4autheapsta-badform | The total number of badly formed authentication EAP start messages on the the R4 interface. | Int32
r4autheapsta-decodeerr | The total number of authentication EAP start messages on the the R4 interface with decode error. | Int32
r4autheapsta-unspecerr | The total number of authentication EAP start messages on the the R4 interface with unspecified error. | Int32
r4autheapsta-missmandtlv | The total number of authentication EAP start messages on the the R4 interface with missing mandatory TLVs. | Int32
r4autheapsta-tlvvalinval | The total number of authentication EAP start messages on the the R4 interface with invalid TLV value. | Int32
r4autheapsta-unknowntlv | The total number of authentication EAP start messages on the the R4 interface with unknown TLVs. | Int32
r4autheapsta-duptlvfound | The total number of authentication EAP start messages on the the R4 interface with duplicate TLVs. | Int32
r4autheapsta-nosessfound | The total number of authentication EAP start messages on the the R4 interface without any session information. | Int32
r4autheapsta-adminprohib | The total number of authentication EAP start messages discarded or denied due to admin prohibit. Triggers: Changes every time an authentication EAP start message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4autheapsta-noresourcedrop | The total number of authentication EAP start messages discarded or denied due to resource unavailability. Triggers: Changes every time an authentication EAP start message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4autheapsta-transiderr | The total number of authentication EAP start messages on the the R4 interface with transaction ID errors. | Int32
r4datapathpreregreq-totsent | The total number of data path pre-registration request messages sent on the the R4 interface. | Int32
r4datapathpreregreq-retranssent | The total number of data path pre-registration request messages re-transmitted on the the R4 interface. | Int32
r4datapathpreregreq-totsendfail | The total number of failures occurred during transaction ID generation and R4 data path pre-registration request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathpreregreq-totrec | The total number of data path pre-registration request messages received on the the R4 interface. | Int32
r4datapathpreregreq-totacc | The total number of data path pre-registration request messages accepted on the the R4 interface. | Int32
r4datapathpreregreq-totrelay | The total number of data path pre-registration request messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a data path pre-registration request message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathpreregreq-totdenied | The total number of data path pre-registration request messages denied on the the R4 interface. | Int32
r4datapathpreregreq-totdiscard | The total number of data path pre-registration request messages discarded on the the R4 interface. | Int32
r4datapathpreregreq-badform | The total number of badly formed data path pre-registration request messages on the the R4 interface. | Int32
r4datapathpreregreq-decodeerr | The total number of data path pre-registration request messages on the the R4 interface with decode error. | Int32
r4datapathpreregreq-unspecerr | The total number of data path pre-registration request messages on the the R4 interface with unspecified error. | Int32
r4datapathpreregreq-missmandtlv | The total number of data path pre-registration request messages on the the R4 interface with missing mandatory TLVs. | Int32
r4datapathpreregreq-tlvvalinval | The total number of data path pre-registration request messages on the the R4 interface with invalid TLV value. | Int32
r4datapathpreregreq-unknowntlv | The total number of data path pre-registration request messages on the the R4 interface with unknown TLVs. | Int32
r4datapathpreregreq-duptlvfound | The total number of data path pre-registration request messages on the the R4 interface with duplicate TLVs. | Int32
r4datapathpreregreq-nosessfound | The total number of data path pre-registration request messages on the the R4 interface without any session information. | Int32
r4datapathpreregreq-adminprohib | The total number of data path pre-registration request messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path pre-registration request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathpreregreq-noresourcedrop | The total number of data path pre-registration request messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path pre-registration request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4datapathpreregreq-transiderr | The total number of data path pre-registration request messages on the the R4 interface with transaction ID errors. | Int32
r4datapathpreregrsp-totsent | The total number of data path pre-registration response messages sent on the the R4 interface. | Int32
r4datapathpreregrsp-retranssent | The total number of data path pre-registration response messages re-transmitted on the the R4 interface. | Int32
r4datapathpreregrsp-totsendfail | The total number of failures occurred during transaction ID generation and R4 data path pre-registration response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathpreregrsp-totrec | The total number of data path pre-registration response messages received on the the R4 interface. | Int32
r4datapathpreregrsp-totacc | The total number of data path pre-registration response messages accepted on the the R4 interface. | Int32
r4datapathpreregrsp-totrelay | The total number of data path pre-registration response messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a data path pre-registration response message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathpreregrsp-totdenied | The total number of data path pre-registration response messages denied on the the R4 interface. | Int32
r4datapathpreregrsp-totdiscard | The total number of data path pre-registration response messages discarded on the the R4 interface. | Int32
r4datapathpreregrsp-badform | The total number of badly formed data path pre-registration response messages on the the R4 interface. | Int32
r4datapathpreregrsp-decodeerr | The total number of data path pre-registration response messages on the the R4 interface with decode error. | Int32
r4datapathpreregrsp-unspecerr | The total number of data path pre-registration response messages on the the R4 interface with unspecified error. | Int32
r4datapathpreregrsp-missmandtlv | The total number of data path pre-registration response messages on the the R4 interface with missing mandatory TLVs. | Int32
r4datapathpreregrsp-tlvvalinval | The total number of data path pre-registration response messages on the the R4 interface with invalid TLV value. | Int32
r4datapathpreregrsp-unknowntlv | The total number of data path pre-registration response messages on the the R4 interface with unknown TLVs. | Int32
r4datapathpreregrsp-duptlvfound | The total number of data path pre-registration response messages on the the R4 interface with duplicate TLVs. | Int32
r4datapathpreregrsp-nosessfound | The total number of data path pre-registration response messages on the the R4 interface without any session information. | Int32
r4datapathpreregrsp-adminprohib | The total number of data path pre-registration response messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path pre-registration response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathpreregrsp-noresourcedrop | The total number of data path pre-registration response messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path pre-registration response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4datapathpreregrsp-transiderr | The total number of data path pre-registration response messages on the the R4 interface with transaction ID errors. | Int32
r4datapathpreregack-totsent | The total number of data path pre-registration acknowledgement messages sent on the the R4 interface. | Int32
r4datapathpreregack-retranssent | The total number of data path pre-registration acknowledgement messages re-transmitted on the the R4 interface. | Int32
r4datapathpreregack-totsendfail | The total number of failures occurred during transaction ID generation and R4 data path pre-registration acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathpreregack-totrec | The total number of data path pre-registration acknowledgement messages received on the the R4 interface. | Int32
r4datapathpreregack-totacc | The total number of data path pre-registration acknowledgement messages accepted on the the R4 interface. | Int32
r4datapathpreregack-totrelay | The total number of data path pre-registration acknowledgement messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a data path pre-registration acknowledgement message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathpreregack-totdenied | The total number of data path pre-registration acknowledgement messages denied on the the R4 interface. | Int32
r4datapathpreregack-totdiscard | The total number of data path pre-registration acknowledgement messages discarded on the the R4 interface. | Int32
r4datapathpreregack-badform | The total number of badly formed data path pre-registration acknowledgement messages on the the R4 interface. | Int32
r4datapathpreregack-decodeerr | The total number of data path pre-registration acknowledgement messages on the the R4 interface with decode error. | Int32
r4datapathpreregack-unspecerr | The total number of data path pre-registration acknowledgement messages on the the R4 interface with unspecified error. | Int32
r4datapathpreregack-missmandtlv | The total number of data path pre-registration acknowledgement messages on the the R4 interface with missing mandatory TLVs. | Int32
r4datapathpreregack-tlvvalinval | The total number of data path pre-registration acknowledgement messages on the the R4 interface with invalid TLV value. | Int32
r4datapathpreregack-unknowntlv | The total number of data path pre-registration acknowledgement messages on the the R4 interface with unknown TLVs. | Int32
r4datapathpreregack-duptlvfound | The total number of data path pre-registration acknowledgement messages on the the R4 interface with duplicate TLVs. | Int32
r4datapathpreregack-nosessfound | The total number of data path pre-registration acknowledgement messages on the the R4 interface without any session information. | Int32
r4datapathpreregack-adminprohib | The total number of data path pre-registration acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path pre-registration acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathpreregack-noresourcedrop | The total number of data path pre-registration acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path pre-registration acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4datapathpreregack-transiderr | The total number of data path pre-registration acknowledgement messages on the the R4 interface with transaction ID errors. | Int32
r4datapathregreq-totsent | The total number of data path registration request messages sent on the the R4 interface. | Int32
r4datapathregreq-retranssent | The total number of data path registration request messages re-transmitted on the the R4 interface. | Int32
r4datapathregreq-totsendfail | The total number of failures occurred during transaction ID generation and R4 data path registration request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathregreq-totrec | The total number of data path registration request messages received on the the R4 interface. | Int32
r4datapathregreq-totacc | The total number of data path registration request messages accepted on the the R4 interface. | Int32
r4datapathregreq-totrelay | The total number of data path registration request messages received from the base station and relayed on the the the R4 interface. Triggers: Changes every time a data path registration request message is relayed by the the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathregreq-totdenied | The total number of data path registration request messages denied on the the R4 interface. | Int32
r4datapathregreq-totdiscard | The total number of data path registration request messages discarded on the the R4 interface. | Int32
r4datapathregreq-badform | The total number of badly formed data path registration request messages on the the R4 interface. | Int32
r4datapathregreq-decodeerr | The total number of data path registration request messages on the the R4 interface with decode error. | Int32
r4datapathregreq-unspecerr | The total number of data path registration request messages on the R4 interface with unspecified error. | Int32
r4datapathregreq-missmandtlv | The total number of data path registration request messages on the R4 interface with missing mandatory TLVs. | Int32
r4datapathregreq-tlvvalinval | The total number of data path registration request messages on the R4 interface with invalid TLV value. | Int32
r4datapathregreq-unknowntlv | The total number of data path registration request messages on the R4 interface with unknown TLVs. | Int32
r4datapathregreq-duptlvfound | The total number of data path registration request messages on the R4 interface with duplicate TLVs. | Int32
r4datapathregreq-nosessfound | The total number of data path registration request messages on the R4 interface without any session information. | Int32
r4datapathregreq-adminprohib | The total number of data path registration request messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path registration request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathregreq-noresourcedrop | The total number of data path registration request messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path registration request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r4datapathregreq-transiderr | The total number of data path registration request messages on the R4 interface with transaction ID errors. | Int32
r4datapathregrsp-totsent | The total number of data path registration response messages sent on the R4 interface. | Int32
r4datapathregrsp-retranssent | The total number of data path registration response messages re-transmitted on the R4 interface. | Int32
r4datapathregrsp-totsendfail | The total number of failures occurred during transaction ID generation and R4 data path registration response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathregrsp-totrec | The total number of data path registration response messages received on the R4 interface. | Int32
r4datapathregrsp-totacc | The total number of data path registration response messages accepted on the R4 interface. | Int32
r4datapathregrsp-totrelay | The total number of data path registration response messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a data path registration response message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathregrsp-totdenied | The total number of data path registration response messages denied on the R4 interface. | Int32
r4datapathregrsp-totdiscard | The total number of data path registration response messages discarded on the R4 interface. | Int32
r4datapathregrsp-badform | The total number of badly formed data path registration response messages on the R4 interface. | Int32
r4datapathregrsp-decodeerr | The total number of data path registration response messages on the R4 interface with decode error. | Int32
r4datapathregrsp-unspecerr | The total number of data path registration response messages on the R4 interface with unspecified error. | Int32
r4datapathregrsp-missmandtlv | The total number of data path registration response messages on the R4 interface with missing mandatory TLVs. | Int32
r4datapathregrsp-tlvvalinval | The total number of data path registration response messages on the R4 interface with invalid TLV value. | Int32
r4datapathregrsp-unknowntlv | The total number of data path registration response messages on the R4 interface with unknown TLVs. | Int32
r4datapathregrsp-duptlvfound | The total number of data path registration response messages on the R4 interface with duplicate TLVs. | Int32
r4datapathregrsp-nosessfound | The total number of data path registration response messages on the R4 interface without any session information. | Int32
r4datapathregrsp-adminprohib | The total number of data path registration response messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path registration response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathregrsp-noresourcedrop | The total number of data path registration response messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path registration response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4datapathregrsp-transiderr | The total number of data path registration response messages on the R4 interface with transaction ID errors. | Int32
r4datapathregack-totsent | The total number of data path registration acknowledgement messages sent on the R4 interface. | Int32
r4datapathregack-retranssent | The total number of data path registration acknowledgement messages re-transmitted on the R4 interface. | Int32
r4datapathregack-totsendfail | The total number of failures occurred during transaction id generation and R4 data path registration acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathregack-totrec | The total number of data path registration acknowledgement messages received on the R4 interface. | Int32
r4datapathregack-totacc | The total number of data path registration acknowledgement messages accepted on the R4 interface. | Int32
r4datapathregack-totrelay | The total number of data path registration acknowledgement messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a data path registration acknowledgement message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathregack-totdenied | The total number of data path registration acknowledgement messages denied on the R4 interface. | Int32
r4datapathregack-totdiscard | The total number of data path registration acknowledgement messages discarded on the R4 interface. | Int32
r4datapathregack-badform | The total number of badly formed data path registration acknowledgement messages on the R4 interface. | Int32
r4datapathregack-decodeerr | The total number of data path registration acknowledgement messages on the R4 interface with decode error. | Int32
r4datapathregack-unspecerr | The total number of data path registration acknowledgement messages on the R4 interface with unspecified error. | Int32
r4datapathregack-missmandtlv | The total number of data path registration acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4datapathregack-tlvvalinval | The total number of data path registration acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4datapathregack-unknowntlv | The total number of data path registration acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4datapathregack-duptlvfound | The total number of data path registration acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4datapathregack-nosessfound | The total number of data path registration acknowledgement messages on the R4 interface without any session information. | Int32
r4datapathregack-adminprohib | The total number of data path registration acknowledgement messages denied on the R4 interface. | Int32
r4datapathregack-noresourcedrop | The total number of data path registration acknowledgement messages discarded or denied due on the R4 interface to resource unavailability. | Int32
r4datapathregack-transiderr | The total number of data path registration acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4pathmodreq-totsent | The total number of data path modification request messages sent on the R4 interface. | Int32
r4pathmodreq-retranssent | The total number of data path modification request messages re-transmitted on the R4 interface. | Int32
r4pathmodreq-totsendfail | The total number of failed data path modification requests that occurred. This counter is used to count the error while sending the R4 packets. | Int32
r4pathmodreq-totrec | The total number of data path modification request messages received on the R4 interface. | Int32
r4pathmodreq-totacc | The total number of data path modification request messages accepted on the R4 interface. | Int32
r4pathmodreq-totrelay | The total number of data path modification request messages received from the base station and relayed on the the R4 interface. | Int32
r4pathmodreq-totdenied | The total number of data path modification request messages denied on the R4 interface. | Int32
r4pathmodreq-totdiscard | The total number of data path modification request messages discarded on the R4 interface. | Int32
r4pathmodreq-badform | The total number of badly formed data path modification request messages on the R4 interface. | Int32
r4pathmodreq-decodeerr | The total number of data path modification request messages on the R4 interface with decode error. | Int32
r4pathmodreq-unspecerr | The total number of data path modification request messages on the R4 interface with unspecified error. | Int32
r4pathmodreq-missmandtlv | The total number of data path modification request messages on the R4 interface with missing mandatory TLVs. | Int32
r4pathmodreq-tlvvalinval | The total number of data path modification request messages on the R4 interface with invalid TLV value. | Int32
r4pathmodreq-unknowntlv | The total number of data path modification request messages on the R4 interface with unknown TLVs. | Int32
r4pathmodreq-duptlvfound | The total number of data path modification request messages on the R4 interface with duplicate TLVs. | Int32
r4pathmodreq-nosessfound | The total number of data path modification request messages on the R4 interface without any session information. | Int32
r4pathmodreq-adminprohib | The total number of administratively prohibited data path modification request messages on the R4 interface. | Int32
r4pathmodreq-noresourcedrop | The total number of data path modification request messages discarded or denied on the R4 interface due to a lack of resources. | Int32
r4pathmodreq-transiderr | The total number of data path modification request messages on the R4 interface with transaction ID errors. | Int32
r4pathmodrsp-totsent | The total number of data path modification response messages sent on the R4 interface. | Int32
r4pathmodrsp-retranssent | The total number of data path modification response messages re-transmitted on the R4 interface. | Int32
r4pathmodrsp-totsendfail | The total number of failed data path modification response that occurred. This counter is used to count the error while sending the R4 packets. | Int32
r4pathmodrsp-totrec | The total number of data path modification response messages received on the R4 interface. | Int32
r4pathmodrsp-totacc | The total number of data path modification response messages accepted on the R4 interface. | Int32
r4pathmodrsp-totrelay | The total number of data path modification response messages received from the base station and relayed on the the R4 interface. | Int32
r4pathmodrsp-totdenied | The total number of data path modification response messages denied on the R4 interface. | Int32
r4pathmodrsp-totdiscard | The total number of data path modification response messages discarded on the R4 interface. | Int32
r4pathmodrsp-badform | The total number of badly formed data path modification response messages on the R4 interface. | Int32
r4pathmodrsp-decodeerr | The total number of data path modification response messages on the R4 interface with decode error. | Int32
r4pathmodrsp-unspecerr | The total number of data path modification response messages on the R4 interface with unspecified error. | Int32
r4pathmodrsp-missmandtlv | The total number of data path modification response messages on the R4 interface with missing mandatory TLVs. | Int32
r4pathmodrsp-tlvvalinval | The total number of data path modification response messages on the R4 interface with invalid TLV value. | Int32
r4pathmodrsp-unknowntlv | The total number of data path modification response messages on the R4 interface with unknown TLVs. | Int32
r4pathmodrsp-duptlvfound | The total number of data path modification response messages on the R4 interface with duplicate TLVs. | Int32
r4pathmodrsp-nosessfound | The total number of data path modification response messages on the R4 interface without any session information. | Int32
r4pathmodrsp-adminprohib | The total number of administratively prohibited data path modification response messages on the R4 interface. | Int32
r4pathmodrsp-noresourcedrop | The total number of data path modification response messages discarded or denied on the R4 interface due to resource unavailability. | Int32
r4pathmodrsp-transiderr | The total number of data path modification response messages on the R4 interface with transaction ID errors. | Int32
r4pathmodack-totsent | The total number of data path modification acknowledgement messages sent on the R4 interface. | Int32
r4pathmodack-retranssent | The total number of data path modification acknowledgement messages re-transmitted on the R4 interface. | Int32
r4pathmodack-totsendfail | The total number of failed data path modification acknowledgement that occurred. This counter is used to count the error while sending the R4 packets. | Int32
r4pathmodack-totrec | The total number of data path modification acknowledgement messages received on the R4 interface. | Int32
r4pathmodack-totacc | The total number of data path modification acknowledgement messages accepted on the R4 interface. | Int32
r4pathmodack-totrelay | The total number of data path modification acknowledgement messages received from the base station and relayed on the the R4 interface. | Int32
r4pathmodack-totdenied | The total number of data path modification acknowledgement messages denied on the R4 interface. | Int32
r4pathmodack-totdiscard | The total number of data path modification acknowledgement messages discarded on the R4 interface. | Int32
r4pathmodack-badform | The total number of badly formed data path modification acknowledgement messages on the R4 interface. | Int32
r4pathmodack-decodeerr | The total number of data path modification acknowledgement messages on the R4 interface with decode error. | Int32
r4pathmodack-unspecerr | The total number of data path modification acknowledgement messages on the R4 interface with unspecified error. | Int32
r4pathmodack-missmandtlv | The total number of data path modification acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4pathmodack-tlvvalinval | The total number of data path modification acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4pathmodack-unknowntlv | The total number of data path modification acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4pathmodack-duptlvfound | The total number of data path modification acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4pathmodack-nosessfound | The total number of data path modification acknowledgement messages on the R4 interface without any session information. | Int32
r4pathmodack-adminprohib | The total number of administratively prohibited data path modification acknowledgement messages on the R4 interface. | Int32
r4pathmodack-noresourcedrop | The total number of data path modification acknowledgement messages discarded or denied on the R4 interface due to resource unavailability. | Int32
r4pathmodack-transiderr | The total number of data path modification acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4datapathderegreq-totsent | The total number of data path deregistration request messages sent on the R4 interface. | Int32
r4datapathderegreq-retranssent | The total number of data path deregistration request messages re-transmitted on the R4 interface. | Int32
r4datapathderegreq-totsendfail | The total number of failures occurred during transaction id generation and R4 data path de-registration request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathderegreq-totrec | The total number of data path deregistration request messages received on the R4 interface. | Int32
r4datapathderegreq-totacc | The total number of data path deregistration request messages accepted on the R4 interface. | Int32
r4datapathderegreq-totrelay | The total number of data path de-registration request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a data path de-registration request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathderegreq-totdenied | The total number of data path deregistration request messages denied on the R4 interface. | Int32
r4datapathderegreq-totdiscard | The total number of data path deregistration request messages discarded on the R4 interface. | Int32
r4datapathderegreq-badform | The total number of badly formed data path deregistration request messages on the R4 interface. | Int32
r4datapathderegreq-decodeerr | The total number of data path deregistration request messages on the R4 interface with decode error. | Int32
r4datapathderegreq-unspecerr | The total number of data path deregistration request messages on the R4 interface with unspecified error. | Int32
r4datapathderegreq-missmandtlv | The total number of data path deregistration request messages on the R4 interface with missing mandatory TLVs. | Int32
r4datapathderegreq-tlvvalinval | The total number of data path deregistration request messages on the R4 interface with invalid TLV value. | Int32
r4datapathderegreq-unknowntlv | The total number of data path deregistration request messages on the R4 interface with unknown TLVs. | Int32
r4datapathderegreq-duptlvfound | The total number of data path deregistration request messages on the R4 interface with duplicate TLVs. | Int32
r4datapathderegreq-nosessfound | The total number of data path deregistration request messages on the R4 interface without any session information. | Int32
r4datapathderegreq-adminprohib | The total number of data path de-registration request messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path de-registration request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathderegreq-noresourcedrop | The total number of data path de-registration request messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path de-registration request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4datapathderegreq-transiderr | The total number of data path deregistration request messages on the R4 interface with transaction ID errors. | Int32
r4datapathderegrsp-totsent | The total number of data path deregistration response messages sent on the R4 interface. | Int32
r4datapathderegrsp-retranssent | The total number of data path deregistration response messages re-transmitted on the R4 interface. | Int32
r4datapathderegrsp-totsendfail | The total number of failures occurred during transaction id generation and R4 data path de-registration response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathderegrsp-totrec | The total number of data path deregistration response messages received on the R4 interface. | Int32
r4datapathderegrsp-totacc | The total number of data path deregistration response messages accepted on the R4 interface. | Int32
r4datapathderegrsp-totrelay | The total number of data path de-registration response messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a data path de-registration response message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4datapathderegrsp-totdenied | The total number of data path deregistration response messages denied on the R4 interface. | Int32
r4datapathderegrsp-totdiscard | The total number of data path deregistration response messages discarded on the R4 interface. | Int32
r4datapathderegrsp-badform | The total number of badly formed data path deregistration response messages on the R4 interface. | Int32
r4datapathderegrsp-decodeerr | The total number of data path deregistration response messages on the R4 interface with decode error. | Int32
r4datapathderegrsp-unspecerr | The total number of data path deregistration response messages on the R4 interface with unspecified error. | Int32
r4datapathderegrsp-missmandtlv | The total number of data path deregistration response messages on the R4 interface with missing mandatory TLVs. | Int32
r4datapathderegrsp-tlvvalinval | The total number of data path deregistration response messages on the R4 interface with invalid TLV value. | Int32
r4datapathderegrsp-unknowntlv | The total number of data path deregistration response messages on the R4 interface with unknown TLVs. | Int32
r4datapathderegrsp-duptlvfound | The total number of data path deregistration response messages on the R4 interface with duplicate TLVs. | Int32
r4datapathderegrsp-nosessfound | The total number of data path deregistration response messages on the R4 interface without any session information. | Int32
r4datapathderegrsp-adminprohib | The total number of data path de-registration response messages discarded or denied due to admin prohibit. Triggers: Changes every time a data path de-registration response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathderegrsp-noresourcedrop | The total number of data path de-registration response messages discarded or denied due to resource unavailability. Triggers: Changes every time a data path de-registration response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4datapathderegrsp-transiderr | The total number of data path deregistration response messages on the R4 interface with transaction ID errors. | Int32
r4keychadir-totsent | The total number of key change directive messages sent on the R4 interface. | Int32
r4keychadir-retranssent | The total number of key change directive messages re-transmitted on the R4 interface. | Int32
r4keychadir-totsendfail | The total number of failures occurred during transaction id generation and R4 Key Change Directive message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4keychadir-totrec | The total number of key change directive messages received on the R4 interface. | Int32
r4keychadir-totacc | The total number of key change directive messages accepted on the R4 interface. | Int32
r4keychadir-totrelay | The total number of key change directive messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a key change directive message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4keychadir-totdenied | The total number of key change directive messages denied on the R4 interface. | Int32
r4keychadir-totdiscard | The total number of key change directive messages discarded on the R4 interface. | Int32
r4keychadir-badform | The total number of badly formed key change directive messages on the R4 interface. | Int32
r4keychadir-decodeerr | The total number of key change directive messages on the R4 interface with decode error. | Int32
r4keychadir-unspecerr | The total number of key change directive messages on the R4 interface with unspecified error. | Int32
r4keychadir-missmandtlv | The total number of key change directive messages on the R4 interface with missing mandatory TLVs. | Int32
r4keychadir-tlvvalinval | The total number of key change directive messages on the R4 interface with invalid TLV value. | Int32
r4keychadir-unknowntlv | The total number of key change directive messages on the R4 interface with unknown TLVs. | Int32
r4keychadir-duptlvfound | The total number of key change directive messages on the R4 interface with duplicate TLVs. | Int32
r4keychadir-nosessfound | The total number of key change directive messages on the R4 interface without any session information. | Int32
r4keychadir-adminprohib | The total number of key change directive messages discarded or denied due to admin prohibit. Triggers: Changes every time a key change directive message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4keychadir-noresourcedrop | The total number of key change directive messages discarded or denied due to resource unavailability. Triggers: Changes every time a key change directive message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4keychadir-transiderr | The total number of key change directive messages on the R4 interface with transaction ID errors. | Int32
r4keychaack-totsent | The total number of key change acknowledgement messages sent on the R4 interface. | Int32
r4keychaack-retranssent | The total number of key change acknowledgement messages re-transmitted on the R4 interface. | Int32
r4keychaack-totsendfail | The total number of failures occurred during transaction id generation and R4 Key Change acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4keychaack-totrec | The total number of key change acknowledgement messages received on the R4 interface. | Int32
r4keychaack-totacc | The total number of key change acknowledgement messages accepted on the R4 interface. | Int32
r4keychaack-totrelay | The total number of key change acknowledgement messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a key change acknowledgement message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4keychaack-totdenied | The total number of key change acknowledgement messages denied on the R4 interface. | Int32
r4keychaack-totdiscard | The total number of key change acknowledgement messages discarded on the R4 interface. | Int32
r4keychaack-badform | The total number of badly formed key change acknowledgement messages on the R4 interface. | Int32
r4keychaack-decodeerr | The total number of key change acknowledgement messages on the R4 interface with decode error. | Int32
r4keychaack-unspecerr | The total number of key change acknowledgement messages on the R4 interface with unspecified error. | Int32
r4keychaack-missmandtlv | The total number of key change acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4keychaack-tlvvalinval | The total number of key change acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4keychaack-unknowntlv | The total number of key change acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4keychaack-duptlvfound | The total number of key change acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4keychaack-nosessfound | The total number of key change acknowledgement messages on the R4 interface without any session information. | Int32
r4keychaack-adminprohib | The total number of key change acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a key change acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4keychaack-noresourcedrop | The total number of key change acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a key change acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4keychaack-transiderr | The total number of key change acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4keychacnf-totrec | The total number of key change confirm messages received on the R4 interface. | Int32
r4keychacnf-totacc | The total number of key change confirm messages accepted on the R4 interface. | Int32
r4keychacnf-totrelay | The total number of key change confirm messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a key change confirm message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4keychacnf-totdenied | The total number of key change confirm messages denied on the R4 interface. | Int32
r4keychacnf-totdiscard | The total number of key change confirm messages discarded on the R4 interface. | Int32
r4keychacnf-badform | The total number of badly formed key change confirm messages on the R4 interface. | Int32
r4keychacnf-decodeerr | The total number of key change confirm messages on the R4 interface with decode error. | Int32
r4keychacnf-unspecerr | The total number of key change confirm messages on the R4 interface with unspecified error. | Int32
r4keychacnf-missmandtlv | The total number of key change confirm messages on the R4 interface with missing mandatory TLVs. | Int32
r4keychacnf-tlvvalinval | The total number of key change confirm messages on the R4 interface with invalid TLV value. | Int32
r4keychacnf-unknowntlv | The total number of key change confirm messages on the R4 interface with unknown TLVs. | Int32
r4keychacnf-duptlvfound | The total number of key change confirm messages on the R4 interface with duplicate TLVs. | Int32
r4keychacnf-nosessfound | The total number of key change confirm messages on the R4 interface without any session information. | Int32
r4keychacnf-adminprohib | The total number of key change confirm messages discarded or denied due to admin prohibit. Triggers: Changes every time a key change confirm message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4keychacnf-noresourcedrop | The total number of key change confirm messages discarded or denied due to resource unavailability. Triggers: Changes every time a key change confirm message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4keychacnf-transiderr | The total number of key change confirm messages on the R4 interface with transaction ID errors. | Int32
r4cmackeycounupd-totsent | The total number of CMAC key count update messages sent on the R4 interface. | Int32
r4cmackeycounupd-retranssent | The total number of CMAC key count update messages re-transmitted on the R4 interface. | Int32
r4cmackeycounupd-totsendfail | The total number of failures occurred during transaction id generation and R4 CMAC key count update message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4cmackeycounupd-totrec | The total number of CMAC key count update messages received on the R4 interface. | Int32
r4cmackeycounupd-totacc | The total number of CMAC key count update messages accepted on the R4 interface. | Int32
r4cmackeycounupd-totrelay | The total number of CMAC key count update messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a CMAC key count update message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4cmackeycounupd-totdenied | The total number of CMAC key count update messages denied on the R4 interface. | Int32
r4cmackeycounupd-totdiscard | The total number of CMAC key count update messages discarded on the R4 interface. | Int32
r4cmackeycounupd-badform | The total number of badly formed CMAC key count update messages on the R4 interface. | Int32
r4cmackeycounupd-decodeerr | The total number of CMAC key count update messages on the R4 interface with decode error. | Int32
r4cmackeycounupd-unspecerr | The total number of CMAC key count update messages on the R4 interface with unspecified error. | Int32
r4cmackeycounupd-missmandtlv | The total number of CMAC key count update messages on the R4 interface with missing mandatory TLVs. | Int32
r4cmackeycounupd-tlvvalinval | The total number of CMAC key count update messages on the R4 interface with invalid TLV value. | Int32
r4cmackeycounupd-unknowntlv | The total number of CMAC key count update messages on the R4 interface with unknown TLVs. | Int32
r4cmackeycounupd-duptlvfound | The total number of CMAC key count update messages on the R4 interface with duplicate TLVs. | Int32
r4cmackeycounupd-nosessfound | The total number of CMAC key count update messages on the R4 interface without any session information. | Int32
r4cmackeycounupd-adminprohib | The total number of CMAC key count update messages discarded or denied due to admin prohibit. Triggers: Changes every time a CMAC key count update message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4cmackeycounupd-noresourcedrop | The total number of CMAC key count update messages discarded or denied due to resource unavailability. Triggers: Changes every time a CMAC key count update message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4cmackeycounupd-transiderr | The total number of CMAC key count update messages on the R4 interface with transaction ID errors. | Int32
r4cmackeycounack-totsent | The total number of CMAC key count acknowledgement messages sent on the R4 interface. | Int32
r4cmackeycounack-retranssent | The total number of CMAC key count acknowledgement messages re-transmitted on the R4 interface. | Int32
r4cmackeycounack-totsendfail | The total number of failures occurred during transaction id generation and R4 CMAC key count acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4cmackeycounack-totrec | The total number of CMAC key count acknowledgement messages received on the R4 interface. | Int32
r4cmackeycounack-totacc | The total number of CMAC key count acknowledgement messages accepted on the R4 interface. | Int32
r4cmackeycounack-totrelay | The total number of CMAC key count acknowledgement messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time a CMAC key count acknowledgement message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4cmackeycounack-totdenied | The total number of CMAC key count acknowledgement messages denied on the R4 interface. | Int32
r4cmackeycounack-totdiscard | The total number of CMAC key count acknowledgement messages discarded on the R4 interface. | Int32
r4cmackeycounack-badform | The total number of badly formed CMAC key count acknowledgement messages on the R4 interface. | Int32
r4cmackeycounack-decodeerr | The total number of CMAC key count acknowledgement messages on the R4 interface with decode error. | Int32
r4cmackeycounack-unspecerr | The total number of CMAC key count acknowledgement messages on the R4 interface with unspecified error. | Int32
r4cmackeycounack-missmandtlv | The total number of CMAC key count acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4cmackeycounack-tlvvalinval | The total number of CMAC key count acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4cmackeycounack-unknowntlv | The total number of CMAC key count acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4cmackeycounack-duptlvfound | The total number of CMAC key count acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4cmackeycounack-nosessfound | The total number of CMAC key count acknowledgement messages on the R4 interface without any session information. | Int32
r4cmackeycounack-adminprohib | The total number of CMAC key count acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a CMAC key count acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4cmackeycounack-noresourcedrop | The total number of CMAC key count acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a CMAC key count acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4cmackeycounack-transiderr | The total number of CMAC key count acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4imentstachareq-totsent | The total number of R4 idle mode entry MS state change request messages sent on the R4 interface. | Int32
r4imentstachareq-retranssent | The total number of R4 idle mode entry MS state change request messages re-transmitted on the R4 interface. | Int32
r4imentstachareq-totsendfail | The total number of failures occurred during transaction id generation and R4 idle mode entry MS state change request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imentstachareq-totrec | The total number of R4 idle mode entry MS state change request messages received on the R4 interface. | Int32
r4imentstachareq-totacc | The total number of R4 idle mode entry MS state change request messages accepted on the R4 interface. | Int32
r4imentstachareq-totrelay | The total number of R4 idle mode entry MS state change request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 idle mode entry MS state change request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4imentstachareq-totdenied | The total number of R4 idle mode entry MS state change request messages denied on the R4 interface. | Int32
r4imentstachareq-totdiscard | The total number of R4 idle mode entry MS state change request messages discarded on the R4 interface. | Int32
r4imentstachareq-badform | The total number of badly formed R4 idle mode entry MS state change request messages on the R4 interface. | Int32
r4imentstachareq-decodeerr | The total number of R4 idle mode entry MS state change request messages on the R4 interface with decode error. | Int32
r4imentstachareq-unspecerr | The total number of R4 idle mode entry MS state change request messages on the R4 interface with unspecified error. | Int32
r4imentstachareq-missmandtlv | The total number of R4 idle mode entry MS state change request messages on the R4 interface with missing mandatory TLVs. | Int32
r4imentstachareq-tlvvalinval | The total number of R4 idle mode entry MS state change request messages on the R4 interface with invalid TLV value. | Int32
r4imentstachareq-unknowntlv | The total number of R4 idle mode entry MS state change request messages on the R4 interface with unknown TLVs. | Int32
r4imentstachareq-duptlvfound | The total number of R4 idle mode entry MS state change request messages on the R4 interface with duplicate TLVs. | Int32
r4imentstachareq-nosessfound | The total number of R4 idle mode entry MS state change request messages on the R4 interface without any session information. | Int32
r4imentstachareq-adminprohib | The total number of R4 idle mode entry MS state change request messages discarded or denied due to admin prohibit. Triggers: Changes every time a R4 idle mode entry MS state change request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imentstachareq-noresourcedrop | The total number of R4 idle mode entry MS state change request messages discarded or denied due to resource unavailability. Triggers: Changes every time a R4 idle mode entry MS state change request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imentstachareq-transiderr | The total number of R4 idle mode entry MS state change request messages on the R4 interface with transaction ID errors. | Int32
r4imentstacharsp-totsent | The total number of R4 idle mode entry MS state change response messages sent on the R4 interface. | Int32
r4imentstacharsp-retranssent | The total number of R4 idle mode entry MS state change response messages re-transmitted on the R4 interface. | Int32
r4imentstacharsp-totsendfail | The total number of failures occurred during transaction id generation and R4 idle mode entry MS state change response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imentstacharsp-totrec | The total number of R4 idle mode entry MS state change response messages received on the R4 interface. | Int32
r4imentstacharsp-totacc | The total number of R4 idle mode entry MS state change response messages accepted on the R4 interface. | Int32
r4imentstacharsp-totrelay | The total number of R4 idle mode entry MS state change response messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 idle mode entry MS state change response message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4imentstacharsp-totdenied | The total number of R4 idle mode entry MS state change response messages denied on the R4 interface. | Int32
r4imentstacharsp-totdiscard | The total number of R4 idle mode entry MS state change response messages discarded on the R4 interface. | Int32
r4imentstacharsp-badform | The total number of badly formed R4 idle mode entry MS state change response messages on the R4 interface. | Int32
r4imentstacharsp-decodeerr | The total number of R4 idle mode entry MS state change response messages on the R4 interface with decode error. | Int32
r4imentstacharsp-unspecerr | The total number of R4 idle mode entry MS state change response messages on the R4 interface with unspecified error. | Int32
r4imentstacharsp-missmandtlv | The total number of R4 idle mode entry MS state change response messages on the R4 interface with missing mandatory TLVs. | Int32
r4imentstacharsp-tlvvalinval | The total number of R4 idle mode entry MS state change response messages on the R4 interface with invalid TLV value. | Int32
r4imentstacharsp-unknowntlv | The total number of R4 idle mode entry MS state change response messages on the R4 interface with unknown TLVs. | Int32
r4imentstacharsp-duptlvfound | The total number of R4 idle mode entry MS state change response messages on the R4 interface with duplicate TLVs. | Int32
r4imentstacharsp-nosessfound | The total number of R4 idle mode entry MS state change response messages on the R4 interface without any session information. | Int32
r4imentstacharsp-adminprohib | The total number of R4 idle mode entry MS state change response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 idle mode entry MS state change response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imentstacharsp-noresourcedrop | The total number of R4 idle mode entry MS state change response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 idle mode entry MS state change response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imentstacharsp-transiderr | The total number of R4 idle mode entry MS state change response messages on the R4 interface with transaction ID errors. | Int32
r4imentstachaack-totsent | The total number of R4 idle mode entry state change acknowledgement messages sent on the R4 interface. | Int32
r4imentstachaack-retranssent | The total number of R4 idle mode entry state change acknowledgement messages re-transmitted on the R4 interface. | Int32
r4imentstachaack-totsendfail | The total number of failures occurred during transaction id generation and R4 idle mode entry state change acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imentstachaack-totrec | The total number of R4 idle mode entry state change acknowledgement messages received on the R4 interface. | Int32
r4imentstachaack-totacc | The total number of R4 idle mode entry state change acknowledgement messages accepted on the R4 interface. | Int32
r4imentstachaack-totrelay | The total number of R4 idle mode entry state change acknowledgement messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 idle mode entry state change acknowledgement message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4imentstachaack-totdenied | The total number of R4 idle mode entry state change acknowledgement messages denied on the R4 interface. | Int32
r4imentstachaack-totdiscard | The total number of R4 idle mode entry state change acknowledgement messages discarded on the R4 interface. | Int32
r4imentstachaack-badform | The total number of badly formed R4 idle mode entry state change acknowledgement messages on the R4 interface. | Int32
r4imentstachaack-decodeerr | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with decode error. | Int32
r4imentstachaack-unspecerr | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with unspecified error. | Int32
r4imentstachaack-missmandtlv | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4imentstachaack-tlvvalinval | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4imentstachaack-unknowntlv | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4imentstachaack-duptlvfound | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4imentstachaack-nosessfound | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface without any session information. | Int32
r4imentstachaack-adminprohib | The total number of R4 idle mode entry state change acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 idle mode entry state change acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imentstachaack-noresourcedrop | The total number of R4 idle mode entry state change acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 idle mode entry state change acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imentstachaack-transiderr | The total number of R4 idle mode entry state change acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4anchorpcind-totsent | The total number of R4 anchor paging controller indicator messages sent on the R4 interface. | Int32
r4anchorpcind-retranssent | The total number of R4 anchor paging controller indicator messages re-transmitted on the R4 interface. | Int32
r4anchorpcind-totsendfail | The total number of failures occurred during transaction id generation and R4 anchor paging controller indicator message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4anchorpcind-totrec | The total number of R4 anchor paging controller indicator messages received on the R4 interface. | Int32
r4anchorpcind-totacc | The total number of R4 anchor paging controller indicator messages accepted on the R4 interface. | Int32
r4anchorpcind-totrelay | The total number of R4 anchor paging controller indicator messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 anchor paging controller indicator message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4anchorpcind-totdenied | The total number of R4 anchor paging controller indicator messages denied on the R4 interface. | Int32
r4anchorpcind-totdiscard | The total number of R4 anchor paging controller indicator messages discarded on the R4 interface. | Int32
r4anchorpcind-badform | The total number of badly formed R4 anchor paging controller indicator messages on the R4 interface. | Int32
r4anchorpcind-decodeerr | The total number of R4 anchor paging controller indicator messages on the R4 interface with decode error. | Int32
r4anchorpcind-unspecerr | The total number of R4 anchor paging controller indicator messages on the R4 interface with unspecified error. | Int32
r4anchorpcind-missmandtlv | The total number of R4 anchor paging controller indicator messages on the R4 interface with missing mandatory TLVs. | Int32
r4anchorpcind-tlvvalinval | The total number of R4 anchor paging controller indicator messages on the R4 interface with invalid TLV value. | Int32
r4anchorpcind-unknowntlv | The total number of R4 anchor paging controller indicator messages on the R4 interface with unknown TLVs. | Int32
r4anchorpcind-duptlvfound | The total number of R4 anchor paging controller indicator messages on the R4 interface with duplicate TLVs. | Int32
r4anchorpcind-nosessfound | The total number of R4 anchor paging controller indicator messages on the R4 interface without any session information. | Int32
r4anchorpcind-adminprohib | The total number of R4 anchor paging controller indicator messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 anchor paging controller indicator message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4anchorpcind-noresourcedrop | The total number of R4 anchor paging controller indicator messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 anchor paging controller indicator message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4anchorpcind-transiderr | The total number of R4 anchor paging controller indicator messages on the R4 interface with transaction ID errors. | Int32
r4anchorpcack-totsent | The total number of R4 anchor paging controller acknowledgement messages sent on the R4 interface. | Int32
r4anchorpcack-retranssent | The total number of R4 anchor paging controller acknowledgement messages re-transmitted on the R4 interface. | Int32
r4anchorpcack-totsendfail | The total number of failures occurred during transaction id generation and R4 anchor paging controller acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4anchorpcack-totrec | The total number of R4 anchor paging controller acknowledgement messages received on the R4 interface. | Int32
r4anchorpcack-totacc | The total number of R4 anchor paging controller acknowledgement messages accepted on the R4 interface. | Int32
r4anchorpcack-totrelay | The total number of R4 anchor paging controller acknowledgement messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 anchor paging controller acknowledgement message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4anchorpcack-totdenied | The total number of R4 anchor paging controller acknowledgement messages denied on the R4 interface. | Int32
r4anchorpcack-totdiscard | The total number of R4 anchor paging controller acknowledgement messages discarded on the R4 interface. | Int32
r4anchorpcack-badform | The total number of badly formed R4 anchor paging controller acknowledgement messages on the R4 interface. | Int32
r4anchorpcack-decodeerr | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with decode error. | Int32
r4anchorpcack-unspecerr | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with unspecified error. | Int32
r4anchorpcack-missmandtlv | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4anchorpcack-tlvvalinval | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4anchorpcack-unknowntlv | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4anchorpcack-duptlvfound | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4anchorpcack-nosessfound | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface without any session information. | Int32
r4anchorpcack-adminprohib | The total number of R4 anchor paging controller acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 anchor paging controller acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4anchorpcack-noresourcedrop | The total number of R4 anchor paging controller acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 anchor paging controller acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4anchorpcack-transiderr | The total number of R4 anchor paging controller acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4imexitstachareq-totsent | The total number of R4 idle mode exit MS state change request messages sent on the R4 interface. | Int32
r4imexitstachareq-retranssent | The total number of R4 idle mode exit MS state change request messages re-transmitted on the R4 interface. | Int32
r4imexitstachareq-totsendfail | The total number of failures occurred during transaction id generation and R4 idle mode exit MS state change request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imexitstachareq-totrec | The total number of R4 idle mode exit MS state change request messages received on the R4 interface. | Int32
r4imexitstachareq-totacc | The total number of R4 idle mode exit MS state change request messages accepted on the R4 interface. | Int32
r4imexitstachareq-totrelay | The total number of R4 idle mode exit MS state change request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 idle mode exit MS state change request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4imexitstachareq-totdenied | The total number of R4 idle mode exit MS state change request messages denied on the R4 interface. | Int32
r4imexitstachareq-totdiscard | The total number of R4 idle mode exit MS state change request messages discarded on the R4 interface. | Int32
r4imexitstachareq-badform | The total number of badly formed R4 idle mode exit MS state change request messages on the R4 interface. | Int32
r4imexitstachareq-decodeerr | The total number of R4 idle mode exit MS state change request messages on the R4 interface with decode error. | Int32
r4imexitstachareq-unspecerr | The total number of R4 idle mode exit MS state change request messages on the R4 interface with unspecified error. | Int32
r4imexitstachareq-missmandtlv | The total number of R4 idle mode exit MS state change request messages on the R4 interface with missing mandatory TLVs. | Int32
r4imexitstachareq-tlvvalinval | The total number of R4 idle mode exit MS state change request messages on the R4 interface with invalid TLV value. | Int32
r4imexitstachareq-unknowntlv | The total number of R4 idle mode exit MS state change request messages on the R4 interface with unknown TLVs. | Int32
r4imexitstachareq-duptlvfound | The total number of R4 idle mode exit MS state change request messages on the R4 interface with duplicate TLVs. | Int32
r4imexitstachareq-nosessfound | The total number of R4 idle mode exit MS state change request messages on the R4 interface without any session information. | Int32
r4imexitstachareq-adminprohib | The total number of R4 idle mode exit MS state change request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 idle mode exit MS state change request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imexitstachareq-noresourcedrop | The total number of R4 idle mode exit MS state change request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 idle mode exit MS state change request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imexitstachareq-transiderr | The total number of R4 idle mode exit MS state change request messages on the R4 interface with transaction ID errors. | Int32
r4imexitstacharsp-totsent | The total number of R4 idle mode exit MS state change response messages sent on the R4 interface. | Int32
r4imexitstacharsp-retranssent | The total number of R4 idle mode exit MS state change response messages re-transmitted on the R4 interface. | Int32
r4imexitstacharsp-totsendfail | The total number of failures that occurred during transaction id generation and R4 idle mode exit MS state change response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imexitstacharsp-totrec | The total number of R4 idle mode exit MS state change response messages received on the R4 interface. | Int32
r4imexitstacharsp-totacc | The total number of R4 idle mode exit MS state change response messages accepted on the R4 interface. | Int32
r4imexitstacharsp-totrelay | The total number of R4 idle mode exit MS state change response messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 idle mode exit MS state change response message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4imexitstacharsp-totdenied | The total number of R4 idle mode exit MS state change response messages denied on the R4 interface. | Int32
r4imexitstacharsp-totdiscard | The total number of R4 idle mode exit MS state change response messages discarded on the R4 interface. | Int32
r4imexitstacharsp-badform | The total number of badly formed R4 idle mode exit MS state change response messages on the R4 interface. | Int32
r4imexitstacharsp-decodeerr | The total number of R4 idle mode exit MS state change response messages on the R4 interface with decode error. | Int32
r4imexitstacharsp-unspecerr | The total number of R4 idle mode exit MS state change response messages on the R4 interface with unspecified error. | Int32
r4imexitstacharsp-missmandtlv | The total number of R4 idle mode exit MS state change response messages on the R4 interface with missing mandatory TLVs. | Int32
r4imexitstacharsp-tlvvalinval | The total number of R4 idle mode exit MS state change response messages on the R4 interface with invalid TLV value. | Int32
r4imexitstacharsp-unknowntlv | The total number of R4 idle mode exit MS state change response messages on the R4 interface with unknown TLVs. | Int32
r4imexitstacharsp-duptlvfound | The total number of R4 idle mode exit MS state change response messages on the R4 interface with duplicate TLVs. | Int32
r4imexitstacharsp-nosessfound | The total number of R4 idle mode exit MS state change response messages on the R4 interface without any session information. | Int32
r4imexitstacharsp-adminprohib | The total number of R4 idle mode exit MS state change response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 idle mode exit MS state change response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imexitstacharsp-noresourcedrop | The total number of R4 idle mode exit MS state change response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 idle mode exit MS state change response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imexitstacharsp-transiderr | The total number of R4 idle mode exit MS state change response messages on the R4 interface with transaction ID errors. | Int32
r4inipagreq-totsent | The total number of R4 initial paging request messages sent on the R4 interface. | Int32
r4inipagreq-retranssent | The total number of R4 initial paging request messages re-transmitted on the R4 interface. | Int32
r4inipagreq-totsendfail | The total number of failures occurred during transaction id generation and R4 initial paging request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4inipagreq-totrec | The total number of R4 initial paging request messages received on the R4 interface. | Int32
r4inipagreq-totacc | The total number of R4 initial paging request messages accepted on the R4 interface. | Int32
r4inipagreq-totrelay | The total number of R4 initial paging request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 initial paging request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4inipagreq-totdenied | The total number of R4 initial paging request messages denied on the R4 interface. | Int32
r4inipagreq-totdiscard | The total number of R4 initial paging request messages discarded on the R4 interface. | Int32
r4inipagreq-badform | The total number of badly formed R4 initial paging request messages on the R4 interface. | Int32
r4inipagreq-decodeerr | The total number of R4 initial paging request messages on the R4 interface with decode error. | Int32
r4inipagreq-unspecerr | The total number of R4 initial paging request messages on the R4 interface with unspecified error. | Int32
r4inipagreq-missmandtlv | The total number of R4 initial paging request messages on the R4 interface with missing mandatory TLVs. | Int32
r4inipagreq-tlvvalinval | The total number of R4 initial paging request messages on the R4 interface with invalid TLV value. | Int32
r4inipagreq-unknowntlv | The total number of R4 initial paging request messages on the R4 interface with unknown TLVs. | Int32
r4inipagreq-duptlvfound | The total number of R4 initial paging request messages on the R4 interface with duplicate TLVs. | Int32
r4inipagreq-nosessfound | The total number of R4 initial paging request messages on the R4 interface without any session information. | Int32
r4inipagreq-adminprohib | The total number of R4 initial paging request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 initial paging request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4inipagreq-noresourcedrop | The total number of R4 initial paging request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 initial paging request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4inipagreq-transiderr | The total number of R4 initial paging request messages on the R4 interface with transaction ID errors. | Int32
r4inipagrsp-totsent | The total number of R4 initial paging response messages sent on the R4 interface. | Int32
r4inipagrsp-retranssent | The total number of R4 initial paging response messages re-transmitted on the R4 interface. | Int32
r4inipagrsp-totsendfail | The total number of failures occurred during transaction id generation and R4 initial paging response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4inipagrsp-totrec | The total number of R4 initial paging response messages received on the R4 interface. | Int32
r4inipagrsp-totacc | The total number of R4 initial paging response messages accepted on the R4 interface. | Int32
r4inipagrsp-totrelay | The total number of R4 initial paging response messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 initial paging response message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4inipagrsp-totdenied | The total number of R4 initial paging response messages denied on the R4 interface. | Int32
r4inipagrsp-totdiscard | The total number of R4 initial paging response messages discarded on the R4 interface. | Int32
r4inipagrsp-badform | The total number of badly formed R4 initial paging response messages on the R4 interface. | Int32
r4inipagrsp-decodeerr | The total number of R4 initial paging response messages on the R4 interface with decode error. | Int32
r4inipagrsp-unspecerr | The total number of R4 initial paging response messages on the R4 interface with unspecified error. | Int32
r4inipagrsp-missmandtlv | The total number of R4 initial paging response messages on the R4 interface with missing mandatory TLVs. | Int32
r4inipagrsp-tlvvalinval | The total number of R4 initial paging response messages on the R4 interface with invalid TLV value. | Int32
r4inipagrsp-unknowntlv | The total number of R4 initial paging response messages on the R4 interface with unknown TLVs. | Int32
r4inipagrsp-duptlvfound | The total number of R4 initial paging response messages on the R4 interface with duplicate TLVs. | Int32
r4inipagrsp-nosessfound | The total number of R4 initial paging response messages on the R4 interface without any session information. | Int32
r4inipagrsp-adminprohib | The total number of R4 initial paging response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 initial paging response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4inipagrsp-noresourcedrop | The total number of R4 initial paging response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 initial paging response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4inipagrsp-transiderr | The total number of R4 initial paging response messages on the R4 interface with transaction ID errors. | Int32
r4delmsentreq-totsent | The total number of R4 delete MS entry request messages sent on the R4 interface. | Int32
r4delmsentreq-retranssent | The total number of R4 delete MS entry request messages re-transmitted on the R4 interface. | Int32
r4delmsentreq-totsendfail | The total number of failures occurred during transaction id generation and R4 delete MS entry request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4delmsentreq-totrec | The total number of R4 delete MS entry request messages received on the R4 interface. | Int32
r4delmsentreq-totacc | The total number of R4 delete MS entry request messages accepted on the R4 interface. | Int32
r4delmsentreq-totrelay | The total number of R4 delete MS entry request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 delete MS entry request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4delmsentreq-totdenied | The total number of R4 delete MS entry request messages denied on the R4 interface. | Int32
r4delmsentreq-totdiscard | The total number of R4 delete MS entry request messages discarded on the R4 interface. | Int32
r4delmsentreq-badform | The total number of badly formed R4 delete MS entry request messages on the R4 interface. | Int32
r4delmsentreq-decodeerr | The total number of R4 delete MS entry request messages on the R4 interface with decode error. | Int32
r4delmsentreq-unspecerr | The total number of R4 delete MS entry request messages on the R4 interface with unspecified error. | Int32
r4delmsentreq-missmandtlv | The total number of R4 delete MS entry request messages on the R4 interface with missing mandatory TLVs. | Int32
r4delmsentreq-tlvvalinval | The total number of R4 delete MS entry request messages on the R4 interface with invalid TLV value. | Int32
r4delmsentreq-unknowntlv | The total number of R4 delete MS entry request messages on the R4 interface with unknown TLVs. | Int32
r4delmsentreq-duptlvfound | The total number of R4 delete MS entry request messages on the R4 interface with duplicate TLVs. | Int32
r4delmsentreq-nosessfound | The total number of R4 delete MS entry request messages on the R4 interface without any session information. | Int32
r4delmsentreq-adminprohib | The total number of R4 delete MS entry request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 delete MS entry request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4delmsentreq-noresourcedrop | The total number of R4 delete MS entry request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 delete MS entry request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4delmsentreq-transiderr | The total number of R4 delete MS entry request messages on the R4 interface with transaction ID errors. | Int32
r4delmsentrsp-totsent | The total number of R4 delete MS entry response messages sent on the R4 interface. | Int32
r4delmsentrsp-retranssent | The total number of R4 delete MS entry response messages re-transmitted on the R4 interface. | Int32
r4delmsentrsp-totsendfail | The total number of failures occurred during transaction id generation and R4 delete MS entry response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4delmsentrsp-totrec | The total number of R4 delete MS entry response messages received on the R4 interface. | Int32
r4delmsentrsp-totacc | The total number of R4 delete MS entry response messages accepted on the R4 interface. | Int32
r4delmsentrsp-totrelay | The total number of R4 delete MS entry response messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 delete MS entry response message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4delmsentrsp-totdenied | The total number of R4 delete MS entry response messages denied on the R4 interface. | Int32
r4delmsentrsp-totdiscard | The total number of R4 delete MS entry response messages discarded on the R4 interface. | Int32
r4delmsentrsp-badform | The total number of badly formed R4 delete MS entry response messages on the R4 interface. | Int32
r4delmsentrsp-decodeerr | The total number of R4 delete MS entry response messages on the R4 interface with decode error. | Int32
r4delmsentrsp-unspecerr | The total number of R4 delete MS entry response messages on the R4 interface with unspecified error. | Int32
r4delmsentrsp-missmandtlv | The total number of R4 delete MS entry response messages on the R4 interface with missing mandatory TLVs. | Int32
r4delmsentrsp-tlvvalinval | The total number of R4 delete MS entry response messages on the R4 interface with invalid TLV value. | Int32
r4delmsentrsp-unknowntlv | The total number of R4 delete MS entry response messages on the R4 interface with unknown TLVs. | Int32
r4delmsentrsp-duptlvfound | The total number of R4 delete MS entry response messages on the R4 interface with duplicate TLVs. | Int32
r4delmsentrsp-nosessfound | The total number of R4 delete MS entry response messages on the R4 interface without any session information. | Int32
r4delmsentrsp-adminprohib | The total number of R4 delete MS entry response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 delete MS entry response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4delmsentrsp-noresourcedrop | The total number of R4 delete MS entry response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 delete MS entry response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4delmsentrsp-transiderr | The total number of R4 delete MS entry response messages on the R4 interface with transaction ID errors. | Int32
r4horeq-totsent | The total number of R4 handover request messages sent on the R4 interface. | Int32
r4horeq-retranssent | The total number of R4 handover request messages re-transmitted on the R4 interface. | Int32
r4horeq-totsendfail | The total number of failures occurred during transaction id generation and R4 handover request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4horeq-totrec | The total number of R4 handover request messages received on the R4 interface. | Int32
r4horeq-totacc | The total number of R4 handover request messages accepted on the R4 interface. | Int32
r4horeq-totrelay | The total number of R4 handover request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 handover request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4horeq-totdenied | The total number of R4 handover request messages denied on the R4 interface. | Int32
r4horeq-totdiscard | The total number of R4 handover request messages discarded on the R4 interface. | Int32
r4horeq-badform | The total number of badly formed R4 handover request messages on the R4 interface. | Int32
r4horeq-decodeerr | The total number of R4 handover request messages on the R4 interface with decode error. | Int32
r4horeq-unspecerr | The total number of R4 handover request messages on the R4 interface with unspecified error. | Int32
r4horeq-missmandtlv | The total number of R4 handover request messages on the R4 interface with missing mandatory TLVs. | Int32
r4horeq-tlvvalinval | The total number of R4 handover request messages on the R4 interface with invalid TLV value. | Int32
r4horeq-unknowntlv | The total number of R4 handover request messages on the R4 interface with unknown TLVs. | Int32
r4horeq-duptlvfound | The total number of R4 handover request messages on the R4 interface with duplicate TLVs. | Int32
r4horeq-nosessfound | The total number of R4 handover request messages on the R4 interface without any session information. | Int32
r4horeq-adminprohib | The total number of R4 handover request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 handover request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4horeq-noresourcedrop | The total number of R4 handover request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 handover request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4horeq-transiderr | The total number of R4 handover request messages on the R4 interface with transaction ID errors. | Int32
r4horsp-totsent | The total number of R4 handover response messages sent on the R4 interface. | Int32
r4horsp-retranssent | The total number of R4 handover response messages re-transmitted on the R4 interface. | Int32
r4horsp-totsendfail | The total number of failures occurred during transaction id generation and R4 handover response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4horsp-totrec | The total number of R4 handover response messages received on the R4 interface. | Int32
r4horsp-totacc | The total number of R4 handover response messages accepted on the R4 interface. | Int32
r4horsp-totrelay | The total number of R4 handover request messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 handover request message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4horsp-totdenied | The total number of R4 handover response messages denied on the R4 interface. | Int32
r4horsp-totdiscard | The total number of R4 handover response messages discarded on the R4 interface. | Int32
r4horsp-badform | The total number of badly formed R4 handover response messages on the R4 interface. | Int32
r4horsp-decodeerr | The total number of R4 handover response messages on the R4 interface with decode error. | Int32
r4horsp-unspecerr | The total number of R4 handover response messages on the R4 interface with unspecified error. | Int32
r4horsp-missmandtlv | The total number of R4 handover response messages on the R4 interface with missing mandatory TLVs. | Int32
r4horsp-tlvvalinval | The total number of R4 handover response messages on the R4 interface with invalid TLV value. | Int32
r4horsp-unknowntlv | The total number of R4 handover response messages on the R4 interface with unknown TLVs. | Int32
r4horsp-duptlvfound | The total number of R4 handover response messages on the R4 interface with duplicate TLVs. | Int32
r4horsp-nosessfound | The total number of R4 handover response messages on the R4 interface without any session information. | Int32
r4horsp-adminprohib | The total number of R4 handover response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 handover response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4horsp-noresourcedrop | The total number of R4 handover response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 handover response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4horsp-transiderr | The total number of R4 handover response messages on the R4 interface with transaction ID errors. | Int32
r4hoack-totsent | The total number of R4 handover acknowledgement messages sent on the R4 interface. | Int32
r4hoack-retranssent | The total number of R4 handover acknowledgement messages re-transmitted on the R4 interface. | Int32
r4hoack-totsendfail | The total number of failures occurred during transaction id generation and R4 handover acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4hoack-totrec | The total number of R4 handover acknowledgement messages received on the R4 interface. | Int32
r4hoack-totacc | The total number of R4 handover acknowledgement messages accepted on the R4 interface. | Int32
r4hoack-totrelay | The total number of R4 handover acknowledgement messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 handover acknowledgement message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4hoack-totdenied | The total number of R4 handover acknowledgement messages denied on the R4 interface. | Int32
r4hoack-totdiscard | The total number of R4 handover acknowledgement messages discarded on the R4 interface. | Int32
r4hoack-badform | The total number of badly formed R4 handover acknowledgement messages on the R4 interface. | Int32
r4hoack-decodeerr | The total number of R4 handover acknowledgement messages on the R4 interface with decode error. | Int32
r4hoack-unspecerr | The total number of R4 handover acknowledgement messages on the R4 interface with unspecified error. | Int32
r4hoack-missmandtlv | The total number of R4 handover acknowledgement messages on the R4 interface with missing mandatory TLVs. | Int32
r4hoack-tlvvalinval | The total number of R4 handover acknowledgement messages on the R4 interface with invalid TLV value. | Int32
r4hoack-unknowntlv | The total number of R4 handover acknowledgement messages on the R4 interface with unknown TLVs. | Int32
r4hoack-duptlvfound | The total number of R4 handover acknowledgement messages on the R4 interface with duplicate TLVs. | Int32
r4hoack-nosessfound | The total number of R4 handover acknowledgement messages on the R4 interface without any session information. | Int32
r4hoack-adminprohib | The total number of R4 handover acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 handover acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4hoack-noresourcedrop | The total number of R4 handover acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 handover acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4hoack-transiderr | The total number of R4 handover acknowledgement messages on the R4 interface with transaction ID errors. | Int32
r4hocnf-totsent | The total number of R4 handover confirm messages sent on the R4 interface. | Int32
r4hocnf-retranssent | The total number of R4 handover confirm messages re-transmitted on the R4 interface. | Int32
r4hocnf-totsendfail | The total number of failures occurred during transaction id generation and R4 handover confirm message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4hocnf-totrec | The total number of R4 handover confirm messages received on the R4 interface. | Int32
r4hocnf-totacc | The total number of R4 handover confirm messages accepted on the R4 interface. | Int32
r4hocnf-totrelay | The total number of R4 handover confirm messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 handover confirm message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4hocnf-totdenied | The total number of R4 handover confirm messages denied on the R4 interface. | Int32
r4hocnf-totdiscard | The total number of R4 handover confirm messages discarded on the R4 interface. | Int32
r4hocnf-badform | The total number of badly formed R4 handover confirm messages on the R4 interface. | Int32
r4hocnf-decodeerr | The total number of R4 handover confirm messages on the R4 interface with decode error. | Int32
r4hocnf-unspecerr | The total number of R4 handover confirm messages on the R4 interface with unspecified error. | Int32
r4hocnf-missmandtlv | The total number of R4 handover confirm messages on the R4 interface with missing mandatory TLVs. | Int32
r4hocnf-tlvvalinval | The total number of R4 handover confirm messages on the R4 interface with invalid TLV value. | Int32
r4hocnf-unknowntlv | The total number of R4 handover confirm messages on the R4 interface with unknown TLVs. | Int32
r4hocnf-duptlvfound | The total number of R4 handover confirm messages on the R4 interface with duplicate TLVs. | Int32
r4hocnf-nosessfound | The total number of R4 handover confirm messages on the R4 interface without any session information. | Int32
r4hocnf-adminprohib | The total number of R4 handover confirm messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 handover confirm message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4hocnf-noresourcedrop | The total number of R4 handover confirm messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 handover confirm message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4hocnf-transiderr | The total number of R4 handover confirm messages on the R4 interface with transaction ID errors. | Int32
r4hocmpl-totsent | The total number of R4 handover complete messages sent on the R4 interface. | Int32
r4hocmpl-retranssent | The total number of R4 handover complete messages re-transmitted on the R4 interface. | Int32
r4hocmpl-totsendfail | The total number of failures occurred during transaction id generation and R4 handover complete message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4hocmpl-totrec | The total number of R4 handover complete messages received on the R4 interface. | Int32
r4hocmpl-totacc | The total number of R4 handover complete messages accepted on the R4 interface. | Int32
r4hocmpl-totrelay | The total number of R4 handover complete messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 handover complete message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4hocmpl-totdenied | The total number of R4 handover complete messages denied on the R4 interface. | Int32
r4hocmpl-totdiscard | The total number of R4 handover complete messages discarded on the R4 interface. | Int32
r4hocmpl-badform | The total number of badly formed R4 handover complete messages on the R4 interface. | Int32
r4hocmpl-decodeerr | The total number of R4 handover complete messages on the R4 interface with decode error. | Int32
r4hocmpl-unspecerr | The total number of R4 handover complete messages on the R4 interface with unspecified error. | Int32
r4hocmpl-missmandtlv | The total number of R4 handover complete messages on the R4 interface with missing mandatory TLVs. | Int32
r4hocmpl-tlvvalinval | The total number of R4 handover complete messages on the R4 interface with invalid TLV value. | Int32
r4hocmpl-unknowntlv | The total number of R4 handover complete messages on the R4 interface with unknown TLVs. | Int32
r4hocmpl-duptlvfound | The total number of R4 handover complete messages on the R4 interface with duplicate TLVs. | Int32
r4hocmpl-nosessfound | The total number of R4 handover complete messages on the R4 interface without any session information. | Int32
r4hocmpl-adminprohib | The total number of R4 handover complete messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 handover complete message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4hocmpl-noresourcedrop | The total number of R4 handover complete messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 handover complete message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4hocmpl-transiderr | The total number of R4 handover complete messages on the the R4 interface with transaction ID errors. | Int32
r4unknown-totrec | The total number of unknown messages sent on the R4 interface. | Int32
r4unknown-totacc | The total number of unknown messages re-transmitted on the R4 interface. | Int32
r4unknown-totrelay | The total number of R4 unknown messages received from the base station and relayed on the the R4 interface. Triggers: Changes every time an R4 unknown message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4unknown-totdenied | The total number of unknown denied messages received on the R4 interface. | Int32
r4unknown-totdiscard | The total number of unknown discarded messages accepted on the R4 interface. | Int32
r4unknown-badform | The total number of unknown badly formed messages on the R4 interface. | Int32
r4unknown-decodeerr | The total number of unknown messages discarded on the R4 interface. | Int32
r4unknown-unspecerr | The total number of unknown unspecified error messages on the R4 interface. | Int32
r4unknown-missmandtlv | The total number of unknown messages on the R4 interface with missing mandatory TLV. | Int32
r4unknown-tlvvalinval | The total number of unknown messages on the R4 interface with an invalid TLV. | Int32
r4unknown-unknowntlv | The total number of unknown messages on the R4 interface with unknown TLVs. | Int32
r4unknown-duptlvfound | The total number of messages on the R4 interface with duplicate TLV values. | Int32
r4unknown-nosessfound | The total number of messages on the R4 interface with no session information. | Int32
r4unknown-adminprohib | The total number of R4 unknown messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 unknown message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4unknown-noresourcedrop | The total number of R4 unknown messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 unknown message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4unknown-transiderr | The total number of unknown messages on the R4 interface with transaction ID errors. | Int32
r4datagrerec-totpackrec | The total number of data packets received through the GRE tunnel on the R4 interface. | Int32
r4datagrerec-prottyperrror | Total number of protected type errors received through the GRE tunnel the R4 interface. | Int32
r4datagrerec-totbytrec | The total number of data bytes received through the GRE tunnel the R4 interface. | Int32
r4datagrerec-grekeyabs | The total number of data message received without the GRE key through GRE tunnel the R4 interface. | Int32
r4datagrerec-grechkerr | The total number of data message received with checksum error through the GRE tunnel the R4 interface. | Int32
r4datagrerec-invpacklen | Total number of protectd type errors received throughthe GRE tunnel the R4 interface. | Int32
r4datagrerec-nosessfou | The total number of data bytes received through the GRE tunnel the R4 interface. | Int32
r4datagrerec-unspecerr | The total number of data message received without a GRE key through the GRE tunnel the R4 interface. | Int32
r4pcrelocind-totsent | The total number of R4 PC Relocation Indication messages sent to the ASNPC. | Int32
r4pcrelocind-retranssent | The total number of PC Relocation Indication messages retransmitted on the the R4 interface to the ASNPC. | Int32
r4pcrelocind-totsendfail | The total number of PC Relocation Indication message failures received from the ASNPC and relayed on the the R4 interface. This counter is used to count the error while sending the R4 packets. | Int32
r4pcrelocind-totrec | The total number of R4 PC Relocation Indication messages received by the ASNPC. | Int32
r4pcrelocind-totacc | The total number of R4 PC Relocation Indication messages accepted by the ASNPC. | Int32
r4pcrelocind-totrelay | The total number of R4 PC Relocation Indication messages sent to the ASNPC and relayed on the R6 interface. Triggers: Changes every time an R4 PC Relocation Indication message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4pcrelocind-totdenied | The total number of PC Relocation Indication messages denied on the the R4 interface. | Int32
r4pcrelocind-totdiscard | The total number of PC Relocation Indication messages discarded on the the R4 interface. | Int32
r4pcrelocind-badform | The total number of badly formed R4 PC Relocation Indication messages sent to the ASNPC. | Int32
r4pcrelocind-decodeerr | The total number of R4 PC Relocation Indication messages sent to the ASNPC with decode errors. | Int32
r4pcrelocind-unspecerr | The total number of R4 PC Relocation Indication messages sent to the ASNPC with unspecified errors. | Int32
r4pcrelocind-missmandtlv | The total number of R4 PC Relocation Indication messages sent to the ASNPC with missing mandatory TLVs. | Int32
r4pcrelocind-tlvvalinval | The total number of R4 PC Relocation Indication messages sent to the ASNPC with an invalid TLV. | Int32
r4pcrelocind-unknowntlv | The total number ofR4 PC Relocation Indication messages sent to the ASNPC with an unknown TLV. | Int32
r4pcrelocind-duptlvfound | The total number of R4 PC Relocation Indication messages sent to the ASNPC with duplicate TLVs. | Int32
r4pcrelocind-nosessfound | The total number ofR4 PC Relocation Indication messages sent to the ASNPC without any session information. | Int32
r4pcrelocind-admprohibit | The total number of R4 PC Relocation Indication messages sent to the ASNPC that were discarded or denied due to admin prohibit. Triggers: Changes every time an R4 PC Relocation Indication message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r4pcrelocind-noresourcedrop | The total number of R4 PC Relocation Indication messages sent to the ASNPC that were discarded or denied due to resource unavailability. Triggers: Changes every time an R4 PC Relocation Indication message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r4pcrelocind-transiderr | The total number of R4 PC Relocation Indication messages sent to the ASNPC with a transaction ID error. | Int32
r4imexitstaind-totsent | The total number of Idle Mode Exit State Indication messages sent to the peer ASNGW. | Int32
r4imexitstaind-retranssent | The total number of Idle Mode Exit State Indication messages retransmitted on the the R4 interface to the peer ASNGW. | Int32
r4imexitstaind-totsendfail | The total number of Idle Mode Exit State Indication message failures received from the peer ASNGW and relayed on the the R4 interface. This counter is used to count the error while sending the R4 packets. | Int 32
r4imexitstaind-totrec | The total number of R4 Idle Mode Exit State Indication messages received by the peer ASNGW. | Int32
r4imexitstaind-totacc | The total number of R4 Idle Mode Exit State Indication messages accepted by the peer ASNGW. | Int32
r4imexitstaind-totrelay | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNPC and relayed on the R6 interface. Triggers: Changes every time an R4 Idle Mode Exit State Indication message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int32
r4imexitstaind-totdenied | The total number of Idle Mode Exit State Indication messages to the peer ASNGW that were denied on the the R4 interface. | Int32
r4imexitstaind-totdiscard | The total number of Idle Mode Exit State Indication messages sent to the peer ASNGW that were discarded on the the R4 interface. | Int32
r4imexitstaind-badform | The total number of badly formed R4 Idle Mode Exit State Indication messages sent to the peer ASNGW. | Int32
r4imexitstaind-decodeerr | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with decode errors. | Int32
r4imexitstaind-unspecerr | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with unspecified errors. | Int32
r4imexitstaind-missmandtlv | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with missing mandatory TLVs. | Int32
r4imexitstaind-tlvvalinval | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with an invalid TLV. | Int32
r4imexitstaind-unknowntlv | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with an unknown TLV. | Int32
r4imexitstaind-duptlvfound | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with duplicate TLVs. | Int32
r4imexitstaind-nosessfound | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW without any session information. | Int32
r4imexitstaind-admprohibit | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW that were discarded or denied due to admin prohibit. Triggers: Changes every time an Idle Mode Exit State Indication message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r4imexitstaind-noresourcedrop | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW that were discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Idle Mode Exit State Indication message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r4imexitstaind-transiderr | The total number of R4 Idle Mode Exit State Indication messages sent to the peer ASNGW with a transaction ID error. | Int32
r4pcrelocack-totsent | The number of PC Relocation Acknowledgement messages sent to the ASNPC. | Int32
r4pcrelocack-retranssent | The total number of PC Relocation Acknowledgement messages retransmitted on the the R4 interface to the ASNPC. | Int32
r4pcrelocack-totsendfail | The total number of PC Relocation Acknowledgement message failures sent to the ASNPC and relayed on the the R4 interface. This counter is used to count the error while sending the R4 packets. | Int32
r4pcrelocack-totrec | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC. | Int32
r4pcrelocack-totacc | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC. | Int32
r4pcrelocack-totrelay | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC and relayed on the the R4 interface. Triggers: Changes every time an R4 Idle Mode Exit State Indication message is relayed by the the R4 interface. Availability: across all ASNGW services. | Int 32
r4pcrelocack-totdenied | The total number of PC Relocation Acknowledgement messages sent to the ASNPC that were denied on the the R4 interface. | Int32
r4pcrelocack-totdiscard | The total number of PC Relocation Acknowledgement messages sent to the ASNPC that were discarded on the the R4 interface. | Int32
r4pcrelocack-badform | The total number of badly formed R4 PC Relocation Acknowledgement messages sent to the ASNPC. | Int32
r4pcrelocack-decodeerr | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC with decode errors. | Int32
r4pcrelocack-unspecerr | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC with unspecified errors. | Int32
r4pcrelocack-missmandtlv | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC with missing mandatory TLVs. | Int32
r4pcrelocack-tlvvalinval | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC with an invalid TLV. | Int32
r4pcrelocack-unknowntlv | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC with an unknown TLV. | Int32
r4pcrelocack-duptlvfound | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC with duplicate TLVs. | Int32
r4pcrelocack-nosessfound | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC without any session information. | Int32
r4pcrelocack-admprohibit | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC that were discarded or denied due to admin prohibit. Triggers: Changes every time an R4 PC Relocation Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r4pcrelocack-noresourcedrop | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNPC that were discarded or denied due to resource unavailability. Triggers: Changes every time an R4 PC Relocation Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r4pcrelocack-transiderr | The total number of R4 IPC Relocation Acknowledgement messages sent to the ASNPC with a transaction ID error. | Int32
r4imexitstaindack-totsent | The total number of Idle Mode Exit State Indication Acknowledgement messages sent to the peer ASNGW. | Int32
r4imexitstaindack-retranssent | The total number of Idle Mode Exit State Indication Acknowledgement messages retransmitted on the the R4 interface to the peer ASNGW. | Int32
r4imexitstaindack-totsendfail | The total number of Idle Mode Exit State Indication Acknowledgement message sent to the peer ASNGW that failed. | Int32
r4imexitstaindack-totrec | The total number of Idle Mode Exit State Indication Acknowledgement messages received on the the R4 interface to the peer ASNGW. | Int32
r4imexitstaindack-totacc | The total number of accepted Idle Mode Exit State Indication Acknowledgement messages sent to the peer ASNGW. | Int32
r4imexitstaindack-totrelay | The total number of Idle Mode Exit State Indication Acknowledgement messages relayed on the the R4 interface to the peer ASNGW. | Int32
r4imexitstaindack-totdenied | The total number of denied Idle Mode Exit State Indication Acknowledgement messages sent to the peer ASNGW. | Int32
r4imexitstaindack-totdiscard | The total number of discarded Idle Mode Exit State Indication Acknowledgement messages sent on the the R4 interface to the peer ASNGW. | Int32
r4imexitstaindack-badform | The total number of badly formed Idle Mode Exit State Indication Acknowledgement messages sent to the peer ASNG | Int32
r4imexitstaindack-decodeerr | The total number of Idle Mode Exit State Indication Acknowledgement messages retransmitted on the the R4 interface to the peer ASNGW with decode errors. | Int32
r4imexitstaindack-unspecerr | The total number of Idle Mode Exit State Indication messages sent to the peer ASNGW on the the R4 interface with unspecified errors. | Int32
r4imexitstaindack-missmandtlv | The total number of Idle Mode Exit State Acknowledgement Indication messages sent to the peer ASNGW with missing mandatory TLVs.. | Int32
r4imexitstaindack-tlvvalinval | The total number of Idle Mode Exit State Acknowledgement Indication messages sent to the peer ASNGW with an invalid TLV. | Int32
r4imexitstaindack-unknowntlv | The total number of Idle Mode Exit State Acknowledgement Indication messages with an unknown TLV sent to the peer ASNGW on the the R4 interface. | Int32
r4imexitstaindack-duptlvfound | The total number of Idle Mode Exit State Acknowledgement Indication messages with duplicate TLVs sent to the peer ASNGW over the the R4 interface. | Int32
r4imexitstaindack-nosessfound | The total number of Idle Mode Exit State Acknowledgement Indication messages sent to the peer ASNGW over the the R4 interface with no session information. | Int32
r4imexitstaindack-admprohibit | The total number of Idle Mode Exit State Indication Acknowledgement messages sent on the the R4 interface to the peer ASNGW discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Idle Mode Exit State Indication message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imexitstaindack-noresourcedrop | The total number of Idle Mode Exit State Indication Acknowledgement messages sent to the peer ASNGW on the the R4 interface that were discarded or denied due to resource unavailability. Triggers: Changes every time an Idle Mode Exit State Indication Acknowledgement message is discarded or denied due to resource unavailability. This counter is used to count the error while sending the R4 packets. | Int 32
r4imexitstaindack-transiderr | The total number of R4 Idle Mode Exit State Indication Acknowledgement messages sent to the peer ASNGW on the the R4 interface with transaction errors. | Int32
r4datapathderegack-totsent | The total number of Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-retranssent | The total number retransmitted Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-totsendfail | The total number of failed Data Path Deregistration Acknowledgement messages sent on the the R4 interface to the peer ASNGW. | Int32
r4datapathderegack-totrec | The total number of received Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-totacc | The total number of accepted Data Path Deregistration Acknowledgement messages sent on the the R4 interface to the peer ASNGW. | Int32
r4datapathderegack-totrelay | The total number of relayed Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-totdenied | The total number of denied Data Path Deregistration Acknowledgement messages sent on the the R4 interface to the peer ASNGW. | Int32
r4datapathderegack-totdiscard | The total number of discarded Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-badform | The total number of badly formed Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathderegack-decodeerr | The total number of Data Path Deregistration Acknowledgement messages sent to the peer ASNGW with decode errors. | Int32
r4datapathderegack-unspecerr | The total number of Data Path Deregistration Acknowledgement messages with unspecified errors sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-missmandtlv | The total number of Data Path Deregistration Acknowledgement messages with missing mandatory TLVs sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-tlvvalinval | The total number of Data Path Deregistration Acknowledgement messages with invalid TLVs sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-unknowntlv | The total number of Data Path Deregistration Acknowledgement messages with unknown TLVs sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-duptlvfound | The total number of Data Path Deregistration Acknowledgement messages with duplicate TLVs sent to the peer ASNGW on the the R4 interface. | Int32
r4datapathderegack-nosessfound | The total number of Data Path Deregistration Acknowledgement messages sent to the peer ASNGW over the the R4 interface with no session information. | Int32
r4datapathderegack-admprohibit | The total number of Data Path Deregistration Acknowledgement messages sent on the the R4 interface to the peer ASNGW discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Data Path Deregistration Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4datapathderegack-noresourcedrop | The total number of Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface that were discarded or denied due to resource unavailability. Triggers: Changes every time an Data Path Deregistration Acknowledgement message is discarded or denied due to resource unavailability. This counter is used to count the error while sending the R4 packets. | Int32
r4datapathderegack-transiderr | The total number of R4 Data Path Deregistration Acknowledgement messages sent to the peer ASNGW on the the R4 interface with transaction ID errors. | Int32
r6keepalivereq-totsent | The total number of R6 Keep-alive Request messages sent to the base station. | Int32
r6keepalivereq-retranssent | The total number of Keep-alive Request messages retransmitted on the R6 interface to the base station. | Int32
r6keepalivereq-totsendfail | The total number of Keep-alive Request message failures received from the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6keepalivereq-totrec | The total number of R6 Keep-alive Request messages received by the base station. | Int32
r6keepalivereq-totacc | The total number of R6 Keep-alive Request messages accepted by base station. | Int32
r6keepalivereq-totrelay | The total number of R6 Keep-alive Request messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Keep-alive Request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6keepalivereq-totdenied | The total number of Keep-alive Request messages denied on the R6 interface. | Int32
r6keepalivereq-totdiscard | The total number of discarded Keep-alive Request messages relayed on the R6 interface. | Int32
r6keepalivereq-badform | The total number of badly formed R6 Keep-alive Request messages sent to the base station. | Int32
r6keepalivereq-decodeerr | The total number of R6 Keep-alive Request messages sent to the base station with decode errors. | Int32
r6keepalivereq-unspecerr | The total number of R6 Keep-alive Request messages sent to the base station with unspecified errors. | Int32
r6keepalivereq-missmandtlv | The total number of R6 Keep-alive Request messages sent to the base station with missing mandatory TLVs. | Int32
r6keepalivereq-tlvvalinval | The total number of R6 Keep-alive Request messages sent to the base station with an invalid TLV. | Int32
r6keepalivereq-unknowntlv | The total number of R6 Keep-alive Request messages sent to the base station with an unknown TLV. | Int32
r6keepalivereq-duptlvfound | The total number of R6 Keep-alive Request messages sent to the base station with duplicate TLVs. | Int32
r6keepalivereq-nosessfound | The total number of R6 Keep-alive Request messages sent to the base station without any session information. | Int32
r6keepalivereq-admprohibit | The total number of R6 Keep-alive Request messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Keep-alive Request message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6keepalivereq-noresourcedrop | The total number of R6 Keep-alive Request messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Keep-alive Request message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6keepalivereq-transiderr | The total number of R6 Keep-alive Request messages sent to the base station with a transaction ID error. | Int32
r6keepaliversp-totsent | The total number of R6 Keep-alive Response messages sent to the base station. | Int32
r6keepaliversp-retranssent | The total number of Keep-alive Response messages retransmitted on the R6 interface to the base station. | Int 32
r6keepaliversp-totsendfail | The total number of Keep-alive Response message failures received by the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6keepaliversp-totrec | The total number of R6 Keep-alive Response messages received by the base station. | Int32
r6keepaliversp-totacc | The total number of R6 Keep-alive Response messages accepted by base station. | Int32
r6keepaliversp-totrelay | The total number of R6 Keep-alive Response messages relayed to the base station on the R6 interface. Triggers: Changes every time an R6 Keep-alive Response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6keepaliversp-totdenied | The total number of Keep-alive Response messages denied on the R6 interface. | Int32
r6keepaliversp-totdiscard | The total number of Keep-alive Response messages discarded on the R6 interface. | Int32
r6keepaliversp-badform | The total number of badly formed R6 Keep-alive Response messages sent to the base station. | Int32
r6keepaliversp-decodeerr | The total number of R6 Keep-alive Response messages sent to the base station with decode errors. | Int32
r6keepaliversp-unspecerr | The total number of R6 Keep-alive Response messages sent to the base station with unspecified errors. | Int32
r6keepaliversp-missmandtlv | The total number of R6 Keep-alive Response messages sent to the base station with missing mandatory TLVs. | Int32
r6keepaliversp-tlvvalinval | The total number of R6 Keep-alive Response messages sent to the base station with an invalid TLV. | Int32
r6keepaliversp-unknowntlv | The total number of R6 Keep-alive Response messages sent to the base station with an unknown TLV. | Int32
r6keepaliversp-duptlvfound | The total number of R6 Keep-alive Response messages sent to the base station with duplicate TLVs. | Int32
r6keepaliversp-nosessfound | The total number of R6 Keep-alive Response messages sent to the base station without any session information. | Int32
r6keepaliversp-admprohibit | The total number of R6 Keep-alive Response messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Keep-alive Response message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6keepaliversp-noresourcedrop | The total number of R6 Keep-alive Response messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Keep-alive Response message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6keepaliversp-transiderr | The total number of R6 Keep-alive Response messages sent to the base station with a transaction ID error. | Int32
r6capabilityreq-totsent | The total number of capability negotiation request messages sent to the base station on the R6 interface. | Int32
r6capabilityreq-retranssent | The total number of retransmitted capability request negotiation messages retransmitted on the R6 interface to the base station. | Int32
r6capabilityreq-totsendfail | The total number of capability negotiation request message failures received by the base station relayed on the R6 interface. | Int32
r6capabilityreq-totrec | The total number of capability negotiation request messages received by the base station on the R6 interface. | Int32
r6capabilityreq-totacc | The total number of capability negotiation request messages relayed on the R6 interface that were accepted by base station. | Int32
r6capabilityreq-totrelay | The total number of capability negotiation request messages relayed to the base station on the R6 interface. | Int32
r6capabilityreq-totdenied | The total number of denied capability negotiation request messages relayed on the R6 interface. | Int32
r6capabilityreq-totdiscard | The total number of discarded capability negotiation request messages relayed on the R6 interface. | Int32
r6capabilityreq-badform | The total number of badly formed capability negotiation request messages sent to the base station on the R6 interface. | Int32
r6capabilityreq-decodeerr | The total number of R6 capability negotiation request messages sent to the base station with decode errors. | Int32
r6capabilityreq-unspecerr | The total number of R6 capability negotiation request messages sent to the base station with unspecified errors. | Int32
r6capabilityreq-missmandtlv | The total number of R6 capability negotiation request messages sent to the base station with missing mandatory TLVs. | Int32
r6capabilityreq-tlvvalinval | The total number of R6 capability negotiation request messages sent to the base station with an invalid TLV. | Int32
r6capabilityreq-unknowntlv | The total number of R6 capability negotiation request messages sent to the base station with an unknown TLV. | Int32
r6capabilityreq-duptlvfound | The total number of R6 capability negotiation request messages sent to the base station with duplicate TLVs. | Int32
r6capabilityreq-nosessfound | The total number of R6 capability negotiation request messages sent to the base station without any session information. | Int32
r6capabilityreq-admprohibit | The total number of R6 capability negotiation request messages sent to the base station that were discarded or denied due to admin prohibit. | Int32
r6capabilityreq-noresourcedrop | The total number of R6 capability negotiation request messages sent to the base station that were discarded or denied due to resource unavailability. | Int32
r6capabilityreq-transiderr | The total number of R6 capability negotiation request messages sent to the base station with a transaction ID error. | Int32
r6capabilityrsp-totsent | The total number of R6 capability negotiation response messages sent to the base station. | Int32
r6capabilityrsp-retranssent | The total number of retransmitted capability negotiation response messages retransmitted on the R6 interface to the base station. | Int32
r6capabilityrsp-totsendfail | The total number of capability negotiation response message failures received by the base station relayed on the R6 interface. | Int32
r6capabilityrsp-totrec | The total number of capability negotiation response messages received by the base station on the R6 interface. | Int32
r6capabilityrsp-totacc | The total number of capability negotiation response messages relayed on the R6 interface that were accepted by base station. | Int32
r6capabilityrsp-totrelay | The total number of capability negotiation response messages relayed to the base station on the R6 interface. | Int32
r6capabilityrsp-totdenied | The total number of denied capability negotiation response messages relayed on the R6 interface. | Int32
r6capabilityrsp-totdiscard | The total number of discarded capability negotiation response messages relayed on the R6 interface. | Int32
r6capabilityrsp-badform | The total number of badly formed capability negotiation response messages sent to the base station on the R6 interface. | Int32
r6capabilityrsp-decodeerr | The total number of R6 capability negotiation response messages sent to the base station with decode errors. | Int32
r6capabilityrsp-unspecerr | The total number of R6 capability negotiation response messages sent to the base station with unspecified errors. | Int32
r6capabilityrsp-missmandtlv | The total number of R6 capability negotiation response messages sent to the base station with missing mandatory TLVs. | Int32
r6capabilityrsp-tlvvalinval | The total number of R6 capability negotiation response messages sent to the base station with an invalid TLV. | Int32
r6capabilityrsp-unknowntlv | The total number of R6 capability negotiation response messages sent to the base station with an unknown TLV. | Int32
r6capabilityrsp-duptlvfound | The total number of R6 capability negotiation response messages sent to the base station with duplicate TLVs. | Int32
r6capabilityrsp-nosessfound | The total number of R6 capability negotiation response messages sent to the base station without any session information. | Int32
r6capabilityrsp-admprohibit | The total number of R6 capability negotiation response messages sent to the base station that were discarded or denied due to admin prohibit. | Int32
r6capabilityrsp-noresourcedrop | The total number of R6 capability negotiation response messages sent to the base station that were discarded or denied due to resource unavailability. | Int32
r6capabilityrsp-transiderr | The total number of R6 capability negotiation response messages sent to the base station with a transaction ID error. | Int32
r6capabilityack-totsent | The total number of capability negotiation acknowledgement messages sent to the base station on the R6 interface. | Int32
r6capabilityack-retranssent | The total number of R6 capability negotiation acknowledgement messages retransmitted to the base station. | Int32
r6capabilityack-totsendfail | The total number of capability negotiation acknowledgment message failures received by the base station relayed on the R6 interface. | Int32
r6capabilityack-totrec | The total number of capability negotiation acknowledgment messages received by the base station on the R6 interface. | Int32
r6capabilityack-totacc | The total number of capability negotiation acknowledgment messages relayed on the R6 interface that were accepted by base station. | Int32
r6capabilityack-totrelay | The total number of capability negotiation acknowledgment messages relayed to the base station on the R6 interface. | Int32
r6capabilityack-totdenied | The total number of denied capability negotiation acknowledgment messages relayed on the R6 interface. | Int32
r6capabilityack-totdiscard | The total number of discarded capability negotiation acknowledgment messages relayed on the R6 interface. | Int32
r6capabilityack-badform | The total number of badly formed capability negotiation acknowledgment messages sent to the base station on the R6 interface. | Int32
r6capabilityack-decodeerr | The total number of R6 capability negotiation acknowledgment messages sent to the base station with decode errors. | Int32
r6capabilityack-unspecerr | The total number of R6 capability negotiation acknowledgment messages sent to the base station with unspecified errors. | Int32
r6capabilityack-missmandtlv | The total number of R6 capability negotiation acknowledgment messages sent to the base station with missing mandatory TLVs. | Int32
r6capabilityack-tlvvalinval | The total number of R6 capability negotiation acknowledgment messages sent to the base station with an invalid TLV. | Int32
r6capabilityack-unknowntlv | The total number of R6 capability negotiation acknowledgment messages sent to the base station with an unknown TLV. | Int32
r6capabilityack-duptlvfound | The total number of R6 capability negotiation acknowledgment messages sent to the base station with duplicate TLVs. | Int32
r6capabilityack-nosessfound | The total number of R6 capability negotiation acknowledgment messages sent to the base station without any session information. | Int32
r6capabilityack-admprohibit | The total number of R6 capability negotiation acknowledgment messages sent to the base station that were discarded or denied due to admin prohibit. | Int32
r6capabilityack-noresourcedrop | The total number of R6 capability negotiation acknowledgment messages sent to the base station that were discarded or denied due to resource unavailability. | Int32
r6capabilityack-transiderr | The total number of R6 capability negotiation acknowledgment messages sent to the base station with a transaction ID error. | Int32
r4capabilityreq-totsent | The total number of capability negotiation request messages sent to the base station on the R4 interface. | Int32
r4capabilityreq-retranssent | The total number of retransmitted capability request negotiation messages retransmitted on the R4 interface to the base station. | Int32
r4capabilityreq-totsendfail | The total number of capability negotiation request message failures received by the base station relayed on the R4 interface. | Int32
r4capabilityreq-totrec | The total number of capability negotiation request messages received by the base station on the R4 interface. | Int32
r4capabilityreq-totacc | The total number of capability negotiation request messages relayed on the R4 interface that were accepted by base station. | Int32
r4capabilityreq-totrelay | The total number of capability negotiation request messages relayed to the base station on the R4 interface. | Int32
r4capabilityreq-totdenied | The total number of denied capability negotiation request messages relayed on the R4 interface. | Int32
r4capabilityreq-totdiscard | The total number of discarded capability negotiation request messages relayed on the R4 interface. | Int32
r4capabilityreq-badform | The total number of badly formed capability negotiation request messages sent to the base station on the R4 interface. | Int32
r4capabilityreq-decodeerr | The total number of R4 capability negotiation request messages sent to the base station with decode errors. | Int32
r4capabilityreq-unspecerr | The total number of R4 capability negotiation request messages sent to the base station with unspecified errors. | Int32
r4capabilityreq-missmandtlv | The total number of R4 capability negotiation request messages sent to the base station with missing mandatory TLVs. | Int32
r4capabilityreq-tlvvalinval | The total number of R4 capability negotiation request messages sent to the base station with an invalid TLV. | Int32
r4capabilityreq-unknowntlv | The total number of R4 capability negotiation request messages sent to the base station with an unknown TLV. | Int32
r4capabilityreq-duptlvfound | The total number of R4 capability negotiation request messages sent to the base station with duplicate TLVs. | Int32
r4capabilityreq-nosessfound | The total number of R4 capability negotiation request messages sent to the base station without any session information. | Int32
r4capabilityreq-admprohibit | The total number of R4 capability negotiation request messages sent to the base station that were discarded or denied due to admin prohibit. | Int32
r4capabilityreq-noresourcedrop | The total number of R4 capability negotiation request messages sent to the base station that were discarded or denied due to resource unavailability. | Int32
r4capabilityreq-transiderr | The total number of R4 capability negotiation request messages sent to the base station with a transaction ID error. | Int32
r4capabilityrsp-totsent | The total number of R4 capability negotiation response messages sent to the base station. | Int32
r4capabilityrsp-retranssent | The total number of retransmitted capability negotiation response messages retransmitted on the R4 interface to the base station. | Int32
r4capabilityrsp-totsendfail | The total number of capability negotiation response message failures received by the base station relayed on the R4 interface. | Int32
r4capabilityrsp-totrec | The total number of capability negotiation response messages received by the base station on the R4 interface. | Int32
r4capabilityrsp-totacc | The total number of capability negotiation response messages relayed on the R4 interface that were accepted by base station. | Int32
r4capabilityrsp-totrelay | The total number of capability negotiation response messages relayed to the base station on the R4 interface. | Int32
r4capabilityrsp-totdenied | The total number of denied capability negotiation response messages relayed on the R4 interface. | Int32
r4capabilityrsp-totdiscard | The total number of discarded capability negotiation response messages relayed on the R4 interface. | Int32
r4capabilityrsp-badform | The total number of badly formed capability negotiation response messages sent to the base station on the R4 interface. | Int32
r4capabilityrsp-decodeerr | The total number of R4 capability negotiation response messages sent to the base station with decode errors. | Int32
r4capabilityrsp-unspecerr | The total number of R4 capability negotiation response messages sent to the base station with unspecified errors. | Int32
r4capabilityrsp-missmandtlv | The total number of R4 capability negotiation response messages sent to the base station with missing mandatory TLVs. | Int32
r4capabilityrsp-tlvvalinval | The total number of R4 capability negotiation response messages sent to the base station with an invalid TLV. | Int32
r4capabilityrsp-unknowntlv | The total number of R4 capability negotiation response messages sent to the base station with an unknown TLV. | Int32
r4capabilityrsp-duptlvfound | The total number of R4 capability negotiation response messages sent to the base station with duplicate TLVs. | Int32
r4capabilityrsp-nosessfound | The total number of R4 capability negotiation response messages sent to the base station without any session information. | Int32
r4capabilityrsp-admprohibit | The total number of R4 capability negotiation response messages sent to the base station that were discarded or denied due to admin prohibit. | Int32
r4capabilityrsp-noresourcedrop | The total number of R4 capability negotiation response messages sent to the base station that were discarded or denied due to resource unavailability. | Int32
r4capabilityrsp-transiderr | The total number of R4 capability negotiation response messages sent to the base station with a transaction ID error. | Int32
r4capabilityack-totsent | The total number of capability negotiation acknowledgement messages sent to the base station on the R4 interface. | Int32
r4capabilityack-retranssent | The total number of R4 capability negotiation acknowledgement messages retransmitted to the base station. | Int32
r4capabilityack-totsendfail | The total number of capability negotiation acknowledgment message failures received by the base station relayed on the R4 interface. | Int32
r4capabilityack-totrec | The total number of capability negotiation acknowledgment messages received by the base station on the R4 interface. | Int32
r4capabilityack-totacc | The total number of capability negotiation acknowledgment messages relayed on the R4 interface that were accepted by base station. | Int32
r4capabilityack-totrelay | The total number of capability negotiation acknowledgment messages relayed to the base station on the R4 interface. | Int32
r4capabilityack-totdenied | The total number of denied capability negotiation acknowledgment messages relayed on the R4 interface. | Int32
r4capabilityack-totdiscard | The total number of discarded capability negotiation acknowledgment messages relayed on the R4 interface. | Int32
r4capabilityack-badform | The total number of badly formed capability negotiation acknowledgment messages sent to the base station on the R4 interface. | Int32
r4capabilityack-decodeerr | The total number of R4 capability negotiation acknowledgment messages sent to the base station with decode errors. | Int32
r4capabilityack-unspecerr | The total number of R4 capability negotiation acknowledgment messages sent to the base station with unspecified errors. | Int32
r4capabilityack-missmandtlv | The total number of R4 capability negotiation acknowledgment messages sent to the base station with missing mandatory TLVs. | Int32
r4capabilityack-tlvvalinval | The total number of R4 capability negotiation acknowledgment messages sent to the base station with an invalid TLV. | Int32
r4capabilityack-unknowntlv | The total number of R4 capability negotiation acknowledgment messages sent to the base station with an unknown TLV. | Int32
r4capabilityack-duptlvfound | The total number of R4 capability negotiation acknowledgment messages sent to the base station with duplicate TLVs. | Int32
r4capabilityack-nosessfound | The total number of R4 capability negotiation acknowledgment messages sent to the base station without any session information. | Int32
r4capabilityack-admprohibit | The total number of R4 capability negotiation acknowledgment messages sent to the base station that were discarded or denied due to admin prohibit. | Int32
r4capabilityack-noresourcedrop | The total number of R4 capability negotiation acknowledgment messages sent to the base station that were discarded or denied due to resource unavailability. | Int32
r4capabilityack-transiderr | The total number of R4 capability negotiation acknowledgment messages sent to the base station with a transaction ID error. | Int32
r4datagresend-totpacksent | The total number of data message received with checksum error through GRE tunnel the R4 interface. | Int32
r4datagresend-senderr | The total number of data message received with invalid packet length error through GRE tunnel the R4 interface. | Int32
r4datagresend-totbytsent | The total number of data message received through GRE tunnel without session information the the R4 interface. | Int32
r4datagresend-unspeerr | The total number of data message received through GRE tunnel with unspecified error the the R4 interface. | Int32
r6mspreattreq-congestion | The total number of R6 MS pre-attachment request messages discarded or denied due to congestion or overload. Triggers: Changes every time an R6 MS pre-attachment request message is discarded or denied due to congestion or overload. Availability: across all the ASNGW service | Int32
total-sessions-connected | The total number of active sessions currently connected through the ASN GW. | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.