# OSPF VRF Configuration Mode Commands

The OSPF VRF Configuration sub-mode is used to configure the virtual routing and forwarding (VRF) context instances for OSPF routing protocol. This mode includes commands that configure VRF instance for OSPF routing parameters.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
area

Configures various parameters, including authentication, area identification, virtual link ID, and delay/interval values for the specified OSPF area using a specific VRF instance.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [no] area { decimal_value | ip_address } {authentication [ message-digest ] | default-cost cost_value  | nssa [default-information-originate] [no-redistribution] [no-summary] [translate-always] [translate-candidate] [translate-never] | stub [no-summary] | virtual-link router_ip_address [authentication {message-digest | null | text}| authentication-key {encrypted
    password encrypted_string | password password_string}| message-digest-key key_id md5 [encrypted
    password encrypted_string | password password_string]} [dead-interval] [hello-interval] [retransmit-interval] [transmit-delay]

no

Disables or removes configured parameters for the specified OSPF area using a specific VRF instance.
ip_address

Specifies the IP address of the area where authentication will be enabled in IPv4 dotted-decimal notation.
decimal_value

Specifies the identification number of the area where parameters to be configured as an integer from 0 through 4294967295.
authentication

Sets the OSPF authentication type to use the simple authentication method.
message-digest

Sets the OSPF authentication type to use the message digest 5 (MD5) authentication method.
default-cost cost_value

Sets the default cost for an OSPF area. cost_value must be an integer from 0 through 16777215.
nssa [default-information-originate] [no-redistribution no-summary] [translate-always] [translate-candidate] [translate-never]

Configures and defines an area as an NSSA (Not So Stubby Area) and configures OSPF parameters for it.

default-information-originate: Configures the OSPF VRF instances to originate default information to the NSSA area.

no-redistribution: Configures the OSPF VRF instance to not to redistribute external routes to the NSSA area.

no-summary: Configures the OSPF VRF instance to not to inject the inter-area routes into NSSA.

translate-always: Configures the NSSA-ABR (Area Border Router) always to translate. By default this is disabled.

translate-candidate: Configures the NSSA-ABR always to translate election. By default this is enabled.

translate-never: Configures the NSSA-ABR never to translate. By default this is disabled.
stub [no-summary]

Specifies an OSPF area as an stub area configures the NSSA-ABR never to translate. By default this is disabled.

no-summary: Disables (stops) the ABR from sending summary LSAs into the stub area.
virtual-link router_id

Specifies the router identifier which provides a virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.

router_id must be an IP address in IPv4 dotted-decimal notation of the ABR to be linked to.
authentication {message-digest | null | text}

Configures the OSPF authentication method to be used by the virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.

message-digest: Set the OSPF authentication type to use the message digest (MD) authentication method.

null: Set the OSPF authentication type to use no authentication, thus disabling either MD or clear text methods.

text: Set the OSPF authentication type to use the clear text authentication method.
authentication-key

Configures the authentication password for the virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.
message-digest-key key_id

Specifies the MD key identifier number for virtual link connection. key_id must be an integer from 1 through 255.
md5

Sets the message digest to MD5 for virtual link connection.
[encrypted] password passwd_string

Specifies the password required for virtual link connection authentications. The keyword password is optional and if specified passwd_string must be an alphanumeric string of 1 through 63 characters. The password specified must be in an encrypted format if the optional keyword encrypted was specified.

The encrypted keyword is intended only for use by the system while saving configuration scripts. The system displays the encrypted keyword in the configuration file as a flag that the variable following the password keyword is the encrypted version of the plain text password. Only the encrypted password is saved as part of the configuration file. encrypted_string is an alphanumeric string of 1 through 523 characters.
dead-interval value

Specifies the dead interval (in seconds) that the router should wait, during which time no packets are received and after the router considers a neighboring router to be off-line. value must be an integer from 1 through 65535.
hello-interval value

Specifies the hello interval (in seconds) before sending a hello packet. value must be an integer from 1 through 65535.
retransmit-interval value

Specifies the delay between retransmission (in seconds) that router should wait before retransmitting a packet. value must be an integer from 1 through 3600.
transmit-delay value

Specifies the interval (in seconds) that the router should wait before transmitting a packet. value must be an integer from 1 through 3600.
Usage:

Use this command to configure/set the various network/connection/authentication parameters of OPSF areas using specific VRF instance.
Example:
The following command enables authentication for an OSPF area defined by the IP address 192.168.100.10 and the OSPF authentication type to MD5:

    area 192.168.100.10
    authentication message-digest

The following command defines the area designated by the IP address 192.168.100.10 as an NSSA area where translation of NSSA candidate is enabled by default:

    area 192.168.100.10 nssa

The following command defines the OSPF area defined by the IP address 192.168.100.10 as a stub area:

    area 192.168.100.10 stub

The following command creates a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20:

    area 192.168.100.10
    virtual-link 192.168.200.20

The following command sets the authentication method for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20 to use no authentication:

    area 192.168.100.10
    virtual-link 192.168.200.20 null

The following command creates an authentication password of 123456 for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20:

    area 192.168.100.10
    virtual-link 192.168.200.20 authentication-key password 123456

The following command enables the use of MD5-based OSPF authentication for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20, sets the MD5 Key ID to 25, and the password to 123456:

    area 192.168.100.10
    virtual-link 192.168.200.20 message-digest-key 25 md5 password 123456

The following command sets the retransmit interval for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20 to 60 seconds:

    area 192.168.100.10
    virtual-link 192.168.200.20 retransmit-interval 60

default-information originate

Creates a default external route into an OSPF routing domain.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    default-information originatedefault-information originate [ always ] [ metric metric_value ] [ metric-type { 1 | 2 } ] [ route-map route_map_name ]no default-information originate

no

Disables the default external route.
always

Always advertise the route regardless of whether or not the software has a default route.
metric metric_value

Sets the OSPF metric used in creating the default rout as an integer from 1 through 16777214.
metric-type { 1 | 2 }

Sets the default route metric type.

1: Sets the OSPF external link type for default routes to Type 1.

2: Sets the OSPF external link type for default routes to Type 2.
route-map route_map_name

Specifies the name of the default route-map to be use as an alphanumeric string of 1 through 79 characters.
Usage:

Use this command to set the default external route into an OSPF routing domain.
Example:

The following command sets the default external route to originate from the route map named rmap1:

    default-information
    originate route-map rmap1

default metric

Configures the default metric value for the OSPF routing protocol.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    default-metric metric_valueno default-metric

metric-value

Sets the metric value expressed as an integer from 1 through 16777214. The default metric value setting is 26385.
no

Enables or disables the default metric value for OSPF.
Usage:

Use this command to set the default metric for routes.
Example:

The following command sets the default metric to 235:

    default-metric 235

distance

Configures the OSPF route administrative distances for all OSPF route types or based on specific route type. Administrative distance is the measure used by Cisco routers to select the best path when there are two or more different routes to the same destination from two different routing protocols. Administrative distance defines the reliability of a routing protocol. Each routing protocol is prioritized in order of most to least reliable (believable) using an administrative distance value. A lower numerical value is preferred.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] distance { distance_value | ospf { [ external distance_value ] [ inter-area distance_value ] [ intra-area distance_value ] } }

no

Disables the OSPF route administrative distances for all OSPF route types.
distance_value

Specifies the OSPF route administrative distances as an integer from 1 to 255. The default distance value is 110.
ospf { [ external distance_value ] [ inter-area distance_value ] [ intra-area distance_value ] }

Set the distance value for the specified route type.

external distance_value: Set the OSPF route administrative distance for routes from other routing domains, learned by redistribution. This must be an integer from 1 through 255. The default is 110.

inter-area distance_value: sets the OSPF route administrative distance for routes from one routing area to another. This must be an integer from 1 through 255. The default is 110.

intra-area distance_value: sets the OSPF route administrative distance for all routes within an area. This must be an integer from 1 through 255. The default is 110.
no

Enables or disables the specified option.
Usage:

Use this command to set the administrative distance for OSPF routes.
Example:

The following command sets the administrative distance for all OSPF route types to 30:

    distance 30

distribute-list

Enables or disables the filtering of networks in outgoing routing updates.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] distribute-list route_access_list out { connected | rip | static }

no

Disables the filtering of networks in outgoing routing updates.
route_access_list

Specifies the name of the OSPF route access list to use for filtering as an alphanumeric string of 1 through 63 characters.
connected

Filters connected routes.
rip

Filters RIP routes. (RIP is not supported at this time.)
static

Filters static routes.
no

Disables the specified option.
Usage:

Use this command to enable the filtering of outgoing route updates by using the specified route access list.
Example:
The following command uses the route access list named ral1 to filter outgoing routing updates for all connected routes:

    distribute-list ral1
    out connected

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
neighbor

Configures OSPF routers that interconnect to non-broadcast networks.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] neighbor  ip_address  [ poll-interval poll_interval_value ] [ priority priority_value ]

no

Disables OSPF routers that interconnect to non-broadcast networks.
ip_address

Specifies the interface IP address of the OSPF neighbor expressed using IPv4 dotted-decimal notation.
poll-interval poll_interval_value

Default: 120

Sets the number of seconds in the dead neighbor polling interval as an integer from 1 through 65535
priority priority_value

Default: 0

Sets the 8-bit number that represents the router priority value of the non-broadcast neighbor associated with the specified IP address. This must be an integer from 0 through 255. This keyword does not apply to point-to-multipoint interfaces.
Usage:

Use this command to configure OSPF routers that connect to non-broadcast networks.
Example:
The following command specifies an OSPF router neighbor with the IP address of 192.168.100.10:

    neighbor 192.168.100.10

network area

Enables OSPF on an interface and defines the OSPF area for that network.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] network network_ip_address / network_mask area { area_id | area_ip_address }

no

Disables OSPF on an interface and defines the OSPF area for that network.
network_ip_address/network_mask

Specifies the network address and mask as well as the interface on which OSPF will be enabled. network_ip_address in entered in IPv4 dotted-decimal notation, followed by the “/” and the mask (CIDR).
area_id

Specifies the OSPF area identification number for the specified network as an integer from 0 through 4294967295.
area_ip_address

Specifies the IP address of the OSPF area for this network. This must be entered in IPv4 dotted-decimal notation.
Usage:

Use this command to specify the IP address of the network interface that the OSPF router will use.
Example:
The following command specified that the OSPF router will use the interface at IP address 192.168.1.0 with a netmask of 24:

    network 192.168.1.0/24

ospf router-id

Configures the router ID for the OSPF process.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    ospf router-id ip_address

    no ospf router-id ip_address

no

Disables ospf router-id.
ip_address

Specifies the router ID for the OSPF process as an IP address entered using IPv4 dotted-decimal notation
Usage:

Use this command to set the router ID for the current OSPF router process.
Example:
The following command sets the router ID to 192.168.200.1:

    ospf router-id 192.168.200.1

passive-interface

Enables or disables the suppression of OSPF routing updates on the specified interface.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] passive-interface interface_name

no

Disables the name assigned to a logical interface within the specific context.
interface_name

Specifies the name assigned to a logical interface within the specific context as an alphanumeric string of 1 through 79 characters.
Usage:

Use this command to suppress router updates on an interface in the current context.
Example:

The following command suppresses OSPF routing updates on the interface named Intfc1:

    passive-interface Intfc1

redistribute

Redistributes routes from other protocols to OSPF neighbors using the OSPF protocol.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    redistribute { connected | rip | static } [ metric metric_value ] [ metric-type { 1 | 2 } ] [ route-map route_map_name ]no redistribute { connected | rip | static }

no

Disables the redistributed routes.
connected

Redistributes connected routes.
rip

Specifies that RIP routes will be redistributed. (RIP is not supported at this time.)
static

Redistributes static routes.
metric metric_value

Sets the OSPF metric used in the redistributed route. This must be an integer from 1 through 16777214.
metric-type { 1 | 2 }

Default: 2

Sets route metric type that is applied to redistributed routes.

1: Sets the OSPF external link type for routes to Type 1.

2: Sets the OSPF external link type for routes to Type 2.
route-map route_map_name

Filter routes through the specified route map before redistribution. route_map_name specifies the name of the route-map to use as an alphanumeric string of 1 through 79 characters.
Usage:

Use this command to define what routing protocols should have their routes redistributed into OSPF.
Example:

The following command defines that BGP routes should be redistributed:

    redistribute connected

refresh timer

Adjusts settings for the OSPF refresh timer.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] refresh  timer value

no

Disables the refresh timer.
value

Default: 10

Specifies the minimum amount of time (in seconds) to wait before refreshing a Link-state Advertisement (LSA). This must be an integer from 10 through 1800.
Usage:

Use this command to define the amount of time to wait before refreshing an LSA.
Example:
The following command sets the refresh timer to 90 seconds:

    refresh timer 90

router-id

Configures the router ID for the OSPF process.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] router-id ip_address

no

Disables the router ID for the OSPF process.

Specifies the router ID for the OSPF process in IPv4 dotted-decimal notation.
Usage:

Use this command to set the router ID for the current OSPF router process.
Example:
The following command sets the router ID to 192.168.200.1:

    router-id 192.168.200.1

timers spf

Sets the Shortest Path First (SPF) timers.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    timers spf delay_value hold_time_valueno timers spf

no

Disables SPF timers.
delay_value

Default: 5

Specifies the delay time (in seconds) between receiving changes to an SPF calculation. This must be an integer from 0 through 4294967295.
hold_time_value

Default: 10

Specifies the hold time (in seconds) between consecutive SPF calculations. This must be an integer from 0 through 4294967295.
Usage:

Use this command to set the SPF delay and hold timers for the current OSPF router process.
Example:
The following command sets the delay timer to 15 and the hold timer to 15:

    timers spf 15 15