# show mipfa

This chapter includes the show mipfa command output tables.
show mipfa full username
Table 1. show mipfa full username Command Output Descriptions

Field | Description
--- | ---
Username | The subscriber’s username.
Callid | The subscriber’s call identification number (callid).
MSID | The subscriber’s Mobile Station Identification number (MSID).
Num Agent Advt Sent | The total number of agent advertisement messages sent by the FA to the subscriber’s mobile node.
Num Agent Solicit Rcvd | The total number of agent solicitation messages received by the FA from the subscriber’s mobile node.
Home Address | The IP address assigned to the subscriber’s mobile node for the duration of the session.
NAI | The subscriber’s Network Access Identifier (NAI).
FA Address | The IP address of the FA that is facilitating the subscriber’s Mobile IP session.
HA Address | The IP address of the Home Agent that is facilitating the subscriber’s Mobile IP session.
Lifetime | The accepted lifetime interval for this session.
Remaining Lifetime | The amount of time that remains after which the session expires and is torn down.
Reverse Tunneling | Displays whether or not reverse tunneling is implemented for the subscriber’s session.
Encapsulation Type | The encapsulation method used for the subscriber’s session.
GRE Key | The key that uniquely identifies the subscriber session when the Generic Routing Encapsulation (GRE) protocol Encapsulation Type
IPSec Required | Indicates whether or not IPSec is required for the subscriber Mobile IP session.
IPSec Ctrl Tunnel Estab. | If IPSec is required for the session, this field indicates whether or not the control tunnel has been established.
IPSec Data Tunnel Estab. | If IPSec is required for the session, this field indicates whether or not the data tunnel has been established.
MN-AAA Removal | Shows if mn-aaa-removal-indication is enable or disabled. The possible values are: enabled disabled
Proxy MIP | Shows if Proxy Mobile IP is enabled or disabled for this subscriber session. Possible values are: enabled disabled
DMU Auth Failures | The total number of failed Dynamic MIP Key Update authentications for this subscriber session.
Send Terminal Verification | Shows if the FA is enabled to send the terminal verification NVSE in the RRQ. for this subscriber session. Possible values are: enabled disabled
Revocation Negotiated | Indicates whether or not MIP Registration Revocation was negotiated between the FA and the HA for this subscriber session. Possible values are : NO YES
Revocation I Bit Negotiated | Indicates whether or not the Revocation I bit was negotiated. Possible values are : NO YES
MN-HA-SPI Present | Status of dynamic MN-HA-SPI received from AAA in RRP for this subscriber session.
MN-HA-SPI | Specifies the dynamic MN-HA Security Parameter Index (SPI) number received from AAA in RRP for this subscriber session.
FA-HA-SPI Present | Status of dynamic FA-HA-SPI received from AAA in RRP for this subscriber session.
FA-HA-SPI | Specifies the dynamic FA-HA Security Parameter Index (SPI) number received from AAA in RRP for this subscriber session.
FA-HA-Key-Present | The security parameter index (SPI) key used to verify a trusted host environment and that communications are to be established between known hosts. Checks for presence of the FA - HA key. Options are: True False
FA-HA-SPI | FA - HA security parameter index (SPI)
HA-RK-Key-Present | The HA root key (RK) received by the HA from the AAA in the Radius Access-Accept. Checks for presence of HA-RK key. Options are: True False Note: True indicates a WiMAX session.
HA-RK-SPI | HA - RK security parameter index (SPI) Note: This field applies to WiMAX sessions only.
HA-RK-Lifetime | The total lifetime applied to an HA-RK. Note: This field applies to WiMAX sessions only.
HA-RK-Remaining-Lifetime | Thew total remaining lifetime for the HA-RK. Note: This field applies to WiMAX sessions only.

show mipfa peers fa-service
Table 2. show mipfa peers fa-service Command Output Descriptions

Field | Description
--- | ---
Context | The name of the context where the FA service is located.
FA Service | The name of the FA service.
Peer Address | The IP address of the peer.
Current Sessions | The number of sessions currently running on the peer.
Total Sessions | The total number of current and past sessions for the peer.
IP Security | Specifies if IP security is enabled or disabled on the peer.
FA-HA Authentication | Specifies if FA-HA authentication is enabled or disabled on the peer.
HA Monitor Status | Specifies if HA monitor is enabled or disabled on the peer.
Total Peers | The total number of peers in the output of this show command.
Total Current Sessions | The total number of sessions across all peers in the output of this show command.