# RP Schema Statistics

The RP schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HSGW
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the RP Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the PDSN service. This is a key variable. | String
vpnid | The identification number of the context configured on the system that is currently facilitating the PDSN service. This is an internal reference number. This is a key variable. | Int32
servname | Displays the name of the PDSN service for which the statistics are displayed. This is a key variable. | String
num-sessions | The current total number of RP sessions | Int32
sess-cursetup | The total number of current sessions per service. | Int32
sess-currevasetup | The total number of current EVDO-Rev A sessions per service. | Int32
sess-ttlsetup | The total sessions setup per service. | Int32
sess-ttlrevasetup | The total EVDO-Rev A sessions setup per service. | Int32
sess-ttlrevareleased | The total EVDO-Rev A sessions released per service. | Int32
sess-ttlrevadowngrade | The total EVDO-Rev A sessions that were downgraded per service. | Int32
sess-ttlreleased | The total number of sessions released per service. | Int32
svctype | Indicates the type of services running for this schema. It is collected at the per service level. | String
a10-cursetup | The total number of current A10s per service. | Int32
a10aux-cursetup | The total number of current aux A10s per service. | Int32
a10main-cursetup | The total number of current main A10s per service. | Int32
a10-ttlsetup | The total number of A10s setup per service. | Int32
a10aux-ttlsetup | The total number of aux A10s setup per service. | Int32
a10main-ttlsetup | The total number of main a10s setup per service. | Int32
a10-ttlreleased | The total number of a10s released per service. | Int32
a10aux-ttlreleased | The total number of aux A10s released per service. | Int32
a10main-ttlreleased | The total number of main A10s released per service. | Int32
sess-release-dereg | The total number of sessions de-registered per service. | Int32
sess-release-expiry | The total number of sessions released due to lifetime expiry per service. | Int32
sess-release-ppplayer | The total number of sessions released due to a PPP Layer command reported per service. | Int32
sess-release-pcfmonfail | The total number of sessions released due to a PCF Monitor failure reported per service. | Int32
sess-release-grekey | The total number of sessions released due to a GRE Key Mismatch reported per service. | Int32
sess-release-purged | The total number of sessions released due to inconsistencies found during audits between the A11 Manager task and the Session Manager task. When an inconsistency is identified, the session is released and accounting stops are issued. | Int32
sess-release-other | The total number of sessions released due to other reasons reported per service. | Int32
recv-total | The total number of registration requests, renewals, and de-registrations received. | Int32
accept-total | The total number of registration requests that have been accepted. | Int32
denied-total | The total number of registration requests that have been rejected. | Int32
reply -total | The total number of registration replies sent. | Int32
discard-total | The total number of registration requests that have been discarded. | Int32
accept-initial | The total number of initial registration requests received and accepted. | Int32
recv-initial | The total number of initial registration requests received. | Int32
accept-intrapdsn | The total number of registration requests received for sessions going through an intra-PDSN handoff. IMPORTANT: This statistic is provided for compatibility only. Please use the accept-active-intrapdsn statistic. | Int32
accept-active-intrapdsn | The total number of registration requests received with ACTIVE START for an intra-PDSN handoff. | Int32
accept-dormant-intrapdsn | The total number of registration requests received with ACTIVE STOP for an intra-PDSN handoff. | Int32
accept-interpdsn | The total number of registration requests received for sessions going through an inter-PDSN handoff. | Int32
reva-rrq-recv | The total number of Rev-A RRQs received per service. | Int32
reva-rrq-accept | The total number of Rev-A RRQs accepted per service. | Int32
reva-rrq-denied | The total number of Rev-A RRQs denied per service. | Int32
reva-rrq-reply | The total number of Rev-A RRQs per service that were replied to. | Int32
denied-initial | The total number of initial registration requests received and rejected. | Int32
discard-initial | The total number of Initial RRQ discarded. | Int32
recv-initial-setupstart | The total number of Initial Setup/Start RRQ received. | Int32
accept-initial-setupstart | The total number of Initial Setup/Start RRQ received and accepted. | Int32
denied-initial-setupstart | The total number of Initial Setup/Start RRQ received and denied. | Int32
discard-initial-setupstart | The total number of initial start or setup registration requests that have been received and discarded. | Int32
accept-renew | The total number of registration request renewals received and accepted. | Int32
denied-renew | The total number of registration request renewals received and rejected. | Int32
recv-renew | The total number of registration request renewals received. | Int32
discard-renew | The total number of registration request renewals received and discarded | Int32
recv-renew-noairlink | The total number of registration request renewals received due to “No airlink”. | Int32
accept-renew-noairlink | The total number of registration request renewals received due to “No airlink” and accepted. | Int32
denied-renew-noairlink | The total number of registration request renewals received due to “No airlink” and denied. | Int32
discard-renew-noairlink | The total number of registration request renewals received due to “No airlink” and discarded. | Int32
active-start-renew | The total number of ACTIVE START registration request renewals received. IMPORTANT: This statistic is provided for compatibility only. Please use the accept-renew-activestart statistic. | Int32
recv-renew-activestart | The total number of RRQ renewals with an Active Start record received. | Int32
accept-renew-activestart | The total number of RRQ renewals with an Active Start record received and accepted. | Int32
denied-renew-activestart | The total number of RRQ renewals with an Active Start record received and denied. | Int32
discard-renew-activestart | The total number of RRQ renewals with an Active Start record received and discarded. | Int32
active-stop-renew | The total number of ACTIVE STOP registration request renewals received. IMPORTANT: This statistic is provided for compatibility only. Please use the accept-renew-activestop statistic. | Int32
recv-renew-activestop | The total number of RRQ renewals with an Active Stop record received. | Int32
accept-renew-activestop | The total number of RRQ renewals with an Active Stop record received and accepted. | Int32
denied-renew-activestop | The total number of RRQ renewals with an Active Stop record received and denied. | Int32
discard-renew-activestop | The total number of RRQ renewals with an Active Stop record received and discarded. | Int32
accept-dereg | The total number of de-registration requests received and accepted. | Int32
denied-dereg | The total number of de-registration request renewals received and rejected. | Int32
recv-dereg | The total number of de-registration request renewals received. | Int32
discard-dereg | The the total number of de-registration requests received and discarded. | Int32
recv-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received. | Int32
accept-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received and accepted. | Int32
denied-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received and denied | Int32
discard-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received and discarded. | Int32
active-stop-dereg | The total number of ACTIVE STOP de-registration request renewals received and accepted. IMPORTANT: This statistic is provided for compatibility only. Please use the accept-dereg-activestop statistic. | Int32
recv-dereg-activestop | The the total number of de-registration request with an Active Stop record received. | Int32
accept-dereg-activestop | The the total number of de-registration request with an Active Stop record received and accepted. | Int32
denied-dereg-activestop | The the total number of de-registration request with an Active Stop record received and denied. | Int32
discard-dereg-activestop | The the total number of de-registration request with an Active Stop record received and discarded. | Int32
recv-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active Access Network Identifier (ANID) received. | Int32
accept-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active ANID received and accepted. | Int32
denied-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active ANID received and denied. | Int32
discard-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active ANID received and discarded. | Int32
recv-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received. | Int32
accept-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received and accepted. | Int32
denied-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received and denied. | Int32
discard-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received and discarded. | Int32
recv-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active Mobility Event Indicator (MEI) and ANID received. | Int32
accept-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active MEI and ANID received and accepted. | Int32
denied-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active MEI and ANID received and denied. | Int32
discard-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active MEI and ANID received and discarded. | Int32
send-error | The total number of registration replies for which errors were experienced during transmission. | Int32
hash-error | The total number of registration requests that had internal hash lookup errors. | Int32
decode-error | The total number of registration requests that had decode errors. | Int32
unhandled | The total number of registration requests that had unhandled errors. | Int32
seqerror | The total number of registration requests that had sequence numbers that were not acceptable. | Int32
deny-unspec | The total number of registration requests that were denied using reply code of 80H (Registration Denied - reason unspecified) | Int32
deny-adminprohib | The total number of registration requests that were denied using reply code of 81H (Registration Denied - administratively prohibited). | Int32
deny-noresource | The total number of registration requests that were denied using reply code of 82H (Registration Denied - insufficient resources). | Int32
deny-auth | The total number of registration requests that were denied using reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
deny-idmismatch | The total number of registration requests that were denied using reply code of 85H (Registration Denied - identification mismatch). | Int32
deny-badrequest | The total number of registration requests that were denied using reply code of 86H (Registration Denied - poorly formed request). | Int32
deny-unknownpdsn | The total number of registration requests that were denied using reply code of 88H (Registration Denied - unknown PDSN address) | Int32
deny-revtununavail | The total number of registration requests that were denied using reply code of 89H (Registration Denied - requested reverse tunnel unavailable). | Int32
deny-revtunreq | The total number of registration requests that were denied using reply code of 8AH (Registration Denied - reverse tunnel is mandatory and “T”-bit not set). | Int32
deny-unrecogvend | The total number of registration requests that were denied using reply code of 8DH (Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE). | Int32
deny-sessclosed | The total number of registration requests that were denied using an error code 0x8E for absent RP sessions. Refer to the session-already-closed keyword for the registration-deny command in the PDSN Configuration Mode chapter of the Command Line Interface Reference for additional information. | Int32
deny-bsninfo | The total number of registration requests that were denied because BSN information was unavailable. | Int32
deny-noresource-nosessmgr | The total number of RRQ denied due to Insufficient resource, no session manager reported per service. | Int32
deny-noresource-nomem | The total number of RRQ denied due to Insufficient resource, no memory reported per service. | Int32
deny-noresource-sessmgrretried | The total number of RRQ denied due to Insufficient resource, session managers retried reported per service. | Int32
deny-noresource-inputq | The total number of RRQ denied due to Insufficient resource, input queue exceeded reported per service. | Int32
deny-noresource-policy | The total number of RRQ denied due to Insufficient resource, policy rejected reported per service. | Int32
deny-noresource-sessmgrrej | The total number of RRQ denied due to Insufficient resource, session manager rejected reported per service. | Int32
deny-noresource-a11mgrrej | The total number of RRQ denied due to Insufficient resource, A11 manager rejected reported per service. | Int32
deny-badrequest-alrdorm | The total number of RRQ denied due to poorly formed request, session already dormant reported per service. | Int32
deny-badrequest-alractive | The total number of RRQ denied due to poorly formed request, already active reported per service. | Int32
deny-badrequest-setupabsent | The total number of RRQ denied due to poorly formed request, airlink setup absent reported per service. | Int32
deny-badrequest-miscoaaddr | The total number of RRQ denied due to poorly formed request, mismatched CoA/Source address reported per service. | Int32
deny-badrequest-pkttooshort | The total number of RRQ denied due to poorly formed request, packet too short reported per service. | Int32
deny-badrequest-pkttoolong | The total number of RRQ denied due to poorly formed request, packet too long reported per service. | Int32
deny-badrequest-fieldlen | The total number of RRQ denied due to poorly formed request, invalid field length reported per service. | Int32
deny-badrequest-flags | The total number of RRQ denied due to poorly formed request, invalid flags reported per service. | Int32
deny-badrequest-hoanonzero | The total number of RRQ denied due to poorly formed request, HOA non-zero reported per service. | Int32
deny-badrequest-sse | The total number of RRQ denied due to poorly formed request, invalid SSE reported per service. | Int32
deny-badrequest-vse | The total number of RRQ denied due to poorly formed request, invalid VSE reported per service. | Int32
deny-badrequest-authextn | The total number of RRQ denied due to poorly formed request, invalid authorization extension reported per service. | Int32
deny-badrequest-unkextn | The total number of RRQ denied due to poorly formed request, invalid unknown extension reported per service. | Int32
deny-badrequest-other | The total number of RRQ denied due to poorly formed request, other reason reported per service. | Int32
deny-unspec-nullpkt | The total number of RRQ denied due to unspecified reason, null packet received reported per service. | Int32
deny-unspec-lifezero | The total number of RRQ denied due to unspecified reason, lifetime zero in initial RRQ reported per service. | Int32
deny-unspec-notready | The total number of RRQ denied due to unspecified reason, session manager not ready reported per service. | Int32
deny-unspec-crphandoff | The total number of RRQ denied due to unspecified reason, Closed RP handoff in progress reported per service. | Int32
deny-unspec-noairlink | The total number of RRQ denied due to unspecified reason, no airlink setup reported per service. | Int32
deny-unspec-intrahandoff | The total number of RRQ Denied due to unspecified reason, intra PDSN handoff triggered reported per service. | Int32
deny-cong-drop | The total number of denied registration replies discarded due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
deny-cong-adminprohib | The total number of denied registration replies that were sent with a reply code of 81H (Registration Denied - administratively prohibited) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
deny-cong-unknownpdsn | The total number of denied registration replies that were sent with a reply code of 88H (Registration Denied - unknown PDSN address) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
upd-total | The total number of registration updates that were transmitted. | Int32
upd-accept | The total number of registration updates that were accepted by the PCF. | Int32
upd-denied | The total number of registration updates that were denied. | Int32
upd-unack | The total number of registration updates that were not acknowledged. | Int32
upd-trans | The total number of initial registration updates that were transmitted. | Int32
upd-ttlnoretrans | The total number of registration updates that were not re-transmitted due to TTL expiration. | Int32
upd-retrans | The total number of registration updates that were re-transmitted. | Int32
upd-received | The total number of registration acknowledgements that were received. | Int32
upd-ack-received | The total number of registration acknowledgements that were received. | Int32
upd-discard | The total number of registration acknowledgements that were discarded. | Int32
upd-senderror | The total number of registration updates for which errors were experienced during transmission. | Int32
upd-upltrinit | The total number of registration updates that were initiated by upper processing layers. IMPORTANT: This statistic is obsolete. | Int32
upd-uplyrinit | The total number of registration updates that were initiated by upper processing layers. IMPORTANT: This statistic is obsolete. | Int32
upd-other | The total number of registration updates that were sent due to reasons other than those listed here. | Int32
upd-handoff | The number of registration updates that were sent due to handoff releases. | Int32
upd-lifetime | The total number of registration updates that the send reason was Lifetime Expiry reported per service. | Int32
upd-smgrexit | The total number of registration updates that the send reason was that the session manager exited reported per service. | Int32
upddeny-unspec | The total number of denied registration updates that were sent with a reply code of 80H (Registration Denied - reason unspecified). | Int32
upddeny-adminprohib | The total number of denied registration updates that were sent with a reply code of 81H (Registration Denied - administratively prohibited). | Int32
upddeny-auth | The total number of denied registration updates that were sent with a reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
upddeny-idmismatch | The total number of denied registration updates that were sent with a reply code of 85H (Registration Denied - identification mismatch). | Int32
upddeny-badrequest | The total number of denied registration updates that were sent with a reply code of 86H (Registration Denied - poorly formed request). | Int32
upd-discard-absent | The total number of registration acknowledgements that were discarded due to the session having been already ended because the acknowledgement was late. | Int32
upd-discard-nomem | The total number of registration acknowledgements that were discarded due to insufficient memory. | Int32
upd-discard-malform | The total number of registration acknowledgements that were discarded due to being poorly formed. | Int32
upd-discard-authfail | The total number of registration acknowledgements that were discarded due to the mobile node failing authentication. | Int32
upd-discard-bounce | The total number of internal communication messages between an A11 Manager task and a Session Manager task that bounced (were not successfully sent). | Int32
upd-discard-inputq | The number of times that the queue in which incoming calls are kept prior to being processed exceeded its capacity. | Int32
upd-discard-mismatchid | The total number of discarded registration acknowledgements due to reply code 85H (Registration Denied - identification mismatch). | Int32
upd-discard-invpktlen | The total number of registration acknowledgements that were discarded due to having an invalid packet length. | Int32
upd-discard-unkpcf | The total number of registration acknowledgements that were discarded due to Unknown PCF. | Int32
upd-discard-unhpkt | The total number of registration acknowledgements that were discarded due to Unhandled Packet. | Int32
upd-discard-misc | The number of registration acknowledgements that were discarded due to reasons other than those listed above. | Int32
disc-absent | IMPORTANT: This statistic has been renamed to upd-discard-absent. However, this statistic name is still provided for compatibility only. | Int32
disc-nomem | IMPORTANT: This statistic has been renamed to upd-discard-nomem. However, this statistic name is still provided for compatibility only. | Int32
disc-malform | IMPORTANT: This statistic has been renamed to upd-discard-malform. However, this statistic name is still provided for compatibility only. | Int32
disc-authfail | IMPORTANT: This statistic has been renamed to upd-discard-authfail. However, this statistic name is still provided for compatibility only. | Int32
disc-bounce | IMPORTANT: This statistic has been renamed to upd-discard-bounce. However, this statistic name is still provided for compatibility only. | Int32
disc-inputq | IMPORTANT: This statistic has been renamed to upd-discard-inputq. However, this statistic name is still provided for compatibility only. | Int32
disc-mismatchid | IMPORTANT: This statistic has been renamed to upd-discard-mismatchid. However, this statistic name is still provided for compatibility only. | Int32
disc-invpktlen | IMPORTANT: This statistic has been renamed to upd-discard-invpktlen. However, this statistic name is still provided for compatibility only. | Int32
disc-misc | IMPORTANT: This statistic has been renamed to upd-discard-misc. However, this statistic name is still provided for compatibility only. | Int32
sec-violations | The total number of security violations that occurred. | Int32
sec-badauth | The total number of security violations that occurred due to a mis-computed authentication field. | Int32
sec-badid | The total number of security violations that occurred due to the receipt of a Security Parameter Index (SPI) that is not configured on the PDSN. | Int32
sec-badspi | The total number of security violations that occurred due to the receipt of a Security Parameter Index (SPI) that was in the reserved range (0 through 255). | Int32
sec-mnhaauth | The total number of security violations that occurred due to missing mobile node-home agent authentication extensions. | Int32
sec-regupdate | The total number of security violations that occurred due to missing registration update authentication extensions | Int32
rrqdiscard-nosessmgr | The total number of registration requests discarded due to no session manager, reported per service. | Int32
rrqdiscard-nomem | The total number of registration requests discarded due to no memory, reported per service. | Int32
rrqdiscard-authfail | The total number of registration requests discarded due to auth failure, reported per service. | Int32
rrqdiscard-smgrdead | The total number of registration requests discarded due to session manager dead, reported per service. | Int32
rrqdiscard-adminprohib | The total number of registration requests discarded due to admin prohibited, reported per service. | Int32
rrqdiscard-smgrnotready | The total number of registration requests discarded due to session manager not ready, reported per service. | Int32
rrqdiscard-unkpdsn | The total number of registration requests discarded due to unknown pdsn, reported per service. | Int32
rrqdiscard-bounce | The total number of registration requests discarded due to internal bounce error, reported per service. | Int32
rrqdiscard-inputq | The total number of registration requests discarded due to input queue exceeded, reported per service. | Int32
rrqdiscard-maxsess | The total number of registration requests discarded due to max sessions reached, reported per service. | Int32
rrqdiscard-invlen | The total number of registration requests discarded due to invalid packet length, reported per service. | Int32
rrqdiscard-grekey | The total number of registration requests discarded due to GRE key changed, reported per service. | Int32
rrqdiscard-overload | The total number of registration requests discarded due to overload/congestion, reported per service. | Int32
rrqdiscard-misc | The total number of registration requests discarded due to miscellaneous errors reported per service. | Int32
ttlprepaid | The total number of Prepaid calls facilitated by the service. | Int32
curprepaid | The total number of Prepaid calls currently being facilitated by the service. | Int32
ttlonlineauthsucc | The total number of successful Online Authentications for the service. | Int32
ttlonlineauthfail | TThe total number of successful Online Authentications for the service. | Int32
rx-pkt-xoff | The total number of packets Received with XOFF per service. | Int32
rx-pkt-xon | The total number of packets Received with XON per Service. | Int32
xontoxoff | The total number of XON->XOFF transitions per service. | Int32
pkt-dropped-xoff | The total number of output packets dropped to XOFF per service. | Int32
bytes-dropped-xoff | The total number of output bytes dropped on XOFF per Service. | Int32
sess-num-transmitted | The total number of RP session update messages transmitted. | Int32
sess-accepted | The total number of RP session update ack messages accepted. | Int32
sess-denied | The total number of RP session update messages denied. | Int32
sess-not-acknowledged | The total number of RP session update messages not acknowledged. | Int32
sess-initial-update | The total number of RP session update messages initially transmitted. | Int32
sess-update-retransmitted | The total number of RP session update messages re-transmitted. | Int32
sess-update-ack-received | The total number of RP session update acknowledgement messages received. | Int32
sess-update-ack-discarded | The total number of RP session update acknowledgement messages discarded. | Int32
sess-update-send-error | The total number of RP session update send errors that occurred. | Int32
sess-updreason-alwayson | The total number of session updates sent due to Always On, reported per service. This is a Rev-A specific statistic. | Int32
sess-updreason-qosinfo | The total number of session updates sent due to QoS Info, reported per service. | Int32
sess-updreason-qostftviol | The total number of session updates sent due to TFT Violation, reported per service. | Int32
sess-updreason-qostrafviol | The total number of session updates sent due to Traffic Violation, reported per service. | Int32
sess-updreason-qostrafpol | The total number of session updates sent due to Traffic Policing, reported per service. | Int32
sess-updreason-qosoptrig | The total number of session updates sent due to Operator Triggered, reported per service. | Int32
sess-always-on-indication | The total number of RP session updates supporting Always-on functionality. | Int32
sess-reason-unspecified | The total number of RP session update messages denied with status code reason-unspecified. | Int32
sess-PDSN-auth-fail | The total number of RP session update messages denied due to message authentication failure at the PCF. IMPORTANT: This statistic is provided for compatibility only. Please use the sess-pdsn-auth-fail statistic. | Int32
sess-pdsn-auth-fail | The total number of RP session update messages denied due to message authentication failure at the PCF. | Int32
sess-ID-mismatch | The total number of RP session update messages denied due to having an ID mismatch at the PCF. IMPORTANT: This statistic is provided for compatibility only. Please use the sess-id-mismatch statistic. | Int32
sess-id-mismatch | The total number of RP session update messages denied due to having an ID mismatch at the PCF. | Int32
sess-poorly-formed-update | The total number of session update messages denied by the PCF due to poorly formed message error. | Int32
sess-para-not-update | The total number of update ack messages received with status code indicating that parameters were not updated. | Int32
sess-upddenied-noresource | The total number of session updates sent due to Insufficient Resources, reported per service. | Int32
sess-upddenied-adminprohib | The total number of session updates denied due to Admin Prohibited, reported per service. | Int32
sess-upddenied-idnotsupp | The total number of session updates denied due to Profile ID Not Supported, reported per service. | Int32
sess-upddenied-handoff | The total number of session updates denied due to handoffs in progress per service. | Int32
sess-absent | The total number of update ack messages that were discarded by the PDSN due to no session being present at the PDSN. | Int32
sess-no-memory | The total number of update ack messages that were discarded by the PDSN due to no memory available. | Int32
sess-malformed | The total number of update ack messages that were discarded by the PDSN due to being malformed. | Int32
sess-auth-fail | The total number of update ack messages that were discarded by the PDSN due to message authentication failure. | Int32
sess-ID-bounce-error | The total number of update ack messages that were discarded by the PDSN due to internal communication error within the PDSN. | Int32
sess-input-Q-exceeded | The total number of update ack messages that were discarded by the PDSN due to exceeding input pacing queues at the PDSN. | Int32
sess-mismatched-ID | The total number of update ack messages that were discarded by the PDSN due to mismatched id in the message. | Int32
sess-invalid-packet-length | The total number of update ack messages that were discarded by the PDSN due to bad packet length. | Int32
sess-misc-reasons | The total number of update ack messages that were discarded by the PDSN due to other reasons. | Int32
sess-updackdisc-sessdisc | Session Update Ack Discard Reasons – Session Disconnecting per service. | Int32
sess-updackdisc-pktnothand | Session Update Ack Discard Reasons – Packet Not Handled per service. | Int32
sess-gre-packet-sent-sdb | The total number of GRE packets transmitted in short data burst (SDB). | Int32
sess-gre-byte-sent-sdb | The total number of GRE bytes transmitted in short data burst (SDB). | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.