# LMA Schema Statistics

The LMA schema provides operational statistics that can be used for monitoring and troubleshooting the following products: P-GW
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the LMA Service Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | Description: The name of the context configured on the system that is currently facilitating the LMA service. This is a key variable. Type: Information | String
vpnid | Description: The identification number of the context configured on the system that is currently facilitating the LMA service. This is an internal reference number. This is a key variable. Type: Information | Int32
servname | Description: Displays the name of the LMA service for which the statistics are displayed. This is a key variable. Type: Information | String
servid | Description: The identification number of the service configured on the system that is currently facilitating the LMA service. This is an internal reference number. This is a key variable. Type: Information | Int32
sess-cur | Description: The total number of sessions currently active in the LMA service. Triggers: Increments when new session is set up. Decremented when session is torn down. Availability: per LMA service Type: Gauge | Int32
mipaaaauth-attempts | Description: The total number of mobile IP AAA Authentication attempts on receiving Binding request message by LMA service. Triggers: Increments when auth attempted on receiving Bind message. Availability: per LMA service Type: Counter | Int32
mipaaaauth-success | Description: The total number of successful mobile IP AAA Authentication attempts made by LMA service. Triggers: Increments when auth is successful when attempted. Availability: per LMA service Type: Counter | Int32
mipaaaauth-totalfailures | Description: The total number of failed mobile IP AAA authentication attempts received by LMA service. Triggers: Increments when auth failed when attempted. Availability: per LMA service Type: Counter | Int32
mipaaaauth-actualauthfailures | Description: The total number of mobile IP AAA authentication failures received by LMA service. Triggers: Increments when actual auth failed when attempted. Availability: per LMA service Type: Counter | Int32
mipaaaauth-miscauthfailures | Description: The total number of miscellaneous mobile IP AAA authentication failures received by LMA service. Triggers: Increments when auth failed due to other reasons when attempted. Availability: per LMA service Type: Counter | Int32
bindupd | Description: The total number of all binding updates received by LMA service. Triggers: Increments when binding updated request is received. Availability: per LMA service Type: Counter | Int32
bindupd-accept | Description: The total number of all binding updates received and accepted by LMA service. Triggers: Increments when binding update request is accepted. Availability: per LMA service Type: Counter | Int32
bindupd-denied | Description: The total number of all binding updates received and denied by LMA service. Triggers: Increments when binding update request is rejected/denied. Availability: per LMA service Type: Counter | Int32
bindupd-discard | Description: The total number of all binding updates received and discarded by LMA service. Triggers: Increments when binding update request is discarded. Availability: per LMA service Type: Counter | Int32
bindupd-initial | Description: The total number of all initial binding updates received by LMA service. Triggers: Increments when initial binding updated request is received. Availability: per LMA service Type: Counter | Int32
bindupd-initialaccept | Description: The total number of initial binding updates received and accepted by LMA service. Triggers: Increments when initial binding update request is accepted. Availability: per LMA service Type: Counter | Int32
bindupd-initialdenied | Description: The total number of initial binding updates received and denied by LMA service. Triggers: Increments when initial binding update request is rejected/denied. Availability: per LMA service Type: Counter | Int32
bindupd-refresh | Description: The total number of all refresh binding update requests received by LMA service. Triggers: Increments when renew binding updated request is received. Availability: per LMA service Type: Counter | Int32
bindupd-refreshaccept | Description: The total number of refresh binding update requests received and accepted by LMA service. Triggers: Increments when renew binding update request is accepted. Availability: per LMA service Type: Counter | Int32
bindupd-refreshdenied | Description: The total number of refresh binding update requests received and denied by LMA service. Triggers: Increments when renew binding update request is rejected/denied. Availability: per LMA service Type: Counter | Int32
bindupd-dereg | Description: The total number of all deregistration request binding updates received by LMA service. Triggers: Increments when dereg binding updated request is received. Availability: per LMA service Type: Counter | Int32
bindupd-deregaccept | Description: The total number of deregistration request binding updates received and accepted by LMA service. Triggers: Increments when dereg binding update request is accepted. Availability: per LMA service Type: Counter | Int32
bindupd-deregdenied | Description: The total number of deregistration request binding updates received and denied by LMA service. Triggers: Increments when dereg binding update request is rejected/denied. Availability: per LMA service Type: Counter | Int32
bindupd-handoff | Description: The total number of all handoff request binding updates received by LMA service. Triggers: Increments when handoff binding updated request is received. Availability: per LMA service Type: Counter | Int32
bindupd-handoffaccept | Description: The total number of handoff request binding updates received and accepted by LMA service. Triggers: Increments when handoff binding update request is accepted. Availability: per LMA service Type: Counter | Int32
bindupd-handoffdenied | Description: The total number of handoff request binding updates received and denied by LMA service. Triggers: Increments when handoff binding update request is rejected/denied. Availability: per LMA service Type: Counter | Int32
bindupd-ack | Description: The total number of all binding update acknowledgements sent by LMA service. Triggers: Increments when binding Ack is sent. Availability: per LMA service Type: Counter | Int32
bindupd-ackacceptreg | Description: The total number of accepted registration binding update acknowledgements sent by LMA service. Triggers: Increments when binding Ack is sent with success status code. Availability: per LMA service Type: Counter | Int32
bindupd-ackacceptdereg | Description: The total number of accepted deregistration binding update acknowledgements sent by LMA service. Triggers: Increments when dereg binding Ack is sent with success status code. Availability: per LMA service Type: Counter | Int32
bindupd-ackdenied | Description: The total number of denied binding update acknowledgements sent by LMA service. Triggers: Increments when binding Ack is denied and sent with error status code. Availability: per LMA service Type: Counter | Int32
bindupd-acksenderror | Description: The total number of send error binding update acknowledgements sent by LMA service. Triggers: Increments when error is encountered while sending binding Ack. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresource | Description: The total number of binding update deny messages, due to insufficient resources, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Insufficient resources”. Availability: per LMA service Type: Counter | Int32
bindupd-denymisid | Description: The total number of binding update deny messages, due to mismatched IDs, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Mismatched ID”. Availability: per LMA service Type: Counter | Int32
bindupd-denymnauthfailure | Description: The total number of binding update deny messages, due to a mobile node authentication failure condition, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Mobility Auth failed”. Availability: per LMA service Type: Counter | Int32
bindupd-denyadmin | Description: The total number of binding update deny messages, due to an admin prohibited condition, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Admin Prohibited”. Availability: per LMA service Type: Counter | Int32
bindupd-denymsgidreq | Description: The total number of binding update deny messages, due to requiring a message ID, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Mesg ID Reqd”. Availability: per LMA service Type: Counter | Int32
bindupd-denydadfailed | Description: The total number of binding update deny messages, due to DAD failure, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “DAD failed”. Availability: per LMA service Type: Counter | Int32
bindupd-denynothomesub | Description: The total number of binding update deny messages, due to an incorrect home subnet, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Not Home Subnet”. Availability: per LMA service Type: Counter | Int32
bindupd-denyseqoow | Description: The total number of binding update deny messages, due to sequence out of window, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Sequence Number out of window”. Availability: per LMA service Type: Counter | Int32
bindupd-denytypchgdis | Description: The total number of binding update deny messages, due to a disallowed registration type change, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Reg Type change Disallowed”. Availability: per LMA service Type: Counter | Int32
bindupd-denyunspec | Description: The total number of binding update deny messages, due to an unspecified reason, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Unspecified reason”. Availability: per LMA service Type: Counter | Int32
bindupd-denyservauthfailed | Description: The total number of binding update deny messages, due to a service authorization failure, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Service authorization failed”. Availability: per LMA service Type: Counter | Int32
bindupd-denyproxyreg | Description: The total number of binding update deny messages, due to a proxy registration not enabled error, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Proxy Reg Not enabled”. Availability: per LMA service Type: Counter | Int32
bindupd-denytimestamp | Description: The total number of binding update deny messages, due to a timestamp mismatch error, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Timestamp mismatch”. Availability: per LMA service Type: Counter | Int32
bindupd-denytimestamplower | Description: The total number of binding update deny messages, due to a timestamp lower than expected reason, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Timestamp lower than expected”. Availability: per LMA service Type: Counter | Int32
bindupd-denymismnid | Description: The total number of binding update deny messages, due to a missing MN-ID option, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Missing MN-ID option”. Availability: per LMA service Type: Counter | Int32
bindupd-denymishnp | Description: The total number of binding update deny messages, due to a missing HNP option, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Missing HNP option”. Availability: per LMA service Type: Counter | Int32
bindupd-denymisaccesstech | Description: The total number of binding update deny messages, due to a missing access technology option, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Missing Access Tech option”. Availability: per LMA service Type: Counter | Int32
bindupd-denymishandoffind | Description: The total number of binding update deny messages, due to a missing handoff indicator option, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Missing Handoff indication option”. Availability: per LMA service Type: Counter | Int32
bindupd-denynotauthhnp | Description: The total number of binding update deny messages, due to a not authorized for HNP reason, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Not Authorized for HNP”. Availability: per LMA service Type: Counter | Int32
bindupd-denynotlmamobile | Description: The total number of binding update deny messages, due to a missing LMA for the MN, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Not LMA for mobile”/ Availability: per LMA service Type: Counter | Int32
bindupd-denynotauthproxyreg | Description: The total number of binding update deny messages, due to a not authorized for proxy registration reason, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “Not Authorized for Proxy Reg”. Availability: per LMA service Type: Counter | Int32
bindupd-denybceprefix | Description: The total number of binding update deny messages, due to a BCE prefix not matching, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “BCE prefix set do not match”. Availability: per LMA service Type: Counter | Int32
bindupd-denygrekey | Description: The total number of binding update deny messages, due to a GRE key option required, sent by LMA service. Triggers: Increments when Binding Ack is sent with status code “GRE key option required”. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresourcesessmgr | Description: The total number of binding update deny messages, due to insufficient resources - no session manager, sent by LMA service.Increments when Binding Update rejected due to No sessmgr. Triggers: Increments when Binding Update rejected due to No sessmgr. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresourcememory | Description: The total number of binding update deny messages, due to insufficient resources - no memory, sent by LMA service. Triggers: Increments when Binding Update rejected due to memory alloc failure. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresourcereject | Description: The total number of binding update deny messages, due to insufficient resources - session manager rejected, sent by LMA service. Triggers: Increments when Binding Update rejected due to sessmgr rejection. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresourceinputq | Description: The total number of binding update deny messages, due to insufficient resources - input queue exceeded, sent by LMA service. Triggers: Increments when Binding Update rejected due to demux queue exceeding limit. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresourcesimulbind | Description: The total number of binding update deny messages, due to insufficient resources - simultaneous bindings exceeded, sent by LMA service. Triggers: Increments when Binding Update rejected due to session exceeding binding limit. Availability: per LMA service Type: Counter | Int32
bindupd-denynoresourceaddallocfail | Description: The total number of binding update deny messages, due to insufficient resources - address allocation failed, sent by LMA service. Triggers: Increments when Binding Update rejected due to address alloc failure. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminprohmnaaaauth | Description: The total number of binding update deny messages, due to an administrator prohibited - MN-AAA auth option missing condition, sent by LMA service. Triggers: Increments when Binding Update rejected due to missing MN-AAA auth option. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminprohhbit | Description: The total number of binding update deny messages, due to an administrator prohibited - H-bit not set condition, sent by LMA service. Triggers: Increments when Binding Update rejected due to H bit not set. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminprohmnaaaspi | Description: The total number of binding update deny messages, due to an administrator prohibited - invalid MN-AAA option SPI condition, sent by LMA service. Triggers: Increments when Binding Update rejected due to invalid SPI in MN-AAA auth option. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminprohmnhaspi | Description: The total number of binding update deny messages, due to an administrator prohibited - invalid MN-HA option SPI condition, sent by LMA service. Triggers: Increments when Binding Update rejected due to invalid SPI in MN-HA auth option. Availability: per LMA service Type: Counter | Int32
bindupd-denyadmincong | Description: The total number of binding update deny messages, due to an administrator prohibited - congestion control condition, sent by LMA service. Triggers: Increments when Binding Update rejected due congestion control. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminpolrej | Description: The total number of binding update deny messages, due to an administrator prohibited - policy rejected condition, sent by LMA service. Triggers: Increments when Binding Update rejected due policy. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminhoa | Description: The total number of binding update deny messages, due to an administrator prohibited - HoA not authorized condition, sent by LMA service. Triggers: Increments when Binding Update rejected due HoA authorization failure. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminperm | Description: The total number of binding update deny messages, due to an administrator prohibited - no permission condition, sent by LMA service. Triggers: Increments when Binding Update rejected due to no permission. Availability: per LMA service Type: Counter | Int32
bindupd-denyadminbadreq | Description: The total number of binding update deny messages, due to an administrator prohibited - bad request condition, sent by LMA service. Triggers: Increments when Binding Update decode fails. Availability: per LMA service Type: Counter | Int32
bindupd-discardcong | Description: The total number of binding update discarded messages, due to congestion, sent by LMA service. Triggers: Increments when Binding Update discarded due to congestion control. Availability: per LMA service Type: Counter | Int32
bindupd-discardchecksum | Description: The total number of binding update discarded messages, due to checksum error(s), sent by LMA service. Triggers: Increments when Binding Update discarded due to checksum error Availability: per LMA service Type: Counter | Int32
bindupd-discardauthpending | Description: The total number of binding update discarded messages, due to an initial authentication pending condition, sent by LMA service. Triggers: Increments when Binding Update discarded when initial registration is still being processed. Availability: per LMA service Type: Counter | Int32
bindupd-discardsessnotfound | Description: The total number of binding update discarded messages, due to a session not found condition, sent by LMA service. Triggers: Increments when Binding Update discarded due to session not found internally when expected. Availability: per LMA service Type: Counter | Int32
bindupd-discardhamgrnotready | Description: The total number of binding update discarded messages, due to an HA manager not found condition, sent by LMA service. Triggers: Increments when Binding Update discarded due to hamgr not ready. Availability: per LMA service Type: Counter | Int32
bindupd-discarddecodefail | Description: The total number of binding update discarded messages, due to a decode failure, sent by LMA service. Triggers: Increments when Binding Update discarded due to decode failure. Availability: per LMA service Type: Counter | Int32
bindupd-discardinvbuflen | Description: The total number of binding update discarded messages, due to an invalid buffer length, sent by LMA service. Triggers: Increments when Binding Update discarded due to packet buffer length. Availability: per LMA service Type: Counter | Int32
bindupd-discardrevoc | Description: The total number of binding update discarded messages, due to a revocation pending, sent by LMA service. Triggers: Increments when Binding Update discarded due to pending revocation. Availability: per LMA service Type: Counter | Int32
bindrev-sent | Description: The total number of binding revocations sent by LMA service. Triggers: Increments when initial Binding Revocation indication is sent. Availability: per LMA service Type: Counter | Int32
bindrev-retriessent | Description: The total number of binding revocation retries sent by LMA service. Triggers: Increments when Binding Revocation indication message is retried. Availability: per LMA service Type: Counter | Int32
bindrev-ackrcvd | Description: The total number of binding revocation acknowledgements received by LMA service. Triggers: Increments when Binding Revocation Acknowledgement is received. Availability: per LMA service Type: Counter | Int32
bindrev-notacked | Description: The total number of binding revocations sent, but not acknowledged, by LMA service. Triggers: Increments when session deleted without receiving ACK after max retries. Availability: per LMA service Type: Counter | Int32
bindrev-rcvd | Description: The total number of binding revocations received by LMA service. Triggers: Increments when Binding revocation indication is received. Availability: per LMA service Type: Counter | Int32
bindrev-acksent | Description: The total number of binding revocation acknowledgements sent by LMA service. Triggers: Increments when Binding revocation Acknowledgement is sent. Availability: per LMA service Type: Counter | Int32
sentrevtrig-reserved | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with a “Reserved” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-unspecified | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Unspecified” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-admin | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Administrative Reason” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-maghoffsameatt | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Inter-MAG Handoff-Same ATT” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-maghoff-unknown | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Inter-MAG - Unknown Handoff” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-maghoff-diffatt | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Inter-MAG Handoff-Diff ATT” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-perpeer | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with a “Per-Peer Policy” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-nodelocal | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with a “Revoking Node Local Policy” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-userinitsess | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with a “User Initiated Session Term” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-accessnwsess | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Access Network Session Term” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-ipv4hoabind | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “IPv4 HoA Binding Only” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-syncbce | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Out-of Sync BCE State” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
sentrevtrig-unknown | Description: The total number of Binding Revocation Indication (BRI) messages sent by LMA service with an “Unknown” revocation trigger reason. Availability: per LMA service Type: Counter | Int32
rcvdrevack-success | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “Success” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-partialsuccess | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “Partial-Success” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-nobinding | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “Binding-Does-Not-Exist” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-noipv4hoabind | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “No IPv4-HoA-Bind” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-revocnotauth | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “Global-Revoc-Not-Authorized” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-bindingnotidentified | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “Cannot-Identify-Binding” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-revocfailmnattch | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with a “Revoc-Failed-MN-Attached” status. Availability: per LMA service Type: Counter | Int32
rcvdrevack-unknown | Description: The total number of Binding Revocation Acknowledgement (BRA) messages received by LMA service with an “Unknown” status. Availability: per LMA service Type: Counter | Int32
bindrev | Description: The total number of binding revocation acknowledgements received and discarded by LMA service. Triggers: Increments when Binding revocation Acknowledgement is discarded. Availability: per LMA service Type: Counter | Int32
bindrev-discardsessnotfound | Description: The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to session not found. Availability: per LMA service Type: Counter | Int32
bindrev-discardbadreq | Description: The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to badly formed message. Availability: per LMA service Type: Counter | Int32
bindrev-discarddecodeerror | Description: The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to decode failure. Availability: per LMA service Type: Counter | Int32
bindrev-discardchecksumerror | Description: The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to checksum error. Availability: per LMA service Type: Counter | Int32
bindrev-discardinvalidmsgtype | Description: The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to invalid message type. Availability: per LMA service Type: Counter | Int32
bindrev-discardhamgrnotready | Description: The total number of binding revocation acknowledgements received and discarded, due to a HAMGR not ready condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to HAMGR not ready. Availability: per LMA service Type: Counter | Int32
bindrev-discardmatchreqnotfound | Description: The total number of binding revocation acknowledgements received and discarded, due to a matching request not found condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded as matching request not found. Availability: per LMA service Type: Counter | Int32
bindrev-discardinvalidbuflen | Description: The total number of binding revocation acknowledgements received and discarded, due to a invalid buffer length condition, by LMA service. Triggers: Increments when Binding revocation Acknowledgement discarded due to invalid packet length. Availability: per LMA service Type: Counter | Int32
rxpackets | Description: The total number of packets received by LMA service. Triggers: Increments when tunneled data packet is received. Availability: per LMA service Type: Counter | Int32
rxpackets-6in6 | Description: The total number of IPv6-in-IPv6 tunnel packets received by LMA service. Triggers: Increments when tunneled IPv6 in IPv6 encapsulated data packet is received. Availability: per LMA service Type: Counter | Int32
rxpackets-4in6 | Description: The total number of IPv4-in-IPv6 tunnel packets received by LMA service. Triggers: Increments when tunneled IPv4 in IPv6 encapsulated data packet is received. Availability: per LMA service Type: Counter | Int32
rxpackets-ipv6greipv4 | Description: The total number of IPv4-in-IPv6 GRE tunnel packets received by LMA service. Triggers: Increments when tunneled IPv4 in IPv6 GRE encapsulated data packet is received. Availability: per LMA service Type: Counter | Int32
rxpackets-ipv6greipv6 | Description: The total number of IPv6-in-IPv6 GRE tunnel packets received by LMA service. Triggers: Increments when tunneled IPv6 in IPv6 GREncapsulated data packet is received. Availability: per LMA service Type: Counter | Int32
rxoctets | Description: The total number of octets received by LMA service. Triggers: Increments with number of bytes received when tunneled data packet is received. Availability: per LMA service Type: Counter | Int32
rxoctets-6in6 | Description: The total number of IPv6-in-IPv6 tunnel octets received by LMA service. Triggers: Increments with number of IPv6 in IPv6 bytes received when tunneled data packet is received. Availability: per LMA service Type: Counter | Int32
rxoctets-4in6 | Description: The total number of IPv4-in-IPv6 tunnel octets received by LMA service. Triggers: Increments with number of IPv4 in IPv6 bytes received when tunneled data packet is received. Availability: per LMA service Type: Counter | Int32
rxoctets-ipv6greipv4 | Description: The total number of IPv4-in-IPv6 GRE tunnel octets received by LMA service. Triggers: Increments with number of IPv4 in IPv6 GRE bytes received when tunneled data packet is received. Availability: per LMA service Type: Counter | Int32
rxoctets-ipv6greipv6 | Description: The total number of IPv6-in-IPv6 GRE tunnel octets received by LMA service. Triggers: Increments with number of IPv6 in IPv6 GRE bytes received when tunneled data packet is received. Availability: per LMA service Type: Counter | Int32
dataerror | Description: The total number of data errors received by LMA service. Triggers: Increments when error is encountered on processing data packet received from the tunnel. Availability: per LMA service Type: Counter | Int32
dataerror-proto | Description: The total number of protocol type data errors received by LMA service. Triggers: Increments when packet received with invalid protocol type. Availability: per LMA service Type: Counter | Int32
dataerror-invpktlen | Description: The total number of invalid packet length data errors received by LMA service. Triggers: Increments when packet received with invalid length. Availability: per LMA service Type: Counter | Int32
dataerror-nosess | Description: The total number of no session found data errors received by LMA service. Triggers: Increments when packet received with session not found. Availability: per LMA service Type: Counter | Int32
txpackets | Description: The total number of packets sent by LMA service. Triggers: Increments when tunneled data packet is sent. Availability: per LMA service Type: Counter | Int32
txpackets-6in6 | Description: The total number of IPv6-in-IPv6 tunnel packets sent by LMA service. Triggers: Increments when tunneled IPv6 in IPv6 encapsulated data packet is sent. Availability: per LMA service Type: Counter | Int32
txpackets-4in6 | Description: The total number of IPv4-in-IPv6 tunnel packets sent by LMA service. Triggers: Increments when tunneled IPv4 in IPv6 encapsulated data packet is sent. Availability: per LMA service Type: Counter | Int32
txpackets-ipv6greipv4 | Description: The total number of IPv4-in-IPv6 GRE tunnel packets sent by LMA service. Triggers: Increments when tunneled IPv4 in IPv6 GRE encapsulated data packet is sent. Availability: per LMA service Type: Counter | Int32
txpackets-ipv6greipv6 | Description: The total number of IPv6-in-IPv6 GRE tunnel packets sent by LMA service. Triggers: Increments when tunneled IPv6 in IPv6 GREncapsulated data packet is sent. Availability: per LMA service Type: Counter | Int32
txoctets | Description: The total number of octets sent by LMA service. Triggers: Increments with number of bytes sent when tunneled data packet is sent. Availability: per LMA service Type: Counter | Int32
txoctets-6in6 | Description: The total number of IPv6-in-IPv6 tunnel octets sent by LMA service. Triggers: Increments with number of IPv6 in IPv6 bytes sent when tunneled data packet is sent. Availability: per LMA service Type: Counter | Int32
txoctets-4in6 | Description: The total number of IPv4-in-IPv6 tunnel octets sent by LMA service. Triggers: Increments with number of IPv4 in IPv6 bytes sent when tunneled data packet is sent. Availability: per LMA service Type: Counter | Int32
txoctets-ipv6greipv4 | Description: The total number of IPv4-in-IPv6 GRE tunnel octets sent by LMA service. Triggers: Increments with number of IPv4 in IPv6 GRE bytes sent when tunneled data packet is sent. Availability: per LMA service Type: Counter | Int32
txoctets-ipv6greipv6 | Description: The total number of IPv6-in-IPv6 GRE tunnel octets sent by LMA service. Triggers: Increments with number of IPv6 in IPv6 GRE bytes sent when tunneled data packet is sent. Availability: per LMA service Type: Counter | Int32
icmpv6-pkttoobigrecv | Description: The total number of tunnel ICMP packets - too big received by LMA service. Triggers: Increments when packet too big received with tunnel. Availability: per LMA service Type: Counter | Int32
icmpv6-pkttoobigdrop | Description: The total number of tunnel ICMP packets - too big dropped by LMA service. Triggers: Increments when packet too big received with tunnel is dropped. Availability: per LMA service Type: Counter | Int32
icmpv6-pkttoobigrelay | Description: The total number of tunnel ICMP packets - too big relayed by LMA service. Triggers: Increments when packet too big received with tunnel is relayed. Availability: per LMA service Type: Counter | Int32
disc | Description: The total number of disconnects initiated by LMA service. Triggers: Increments when LMA session disconnects. Availability: per LMA service Type: Counter | Int32
disclifetime | Description: The total number of disconnects due to lifetime expiry initiated by LMA service. Triggers: Increments when LMA session is disconnected due to lifetime expiry. Availability: per LMA service Type: Counter | Int32
discdereg | Description: The total number sessions disconnected in the LMA service due to peer deregistration. Triggers: Increments when LMA session is disconnected due to deregistration. Availability: per LMA service Type: Counter | Int32
discadmin | Description: The total number of disconnects due to admin drops initiated by LMA service. Triggers: Increments when LMA session disconnects due to Admin reasons. Availability: per LMA service Type: Counter | Int32
discother | Description: The total number of disconnects due to “other reasons” initiated by LMA service. Triggers: Increments when LMA session is disconnected due to misc reasons. Availability: per LMA service Type: Counter | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.