# show pcc-policy

This chapter describes the output of the show pcc-policy command.
show pcc-policy service all
Table 1. show pcc-policy service all Command Output Description

Field | Description
--- | ---
Service name | Indicates the name of the PCC-Policy service instancefor which counters are displayed.
Context name | Indicates the name of the context in which the PCC-Policy service instance is configured and running.
Service State | Displays the state of PCC-Policy service instance on an IPCF node. Possible states are: Initial Connected Disconnected
Diameter | This group displays information of Diameter configuration parameters configured in this PCC-Policy service instance.
Origin | Indicates the name of the Diameter origin host configured in this PCC-Policy service instance.
Dictionary | Indicates the Diameter dictionary configured and used for Diameter session (Gx) in this PCC-Policy service instance.
Associate PCC-Service | Indicates the name of the PCC service which is associated with this PCC-Policy service instance.
Max Policy Sessions | Indicates the maximum limit of policy (Gx) sessions allowed in this PCC-Policy service instance.
Newcall Policy | Indicates the action configured when new calls arrived after reaching a threshold limit in this PCC-Policy service instance to manage the congestion control. If configured possible actions are: drop reject
GPRS-Access-BCM | Indicates the Bearer Control Mode configured in PCC-Policy service instance to access the PCEF in GPRS network. If configured possible modes are: as-requested: the PCC-Policy service is configured to accept the BCM request from Application Server (AS) for PCEF access over Gx interface on IPCF node. This is the default mode. ue-nw: the PCC-Policy service is configured to accept the BCM request from UE and/or network element for PCEF access over Gx interface on IPCF node. ue-only: the PCC-Policy service is configured to accept the BCM request from UE only for PCEF access over Gx interface on IPCF node.
eHRPD-Access-BCM | Indicates the Bearer Control Mode configured in PCC-Policy service instance to access the PCEF in eHRPD network. If configured possible modes are: as-requested: the PCC-Policy service is configured to accept the BCM request from Application Server (AS) for PCEF access over Gxa interface on IPCF node. This is the default mode. ue-nw: the PCC-Policy service is configured to accept the BCM request from UE and/or network element for PCEF access over Gxa interface on IPCF node. ue-only: the PCC-Policy service is configured to accept the BCM request from UE only for PCEF access over Gxa interface on IPCF node.
Subscriber Binding ID | Indicatges the subscriber binding identifier used by bindmux for binding subscriber session to PCC-Policy service instance.If configured possible binding identifiers are: IMSI MSISDN NAI SIP-URI
Subscription-ID Absence Action | Indicatges the action configured for PCC Policy when CCR-I message is received by IPCF/PCRF without a valid Subscription id (IMSI, NAT, E164 etc.). Possible actions are: Continue Reject

show pcc-policy service statistics
Table 2. show pcc-policy service statistics Command Output Description

Field | Description
--- | ---
Total Services | Indicates the total number of PCC-Policy services for which counters are displayed.
Messages Statistics | This group displays the summary statistics of messages in a PCC Policy service instance.
Total Messages Recv | Indicates total number of inbound messages received (CCR + RAA).
Total Messages sent | Indicates total number of outbound messages sent (CCA + RAR).
Total CCR | Indicates total number of known (I/U/T) and unknown CCR received.
CCR-Initial | Indicates total number of CCR-I messages received.
CCR-Updates | Indicates total number of CCR-U messages received.
CCR-Terminate | Indicates total number of CCR-T messages received..
Unknown CCR | Indicates total number of CCR messages received with type not determined.
Total CCA | Indicates total number of known (I/U/T) and unknown CCA sent..
CCA-Initial | Indicates total number of CCA-I messages sent.
CCA-Updates | Indicates total number of CCA-U messages sent.
CCA-Terminate | Indicates total number of CCA-T messages sent.
Unknown CCA | Indicates total number of CCA messages sent as response to CCR with type not determined..
CCA with Success | Indicates total number of CCA messages sent with Result-Code as DIAMETER_SUCCESS(2001).
CCA-I with Success | Indicates total number of CCA-I messages sent with Result-Code as DIAMETER_SUCCESS(2001).
CCA-U with Success | Indicates total number of CCA-U messages sent with Result-Code as DIAMETER_SUCCESS(2001).
CCA-T with Success | Indicates total number of CCA-T messages sent with Result-Code as DIAMETER_SUCCESS(2001).
CCA with Failures | Indicates total number of CCA messages rejected.
CCA-I with Failures | Indicates total number of CCA-I messages rejected.
CCA-U with Failures | Indicates total number of CCA-U messages rejected.
CCA-T with Failures | Indicates total number of CCA-T messages rejected.
Total RAA | Indicates total RAA messages received.
Total RAR | Indicates total RAR messages sent.
RAA with Sucesss | Indicates total RAA messages with Result-Code or Experimental-Result-Code as SUCCESS..
RAA with Failure | Indicates total RAA messages with Result-Code or Experimental-Result-Code depicting FAILURE..
RAA without Result | Indicates total RAA messages with both Result-Code or Experimental-Result-Code absent..
Unexpected RAA | Indicates total RAA messages for the non-existing sessions.
RAA parse Sucesss | Indicates total RAA messages with parsing SUCCESS..
RAA parse Failure | Indicates total RAA messages with parsing FAILURE.
Reauth probes | Indicates total RAA messages with reauthorization triggers for subscriber session due to expiry idle timeout timer.
RAR for Sess Release | Indicates total RAR message with Session Release-Cause.
Unspecified | Indicates total RAR message with Session Release-Cause AVP as UNSPECIFIED (0).
UE-subscription-Reason | Indicates total RAR message with Session Release-Cause AVP as UE_SUBSCRIPTION_CHANGED (1).
Insuff Server Resources | Indicates total RAR message with Session Release-Cause AVP as INSUFFICIENT_SERVER_RESOURCES (2).
Total RAR Timeouts | Indicates total RAR messages for which no RAA response was received from PCEF.
Update RAR Timeouts | Indicates total Timed-out RAR messages which were sent by PCRF for session updates (e.g. RAR with new / modified PCC rules / QoS).
Release RAR Timeouts | Indicates total Timed-out RAR messages which were sent by PCRF for session termination (RAR with Session-Release-Cause AVP).
Session-Level Statistics | This group displays the session level statistics of messages in a PCC Policy service instance.
Current Sessions | Indicates the session counter which keeps track of existing sessions under this PCC-Policy service.
Total Session Created | Indicates cumulative number of sessions created at the PCC-Policy service.
Total Session Updates | Indicates cumulative number of sessions updates at the PCC-Policy service. This will include both PCRF-initiated and PCEF initiated updates.
PCEF-Initiated | Indicates cumulative number of PCEF-initiated sessions updates at the PCC-Policy service. This will include session updates through CCR-U message.
PCRF-Initiated | Indicates cumulative number of PCRF-initiated sessions updates at the PCC-Policy service. This will include session updates through RAR.
Total Session Deleted | Indicates cumulative number of session deletion at the PCC-Policy service.
PCEF-Initiated | Indicates cumulative number of PCEF-initiated session terminations at the PCC-Policy service initiated through CCR-T message.
PCRF-Initiated | Indicates cumulative number of PCRF-initiated session termination at the PCC-Policy service initiated through RAR messages with Session-Release-Cause AVP.
Peer Down Initiated | Indicates cumulative number of sessions terminations due to peer disconnect at the PCC-Policy service..
Initial Reject | Indicates cumulative number of sessions terminations at the PCC-Policy service initiated through CCR-I rejection.
Idle Timeout | Indicates the idle session timeout duration set for a subscriber session timer. Possible range of duration is 1 to 4294967295 in seconds. Special value of 0 indicates that timer is disabled and it is the default behavior.
Setup Timeout | Indicates IPCF setup timeout duration set on a system for setup timer. Possible range of duration is 1 to 120 in seconds. By default Setup timeout value is 60 seconds. Special value of 0 indicates that timer is disabled.
Long-duration Timeout | Indicates the long duration idle session timeout set for a subscriber session timer. Possible range of duration is 1 to 4294967295 in seconds. Special value of 0 indicates that timer is disabled and it is the default behavior.
Failure Statistics | This group displays the statistics of various failure reasons in a PCC Policy service instance.
Missng CCR-Type | Indicates total number of CCR messages with mandatory CC-Request-Type AVP missing.
Unexpected CCR-I | Indicates total number of CCR-I message for existing session.
Unexpected CCR-U | Indicates total number of CCR-U message for non-existing session.
Unexpected CCR-T | Indicates total number of CCR-T message for non-existing session.
Missng CCR-Num | Indicates total number of CCR messages with mandatory CC-Request-Number missing.
Out-of-Order CCR | Indicates total number of CCR messages with out-of-order CC-Request-Number.
PCC-Sess Create Fail | Indicates total number of PCC Session Creation Failure after receiving CCR-I due to miscellaneous reasons.
Policy-Sess Create Fail | Indicates total number of PCC Policy Session Creation Failure after receiving CCR-I due to miscellaneous reasons.
PCC-Sess Lookup Fail | Indicates total number of PCC Session Creation Failure after receiving CCR-U/T due to miscellaneous reasons.
Policy-Sess Lookup Fail | Indicates total number of PCC Policy Session Creation Failure after receiving CCR-U/T due to miscellaneous reasons.
Missing Origin-Host | Indicates total number of CCR messages with mandatory Origin-Host AVP missing.
Invalid Origin-Host | Indicates total number of CCR messages with mandatory Origin-Host AVP invalid.
Missing Origin-Realm | Indicates total number of CCR messages with mandatory Origin-Realm AVP missing.
Invalid Origin-Realm | Indicates total number of CCR messages with mandatory Origin-Realm AVP invalid.
Missing Dest-Realm | Indicates total number of CCR messages with mandatory Destination-Realm AVP missing.
Invalid Dest-Realm | Indicates total number of CCR messages with mandatory Destination-Realm AVP invalid.
Unsubscribed Triggers | Indicates total number of Event-Trigger received from PCEF for which PCRF has not subscribed (E.g. RAT_CHANGE received from PCEF even though it is not supplied previously by PCRF).
Unknwown Triggers | Indicates total number of Event-Trigger received from PCEF which is undefined for the policy version. (E.g. Defaul-EPS-Bearer-QoS-Change received for R7-Gx).
Non-Applicable Triggers | Indicates total number of Event-Trigger received from PCEF which is not applicable for the access-type. (E.g. Defaul-EPS-Bearer-QoS-Change received for R8 GGSN with 3GPP-GPRS access).
Missing Trigger-Param | Indicates total number of Event-Trigger received from PCEF without the related parameter (E.g. PCEF sending RAT_CHANGE without the RAT-Type value).
Invalid Trigger-Param | Indicates total number of Event-Trigger received from PCEF with invalid related parameter (E.g. PCEF sending RAT_CHANGE by RAT-Type reported is same as previous one).
Event-Trigger in CCR-I | Indicates total number of Event-Trigger received from PCEF in CCR-I message.
Event-Trigger in CCR-T | Indicates total number of Event-Trigger received from PCEF in CCR-T message.
Invalid BCM Request | Indicates total number of failure cases where PCEF requests bearer control mode (BCM) as UE-ONLY by sending Network-Request-Not-Supported in CCR-I. However, operator configured BCM is UE-NW. Thus, BCM is not provisioned and PCRF rejects this CCR.
QoS-Auth Fail | Indicates total number of failure when PCRF rejects the CCR in case of QoS-authorization failure in CCR-I message.
Invalid Initial Param | Indicates total number of failure when PCRF rejects the CCR with Experimental Result-Code DIAMETER_ERROR_INITIAL_PARAMETERS due to incorrect information in the request.
Invalid AVP Value | Indicates total number of failure when PCRF rejects the CCR with Result-Code DIAMETER_INVALID_AVP_VALUE due to incorrect AVP value in the request.
Unsupported AVP | Indicates total number of failure when PCRF rejects the CCR with Result-Code DIAMETER_AVP_UNSUPPORTED due to incorrect AVP value in the request.
Missing AVP | Indicates total number of failure when PCRF rejects the CCR with Result-Code DIAMETER_MISSING_AVP due to incorrect AVP value in the request.
Session-Linking Failurre | Indicates total number of failure when PCRF rejects the CCR-I with Result-Code DIAMETER_AUTHORIZATION_REJECTED due to Session Linking failure.
Unavail Srv Credits | Indicates total number of session failure due to unavailability of enough service credits for PCC-Policy Session creation.
Multiple Policy Sess Reject | Indicates total number of session rejection due to no-support for multiple PCC session per subscriber available but attempted by PCEF.
Diameter Statistics | This group displays the statistics of various Diameter interface messages in a PCC Policy service instance.
App Register Success | Indicates total number of successful diabase registrations at this PCC-Policy service due to service addition.
App Register Fail | Indicates total number of failed diabase registrations performed at this PCC-Policy service due to service addition.
App Unregister Success | Indicates total number of successful diabase deregistration at this PCC-Policy service due to service removal.
App Unregister Fail | Indicates total number of failed diabase deregistration performed at this PCC-Policy service due to service removal.
App Reregister Success | Indicates total number of successful diabase re-registrations at this PCC-Policy service due to service modification.
App Reregister Fail | Indicates total number of failed diabase registrations performed at this PCC-Policy service due to service modification.
Total Msg Create Fail | Indicates total number of failure to create diabase messages for CCA and RAR.
CCA Create Fail | Indicates total number of failure to create diabase messages for CCA.
RAR Create Fail | Indicates total number of failure to create diabase messages for RAR.
Total Msg Encode Fail | Indicates total number of failure to encode diabase message AVP for CCA and RAR.
CCA Encode Fail | Indicates total number of failure to encode diabase message AVP for CCA.
RAR Encode Fail | Indicates total number of failure to encode diabase message AVP for RAR.
Total Msg Send Fail | Indicates total number of failure to send diabase messages for CCA and RAR.
CCA Send Fail | Indicates total number of failure to send diabase messages for CCA.
RAR Send Fail | Indicates total number of failure to send diabase messages for RAR.
Termination Cause Statistics | This group displays the statistics of various causes for session termination in a PCC Policy service instance.
Diameter Logout | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_LOGOUT (1).
Serv | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_SERVICE_NOT_PROVIDED (2).
Bad Answer | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_BAD_ANSWER (3).
Administrative | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_ADMINISTRATIVE (4).
Link Broken | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_LINK_BROKEN (5).
Auth Expired | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_AUTH_EXPIRED (6).
User Moved | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_USER_MOVED (7).
Session Timeout | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_SESSION_TIMEOUT (8).
Rule Report Statistics | This group displays the statistics of various Rule Reports in a PCC Policy service instance.
Total Rules Reports | Indicates total number of rule-reports received for various PCC/QoS rules.
Total Install Failures | Indicates total number of rule-reports received for various PCC/QoS rule installation failures.
Total Install Success | Indicates total number of rule-reports received for various successful PCC rule installation.
Total Credit Exhaustion | Indicates total number of rule-reports received for various PCC rule out-of-credit.
Total Credit Reallocs | Indicates total number of rule-reports received for various PCC rule credit reallocation.
Unknown Rule-Names | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as UNKNOWN_RULE_NAME (1).
Rating Group Errors | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as RATING_GROUP_ERROR (2).
Service-ID Errors | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as SERVICE_IDENTIFIER_ERROR (3).
GW-PCEF Malfunctions | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as GW/PCEF_MALFUNCTION (4).
Resource Limitations | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as RESOURCES_LIMITATIONS (5).
Max-NR-Bearers Reached | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as MAX_NR_BEARERS_REACHED (6).
Unknown Bearer ID | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as UNKNOWN_BEARER_ID (7).
Missing BearerID | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as MISSING_BEARER_ID (8).
Missing Flow-Desc | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as MISSING_FLOW_DESCRIPTION (9).
Resource Alloc Fail | Indicates total number of rule-reports received for valrious PCC rule installation failures with Rule-Failure-Code as RESOURCE_ALLOCATION_FAILURE (10).
QoS Validation Fail | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as UNSUCCESSFUL_QOS_VALIDATION (11).
Usage Statistics | This group displays the usage statistics in a PCC Policy service instance.
Total Usage Thresholds | Indicates total number of usage thresholds supplied to PCEF for various monitoring instances.
Rule-Level Thresholds | Indicates total number of PCC-Rule-Level usage thresholds supplied to PCEF for various monitoring instances.
Sess-Level Thresholds | Indicates total number of Session-Level usage thresholds supplied to PCEF for various monitoring instances.
Rule-Level Report Req | Indicates total number of PCRF initiated PCC-Rule-Level usage report requests supplied to PCEF for various monitoring instances.
Sess-Level Report Req | Indicates total number of PCRF initiated session-level usage report requests supplied to PCEF for various monitoring instances.
Rule-Level Disable Requests | Indicates total number of PCRF initiated PCC-Rule-level usage report disable requests supplied to PCEF for various monitoring instances.
Sess-Level Disable Req | Indicates total number of PCRF initiated session-level usage report disable requests supplied to PCEF for various monitoring instances.
SPR Statistics | This group displays the statistics related to SSC/SPR instances and procedures associated with a PCC Policy service instance.
Profile Register | Indicates total messages sent to SPR for Subscriber Profile Registration.
Profile Deregister | Indicates total messages sent to SPR for Subscriber Profile Deregistration.
Usage Register | Indicates total messages sent to SPR for Subscriber Usage Registration.
Usage Deregister | Indicates total messages sent to SPR for Subscriber Usage Deregistration.
Usage Updates | Indicates total messages sent to SPR for Subscriber Usage Update.
RAR-CCR | Indicates total RAR and CCR message collisions.
Update RAR-CCR-U | Indicates total message collision between CCR-U message from PCEF and RAR message sent by PCRF for policy update.
Update RAR-CCR-T | Indicate total message collision between CCR-T message from PCEF and RAR message sent by PCRF for policy update.
Update RAR-CCR-U | Indicates total message collision between CCR-U message from PCEF and RAR message sent by PCRF for session release.
Update RAR-CCR-T | Indicates total message collision between CCR-T message from PCEF and RAR message sent by PCRF for session release.

show pcc-policy session full all
Table 3. show pcc-policy session full all Command Output Description

Field | Description
--- | ---
Callid | Indicates the identity number of the IP-CAN call registered on the PCC-Policy service instancefor which counters are displayed.
Session ID | Indicates the identity number of the IP-CAN session active on the PCC-Policy service instancefor which counters are displayed.
Peer ID | Indicates the identity number (IP address) of the PCEF node used in IP-CAN session within the PCC-Policy service instancefor which counters are displayed.
Service Name | Indicates the name of the PCC-Policy service instancefor which counters are displayed.
Service Type | Indicates the type of IP-CAN session on the PCC-Policy service instancefor which counters are displayed.
IMSI | Indicatges the IMSI number of subscriber used by bindmux for binding subscriber session to PCC-Policy service instance.
MSISDN | Indicatges the MSISDN number of subscriber used by bindmux for binding subscriber session to PCC-Policy service instance.
APN Name | Indicates the name of the APN used by IP-CAN session to serve subscriber in the PCC-Policy service instance.
IMEI | Indicates the IMEI number of UE used by bindmux for binding subscriber session to PCC-Policy service instance.
Session State | Indicates the state of the IP-CAN session on PCC-Policy service instance. Possible states are: Initial Connected Disconnected
Framed-IPv4 | Indicates the IPv4 address, if used, for frame route relay prefix in IP-CAN session on PCC-Policy service instance.
Framed-IPv6 | Indicates the IPv6 address, if used, for frame route relay prefix in IP-CAN session on PCC-Policy service instance.
RAT-Type | Indicates the Radio Access Type used for this IP-CAN session. Possible RAT types are: UTRAN E-UTRAN GPRS
SGSN_MCC | Indicates the Mobile Country Code used in IP-CAN session on PCC-Policy service instance.
SGSN_MNC | Indicates the Mobile Network Code used in IP-CAN session on PCC-Policy service instance.
IP-CAN-Type | Indicates the type of IP-CAN session active on PCC-Policy service instance.
BCM | Indicates the Bearer Control Mode configured in PCC-Policy service instance to access the PCEF in GPRS/eHRPD network. If configured possible modes are: as-requested: the PCC-Policy service is configured to accept the BCM request from Application Server (AS) for PCEF access over Gx interface on IPCF node. This is the default mode. ue-nw: the PCC-Policy service is configured to accept the BCM request from UE and/or network element for PCEF access over Gx interface on IPCF node. ue-only: the PCC-Policy service is configured to accept the BCM request from UE only for PCEF access over Gx interface on IPCF node.
ANC-Address | Indicates the IP address of the Access Network Controller node of the IP-CAN session on the PCC-Policy service instancefor which counters are displayed.
ANC-Identifier | Indicates the identity number of the Access Network Controller node used in IP-CAN session within the PCC-Policy service instancefor which counters are displayed.
Event-Trigger | Indicates the event triggers configured/activated for IP-CAN session within the PCC-Policy service instancefor which counters are displayed.