# OSPF Configuration Mode Commands

The OSPF Configuration sub-mode is used to configure the Open Shortest Path First (OSPF) routing protocol. This mode includes commands that configure OSPF routing parameters.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
area authentication

Enables authentication for the specified OSPF area.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area  { ipaddress | decimal_value } authentication [ message-digest ]

no

Disables authentication for the specified area.
ipaddress

Specifies the IP address of the area where authentication will be enabled in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the area where authentication will be enabled. This must be an integer from 0 through 4294967295.
authentication

Sets the OSPF authentication type to use the simple authentication method.
message-digest

Sets the OSPF authentication type to use the message digest 5 (MD5) authentication method.
Usage:

Use this command to enable authentication of OPSF areas.
Example:

The following command enables authentication for an OSPF area defined by the IP address 192.168.100.10 and the OSPF authentication type to MD5:

    area 192.168.100.10
    authentication message-digest

area default-cost

Configures the default cost for an area.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area { ipaddress | decimal_value }  default-cost  cost_value

no

Deletes the default cost for the area.
ipaddress

Specifies the IP address of the area in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the area as an integer from 0 through 4294967295.
cost_value

Sets the default cost to be configured for the specified area as an integer from 0 through 16777215.
Usage:

Use this command to configure the default cost for an OSPF area.
Example:

The following command sets the default cost for an OSPF area defined by the IP address 192.168.100.10 to 300:

    area 192.168.100.10
    default-cost 300

area nssa

Defines an area as an NSSA (Not So Stubby Area) and configures OSPF parameters for it.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area { ipaddress | decimal_value } nssa [ default-information-originate ] [ no-redistribution ] [ no-summary ] [ translate-always ] [ translate-candidate ] [ translate-never ]

ipaddress

Specifies the IP address of the NSSA in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the NSSA area as an integer from 0 through 4294967295.
default-information-originate

Originates default information to the NSSA area.
no-redistribution

Does not redistribute external routes to the NSSA area.
no-summary

Does not inject inter-area routes into NSSA.
translate-always

Configures the NSSA-ABR (Area Border Router) to always translate
translate-candidate

Configure NSSA-ABR for translate election. (This is enabled by default.)
translate-never

Configure NSSA-ABR to never translate.
Usage:

Use this command to define NSSA areas.
Example:

The following command defines the area designated by the IP address 192.168.100.10 as an NSSA area:

    area 192.168.100.10 nssa

area stub

Defines an area as an OSPF stub area.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HAGGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area { ipaddress | decimal_value } stub [ no-summary ]

ipaddress

Specifies the IP address of the stub area in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the stub area as an integer from 0 through 4294967295.
no-summary

Disables (stops) the ABR (Area Border Router) from sending summary link state advertisements (LSAs) into the stub area.
Usage:

Use this command to define an OPSF area as a stub area.
Example:

The following command defines the OSPF area defined by the IP address 192.168.100.10 as a stub area:

    area 192.168.100.10 stub

area virtual-link

Configures a virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area { ipaddress | decimal_value }  virtual-link router_id_address

no

Disables area virtual-link.
ipaddress

Specifies the IP address of the transit area in IPv4 dotted-decimal notation.
decimal-value

Specifies The identification number of the transit area as an integer from 0 through 4294967295.
router_id_address

Specifies the router id of the ABR to be linked to in IPv4 dotted-decimal notation.
Usage:

Use this command to create a virtual link between an area that is connected to the network backbone and an area that cannot be connected to the network backbone.
Example:

The following command creates a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20:

    area 192.168.100.10
    virtual-link 192.168.200.20

area virtual link authentication

Configures the OSPF authentication method to be used by the virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area { ipaddress | decimal_value } virtual-link router_id_address authentication  { message-digest |  null | text }

no

Disables area virtual link authentication.
ipaddress

Specifies the IP address of the transit ares in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the transit area as an integer from 0 through 4294967295.
router_id_address

Specifies the router id of the ABR to be linked to in IPv4 dotted-decimal notation.
authentication

Sets the OSPF authentication type to use the simple authentication method.
message-digest

Sets the OSPF authentication type to use the message digest (MD) authentication method.
null

Set the OSPF authentication type to use no authentication, thus disabling either MD or clear text methods.
text

Set the OSPF authentication type to use the clear text authentication method.
Usage:

Use this command to set the authentication method for a virtual link between an area that is connected to the network backbone and an area that cannot be connected to the network backbone.
Example:

The following command sets the authentication method for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20 to use no authentication:

    area 192.168.100.10
    virtual-link 192.168.200.2 null

area virtual-link authentication-key

Configures the authentication password for the virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    area { ipaddress | decimal_value } virtual-link router_id_address authentication-key { encrypted password  encrypted_authentication_key | password authentication_key }no area { ipaddress | decimal_value } virtual-link router_id_address authentication-key

no

Disables the area virtual link authentication key.
ipaddress

Specifies the IP address of the transit area in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the transit area as an integer from 0 through 4294967295.
router_id_address

Specifies the router id of the ABR to be linked to in IPv4 dotted-decimal notation.
encrypted password

encrypted_authentication_key is an alphanumeric string of 1 through 523 characters.

Use this if you are pasting a previously encrypted authentication key into the CLI command.
password authentication_key

The password to use for authentication. authentication_key is an alphanumeric string of 1 through 16 characters that denotes the authentication password. This variable is entered in clear text format.
Usage:

Use this command to specify the authentication password for a virtual link between an area that is connected to the network backbone and an area that cannot be connected to the network backbone.
Example:

The following command creates an authentication password of 123456 for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20:

    area 192.168.100.10
    virtual-link 192.168.200.20 authentication-key password 123456

area virtual link intervals

Configures the interval or delay type, and the delay time in seconds, for the virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] area { ipaddress | decimal_value } virtual-link router_id_address  [ dead-interval value ] [ hello-interval value ] [ retransmit-interval value ] [ transmit-delay value ]

no

Disables the area virtual link intervals.
ipaddress

Specifies the IP address of the area in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the transit area as an integer from 0 through 4294967295.
router_id_address

Specifies the router id of the ABR to be linked to in IPv4 dotted-decimal notation.
dead-interval value

Specifies The interval (in seconds) that the router should wait, during which time no packets are received and after the router considers a neighboring router to be off-line. value must be an integer from 1 through 65535.
hello-interval value

Specifies the interval (in seconds) before sending a hello packet. value must be an integer from 1 through 65535.
retransmit-interval value

Specifies the interval (in seconds) that router should wait before retransmitting a packet. value must be an integer from 1 through 3600.
transmit-delay value

Specifies the interval (in seconds) that the router should wait before transmitting a packet. value must be an integer from 1 through 3600.
Usage:

Use this command to set the intervals or delay types for a virtual link between an area that is connected to the network backbone and an area that cannot be connected to the network backbone.
Example:

The following command sets the retransmit interval for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20 to 60 seconds:

    area 192.168.100.10
    virtual-link 192.168.200.20 retransmit-interval 60

area virtual link message-digest-key

Enables the use of MD5-based OSPF authentication for the virtual link between an area that cannot be physically connected to the network backbone and an area that is physically connected to the network backbone.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    area { ipaddress | decimal_value } virtual-link router_id_address message-digest-key key_id  md5 { encrypted password encrypted_authentication_key |
     password authentication_key }no  area { ipaddress | decimal_value } virtual-link router_id_address message-digest-key key_id

no

Disables the area virtual link message digest key.
ipaddress

Specifies the IP address of the transit area in IPv4 dotted-decimal notation.
decimal-value

Specifies the identification number of the transit area as an integer from 0 through 4294967295.
router_id_address

Specifies the router id of the ABR to be linked to in IPV4 dotted-decimal notation.
message-digest-key key_id

Specifies the key identifier number. key_id must be an integer from 1 through 255.
encrypted password

Specifies the use of an encrypted password. encrypted_authentication_key is an alphanumeric string of 1 through 523 characters.

Used this if you are pasting a previously encrypted authentication key into the CLI command.
password authentication_key

Specifies the password to use for authentication. authentication_key is an alphanumeric string from 1 through 16 characters that is entered in clear text format.
Usage:

Use this command to enable the use of MD5-based OSPF authentication for a virtual link between an area that is connected to the network backbone and an area that cannot be connected to the network backbone.
Example:

The following command enables the use of MD5-based OSPF authentication for a virtual link between the OSPF areas defined by the IP address 192.168.100.10 and the IP address 192.168.200.20, sets the MD5 Key ID to 25, and the password to 123456:

    area 192.168.100.10
    virtual-link 192.168.200.20 message-digest-key 25 md5 password 123456

bfd-all-interfaces

Enables or disables Bidirectional Forwarding Detection (BFD) on all OSPF interfaces.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [no] bfd-all-interfaces

no

Disables BFD capability on all interfaces.
Usage:

Use this command to configure BFD on all OSPF interfaces. See the System Administration Guide for additional information on how to configure BFD.
Example:

The following command configures BFD on all OSPF interfaces:

    bfd-all-interfaces

capability graceful-restart

Configures graceful-restart. By default, this capability is set to enabled.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no | default  ] capability graceful-restart

no

Disables the graceful-restart capability.
default

Enables the graceful-restart capability if it has been disabled.
Usage:

Use this command to configure graceful-restart.
Example:

The following command configures graceful-restart:

    capability graceful-restart

default-information originate

Creates a default external route into an OSPF routing domain.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    default-information originatedefault-information originate [ always ] [ metric metric_value ] [ metric-type { 1 | 2 } ] [ route-map route_map_name ]no default-information originate

no

Disables the default external route.
always

Always advertise the route regardless of whether or not the software has a default route.
metric metric_value

Sets the OSPF metric used in creating the default rout as an integer from 1 through 16777214.
metric-type { 1 | 2 }

Sets the default route metric type.

1: Sets the OSPF external link type for default routes to Type 1.

2: Sets the OSPF external link type for default routes to Type 2.
route-map route_map_name

Specifies the name of the default route-map to be use as an alphanumeric string of 1 through 79 characters.
Usage:

Use this command to set the default external route into an OSPF routing domain.
Example:

The following command sets the default external route to originate from the route map named rmap1:

    default-information
    originate route-map rmap1

default-metric

Configures the default metric value for the OSPF routing protocol. All OSPF interfaces have a cost, which is a routing metric that is used in the link-state calculation. Routes with lower total path metrics are preferred over those with higher path metrics. When several equal-cost routes to a destination exist, traffic is distributed equally among them. The default metric is a global parameter that specifies the cost applied to all OSPF routes by default.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    default-metric metric_valueno default-metric

metric-value

Sets the metric value expressed as an integer from 1 through 16777214. Default: 26385.
no

Enables or disables the default metric value for OSPF.
Usage:

Use this command to set the default metric for routes.
Example:

The following command sets the default metric to 235:

    default-metric 235

distance

Configures the OSPF route administrative distances for all OSPF route types or based on specific route type. Administrative distance is the measure used by Cisco routers to select the best path when there are two or more different routes to the same destination from two different routing protocols. Administrative distance defines the reliability of a routing protocol. Each routing protocol is prioritized in order of most to least reliable (believable) using an administrative distance value. A lower numerical value is preferred.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] distance { distance_value | ospf { [ external distance_value ] [ inter-area distance_value ] [ intra-area distance_value ] } }

no

Disables the OSPF route administrative distances for all OSPF route types.
distance_value

Specifies the OSPF route administrative distances as an integer from 1 to 255. The default distance value is 110.
ospf { [ external distance_value ] [ inter-area distance_value ] [ intra-area distance_value ] }

Set the distance value for the specified route type.

external distance_value: Set the OSPF route administrative distance for routes from other routing domains, learned by redistribution. This must be an integer from 1 through 255. The default is 110.

inter-area distance_value: sets the OSPF route administrative distance for routes from one routing area to another. This must be an integer from 1 through 255. The default is 110.

intra-area distance_value: sets the OSPF route administrative distance for all routes within an area. This must be an integer from 1 through 255. The default is 110.
no

Enables or disables the specified option.
Usage:

Use this command to set the administrative distance for OSPF routes.
Example:

The following command sets the administrative distance for all OSPF route types to 30:

    distance 30

distribute-list

Enables or disables the filtering of networks in outgoing routing updates.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] distribute-list route_access_list out { connected | rip | static }

no

Disables the filtering of networks in outgoing routing updates.
route_access_list

Specifies the name of the OSPF route access list to use for filtering as an alphanumeric string of 1 through 63 characters.
connected

Filters connected routes.
rip

Filters RIP routes. (RIP is not supported at this time.)
static

Filters static routes.
no

Disables the specified option.
Usage:

Use this command to enable the filtering of outgoing route updates by using the specified route access list.
Example:
The following command uses the route access list named ral1 to filter outgoing routing updates for all connected routes:

    distribute-list ral1
    out connected

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
ip vrf

Configures the Virtual Routing and Forwarding (VRF) instances for OSPF routing protocol.
Platform:

ASR 5000

ASR 5500
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] ip vrf vrf_name

no

Disables the VRF instances and removes the configured VRF context association for OSPF routing.
vrfvrf_name

Configures Virtual Routing & Forwarding (VRF) parameters.

vrf_name is name of a preconfigured VRF context configured in Context Configuration Mode via the ip vrf command. It is an alphanumeric string of 1 through 63 characters.
Usage:

Use this command to configure the IP VRF forwarding also to associate the preconfigured VRF context with the specific tunnel interface.

This command creates and enters the OSPF VRF Configuration Mode if required to configure the VRF context instances for OSPF routing.
Example:
The following command enables preconfigured VRF context instance ospf_vrf1 for OSPF routing and enters the OSPF VRF Configuration mode:

    ip vrf ospf_vrf1

neighbor

Configures OSPF routers that interconnect to non-broadcast networks.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] neighbor  ip_address  [ poll-interval poll_interval_value ] [ priority priority_value ]

no

Disables OSPF routers that interconnect to non-broadcast networks.
ip_address

Specifies the interface IP address of the OSPF neighbor expressed using IPv4 dotted-decimal notation.
poll-interval poll_interval_value

Default: 120

Sets the number of seconds in the dead neighbor polling interval as an integer from 1 through 65535
priority priority_value

Default: 0

Sets the 8-bit number that represents the router priority value of the non-broadcast neighbor associated with the specified IP address. This must be an integer from 0 through 255. This keyword does not apply to point-to-multipoint interfaces.
Usage:

Use this command to configure OSPF routers that connect to non-broadcast networks.
Example:
The following command specifies an OSPF router neighbor with the IP address of 192.168.100.10:

    neighbor 192.168.100.10

network area

Enables OSPF on an interface and defines the OSPF area for that network.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] network network_ip_address / network_mask area { area_id | area_ip_address }

no

Disables OSPF on an interface and defines the OSPF area for that network.
network_ip_address/network_mask

Specifies the network address and mask as well as the interface on which OSPF will be enabled. network_ip_address in entered in IPv4 dotted-decimal notation, followed by the “/” and the mask (CIDR).
area_id

Specifies the OSPF area identification number for the specified network as an integer from 0 through 4294967295.
area_ip_address

Specifies the IP address of the OSPF area for this network. This must be entered in IPv4 dotted-decimal notation.
Usage:

Use this command to specify the IP address of the network interface that the OSPF router will use.
Example:
The following command specified that the OSPF router will use the interface at IP address 192.168.1.0 with a netmask of 24:

    network 192.168.1.0/24

ospf graceful-restart

Configures OSPF graceful-restart settings.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    ospf graceful-restart { grace-period grace_period  | helper { never | policy { only-reload | only-upgrade } } }

grace-period grace-period

Specifies the OSPF graceful restart grace period (in seconds) as an integer from 1 through 1800. Default grace period is 60 seconds.
helper { never | policy { only-reload | only-upgrade } }

Helps configure OSPF helper settings.

never: Do not allow helper mode.
policy { only-reload | only-upgrade }: Allows ospf graceful-restart helper mode.

- only-reload: Allows ospf graceful-restart helper mode only for a reload.
- only-upgrade: Allows ospf graceful-restart helper mode only for an upgrade.

Default is ospf graceful-restart grace-period.
Usage:

Use this command to configure graceful-restart specific settings.
Example:
The following command sets the graceful restart grace period to 60 seconds:

    ospf graceful-restart
    grace-period 60

    ospf graceful-restart
    helper policy only-reloadL

    ospf graceful-restart
    helper policy only-upgrade

ospf router-id

This command configures the router ID for the OSPF process.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] ospf router-id  ip_address

no

Disables the router ID for the OSPF process.
router-id ip_address

Specifies the router ID for the OSPF process. ip_address is entered using IPv4 dotted-decimal notation.
Usage:

Use this command to set the router ID for the current OSPF router process.
Example:

The following command sets the router ID to 192.168.200.1:

    ospf router-id 192.168.200.1

passive-interface

Enables or disables the suppression of OSPF routing updates on the specified interface.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] passive-interface interface_name

no

Disables the name assigned to a logical interface within the specific context.
interface_name

Specifies the name assigned to a logical interface within the specific context as an alphanumeric string of 1 through 79 characters.
Usage:

Use this command to suppress router updates on an interface in the current context.
Example:

The following command suppresses OSPF routing updates on the interface named Intfc1:

    passive-interface Intfc1

redistribute

Redistributes routes from other protocols to OSPF neighbors using the OSPF protocol.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    redistribute { connected | rip | static } [ metric metric_value ] [ metric-type { 1 | 2 } ] [ route-map route_map_name ]no redistribute { connected | rip | static }

no

Disables the redistributed routes.
connected

Redistributes connected routes.
rip

Specifies that RIP routes will be redistributed. (RIP is not supported at this time.)
static

Redistributes static routes.
metric metric_value

Sets the OSPF metric used in the redistributed route. This must be an integer from 1 through 16777214.
metric-type { 1 | 2 }

Default: 2

Sets route metric type that is applied to redistributed routes.

1: Sets the OSPF external link type for routes to Type 1.

2: Sets the OSPF external link type for routes to Type 2.
route-map route_map_name

Filter routes through the specified route map before redistribution. route_map_name specifies the name of the route-map to use as an alphanumeric string of 1 through 79 characters.
Usage:

Use this command to define what routing protocols should have their routes redistributed into OSPF.
Example:

The following command defines that BGP routes should be redistributed:

    redistribute connected

refresh timer

Adjusts settings for the OSPF refresh timer.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] refresh  timer value

no

Disables the refresh timer.
value

Default: 10

Specifies the minimum amount of time (in seconds) to wait before refreshing a Link-state Advertisement (LSA). This must be an integer from 10 through 1800.
Usage:

Use this command to define the amount of time to wait before refreshing an LSA.
Example:
The following command sets the refresh timer to 90 seconds:

    refresh timer 90

router-id

Configures the router ID for the OSPF process.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] router-id ip_address

no

Disables the router ID for the OSPF process.

Specifies the router ID for the OSPF process in IPv4 dotted-decimal notation.
Usage:

Use this command to set the router ID for the current OSPF router process.
Example:
The following command sets the router ID to 192.168.200.1:

    router-id 192.168.200.1

timers spf

Sets the Shortest Path First (SPF) timers.
Platform:

ASR 5000

ASR 5500
Product:

PDSN, HA, GGSN
Privilege:

Security Administrator, Administrator
Syntax

    timers spf delay_value hold_time_valueno timers spf

no

Disables SPF timers.
delay_value

Default: 5

Specifies the delay time (in seconds) between receiving changes to an SPF calculation. This must be an integer from 0 through 4294967295.
hold_time_value

Default: 10

Specifies the hold time (in seconds) between consecutive SPF calculations. This must be an integer from 0 through 4294967295.
Usage:

Use this command to set the SPF delay and hold timers for the current OSPF router process.
Example:
The following command sets the delay timer to 15 and the hold timer to 15:

    timers spf 15 15