# PCC-Sp-Endpoint Configuration Mode Commands

The PCC-Sp-Endpoint Configuration mode provides a mechanism for Intelligent Policy Control Function (IPCF) to support the Sp interface endpoint. It represents a client end for SSC interactions. The PCC-Sp-Endpoint configuration mode facilitates the configuration of Sp interface, and manages the connection and operational parameters related to its peer.

IMPORTANT:

This configuration mode is supported from StarOS Release 12.1 onward.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
access-type

This command is used to define the type of access protocol to be used with a PCC-Sp-Endpoint instance for IPCF configuration.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    access-type {diameter | ldap}

    default access-type

default

Sets access type protocol to be used by endpoints to default protocol of Diameter protocol in a PCC-Sp-Endpoint instance for IPCF configuration.
diameter

Default: Enabled

Sets access type protocol to be used by endpoints to Diameter protocol in a PCC-Sp-Endpoint instance for IPCF configuration.
ldap

Default: Disabled

Sets access type protocol to be used by endpoints to Lightweight Directory Access Protocol (LDAP) in a PCC-Sp-Endpoint instance for IPCF configuration.
Usage:

Use this command to define the type of access protocol to be used with a PCC-Sp-Endpoint instance for IPCF configuration.
Example:
Following command sets the access type of protocol to Diameter for a PCC-Sp-Endpoint instance.

    default access-type

diameter dictionary

This command is used to assign a Diameter dictionary for interaction with SSC and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    diameter dictionary {sh-custon-starent | sh-custom2 | sh-standard }

    default diameter dictionary

default

Sets the Diameter Sh dictionary to default dictionary sh-custon-starent (3GPP Rel. 8 Sh standard) for Sh interaction and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration.
sh-custom-starent

Default: Enabled

Sets the Diameter Sh dictionary to default dictionary sh-custom-starent for Sh interaction and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration.
sh-custom2

Default: Disabled

Sets the Diameter Sh dictionary to sh-custom2with Cisco ULI AVP support for Sh interaction and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration.
sh-standard

Default: Disabled

Sets the Diameter Sh dictionary to default dictionary sh-standard (3GPP Rel. 8 standard) for Sh interaction and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration.
Usage:

Use this command to assign a Diameter dictionary for Sh interaction and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration.
Example:
Following command sets the Diameter dictionary for Sh interaction and messaging over Sp interface in a PCC-Sp-Endpoint instance of IPCF configuration to 3GPP Rel. 8 standard.

    diameter dictionary sh-standard

diameter origin end-point

This command is used to bind/associate a pre-configured Diameter host/realm (SSC) over Sp interface for SPR interactions with a PCC-Sp-Endpoint instance to be used for subscriber profile and policy management.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    diameter origin endpoint ssc_node_name

    no diameter origin endpoint

no

Removes the associated Diameter Origin Endpoint configuration from PCC-Sp-Endpoint instance configured for IPCF configuration.
ssc_node_name

The ssc_node_name is a predefined Diameter origin endpoint node (SSC) and must be an alphanumerical string from 1 through 63 characters.
Usage:

Use this command to bind the SSC node over Sp interface by associating a pre-configured Diameter Origin Endpoint configuration with a PCC-Sp-Endpoint instance.

The Diameter origin endpoint must be a pre-configured instance in the Context Configuration Mode. For more information on Diameter origin endpoint configuration, refer Diameter Endpoint Configuration Mode Commands chapter.
Example:
Following command associates a pre-configured Diameter endpoint node configuration named ssc_1 with a PCC-Sp-Endpoint instance for subscriber policy profile management.

    diameter origin endpoint ssc_1

Following command removes the pre-associated Diameter endpoint node configuration named ssc_1 from a PCC-Sp-Endpoint instance.

    no diameter origin endpoint

diameter peer-select

This command nominates primary and secondary Diameter peers amongst the peers configured under Diameter Endpoint Configuration instance which is associated with a PCC-Sp-Endpoint configuration.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    diameter peer-select peer pri_peer_name [realm realm_name ] [secondary peer sec_peer_name [realm sec_realm_name ]]

    no diameter peer-select

no

Removes the configured Diameter peer from peer-select process which are configured in Diameter Endpoint configuration associated with PCC-Sp-Endpoint instance configured for IPCF configuration.
peer pri_peer_name

Sets a configured Diameter peer, which is configured in Diameter Endpoint configuration associated with PCC-Sp-Endpoint instance configuration, as primary in Diameter peer selection process for IPCF configuration.

The pri_peer_name is a pre-configured Diameter peer in Diameter Endpoint configuration which is associated with a PCC-Sp-Endpoint configuration and must be an alphanumerical string from 1 through 63 characters. pri_peer_name allows punctuation marks.
realm realm-name

This keyword optionally defines the realm (domain) of a configured primary Diameter peer, which is configured in Diameter Endpoint configuration associated with PCC-Sp-Endpoint instance configuration, in Diameter peer selection process for IPCF configuration.

realm_name is the realm (domain) of the associated primary Diameter peer in Diameter Endpoint configuration which associated with a PCC-Sp-Endpoint configuration. The realm_name must be an alpha and/or numeric string of from 1 to 127 characters. The realm may typically be a company or service name and it allows punctuation marks.
secondary peer sec_peer_name

Sets a configured Diameter peer, which is configured in Diameter Endpoint configuration associated with PCC-Sp-Endpoint instance configuration, as secondary in Diameter peer selection process for IPCF configuration.

The sec_peer_name is a pre-configured Diameter peer in Diameter Endpoint configuration which is associated with a PCC-Sp-Endpoint configuration and must be an alphanumerical string from 1 through 63 characters. sec_peer_name allows punctuation marks.
realm sec_realm-name

This keyword optionally defines the realm (domain) of a configured secondary Diameter peer, which is configured in Diameter Endpoint configuration associated with PCC-Sp-Endpoint instance configuration, in Diameter peer selection process for IPCF configuration.

sec_realm_name is the realm (domain) of the associated primary Diameter peer in Diameter Endpoint configuration which associated with a PCC-Sp-Endpoint configuration. The sec_realm_name must be an alpha and/or numeric string of from 1 to 127 characters. The realm may typically be a company or service name and it allows punctuation marks.
Usage:

Use this command to nominate primary and secondary Diameter peers amongst the peers configured under Diameter Endpoint Configuration instance which is associated with a PCC-Sp-Endpoint configuration. When both primary and secondary are down, the remaining Diameter peers are chosen based on their configured weight in round robin manner.

Multiple Diameter peers can be configured in a PCC-Sp-Endpoint instance by entering this command multiple times.
Example:
Following command nominates a pre-configured Diameter peer dia1 as primary and dia2 as secondary for Diameter peer selection process in a PCC-Sp-Endpoint configuration instance.

    diameter peer-select
    peer dia1 secondary peer dia2

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
profile-data

This command allows the operator to specify data-reference and service indication AVP values used in UDR/SNR message for profile data sent over Sp endpoint when access type is set to Diameter.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    profile-data key data-reference data_ref_value [service-indication svc_ind_value]

    default profile-data key

default

Specifies the data-reference value used in UDR/SNR message for profile data sent over Sp endpoint to default value of ‘0’ (zero) and service indication AVP value to profile data when access type is set to Diameter in PCC-Sp-Endpoint instance.
data-reference data_ref_value

Default: 0

Specifies the data-reference values used in UDR/SNR message for profile data sent over Sp endpoint when access type is set to Diameter in PCC-Sp-Endpoint instance.

The data reference value data_ref_value must be an integer from 1 through 65535.
service-indication svc_ind_value

Specifies the service indication AVP value used in UDR/SNR message for profile data sent over Sp endpoint when access type is set to Diameter in PCC-Sp-Endpoint instance.

IMPORTANT:

The Service-Indication values are set as per application logic and are supposed to be used only with SSC.

The service indication value svc_ind_value must be a string of alpha and/or numeric characters from 1 to 32 characters.
Usage:

Use this command to allow the operator to specify data-reference and service indication AVP values used in UDR/SNR message for profile data sent over Sp endpoint when access type is set to Diameter in PCC-Sp-Endpoint configuration instance.

Default service-indication value varies as per other interface configuration default profile-data key is used to set the service indication value.
Example:
Following command set the data-reference value used in UDR/SNR message for profile data sent over Sp endpoint to default value of ‘0’ (zero) and service-indication value as per application logic when access type is set to Diameter in PCC-Sp-Endpoint instance.

    default profile-data key

profile-update-notification

This command sets the system to indicate whether SSC and IPCF are capable of supporting profile update notifications in a PCC-Sp-Endpoint instance.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    profile-update-notification {allow | disallow}

    default profile-update-notification

default

Set the PCC-Sp-Endpoint instance default mode for supporting profile update notifications in a PCC-Sp-Endpoint instance and also to use the same in a PCC-Sp-Endpoint configuration instance.
allow

Default: Enabled

Set the PCC-Sp-Endpoint instance to support the profile update notifications and also allow to use the same in Sp interaction.
disallow

Default: Disabled

Set the PCC-Sp-Endpoint instance to not to support the profile update notifications and also does not allow to use the same in Sp interaction.
Usage:

Use command to set to indicate whether SSC and IPCF are capable of supporting profile update notifications in a PCC-Sp-Endpoint instance. It also sets that whether profile update notification should be used or not for a PCC-Sp-Endpoint configuration instance.
Example:
Following command indicates that SSC and IPCF are capable of supporting profile update notifications in a PCC-Sp-Endpoint instance and also allow to use it for a PCC-Sp-Endpoint configuration instance.

    default profile-update-notification

spr subscriber identifier

This command sets the PCC-Sp-Endpoint instance to indicate how a subscriber is uniquely identified in SPR database while requesting subscriber data from SSC.
Platform:

ASR 5000
Product:

IPCF
Privilege:

Security Administrator, Administrator
Syntax

    spr subscriber identifier {imsi | msisdn | nai}

    default spr subscriber identifier

default

Sets the PCC-Sp-Endpoint instance to use subscriber IMSI to identify subscriber uniquely in SPR database while requesting subscriber data from SSC.
imsi

Default: Enabled

Sets the PCC-Sp-Endpoint instance to use subscriber IMSI to identify subscriber uniquely in SPR database while requesting subscriber data from SSC.
msisdn

Default: Disabled

Sets the PCC-Sp-Endpoint instance to use subscriber MSISDN to identify subscriber uniquely in SPR database while requesting subscriber data from SSC.
nai

Default: Disabled

Sets the PCC-Sp-Endpoint instance to use Network Address Identifier as token to identify subscriber uniquely in SPR database while requesting subscriber data from SSC.

This token facilitates CDMA users for Policy Control and Charging functions.
Usage:

Use command to set the PCC-Sp-Endpoint instance to indicate how a subscriber is uniquely identified in SPR database on SSC while requesting subscriber data. By default it uses Subscriber IMSI for identification in SPR database.

For IP-CAN session between PDSN and IPCF the subscriber token NAI facilitates the Policy Control and Charging functions to subscribers.
Example:
Following command sets the PCC-Sp-Endpoint instance to use a subscriber IMSI to uniquely identified in SPR database at SSC.

    default spr subscriber identifier