# eGTP-C Service Schema

The eGTP-C schema provides operational statistics that can be used for monitoring and troubleshooting the following products: MME, P-GW, S-GW, SGSN
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the eGTP-C Service Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the eGTP service. This is a key variable. Type: Information | String
vpnid | The identification number of the context configured on the system that is currently facilitating the eGTP service. This is an internal reference number. This is a key variable. Type: Information | Int32
servname | Displays the name of the eGTP service for which the statistics are displayed. This is a key variable. Type: Information | String
servid | The identification number of the service configured on the system that is currently facilitating the eGTP service. This is an internal reference number. This is a key variable. Type: Information | Int32
tun-sent-cresess | The total number of initial tunnel - create session request messages sent by the system. Type: Counter | Int32
tun-sent-retranscresess | The total number of tunnel - retransmitted create session request messages sent by the system. Type: Counter | Int32
tun-recv-cresess | The total number of tunnel - create session request messages received by the system. Type: Counter | Int32
tun-recv-retranscresess | The total number of tunnel - retransmitted create session request messages received by the system. Type: Counter | Int32
tun-sent-cresessresp | The total number of tunnel - create session response messages sent by the system. Type: Counter | Int32
tun-sent-cresessrespaccept | The total number of tunnel - create session response - accepted messages sent by the system. Type: Counter | Int32
tun-sent-cresessrespdenied | The total number of tunnel - create session response - denied messages sent by the system. Type: Counter | Int32
tun-sent-retranscresessresp | The total number of tunnel - retransmitted create session response - messages sent by the system. Type: Counter | Int32
tun-recv-cresessresp | The total number of tunnel - create session response messages received by the system. Type: Counter | Int32
tun-recv-cresessrespaccept | The total number of tunnel - create session response - accepted messages received by the system. Type: Counter | Int32
tun-recv-cresesssrespdenied | The total number of tunnel - create session response - denied messages received by the system. Type: Counter | Int32
tun-sent-crebear | The total number of tunnel - create bearer request messages sent by the system. Type: Counter | Int32
tun-sent-retranscrebear | The total number of tunnel - retransmitted create bearer request messages sent by the system. Type: Counter | Int32
tun-recv-crebear | The total number of tunnel - create bearer request messages received by the system. Type: Counter | Int32
tun-recv-retranscrebear | The total number of tunnel - retransmitted create bearer request messages received by the system. Type: Counter | Int32
tun-sent-crebearresp | The total number of tunnel - create bearer response messages sent by the system. Type: Counter | Int32
tun-sent-crebearrespaccept | The total number of tunnel - create bearer response - accepted messages sent by the system. Type: Counter | Int32
tun-sent-crebearrespdenied | The total number of tunnel - create bearer response - denied messages sent by the system. Type: Counter | Int32
tun-sent-retranscrebearresp | The total number of tunnel - retransmitted create bearer response - messages sent by the system. Type: Counter | Int32
tun-recv-crebearresp | The total number of tunnel - create bearer response messages received by the system. Type: Counter | Int32
tun-recv-crebearrespaccept | The total number of tunnel - create bearer response - accepted messages received by the system. Type: Counter | Int32
tun-recv-crebearrespdenied | The total number of tunnel - create bearer response - denied messages received by the system. Type: Counter | Int32
tun-sent-bearrescmd | The total number of tunnel - bearer resource command messages sent by the system. Type: Counter | Int32
tun-sent-retransbearrescmd | The total number of tunnel - retransmitted bearer resource command messages sent by the system. Type: Counter | Int32
tun-recv-bearrescmd | The total number of tunnel - bearer resource command messages received by the system. Type: Counter | Int32
tun-recv-retransbearrescmd | The total number of tunnel - retransmitted bearer resource command messages received by the system. Type: Counter | Int32
tun-sent-bearrescmd-fail | The total number of tunnel - bearer resource command - failure messages sent by the system. Type: Counter | Int32
tun-sent-retransbearrescmd-fail | The total number of tunnel - retransmitted bearer resource command - failure messages sent by the system. Type: Counter | Int32
tun-recv-bearrescmd-fail | The total number of tunnel - bearer resource command - failure messages received by the system. Type: Counter | Int32
tun-recv-retransbearrescmd-fail | The total number of tunnel - retransmitted bearer resource command - failure messages received by the system. Type: Counter | Int32
tun-sent-modbearreq | The total number of tunnel - modify bearer request messages sent by the system. Type: Counter | Int32
tun-sent-retransmodbearreq | The total number of tunnel - retransmitted modify bearer request messages sent by the system. Type: Counter | Int32
tun-recv-modbearreq | The total number of tunnel - modify bearer request messages received by the system. Type: Counter | Int32
tun-recv-retransmodbearreq | The total number of tunnel - retransmitted modify bearer request messages received by the system. Type: Counter | Int32
tun-sent-modbearresp | The total number of tunnel - modify bearer response - messages sent by the system. Type: Counter | Int32
tun-sent-modbearrespaccept | The total number of tunnel - modify bearer response - accepted messages sent by the system. Type: Counter | Int32
tun-sent-modbearrespdenied | The total number of tunnel - modify bearer response - denied messages sent by the system. Type: Counter | Int32
tun-sent-retransmodbearresp | The total number of tunnel - retransmitted modify bearer response - messages sent by the system. Type: Counter | Int32
tun-recv-modbearresp | The total number of tunnel - modify bearer response messages received by the system. Type: Counter | Int32
tun-recv-modbearrespaccept | The total number of tunnel - modify bearer response - accepted messages received by the system. Type: Counter | Int32
tun-recv-modbearrespdenied | The total number of tunnel - modify bearer response - denied messages received by the system. Type: Counter | Int32
tun-sent-delsessreq | The total number of tunnel - delete session request messages sent by the system. Type: Counter | Int32
tun-sent-retransdelsessreq | The total number of tunnel - retransmitted delete session request messages sent by the system. Type: Counter | Int32
tun-recv-delsessreq | The total number of tunnel - delete session request messages received by the system. Type: Counter | Int32
tun-recv-retransdelsessreq | The total number of tunnel - retransmitted delete session request messages received by the system. Type: Counter | Int32
tun-sent-delsessresp | The total number of tunnel - delete session response messages sent by the system. Type: Counter | Int32
tun-sent-delsessrespaccept | The total number of tunnel - delete session response - accepted messages sent by the system. Type: Counter | Int32
tun-sent-delsessrespdenied | The total number of tunnel - delete session response - denied messages sent by the system. Type: Counter | Int32
tun-recv-delsessresp | The total number of tunnel - delete session response messages received by the system. Type: Counter | Int32
tun-recv-delsessrespaccept | The total number of tunnel - delete session response - accepted messages received by the system. Type: Counter | Int32
tun-recv-delsessrespdenied | The total number of tunnel - delete session response - denied messages received by the system. Type: Counter | Int32
tun-sent-delbearreq | The total number of tunnel - delete bearer request messages sent by the system. Type: Counter | Int32
tun-sent-retransdelbearreq | The total number of tunnel - retransmitted delete bearer request messages sent by the system. Type: Counter | Int32
tun-recv-delbearreq | The total number of tunnel - delete bearer request messages received by the system. Type: Counter | Int32
tun-recv-retransdelbearreq | The total number of tunnel - retransmitted delete bearer request messages received by the system. Type: Counter | Int32
tun-sent-delbearresp | The total number of tunnel - delete bearer response messages sent by the system. Type: Counter | Int32
tun-sent-delbearrespaccept | The total number of tunnel - delete bearer response - accepted messages sent by the system. Type: Counter | Int32
tun-sent-delbearrespdenied | The total number of tunnel - delete bearer response - denied messages sent by the system. Type: Counter | Int32
tun-recv-delbearresp | The total number of tunnel - delete bearer response messages received by the system. Type: Counter | Int32
tun-recv-delbearrespaccept | The total number of tunnel - delete bearer response - accepted messages received by the system. Type: Counter | Int32
tun-recv-delbearrespdenied | The total number of tunnel - delete bearer response - denied messages received by the system. Type: Counter | Int32
tun-sent-dlinknotif | The total number of tunnel - downlink data notification request messages sent by the system. Type: Counter | Int32
tun-sent-retransdlinknotif | The total number of tunnel - retransmitted downlink data notification request messages sent by the system. Type: Counter | Int32
tun-recv-dlinknotif | The total number of tunnel - downlink data notification request messages received by the system. Type: Counter | Int32
tun-recv-retransdlinknotif | The total number of tunnel - retransmitted downlink data notification request messages received by the system. Type: Counter | Int32
tun-recv-dlinknotifack | The total number of tunnel - downlink data notification acknowledgement messages received by the system. Type: Counter | Int32
tun-sent-dlinknotifack | The total number of tunnel - downlink data notification acknowledgement messages sent by the system. Type: Counter | Int32
tun-recv-dlinknotifackaccept | The total number of tunnel - downlink data notification acknowledgement accepted messages received by the system. Type: Counter | Int32
tun-sent-dlinknotifackaccept | The total number of tunnel - downlink data notification acknowledgement accepted messages sent by the system. Type: Counter | Int32
tun-recv-dlinknotifackdenied | The total number of tunnel - downlink data notification acknowledgement denied messages received by the system. Type: Counter | Int32
tun-sent-dlinknotifackdenied | The total number of tunnel - downlink data notification acknowledgement denied messages sent by the system. Type: Counter | Int32
tun-sent-dlinkdatafail | The total number of tunnel - downlink data failure messages sent by the system. Type: Counter | Int32
tun-recv-dlinkdatafail | The total number of tunnel - downlink data failure messages received by the system. Type: Counter | Int32
tun-sent-relaccbearreq | The total number of tunnel - release access bearers request messages sent by the system. Type: Counter | Int32
tun-sent-retransrelaccbearreq | The total number of tunnel - retransmitted release access bearers request messages sent by the system. Type: Counter | Int32
tun-recv-relaccbearreq | The total number of tunnel - release access bearers request messages received by the system. Type: Counter | Int32
tun-recv-retransrelaccbearreq | The total number of tunnel - retransmitted release access bearers request messages received by the system. Type: Counter | Int32
tun-sent-relaccbearresp | The total number of tunnel - release access bearers response messages sent by the system. Type: Counter | Int32
tun-sent-relaccbearrespaccept | The total number of tunnel - release access bearers response accepted messages sent by the system. Type: Counter | Int32
tun-sent-relaccbearrespdenied | The total number of tunnel - release access bearers response denied messages sent by the system. Type: Counter | Int32
tun-sent-retransrelaccbearresp | The total number of tunnel - retransmitted release access bearers response messages sent by the system. Type: Counter | Int32
tun-recv-relaccbearresp | The total number of tunnel - release access bearers response messages received by the system. Type: Counter | Int32
tun-recv-relaccbearrespaccept | The total number of tunnel - release access bearers response accepted messages received by the system. Type: Counter | Int32
tun-recv-relaccbearrespdenied | The total number of tunnel - release access bearers response denied messages received by the system. Type: Counter | Int32
tun-sent-modbearcmd | The total number of tunnel - modify bearer command messages sent by the system. Type: Counter | Int32
tun-sent-retransmodbearcmd | The total number of tunnel - retransmitted modify bearer command messages sent by the system. Type: Counter | Int32
tun-recv-modbearcmd | The total number of tunnel - modify bearer command messages received by the system. Type: Counter | Int32
tun-recv-retransmodbearcmd | The total number of tunnel - retransmitted modify bearer command messages received by the system. Type: Counter | Int32
tun-sent-modbearfail | The total number of tunnel - modify bearer command - failure indication messages sent by the system. Type: Counter | Int32
tun-sent-retransmodbearfail | The total number of tunnel - retransmitted modify bearer command - failure indication messages sent by the system. Type: Counter | Int32
tun-recv-modbearfail | The total number of tunnel - modify bearer command - failure indication messages received by the system. Type: Counter | Int32
tun-recv-retransmodbearfail | The total number of tunnel - retransmitted modify bearer command - failure indication messages received by the system. Type: Counter | Int32
tun-sent-delbearcmd | The total number of tunnel - delete bearer command messages sent by the system. Type: Counter | Int32
tun-sent-retransdelbearcmd | The total number of tunnel - retransmitted delete bearer command messages sent by the system. Type: Counter | Int32
tun-recv-delbearcmd | The total number of tunnel - delete bearer command messages received by the system. Type: Counter | Int32
tun-recv-retransdelbearcmd | The total number of tunnel - retransmitted delete bearer command messages received by the system. Type: Counter | Int32
tun-sent-delbearfail | The total number of tunnel - delete bearer command - failure indication messages sent by the system. Type: Counter | Int32
tun-sent-retransdelbearfail | The total number of tunnel - retransmitted delete bearer command - failure indication messages sent by the system. Type: Counter | Int32
tun-recv-delbearfail | The total number of tunnel - delete bearer command - failure indication messages received by the system. Type: Counter | Int32
tun-recv-retransdelbearfail | The total number of tunnel - retransmitted delete bearer command - failure indication messages received by the system. Type: Counter | Int32
tun-sent-updbearreq | The total number of tunnel - update bearer request messages sent by the system. Type: Counter | Int32
tun-sent-retransupdbearreq | The total number of tunnel - retransmitted update bearer request messages sent by the system. Type: Counter | Int32
tun-recv-updbearreq | The total number of tunnel - update bearer request messages received by the system. Type: Counter | Int32
tun-recv-retransupdbearreq | The total number of tunnel - retransmitted update bearer request messages received by the system. Type: Counter | Int32
tun-sent-updbearresp | The total number of tunnel - update bearer response messages sent by the system. Type: Counter | Int32
tun-sent-updbearrespaccept | The total number of tunnel - update bearer response - accepted messages sent by the system. Type: Counter | Int32
tun-sent-updbearrespdenied | The total number of tunnel - update bearer response - denied messages sent by the system. Type: Counter | Int32
tun-recv-updbearresp | The total number of tunnel - update bearer response messages received by the system. Type: Counter | Int32
tun-recv-updbearrespaccept | The total number of tunnel - update bearer response - accepted messages received by the system. Type: Counter | Int32
tun-recv-updbearrespdenied | The total number of tunnel - update bearer response - denied messages received by the system. Type: Counter | Int32
tun-sent-creinddatafwdngreq | The total number of tunnel - create indicators for data forwarding requests sent by the system. Type: Counter | Int32
tun-sent-retranscreinddatafwdngreq | The total number of tunnel - retransmit indicators for data forwarding requests, sent by the system. Type: Counter | Int32
tun-recv-creinddatafwdngreq | The total number of tunnel - create indicators for data forwarding requests, received by the system. Type: Counter | Int32
tun-recv-retranscreinddatafwdngreq | The total number of tunnel -retransmit indicators for data forwarding requests, received by the system. Type: Counter | Int32
tun-sent-creinddatafwdngrsp | The total number of tunnel - create indicators for data forwarding responses, sent by the system. Type: Counter | Int32
tun-sent-creinddatafwdngrspaccept | The total number of tunnel - create indicators for data forwarding responses accepted, sent by the system. Type: Counter | Int32
tun-sent-creinddatafwdngrspdenied | The total number of tunnel - create indicators for data forwarding responses denied, sent by the system. Type: Counter | Int32
tun-sent-retranscreinddatafwdngrsp | The total number of tunnel - retransmitted create indicators for data forwarding responses, sent by the system. Type: Counter | Int32
tun-recv-creinddatafwdngrsp | The total number of tunnel - create indicators for data forwarding responses, received by the system. Type: Counter | Int32
tun-recv-creinddatafwdngrspaccept | The total number of tunnel - create indicators for data forwarding responses accepted, received by the system. Type: Counter | Int32
tun-recv-creinddatafwdngrspdenied | The total number of tunnel - denied create indicators for data forwarding responses, received by the system. Type: Counter | Int32
tun-sent-delinddatafwdngreq | The total number of tunnel - deleted indicators for data forwarding requests, sent by the system. Type: Counter | Int32
tun-sent-retransdelinddatafwdngreq | The total number of tunnel - retransmitted delete indicators for data forwarding requests, sent by the system. Type: Counter | Int32
tun-recv-delinddatafwdngreq | The total number of tunnel - delete indicators for data forwarding requests, received by the system. Type: Counter | Int32
tun-recv-retransdelinddatafwdngreq | The total number of tunnel - retransmitted delete indicators for data forwarding requests, received by the system. Type: Counter | Int32
tun-sent-delinddatafwdngrsp | The total number of tunnel - delete indicators for data forwarding responses, sent by the system. Type: Counter | Int32
tun-sent-retransdelinddatafwdngrsp | The total number of tunnel - retransmitted delete indicators for data forwarding responses, sent by the system. Type: Counter | Int32
tun-sent-delinddatafwdngrspaccept | The total number of tunnel - delete indicators for data forwarding responses accepted, sent by the system. Type: Counter | Int32
tun-sent-delinddatafwdngrspdenied | The total number of tunnel - delete indicators for data forwarding responses denied, sent by the system. Type: Counter | Int32
tun-recv-delinddatafwdngrsp | The total number of tunnel - delete indicators for data forwarding responses, received by the system. Type: Counter | Int32
tun-recv-delinddatafwdngrspaccept | The total number of tunnel - delete indicators for data forwarding responses accepted, received by the system. Type: Counter | Int32
tun-recv-delinddatafwdngrspdenied | The total number of tunnel - delete indicators for data forwarding responses denied, received by the system. Type: Counter | Int32
tun-sent-changenotfreq | The total number of tunnel - change notification requests, sent by the system. Type: Counter | Int32
tun-sent-retranschangenotfreq | The total number of tunnel - retransmitted change notification requests, sent by the system. Type: Counter | Int32
tun-recv-changenotfreq | The total number of tunnel - change notification requests, received by the system. Type: Counter | Int32
tun-recv-retranschangenotfreq | The total number of tunnel - retransmitted change notification requests, received by the system. Type: Counter | Int32
tun-sent-changenotfresp | The total number of tunnel - change notification responses, sent by the system. Type: Counter | Int32
tun-sent-changenotfrespaccept | The total number of tunnel - change notification accepted responses, sent by the system. Type: Counter | Int32
tun-sent-changenotfrespdenied | The total number of tunnel - change notification denied responses, sent by the system. Type: Counter | Int32
tun-sent-retranschangenotfresp | The total number of tunnel - retransmitted change notification responses, sent by the system. Type: Counter | Int32
tun-recv-changenotfresp | The total number of tunnel - change notification responses, received by the system. Type: Counter | Int32
tun-recv-changenotfrespaccept | The total number of tunnel - change notification accepted responses, received by the system. Type: Counter | Int32
tun-recv-changenotfrespdenied | The total number of tunnel - change notification denied responses, received by the system. Type: Counter | Int32
tun-sent-stoppagingind | The total number of tunnel - Stop paging indications sent by the system. Type: Counter | Int32
tun-recv-stoppagingind | The total number of tunnel - Stop paging indications received by the system. Type: Counter | Int32
csfb-sent-suspendnotf | Circuit-Switched Fallback - The total number of suspend notification messages sent by this service. Type: Counter | Int32
csfb-sent-retranssuspendnotf | Circuit-Switched Fallback - The total number of retransmitted suspend notification messages sent by this service. Type: Counter | Int32
csfb-recv-suspendnotf | Circuit-Switched Fallback - The total number of suspend notification messages received by this service. Type: Counter | Int32
csfb-recv-retranssuspendnotf | Circuit-Switched Fallback - The total number of retransmitted suspend notification messages received by this service. Type: Counter | Int32
csfb-sent-suspendack | Circuit-Switched Fallback - The total number of suspend acknowledgement messages sent by this service. Type: Counter | Int32
csfb-sent-suspendackaccept | Circuit-Switched Fallback - The total number of suspend acknowledgement accepted messages sent by this service. Type: Counter | Int32
csfb-sent-suspendackdenied | Circuit-Switched Fallback - The total number of suspend acknowledgement denied messages sent by this service. Type: Counter | Int32
csfb-recv-suspendack | Circuit-Switched Fallback - The total number of suspend acknowledgement messages received by this service. Type: Counter | Int32
csfb-recv-suspendackaccept | Circuit-Switched Fallback - The total number of suspend acknowledgement accepted messages received by this service. Type: Counter | Int32
csfb-recv-suspenddenied | Circuit-Switched Fallback - The total number of suspend acknowledgement denied messages received by this service. Type: Counter | Int32
csfb-sent-resumenotf | Circuit-Switched Fallback - The total number of resume notification messages sent by this service. Type: Counter | Int32
csfb-sent-retransresumenotf | Circuit-Switched Fallback - The total number of retransmitted resume notification messages sent by this service. Type: Counter | Int32
csfb-recv-resumenotf | Circuit-Switched Fallback - The total number of resume notification messages received by this service. Type: Counter | Int32
csfb-recv-retransresumenotf | Circuit-Switched Fallback - The total number of retransmitted resume notification messages received by this service. Type: Counter | Int32
csfb-sent-resumeack | Circuit-Switched Fallback - The total number of resume acknowledgement message sent by this service. Type: Counter | Int32
csfb-sent-resumeackaccept | Circuit-Switched Fallback - The total number of resume acknowledgement accepted messages sent by this service. Type: Counter | Int32
csfb-sent-resumeackdenied | Circuit-Switched Fallback - The total number of resume acknowledgement denied messages sent by this service. Type: Counter | Int32
csfb-recv-resumeack | Circuit-Switched Fallback - The total number of resume acknowledgement message received by this service. Type: Counter | Int32
csfb-recv-resumeackaccept | Circuit-Switched Fallback - The total number of resume acknowledgement accepted messages received by this service. Type: Counter | Int32
csfb-recv-resumedenied | Circuit-Switched Fallback - The total number of resume acknowledgement denied messages received by this service. Type: Counter | Int32
OutSigPktS5S8PGW | The total number of outgoing signalling packets over the S5/S8 P-GW interface. Type: Counter | Int32
IncSigPktS5S8PGW | The total number of incoming signalling packets over the S5/S8 P-GW interface. Type: Counter | Int32
OutSigOctS5S8PGW | The total number of outgoing signalling octets over the S5/S8 P-GW interface. Type: Counter | Int32
IncSigOctS5S8PGW | The total number of incoming signalling octets over the S5/S8 P-GW interface. Type: Counter | Int32
OutSigPktS5S8SGW | The total number of outgoing signalling packets over the S5/S8 S-GW interface. Type: Counter | Int32
IncSigPktS5S8SGW | The total number of incoming signalling packets over the S5/S8 S-GW interface. Type: Counter | Int32
OutSigOctS5S8SGW | The total number of outgoing signalling octets over the S5/S8 S-GW interface. Type: Counter | Int32
IncSigOctS5S8SGW | The total number of incoming signalling octets over the S5/S8 S-GW interface. Type: Counter | Int32
OutSigPktS11S4SGW | The total number of outgoing signalling packets over the S11 and/or S4 S-GW interface. Type: Counter | Int32
IncSigPktS11S4SGW | The total number of incoming signalling packets over the S11 and/or S4 S-GW interface. Type: Counter | Int32
OutSigOctS11S4SGW | The total number of outgoing signalling octets over the S11 and/or S4 S-GW interface. Type: Counter | Int32
IncSigOctS11S4SGW | The total number of incoming signalling octets over the S11 and/or S4 S-GW interface. Type: Counter | Int32
OutSigPktS11S10MME | The total number of outgoing signalling packets over the S11 and/or S10 MME interface. Type: Counter | Int32
IncSigPktS11S10MME | The total number of incoming signalling packets over the S11 and/or S10 MME interface. Type: Counter | Int32
OutSigOctS11S10MME | The total number of outgoing signalling octets over the S11 and/or S10 MME interface. Type: Counter | Int32
IncSigOctS11S10MME | The total number of incoming signalling octets over the S11 and/or S10 MME interface. Type: Counter | Int32
OutSigPktS4SGSN | The total number of outgoing signalling packets over the S4 SGSN interface. Type: Counter | Int32
IncSigPktS4SGSN | The total number of incoming signalling packets over the S4 SGSN interface. Type: Counter | Int32
OutSigOctS4SGSN | The total number of outgoing signalling octets over the S4 SGSN interface. Type: Counter | Int32
IncSigOctS4SGSN | The total number of incoming signalling octets over the S4 SGSN interface. Type: Counter | Int32
path-sent-echoreq | The total number of path - echo request messages sent by the system. Type: Counter | Int32
path-sent-retransechoreq | The total number of path - retransmitted echo request messages sent by the system. Type: Counter | Int32
path-recv-echoreq | The total number of path - echo request messages received by the system. Type: Counter | Int32
path-sent-echoresp | The total number of path - echo response messages sent by the system. Type: Counter | Int32
path-recv-echoresp | The total number of path - echo response messages received by the system. Type: Counter | Int32
path-sent-versnotsupp | The total number of path - version not supported indication messages sent by the system. Type: Counter | Int32
path-recv-versnotsupp | The total number of path - version not supported indication messages received by the system. Type: Counter | Int32
mobility-sent-ctxreq | The total number of mobility - context request messages sent by the system. Type: Counter | Int32
mobility-sent-retransctxreq | The total number of mobility - retransmitted context request messages sent by the system. Type: Counter | Int32
mobility-recv-ctxreq | The total number of mobility - context request messages received by the system. Type: Counter | Int32
mobility-recv-retransctxreq | The total number of mobility - retransmitted context request messages received by the system. Type: Counter | Int32
mobility-sent-ctxrsp | The total number of mobility - context response messages sent by the system. Type: Counter | Int32
mobility-sent-retransctxrsp | The total number of mobility - retransmitted context response messages sent by the system. Type: Counter | Int32
mobility-recv-ctxrsp | The total number of mobility - context response messages received by the system. Type: Counter | Int32
mobility-recv-retransctxrsp | The total number of mobility - retransmitted context response messages received by the system. Type: Counter | Int32
mobility-sent-ctxrspaccept | The total number of mobility - context response - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-ctxrspdenied | The total number of mobility - context response - denied messages sent by the system. Type: Counter | Int32
mobility-recv-ctxrspaccept | The total number of mobility - context response - accepted messages received by the system. Type: Counter | Int32
mobility-recv-ctxrspdenied | The total number of mobility - context response - denied messages received by the system. Type: Counter | Int32
mobility-sent-ctxack | The total number of mobility - context acknowledge messages sent by the system. Type: Counter | Int32
mobility-sent-retransctxack | The total number of mobility - retransmitted context acknowledge messages sent by the system. Type: Counter | Int32
mobility-recv-ctxack | The total number of mobility - context acknowledge messages received by the system. Type: Counter | Int32
mobility-recv-retransctxack | The total number of mobility - retransmitted context acknowledge messages received by the system. Type: Counter | Int32
mobility-sent-ctxackaccept | The total number of mobility - context acknowledge - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-ctxackdenied | The total number of mobility - context acknowledge - denied messages sent by the system. Type: Counter | Int32
mobility-recv-ctxackaccept | The total number of mobility - context acknowledge - accepted messages received by the system. Type: Counter | Int32
mobility-recv-ctxackdenied | The total number of mobility - context acknowledge - denied messages received by the system. Type: Counter | Int32
mobility-sent-idtreq | The total number of mobility - identity request messages sent by the system. Type: Counter | Int32
mobility-sent-retransidtreq | The total number of mobility - retransmitted identity request messages sent by the system. Type: Counter | Int32
mobility-recv-idtreq | The total number of mobility - identity request messages received by the system. Type: Counter | Int32
mobility-recv-retransidtreq | The total number of mobility - retransmitted identity request messages received by the system. Type: Counter | Int32
mobility-sent-idtrsp | The total number of mobility - identity response messages sent by the system. Type: Counter | Int32
mobility-sent-retransidtrsp | The total number of mobility - retransmitted identity response messages sent by the system. Type: Counter | Int32
mobility-recv-idtrsp | The total number of mobility - identity response messages received by the system. Type: Counter | Int32
mobility-recv-retransidtrsp | The total number of mobility - retransmitted identity response messages received by the system. Type: Counter | Int32
mobility-sent-idtrspaccept | The total number of mobility - identity response - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-idtrspdenied | The total number of mobility - identity response - denied messages sent by the system. Type: Counter | Int32
mobility-recv-idtrspaccept | The total number of mobility - identity response - accepted messages received by the system. Type: Counter | Int32
mobility-recv-idtrspdenied | The total number of mobility - identity response - denied messages received by the system. Type: Counter | Int32
mobility-sent-fwdrelreq | The total number of mobility - forward relocation request messages sent by the system. Type: Counter | Int32
mobility-sent-retransfwdrelreq | The total number of mobility - retransmitted forward relocation request messages sent by the system. Type: Counter | Int32
mobility-recv-fwdrelreq | The total number of mobility - forward relocation request messages received by the system. Type: Counter | Int32
mobility-recv-retransfwdrelreq | The total number of mobility - retransmitted forward relocation request messages received by the system. Type: Counter | Int32
mobility-sent-fwdrelrsp | The total number of mobility - forward relocation response messages sent by the system. Type: Counter | Int32
mobility-sent-retransfwdrelrsp | The total number of mobility - retransmitted forward relocation response messages sent by the system. Type: Counter | Int32
mobility-recv-fwdrelrsp | The total number of mobility - forward relocation response messages received by the system. Type: Counter | Int32
mobility-recv-retransfwdrelrsp | The total number of mobility - retransmitted forward relocation response messages received by the system. Type: Counter | Int32
mobility-sent-fwdrelrspaccept | The total number of mobility - forward relocation response - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-fwdrelrspdenied | The total number of mobility - forward relocation response - denied messages sent by the system. Type: Counter | Int32
mobility-recv-fwdrelrspaccept | The total number of mobility - forward relocation response - accepted messages received by the system. Type: Counter | Int32
mobility-recv-fwdrelrspdenied | The total number of mobility - forward relocation response - denied messages received by the system. Type: Counter | Int32
mobility-sent-fwdaccnotf | The total number of mobility - forward access context notification messages sent by the system. Type: Counter | Int32
mobility-sent-retransfwdaccnotf | The total number of mobility - retransmitted forward access context notification messages sent by the system. Type: Counter | Int32
mobility-recv-fwdaccnotf | The total number of mobility - forward access context notification messages received by the system. Type: Counter | Int32
mobility-recv-retransfwdaccnotf | The total number of mobility - retransmitted forward access context notification messages received by the system. Type: Counter | Int32
mobility-sent-fwdaccack | The total number of mobility - forward access context acknowledge messages sent by the system. Type: Counter | Int32
mobility-sent-retransfwdaccack | The total number of mobility - retransmitted forward access context acknowledge messages sent by the system. Type: Counter | Int32
mobility-recv-fwdaccack | The total number of mobility - forward access context acknowledge messages received by the system. Type: Counter | Int32
mobility-recv-retransfwdaccack | The total number of mobility - retransmitted forward access context acknowledge messages received by the system. Type: Counter | Int32
mobility-sent-fwdaccackaccept | The total number of mobility - forward access context acknowledge - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-fwdaccackdenied | The total number of mobility - forward access context acknowledge - denied messages sent by the system. Type: Counter | Int32
mobility-recv-fwdaccackaccept | The total number of mobility - forward access context acknowledge - accepted messages received by the system. Type: Counter | Int32
mobility-recv-fwdaccackdenied | The total number of mobility - forward access context acknowledge - denied messages received by the system. Type: Counter | Int32
mobility-sent-fwdrelcmpnotf | The total number of mobility - forward relocation complete notification messages sent by the system. Type: Counter | Int32
mobility-sent-retransfwdrelcmpnotf | The total number of mobility - retransmitted forward relocation complete notification messages sent by the system. Type: Counter | Int32
mobility-recv-fwdrelcmpnotf | The total number of mobility - forward relocation complete notification messages received by the system. Type: Counter | Int32
mobility-recv-retransfwdrelcmpnotf | The total number of mobility - retransmitted forward relocation complete notification messages received by the system. Type: Counter | Int32
mobility-sent-fwdrelcmpack | The total number of mobility - forward relocation complete acknowledge messages sent by the system. Type: Counter | Int32
mobility-sent-retransfwdrelcmpack | The total number of mobility - retransmitted forward relocation complete acknowledge messages sent by the system. Type: Counter | Int32
mobility-recv-fwdrelcmpack | The total number of mobility - forward relocation complete acknowledge messages received by the system. Type: Counter | Int32
mobility-recv-retransfwdrelcmpack | The total number of mobility - retransmitted forward relocation complete acknowledge messages received by the system. Type: Counter | Int32
mobility-sent-fwdrelcmpackaccept | The total number of mobility - forward relocation complete acknowledge - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-fwdrelcmpackdenied | The total number of mobility - forward relocation complete acknowledge - denied messages sent by the system. Type: Counter | Int32
mobility-recv-fwdrelcmpackaccept | The total number of mobility - forward relocation complete acknowledge - accepted messages received by the system. Type: Counter | Int32
mobility-recv-fwdrelcmpackdenied | The total number of mobility - forward relocation complete acknowledge - denied messages received by the system. Type: Counter | Int32
mobility-sent-relcancelreq | The total number of mobility - relocation cancel request messages sent by the system. Type: Counter | Int32
mobility-sent-retransrelcancelreq | The total number of mobility - retransmitted relocation cancel request messages sent by the system. Type: Counter | Int32
mobility-recv-relcancelreq | The total number of mobility - relocation cancel request messages received by the system. Type: Counter | Int32
mobility-recv-retransrelcancelreq | The total number of mobility - retransmitted relocation cancel request messages received by the system. Type: Counter | Int32
mobility-sent-relcancelrsp | The total number of mobility - relocation cancel response messages sent by the system. Type: Counter | Int32
mobility-sent-retransrelcancelrsp | The total number of mobility - retransmitted relocation cancel response messages sent by the system. Type: Counter | Int32
mobility-recv-relcancelrsp | The total number of mobility - relocation cancel response messages received by the system. Type: Counter | Int32
mobility-recv-retransrelcancelrsp | The total number of mobility - retransmitted relocation cancel response messages received by the system. Type: Counter | Int32
mobility-sent-relcancelrspaccept | The total number of mobility - relocation cancel response - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-relcancelrspdenied | The total number of mobility - relocation cancel response - denied messages sent by the system. Type: Counter | Int32
mobility-recv-relcancelrspaccept | The total number of mobility - relocation cancel response - accepted messages received by the system. Type: Counter | Int32
mobility-recv-relcancelrspdenied | The total number of mobility - relocation cancel response - denied messages received by the system. Type: Counter | Int32
mobility-sent-cspagingind | The total number of mobility - CS paging indication - messages sent by the system. Type: Counter | Int32
mobility-recv-cspagingind | The total number of mobility - CS paging indication - messages received by the system. Type: Counter | Int32
mobility-sent-alertmmenotf | The total number of mobility - alert MME notification - messages sent by the system. Type: Counter | Int32
mobility-sent-retransalertmmenotf | The total number of mobility - retransmitted alert MME notification - messages sent by the system. Type: Counter | Int32
mobility-recv-alertmmenotf | The total number of mobility - alert MME notification - messages received by the system. Type: Counter | Int32
mobility-recv-retransalertmmenotf | The total number of mobility - retransmitted alert MME notification - messages received by the system. Type: Counter | Int32
mobility-sent-alertmmeack | The total number of mobility - alert MME - acknowledge messages sent by the system. Type: Counter | Int32
mobility-sent-retransalertmmeack | The total number of mobility - retransmitted alert MME - acknowledge messages sent by the system. Type: Counter | Int32
mobility-recv-alertmmeack | The total number of mobility - alert MME - acknowledge messages received by the system. Type: Counter | Int32
mobility-recv-retransalertmmeack | The total number of mobility - retransmitted alert MME - acknowledge messages received by the system. Type: Counter | Int32
mobility-sent-alertmmeackaccept | The total number of mobility - alert MME acknowledge - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-alertmmeackdenied | The total number of mobility - alert MME acknowledge - denied messages sent by the system. Type: Counter | Int32
mobility-recv-alertmmeackaccept | The total number of mobility - alert MME acknowledge - accepted messages received by the system. Type: Counter | Int32
mobility-recv-alertmmeackdenied | The total number of mobility - alert MME acknowledge - denied messages received by the system. Type: Counter | Int32
mobility-sent-ueactivitynotf | The total number of mobility - UE activity notification - messages sent by the system. Type: Counter | Int32
mobility-sent-ueactivitynotf | The total number of mobility - UE activity notification - messages sent by the system. Type: Counter | Int32
mobility-sent-retransueactivitynotf | The total number of mobility - retransmitted UE activity notification - messages sent by the system. Type: Counter | Int32
mobility-recv-ueactivitynotf | The total number of mobility - UE activity notification - messages received by the system. Type: Counter | Int32
mobility-recv-retransueactivitynotf | The total number of mobility - retransmitted UE activity notification - messages received by the system. Type: Counter | Int32
mobility-sent-ueactivityack | The total number of mobility - UE activity - acknowledge messages sent by the system. Type: Counter | Int32
mobility-sent-retransueactivityack | The total number of mobility - retransmitted UE activity - acknowledge messages sent by the system. Type: Counter | Int32
mobility-recv-ueactivityack | The total number of mobility - UE activity - acknowledge messages received by the system. Type: Counter | Int32
mobility-recv-retransueactivityack | The total number of mobility - retransmitted UE activity - acknowledge messages received by the system. Type: Counter | Int32
mobility-sent-ueactivityackaccept | The total number of mobility - UE activity acknowledge - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-ueactivityackdenied | The total number of mobility - UE activity acknowledge - denied messages sent by the system. Type: Counter | Int32
mobility-recv-ueactivityackaccept | The total number of mobility - UE activity acknowledge - accepted messages received by the system. Type: Counter | Int32
mobility-recv-ueactivityackdenied | The total number of mobility - UE activity acknowledge - denied messages received by the system. Type: Counter | Int32
mobility-sent-ranInforelay | The total number of mobility - RAN information relay messages sent by the system. Type: Counter | Int32
mobility-recv-ranInforelay | The total number of mobility - RAN information relay messages received by the system. Type: Counter | Int32
mobility-sent-configxfertun | The total number of mobility - configuration transfer tunnel messages sent by the system. Type: Counter | Int32
mobility-recv-configxfertun | The total number of mobility - configuration transfer tunnel messages received by the system. Type: Counter | Int32
mobility-sent-detachnotf | The total number of mobility - detach notification - messages sent by the system. Type: Counter | Int32
mobility-sent-retransdetachnotf | The total number of mobility - retransmitted detach notification - messages sent by the system. Type: Counter | Int32
mobility-recv-detachnotf | The total number of mobility - detach notification - messages received by the system. Type: Counter | Int32
mobility-recv-retransdetachnotf | The total number of mobility - retransmitted detach notification - messages received by the system. Type: Counter | Int32
mobility-sent-detachack | The total number of mobility - detach - acknowledge messages sent by the system. Type: Counter | Int32
mobility-recv-detachack | The total number of mobility - detach - acknowledge messages received by the system. Type: Counter | Int32
mobility-sent-detachackaccept | The total number of mobility - detach acknowledge - accepted messages sent by the system. Type: Counter | Int32
mobility-sent-detachackdenied | The total number of mobility - detach acknowledge - denied messages sent by the system. Type: Counter | Int32
mobility-recv-detachackaccept | The total number of mobility - detach acknowledge - accepted messages received by the system. Type: Counter | Int32
mobility-recv-detachackdenied | The total number of mobility - detach acknowledge - denied messages received by the system. Type: Counter | Int32
trace-sent-activate | The total number of trace - activate messages sent by the system. Type: Counter | Int32
trace-recv-activate | The total number of trace - activate messages received by the system. Type: Counter | Int32
trace-sent-deactivate | The total number of trace - deactivate messages sent by the system. Type: Counter | Int32
trace-recv-deactivate | The total number of trace - deactivate messages received by the system. Type: Counter | Int32
srvcc-sent-pstocsreq | The total number of PS (Packet Switched) to CS (Circuit Switched) request messages sent by this system, the specified service, or the specified interface. Type: Counter | Int32
srvcc-sent-retranspstocsreq | The total number of PS (Packet Switched) to CS (Circuit Switched) request messages retransmitted. Type: Counter | Int32
srvcc-recv-pstocsrsp | The total number of PS (Packet Switched) to CS (Circuit Switched) request messages received. Type: Counter | Int32
srvcc-recv-pstocsrspaccept | The total number of accepted PS (Packet Switched) to CS (Circuit Switched) response messages received. Type: Counter | Int32
srvcc-recv-pstocsrspdenied | The total number of denied PS (Packet Switched) to CS (Circuit Switched) response messages received. Type: Counter | Int32
srvcc-recv-pstocscmpnotf | The total number of PS (Packet Switched) to CS (Circuit Switched) complete notification messages received. Type: Counter | Int32
srvcc-recv-retranspstocscmpnotf | The total number of retransmitted PS (Packet Switched) to CS (Circuit Switched) complete notification messages received. Type: Counter | Int32
srvcc-sent-pstocscmpack | The total number of PS (Packet Switched) to CS (Circuit Switched) complete acknowledge messages sent. Type: Counter | Int32
srvcc-sent-retranspstocscmpack | The total number of retransmitted PS (Packet Switched) to CS (Circuit Switched) complete acknowledge messages sent. Type: Counter | Int32
srvcc-sent-pstocscmpackaccept | The total number of accepted PS (Packet Switched) to CS (Circuit Switched) complete acknowledge messages sent. Type: Counter | Int32
srvcc-sent-pstocscmpackdenied | The total number of denied PS (Packet Switched) to CS (Circuit Switched) complete acknowledge messages sent. Type: Counter | Int32
srvcc-sent-pstocscancelnotf | The total number of PS (Packet Switched) to CS (Circuit Switched) cancel notification messages sent. Type: Counter | Int32
srvcc-sent-retranspstocscancelnotf | The total number of retransmitted PS (Packet Switched) to CS (Circuit Switched) cancel notification messages sent. Type: Counter | Int32
srvcc-recv-pstocscancelack | The total number of PS (Packet Switched) to CS (Circuit Switched) cancel acknowledge messages received. Type: Counter | Int32
srvcc-recv-pstocscanelackaccept | The total number of accepted PS (Packet Switched) to CS (Circuit Switched) cancel acknowledge messages received. Type: Counter | Int32
srvcc-recv-pstocscancelackdenied | The total number of denied PS (Packet Switched) to CS (Circuit Switched) cancel acknowledge messages received. Type: Counter | Int32
gtpv1path-sent-echoreq | The total number of GTPv1 path - echo request messages sent by the system. Type: Counter | Int32
gtpv1path-recv-echoreq | The total number of GTPv1 path - echo request messages received by the system. Type: Counter | Int32
gtpv1path-sent-echoresp | The total number of GTPv1 path - echo response messages sent by the system. Type: Counter | Int32
gtpv1path-recv-echoresp | The total number of GTPv1 path - echo response messages received by the system. Type: Counter | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.