# HNB-RN PLMN Configuration Mode Commands

This HNB Radio Network PLMN configuration mode defines the radio network PLMN parameters related to the HNB-GW connection with a UMTS Femto radio network.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
associate cs-network

From StarOS Release 14.0 onward this command is deprecated.
associate ps-network

From StarOS Release 14.0 onward this command is deprecated.
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
rnc-id

Configures the Radio Network Concentrator (RNC) identifier in a Radio Network PLMN associated with HNB-GW service. The RNC identifier is provided to the HNB during HNB-REGISTRATION.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] rnc-id rnc_id

no

Deletes the RNC id from the system configuration.
rnc-id

Specifies the RNC identifier as an integer from 0 through 4095.
Usage:

Use this command to configure RNC id for Radio Network PLMN which will be sent to HNBs from HNB-GW during HNB-REGISTRATION procedure. Depending upon the requirement the RNC Identifier can be provided at the desired granularity.
Example:
The following command configures the HNB-GW service to return an RNC identifier as 102 when an HNB-REGISTRATION request is received:

    global rnc-id 102