# LTE Policy Configuration Mode Commands

The LTE Policy Configuration Mode is used to create and manage the LTE policies supporting MME and S-GW configurations on the system.

IMPORTANT:

Available commands or keywords/variables vary based on platform type, product version, and installed license(s).
congestion-action-profile

Creates an action profile for MME critical, major and minor congestion thresholds. The profile defines the action to be taken when these thresholds are exceeded.
Platform:

ASR 5000
Product:

MME
Privilege:

Administrator
Syntax

    [ no ] congestion-action-profile profile_name

no

Removes the specified profile from the system.
profile_name

Specifies the name of the action profile. If the entered name does not refer to an existing profile, a new profile is created. profile_name is an alphanumeric string of 1 through 64 characters.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
Usage:

Use this command to establish MME action profiles to be associated with critical, major and minor congestion thresholds. This command is also used to remove an existing profile.

Note:

This command is part of a licensed feature and requires a proper license to function: MME Resiliency Bundle.

For information on setting the action to be taken within this profile, see the Congestion Action Profile Configuration Mode Commands chapter in this guide, and the Congestion Control chapter in the System Administration Guide.
Example:
The following command creates a major congestion action profile named mme_major_profile and moves to the Congestion Action Profile Configuration mode:

    congestion-action-profile
    mme_major_profile

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
ho-restrict-list

Creates a handover (HO) restriction list or specifies an existing HO restriction list and enters the Handover Restriction List Configuration Mode.
Platform:

ASR 5000

ASR 5500
Product:

MME, SAEGW, S-GW
Privilege:

Administrator
Syntax

    [ no ] ho-restrict-list list_name [ -noconfirm ]

no

Removes the specified restriction list from the system.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
list_name

Specifies the name of the HO restriction list. If the entered list name does not refer to an existing list, a new list is created. list_name is an alphanumeric string of 1 through 64 characters.
Usage:

Use this command to enter the Handover Restriction List Configuration Mode for an existing list or for a newly defined list. This command is also used to remove an existing list.

Entering this command results in the following prompt:

    [context_name]hostname(ho-restrict-list)#

Handover Restriction List Configuration Mode commands are defined in the LTE Handover Restriction List Configuration Mode Commands chapter.
Example:
The following command enters the Handover Restriction List Configuration Mode for a new or existing list named ho_restricit_list1:

    ho-restrict-list ho_restrict_list1

lte-emergency-profile

Creates an LTE emergency profile or specifies an existing emergency profile and enters the LTE Emergency Profile Configuration Mode.
Platform:

ASR 5000

ASR 5500
Product:

MME, SAEGW, S-GW
Privilege:

Administrator
Syntax

    [ no ] lte-emergency-profile profile_name [ -noconfirm ]

no

Removes an LTE emergency profile from the system.
profile_name

Specifies the name of the LTE emergency profile being created or accessed. If the profile name does not refer to an existing profile, a new profile is created. profile_name is an alphanumeric string of 1 through 64 characters.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
Usage:

Use this command to enter the LTE Emergency Profile Configuration Mode for an existing profile or for a newly defined profile. This command is also used to remove an existing profile.

IMPORTANT:

A maximum of four LTE emergency profiles are allowed per system.

Entering this command results in the following prompt:

    [context_name]hostname(lte-emergency-profile)#

LTE Emergency Profile Configuration Mode commands are defined in the LTE Emergency Profile Configuration Mode Commands chapter.
Example:
The following command enters the LTE Emergency Profile Configuration Mode for a new or existing profile named emergency_profile3:

    lte-emergency-profile emergency_profile3

network-global-mme-id-mgmt-db

Creates a new, or enters the existing MME group ID management database.
Platform:

ASR 5000

ASR 5500
Product:

MME, SAEGW, S-GW, SGSN

IMPORTANT:

Currently, the SGSN is not supported on the ASR 5000 platform.
Privilege:

Administrator
Syntax

    [ no ] network-global-mme-id-mgmt-db

no

Remove the global MME ID management database from the system.
Usage:

Use this command to create a new, or enter the existing MME group ID management database. The MME group ID management database is used to create associations between PLMN IDs and ranges of MME group IDs.

On the S4-SGSN, this command enables operators to create a MME group ID management database that can be associated with an SGSN service.

IMPORTANT:

Only one MME group ID management database can be created per system.

Entering this command results in the following prompt:

    [context_name]hostname(network-global-mme-id-mgmt-db)#

Global MME ID management database commands are defined in the LTE Network Global MME ID Management Database Configuration Mode Commands chapter.
paging-map

Creates a paging map or specifies an existing paging map and enters the Paging Map Configuration Mode.
Platform:

ASR 5000
Product:

MME
Privilege:

Administrator
Syntax

    [ no ] paging-map paging_map_name [ -noconfirm ]

no

Remove the paging map from the system.
paging_map_name

Specifies the name of the paging map being created or accessed. If the map name does not refer to an existing map, a new map is created. paging_map_name must be an alphanumeric string of 1 through 64 characters.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
Usage:

Enter the Paging Map Configuration Mode for an existing or newly defined map. This command is also used to remove an existing map.

Entering this command results in the following prompt:

    hostname(paging-map)#

Paging Map Configuration Mode commands are defined in the LTE Paging Map Configuration Mode Commands chapter.

Refer to the Heuristic and Intelligent Paging chapter in the MME Administration Guide for more information about Paging Maps.
Example:
The following command enters the existing Paging Map Configuration Mode (or creates it if it does not already exist) for the map named map1:

    paging-map map1

paging-profile

Creates a paging profile or specifies an existing paging profile and enters the Paging Profile Configuration Mode.
Platform:

ASR 5000
Product:

MME
Privilege:

Administrator
Syntax

    [ no ] paging-profile paging_profile_name [ -noconfirm ]

no

Remove the paging map from the system.
paging_profile_name

Specifies the name of the paging profile being created or accessed. If the profile name does not refer to an existing profile, a new profile is created. paging_profile_name must be an alphanumeric string of 1 through 64 characters.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
Usage:

Enter the Paging Profile Configuration Mode for an existing or newly defined paging profile. This command is also used to remove an existing profile.

Entering this command results in the following prompt:

    hostname(paging-profile)#

Paging Profile Configuration Mode commands are defined in the LTE Paging Profile Configuration Mode Commands chapter.

Refer to the Heuristic and Intelligent Paging chapter in the MME Administration Guide for more information about Paging Profiles.
Example:
The following command enters the existing Paging Profile Configuration Mode (or creates it if it does not already exist) for the profile named profile1:

    paging-profile profile1

subscriber-map

Creates a subscriber map or specifies an existing subscriber map and enters the Subscriber Map Configuration Mode.
Platform:

ASR 5000

ASR 5500
Product:

MME, SAEGW, S-GW
Privilege:

Administrator
Syntax

    [ no ] subscriber-map map_name [ -noconfirm ]

no

Removes the specified subscriber map from the system.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
map_name

Specifies the name of the subscriber map. If the map name does not refer to an existing map, a new map is created. map_name must be an alphanumeric string of 1 through 64 characters.
Usage:

Enter the Subscriber Map Configuration Mode for an existing or newly defined map. This command is also used to remove an existing map.

Entering this command results in the following prompt:

    hostname(subscriber-map)#

Subscriber Map Configuration Mode commands are defined in the LTE Subscriber Map Configuration Mode Commands chapter.
Example:
The following command enters the existing Subscriber Map Configuration Mode (or creates it if it does not already exist) for the map named map1:

    subscriber-map map1

tai-mgmt-db

Creates a Tracking Area Identifier (TAI) Management Database or specifies an existing database and enters the TAI Management Database Configuration mode. On an S4-SGSN, this command is used as part of configuring S-GWs and their associated RAIs to bypass DNS resolution of RAI FQDN for obtaining the S-GW address.
Platform:

ASR 5000

ASR 5500
Product:

MME, SAEGW, S-GW, SGSN

IMPORTANT:

Currently, the SGSN is not supported on the ASR 5500 platform.
Privilege:

Administrator
Syntax

    [ no ] tai-mgmt-db db_name [ -noconfirm ]

no

Removes the specified management database from the system.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
db_name

Specifies the name of the management database. If the name does not refer to an existing database, a new database is created. db_name is an alphanumeric string of 1 through 64 characters.
Usage:

Enter the TAI Management Database Configuration Mode for an existing or newly defined database. This command is also used to remove an existing database.

On the S4-SGSN, once you have created a new, or accessed an existing, TAI Management database, a TAI Management Object must be created or accessed and the S-GWs and their associated RAIs configured using the rai and sgw-address commands. Refer to the LTE TAI Object Configuration Mode chapter for details on these two commands.

Entering this command results in the following prompt:

    [context_name]hostname(tai-mgmt-db)#

TAI Management Database Configuration Mode commands are defined in the TAI Management Database Configuration Mode Commands chapter.
Example:
The following command enters the existing TAI Management Database configuration mode (or creates it if it does not already exist) for the database named tai_db1:

    tai-mgmt-db tai_db1