# show egtp

This chapter includes the show egtp command output tables.
show egtpc peers interface
Table 1. show egtpc peers interface Command Output Descriptions

Field | Description
--- | ---
Status | The status of the GTPC session. - A: Online/Active - I: Offline/Inactive
GTPC Echo | Displays whether GTPC echo is enable or not. - D: Disabled - E: Enabled
Restart Counter | Displays whether restart counter messages have been sent or not. - S: Sent - N: Not Sent
Peer Restart Counter | Displays the status of the peer restart counter. - K: Known - U: Unknown
Type of Node | Indicates the type of node with which the interface communicates. - S: SGW - P: PGW - M: MME - G: SGSN
Service ID | The Service ID for the eGTP service
Peer Address | Indicates the IP address of the peer service (MME/P-GW/S-GW).
Restart Counter | Indicates the restart counter value.
No. of restarts | Indicates the number of restarts of the peer node (MME/S-GW/P-GW).
Current sessions | Indicates the number of sessions currently active on eGTP service.
Max sessions | Indicates the total number of sessions allowed on this eGTP service.

show egtpc sessions
Table 2. show egtpc sessions Command Output Descriptions

Field | Description
--- | ---
vvvv | From left to right, the first value indicates the Interface Type. - M: MME Egress - P: PGW Ingress - S: SGW Ingress vs: SGW Egress - G: SGSN Egress The second value indicates the PDN Type. - N: Non-Data Forwarding - F: Data Forwarding The third value indicates the UEID Type. - M: MEI (Mobile Equipment ID) - I: IMSI (International Mobile Subscriber Identity) The fourth value is a string of characters that indicate the Bearer States. - A: Active - C: Create Session Pending - D: Delete Session Pending - d: Delete Bearer Pending - M: Modify Bearer Pending - R: Release Access Bearer Pending - L: Downlink Data Notification Pending - u: Update User Plane Pending - c: Create Bearer Pending - U: Update Bearer Pending - E: Delete Bearer Command Pending - B: Bearer Resource Command Pending
vvvv (cont.) | - m: Modify Bearer Command Pending - I: Create Indirect Data Forwarding Pending - i: Delete Indirect Forwarding Pending - t: Context Acknowledge Pending - T: Context Request Pending - F: Identification Request Pending - W: Forward Relocation Pending - X: Forward Access Context Notification Pending - w: Forward Relocation Complete Pending - r: Release Cancel pending - S: Suspend Pending - Y: Resume Pending - P: PS to CS Response Pending - p: PS to CS Complete Pending - Q: PS to CS Cancel Pending - .: Inactive
SVC ID | Displays the Service ID.
IMSI/MEI | Displays the IMSI or MEI number.
Def EBI | Displays the default EPS Bearer Identity
EBIs | EBI Bearer States (see fourth value indicators described above).
Control TEIDs | Lists the Tunnel Endpoint Identifiers (TEIDs)
Local | Local TEID.
Remote | Remote TEID.
CallID | Displays the Call Identifier.
Peer Address | Displays the IP address of the eGTP-C peer.
Total sessions matching specified criteria | Displays the total number of eGTP-C sessions matching the specified criteria.

show egtpc statistics
Table 3. show egtpc statistics Command Output Descriptions

Field | Description
--- | ---
Tunnel Management Messages
Create Session Request
Total TX | The total number of tunnel - create session request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - create session request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted create session request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted create session request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted create session request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted create session request messages received by this system, the specified service, or the specified interface.
Create Session Response
Total TX | The total number of tunnel - create session response messages sent by this system, a specified service, or a specified interface.
Total RX | The total number of tunnel - create session response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted create session response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create session response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted create session request messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create session response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted create session response messages sent by this system, the specified service, or the specified interface.
Modify Bearer Request
Total TX | The total number of tunnel - modify bearer request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - modify bearer request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted modify bearer request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted modify bearer request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted modify bearer request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted modify bearer request messages received by this system, the specified service, or the specified interface.
Modify Bearer Response
Total TX | The total number of tunnel - modify bearer response messages sent by this system, a specified service, or a specified interface.
Total RX | The total number of tunnel - modify bearer response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted modify bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted modify bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted modify bearer request messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted modify bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted modify bearer response messages sent by this system, the specified service, or the specified interface.
Delete Session Request
Total TX | The total number of tunnel - delete session request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - delete session request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted delete session request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted delete session request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted delete session request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted delete session request messages received by this system, the specified service, or the specified interface.
Delete Session Response
Total TX Accepted Denied | The total number of tunnel - delete session response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - delete session response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Total RX Accepted Denied | The total number of tunnel - delete session request messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - delete session response (accept or denied) messages received by the system, the specified service, or the specified interface.
Downlink Data Notification Request
Total TX | The total number of tunnel - downlink data notification request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - downlink data notification request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted downlink data notification request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted downlink data notification request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted downlink data notification request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted downlink data notification request messages received by this system, the specified service, or the specified interface.
Downlink Data Notification Response
Total TX | The total number of tunnel - downlink data notification response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - downlink data notification response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted downlink data notification response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted downlink data notification response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted downlink data notification response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted downlink data notification response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted downlink data notification response messages sent by the system, the specified service, or the specified interface.
Downlink Data Failure Indication
Initial TX | The total number of tunnel - initially transmitted downlink data failure indication messages sent by this system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted downlink data failure indication messages received by this system, the specified service, or the specified interface.
Release Access Bearers Request
Total TX | The total number of tunnel - release access bearers request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - release access bearers request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted release access bearers request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted release access bearers request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted release access bearers request messages sent by this system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted release access bearers request messages received by this system, the specified service, or the specified interface.
Release Access Bearer Response
Total TX | The total number of tunnel - release access bearer response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - release access bearer response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted release access bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted release access bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted release access bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted release access bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted release access bearer response messages sent by the system, the specified service, or the specified interface.
Create Bearer Request
Total TX | The total number of tunnel - create bearer request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - create bearer request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted create bearer request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted create bearer request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted create bearer request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted create bearer request messages received by this system, the specified service, or the specified interface.
Create Bearer Response
Total TX | The total number of tunnel - create bearer response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - create bearer response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted create bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted create bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted create bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted create bearer response messages sent by the system, the specified service, or the specified interface.
Update Bearer Request
Total TX | The total number of tunnel - update bearer request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - update bearer request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted update bearer request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted update bearer request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted update bearer request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted update bearer request messages received by this system, the specified service, or the specified interface.
Update Bearer Response
Total TX | The total number of tunnel - update bearer response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - update bearer response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted update bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted update bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted update bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - initially transmitted update bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
Delete Bearer Request
Total TX | The total number of tunnel - delete bearer request messages sent by the system, the specified service, or the specified interface.
Total RX | The total number of tunnel - delete bearer request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted delete bearer request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted delete bearer request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted delete bearer request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted delete bearer request messages received by this system, the specified service, or the specified interface.
Delete Bearer Response
Total TX Accepted Denied | The total number of tunnel - delete bearer response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - delete bearer response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Total RX Accepted Denied | The total number of tunnel - initially transmitted update bearer response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of tunnel - delete bearer response (accept or denied) messages received by the system, the specified service, or the specified interface.
Modify Bearer Command
Total TX | The total number of tunnel - modify bearer command messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - modify bearer command messages received by this system, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted modify bearer command messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted modify bearer command messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted modify bearer command messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted modify bearer command messages received by this system, the specified service, or the specified interface.
Modify Bearer Failure Indication
Total TX | The total number of tunnel - modify bearer failure indication messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - modify bearer failure indication messages received by this system, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted modify bearer failure indication messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted modify bearer failure indication messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted modify bearer failure indication messages sent by the system, the specified service, or the specified interface.
Bearer Resource Command
Total TX | The total number of tunnel - bearer resource command messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - bearer resource command messages received by this system, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted bearer resource command messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted bearer resource command messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted bearer resource command messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted bearer resource command messages received by this system, the specified service, or the specified interface.
Bearer Resource Failure Indication
Total TX | The total number of tunnel - bearer resource failure indication messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - bearer resource failure indication messages received by this system, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted bearer resource failure indication messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted bearer resource failure indication messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted bearer resource failure indication messages sent by the system, the specified service, or the specified interface.
Delete Bearer Command
Total TX | The total number of tunnel - delete bearer command messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - delete bearer command messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted delete bearer command messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted delete bearer command messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted delete bearer command messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted delete bearer command messages received by this system, the specified service, or the specified interface.
Delete Bearer Failure Indication
Total TX | The total number of tunnel - delete bearer failure indication messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - delete bearer failure indication messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted delete bearer failure indication messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted delete bearer failure indication messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted delete bearer failure indication messages sent by the system, the specified service, or the specified interface.
Create Ind Data Forwarding Tunnel Request
Total TX | The total number of tunnel - create indirect data forwarding tunnel requests sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - create indirect data forwarding tunnel requests received by this system, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted create indirect data forwarding tunnel requests sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted create indirect data forwarding tunnel requests received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted create indirect data forwarding tunnel requests sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted create indirect data forwarding tunnel requests received by this system, the specified service, or the specified interface.
Create Ind Data Forwarding Tunnel Response
Total TX | The total number of tunnel - create indirect data forwarding tunnel response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - create indirect data forwarding tunnel response messages received by this system, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted create indirect data forwarding tunnel response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of create indirect data forwarding tunnel response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted create indirect data forwarding tunnel response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of create indirect data forwarding tunnel response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted create indirect data forwarding tunnel response messages sent by the system, the specified service, or the specified interface.
Delete Ind Data Forwarding Tunnel Request
Total TX | The total number of tunnel - delete indirect data forwarding tunnel requests sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - delete indirect data forwarding tunnel requests received by this system, or the specified interface.
Initial TX | The total number of tunnel - initially transmitted delete indirect data forwarding tunnel requests sent by the system, the specified service, or the specified interface.
Initial RX | The total number of tunnel - initially transmitted delete indirect data forwarding tunnel requests received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted delete indirect data forwarding tunnel requests sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of tunnel - retransmitted delete indirect data forwarding tunnel requests received by this system, the specified service, or the specified interface.
Delete Ind Data Forwarding Tunnel Response
Total TX | The total number of tunnel - delete indirect data forwarding tunnel response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of tunnel - delete indirect data forwarding tunnel response messages received by this system, or the specified interface.
Initial TX Accepted Denied | The total number of tunnel - initially transmitted delete indirect data forwarding tunnel response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of delete indirect data forwarding tunnel response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of tunnel - initially transmitted delete indirect data forwarding tunnel response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of delete indirect data forwarding tunnel response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of tunnel - retransmitted delete indirect data forwarding tunnel response messages sent by the system, the specified service, or the specified interface.
Change Notification Request
Total TX | The total number of change notification request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of change notification request messages received by this system, or the specified interface.
Initial TX | The total number of initially transmitted change notification request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of initially transmitted change notification request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted change notification request messages sent by the system, the specified service, or the specified interface.
Change Notification Response
Total TX | The total number of change notification response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of change notification response messages received by this system, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted change notification response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of change notification response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted change notification response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of change notification response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted change notification response messages sent by the system, the specified service, or the specified interface.
Stop Paging Indication
Total TX | The total number of stop paging indication messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of stop paging indication messages received by this system, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted stop paging indication messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of stop paging indication (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted stop paging indication messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of delete indirect data forwarding tunnel response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted stop paging indication messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of retransmitted stop paging indication messages sent by the system, the specified service, or the specified interface.
Path Management Messages
Echo Request
Total TX | The total number of path - echo request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of path - echo request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of path - initially transmitted echo request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of path - initially transmitted echo request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of path - retransmitted echo request messages sent by the system, the specified service, or the specified interface.
Echo Response
Total TX | The total number of path - echo response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of path - echo response messages received by this system, the specified service, or the specified interface.
Version Not Supported
Total TX | The total number of path - version not supported messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of path - version not supported messages received by this system, the specified service, or the specified interface.
Mobility Management Messages
Context Request
Total TX | The total number of mobility - context request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - context request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of mobility - initially transmitted context request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of mobility - initially transmitted context request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted context request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of mobility - retransmitted context request messages received by the system, the specified service, or the specified interface.
Context Response
Total TX | The total number of mobility - context response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - context response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of mobility - initially transmitted context response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted context response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of mobility - initially transmitted context response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted context response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted context response messages sent by the system, the specified service, or the specified interface.
Context Acknowledge
Total TX | The total number of mobility - context acknowledge messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - context acknowledge messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of mobility - initially transmitted context acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted context acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of mobility - initially transmitted context acknowledge messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted context acknowledge (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted context acknowledge messages sent by the system, the specified service, or the specified interface.
Identification Request
Total TX | The total number of mobility - identification request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - identification request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of mobility - initially transmitted identification request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of mobility - initially transmitted identification request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted identification request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of mobility - retransmitted identification request messages received by the system, the specified service, or the specified interface.
Identification Response
Total TX Accepted Denied | The total number of mobility - identification response messages sent by this system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - identification response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Total RX Accepted Denied | The total number of mobility - identification response messages received by this system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - identification response (accept or denied) messages received by the system, the specified service, or the specified interface.
Forward Relocation Request
Total TX | The total number of mobility - forward relocation request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - forward relocation request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of mobility - initially transmitted forward relocation request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of mobility - initially transmitted forward relocation request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted forward relocation request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of mobility - retransmitted forward relocation request messages received by the system, the specified service, or the specified interface.
Forward Relocation Response
Total TX | The total number of mobility - forward relocation response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - forward relocation response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of mobility - initially transmitted forward relocation response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted forward relocation response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of mobility - initially transmitted forward relocation response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted forward relocation response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted forward relocation response messages sent by the system, the specified service, or the specified interface.
Forward Access Context Notification
Total TX | The total number of mobility - forward access context notification messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - forward access context notification messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of mobility - initially transmitted forward access context notification messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of mobility - initially transmitted forward access context notification messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted forward access context notification messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of mobility - retransmitted forward access context notification messages received by the system, the specified service, or the specified interface.
Forward Access Context Acknowledge
Total TX | The total number of mobility - forward access context acknowledge messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - forward access context acknowledge messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of mobility - initially transmitted forward access context acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted forward access context acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of mobility - initially transmitted forward access context acknowledge messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted forward access context acknowledge (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted forward access context acknowledge messages sent by the system, the specified service, or the specified interface.
Forward Relocation Complete Notification
Total TX | The total number of mobility - forward relocation complete notification messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - forward relocation complete notification messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of mobility - initially transmitted forward relocation complete notification messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of mobility - initially transmitted forward relocation complete notification messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted forward relocation complete notification messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of mobility - retransmitted forward relocation complete notification messages received by the system, the specified service, or the specified interface.
Forward Relocation Complete Acknowledge
Total TX | The total number of mobility - forward relocation complete acknowledge messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - forward relocation complete acknowledge messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of mobility - initially transmitted forward relocation complete acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted forward relocation complete acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of mobility - initially transmitted forward relocation complete acknowledge messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted forward relocation complete acknowledge (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted forward relocation complete acknowledge messages sent by the system, the specified service, or the specified interface.
Relocation Cancel Request
Total TX | The total number of mobility - relocation cancel request messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - relocation cancel request messages received by this system, the specified service, or the specified interface.
Initial TX | The total number of mobility - initially transmitted relocation cancel request messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of mobility - initially transmitted relocation cancel request messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted relocation cancel request messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of mobility - retransmitted relocation cancel request messages received by the system, the specified service, or the specified interface.
Relocation Cancel Response
Total TX | The total number of mobility - relocation cancel response messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of mobility - relocation cancel response messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of mobility - initially transmitted relocation cancel response messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted relocation cancel response (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of mobility - initially transmitted relocation cancel response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of mobility - initially transmitted relocation cancel response (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of mobility - retransmitted relocation cancel response messages sent by the system, the specified service, or the specified interface.
RAN Information Relay
Initial TX | The total number of initially transmitted RAN Information Management (RIM) messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of initially transmitted RAN Information Management (RIM) messages received by the system, the specified service, or the specified interface.
Configuration Transfer Tunnel
Initial TX | The total number of initially transmitted configuration transfer tunnel messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of initially transmitted configuration transfer tunnel messages received by the system, the specified service, or the specified interface.
Detach Notification
Total TX | The total number of detach notification messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of detach notification messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted detach notification messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of detach notification (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted detach notification messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of detach notification (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted detach notification messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of retransmitted detach notification messages received by the system, the specified service, or the specified interface.
Detach Acknowledge
Total TX | The total number of detach acknowledge messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of detach acknowledge messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted detach acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of detach acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted detach acknowledge messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of detach acknowledge (accept or denied) messages received by the system, the specified service, or the specified interface.
Alert MME Notification
Total TX | The total number of alert MME notification messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of alert MME notification messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted alert MME notification messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of alert MME notification (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted alert MME notification messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of alert MME notification (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted alert MME notification messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of retransmitted alert MME notification messages received by the system, the specified service, or the specified interface.
Alert MME Acknowledge
Total TX | The total number of alert MME acknowledge messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of alert MME acknowledge messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted alert MME acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of detach notification (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted alert MME acknowledge messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of alert MME acknowledge (accept or denied) messages received by the system, the specified service, or the specified interface.
UE Activation Notification
Total TX | The total number of UE activation messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of UE activation messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted UE activation messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of UE activation (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted UE activation messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of UE activation (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted UE activation messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of retransmitted UE activation messages received by the system, the specified service, or the specified interface.
UE Activity Acknowledge
Total TX | The total number of UE activity acknowledge messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of UE activity acknowledge messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted UE activity acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of UE activity acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted UE activity acknowledge messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of UE activity acknowledge (accept or denied) messages received by the system, the specified service, or the specified interface.
CS Paging Indication
Total TX | The total number of CS (Circuit Switched) paging indication messages sent by this system, the specified service, or the specified interface.
Total RX | The total number of CS paging indication messages received by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted CS paging indication messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of CS paging indication (accept or denied) messages sent by the system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted CS paging indication messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of CS paging indication (accept or denied) messages received by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted CS paging indication messages sent by the system, the specified service, or the specified interface.
Retrans RX | The total number of retransmitted CS paging indication messages received by the system, the specified service, or the specified interface.
SRVCC Messages (Single Radio Voice Call Continuity)
PS to CS Request
Total TX | The total number of PS (Packet Switched) to CS (Circuit Switched) request messages sent by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted PS to CS request messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of PS to CS request (accept or denied) messages sent by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted PS to CS request messages sent by the system, the specified service, or the specified interface.
PS to CS Response
Total RX | The total number of PS (Packet Switched) to CS (Circuit Switched) response messages received by this system, the specified service, or the specified interface.
Initial RX Accepted Denied | The total number of initially transmitted PS to CS response messages received by the system, the specified service, or the specified interface. Accepted and Denied display the total number of PS to CS response (accept or denied) messages received by the system, the specified service, or the specified interface.
PS to CS Complete Notification
Total RX | The total number of PS (Packet Switched) to CS (Circuit Switched) complete notification messages received by this system, the specified service, or the specified interface.
Initial RX | The total number of initially transmitted PS to CS complete notification messages received by the system, the specified service, or the specified interface.
Retrans RX | The total number of retransmitted PS to CS complete notification messages received by the system, the specified service, or the specified interface.
PS to CS Complete Acknowledge
Total TX | The total number of PS (Packet Switched) to CS (Circuit Switched) complete acknowledge messages sent by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted PS to CS complete acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of PS to CS complete acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted PS to CS complete acknowledge messages sent by the system, the specified service, or the specified interface.
PS to CS Cancel Notification
Total TX | The total number of PS (Packet Switched) to CS (Circuit Switched) cancel notification messages sent by this system, the specified service, or the specified interface.
Initial TX | The total number of initially transmitted PS to CS cancel notification messages sent by the system, the specified service, or the specified interface.
Retrans TX | The total number of retransmitted PS to CS cancel notification messages sent by the system, the specified service, or the specified interface.
PS to CS Cancel Acknowledge
Total TX | The total number of PS (Packet Switched) to CS (Circuit Switched) cancel acknowledge messages sent by this system, the specified service, or the specified interface.
Initial TX Accepted Denied | The total number of initially transmitted PS to CS cancel acknowledge messages sent by the system, the specified service, or the specified interface. Accepted and Denied display the total number of PS to CS cancel acknowledge (accept or denied) messages sent by the system, the specified service, or the specified interface.
Trace Management Messages
Trace Session Activation
Initial TX | The total number of trace - initially transmitted session activation messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of trace - initially transmitted session activation messages received by the system, the specified service, or the specified interface.
Trace Session Deactivation
Initial TX | The total number of trace - initially transmitted session deactivation messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of trace - initially transmitted session deactivation messages received by the system, the specified service, or the specified interface.
CS Fallback Messages (CSFB)
Suspend Notification
Initial TX | The total number of CSFB (Circuit Switched Fallback) - initially transmitted suspend notification messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of CSFB - initially transmitted suspend notification messages received by the system, the specified service, or the specified interface.
Suspend Acknowledge
Initial TX | The total number of CSFB - initially transmitted suspend acknowledge messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of CSFB - initially transmitted suspend acknowledge messages received by the system, the specified service, or the specified interface.
Resume Notification
Initial TX | The total number of CSFB - initially transmitted resume notification messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of CSFB - initially transmitted resume notification messages received by the system, the specified service, or the specified interface.
Resume Acknowledge
Initial TX | The total number of CSFB - initially transmitted resume acknowledge messages sent by the system, the specified service, or the specified interface.
Initial RX | The total number of CSFB - initially transmitted resume acknowledge messages received by the system, the specified service, or the specified interface.
Total Signalling Packets
TX | The total number of signalling packets sent by the system, the specified service, or the specified interface.
RX | The total number of signalling packets received by the system, the specified service, or the specified interface.
Total Signalling Bytes
TX | The total number of signalling bytes sent by the system, the specified service, or the specified interface.
RX | The total number of signalling bytes received by the system, the specified service, or the specified interface.

show egtpc statistics verbose

3GPP Release 9, 29.274

The show egtpc statistics verbosecommand includes all of the data provided in the show egtpc statistics command and appends detailed rejection statistics for the following call request/response/notification denials [3GPP Release 9, 29.274]:

- Reject Statistics
- Modify Bearer Request Denied
- Delete Bearer Request Denied
- Delete Session Request Denied
- Downlink Data Notification Denied
- Release Access Bearers Denied
- Create Bearer Denied
- Update Bearer Denied
- Delete Bearer Command Denied
- Modify Bearer Command Denied
- Bearer Resource Command Denied
- Create Indirect Data Forwarding Tunnel Request Denied
- Delete Indirect Data Forwarding Tunnel Request Denied
- Change Notification Request Denied
- Context Request Denied
- Context Response Denied
- Identification Request Denied
- Forward Relocation Request Denied
- Forward Access Context Notification Denied
- Forward Relocation Complete Notification Denied
- Relocation Cancel Request Denied
- Suspend Notification Denied
- Resume Notification Denied

The table below lists and describes the transmit and receive parameters output for all of the call denials listed above.
Table 4. show egtpc statistics verbose Command Output Descriptions -- 3GPP Release 9, 29.274

Field | Description
--- | ---
Context not existent TX | The total number of Context Does Not Exist messages sent by this system, the specified service, or the specified interface.
Context not existent RX | The total number of Context Does Not Exist messages received by this system, the specified service, or the specified interface.
Invalid message format TX | The total number of Invalid Message Format messages sent by the system, the specified service, or the specified interface.
Invalid message format RX | The total number of Invalid Message Format messages received by the system, the specified service, or the specified interface.
Version not supported TX | The total number of Version Not Supported messages sent by the system, the specified service, or the specified interface.
Version not supported RX | The total number of Version Not Supported messages received by this system, the specified service, or the specified interface.
Invalid length TX | The total number of Invalid Length messages sent by the system, the specified service, or the specified interface.
Invalid length RX | The total number of Invalid Length messages received by this system, the specified service, or the specified interface.
Mandatory IE incorrect TX | The total number of Mandatory IE (Information Element) Incorrect messages sent by the system, the specified service, or the specified interface.
Mandatory IE incorrect RX | The total number of Mandatory IE Incorrect messages received by this system, the specified service, or the specified interface.
Mandatory IE missing TX | The total number of Mandatory IE Missing messages sent by the system, the specified service, or the specified interface.
Mandatory IE missing RX | The total number of Mandatory IE Missing messages received by this system, the specified service, or the specified interface.
System failure TX | The total number of System Failure messages sent by the system, the specified service, or the specified interface.
System failure RX | The total number of System Failure messages received by this system, the specified service, or the specified interface.
No resources available TX | The total number of No Resources Available messages sent by the system, the specified service, or the specified interface.
No resources available RX | The total number of No Resources Available messages received by the system, the specified service, or the specified interface.
Semantic error in TFT TX | The total number of Semantic Error in TFT (Traffic Flow Template) messages sent by the system, the specified service, or the specified interface.
Semantic error in TFT RX | The total number of Semantic Error in TFT messages received by this system, the specified service, or the specified interface.
Syntactic error in TFT TX | The total number of Syntactic Error in TFT messages sent by the system, the specified service, or the specified interface.
Syntactic error in TFT RX | The total number of Syntactic Error in TFT messages received by this system, the specified service, or the specified interface.
Semantic error in Pkt Fltr TX | The total number of Semantic Error in Packet Filtering messages sent by the system, the specified service, or the specified interface.
Semantic error in Pkt Fltr RX | The total number of Semantic Error in Packet Filtering messages received by this system, the specified service, or the specified interface.
Syntactic error in Pkt Fltr TX | The total number of Syntactic Error in Packet Filtering messages sent by the system, the specified service, or the specified interface.
Syntactic error in Pkt Fltr RX | The total number of Syntactic Error in Packet Filtering messages received by this system, the specified service, or the specified interface.
Missing or unknown APN TX | The total number of Missing or Unknown APN (Access Point number) messages sent by the system, the specified service, or the specified interface.
Missing or unknown APN RX | The total number of Missing or Unknown APN messages received by this system, the specified service, or the specified interface.
GRE key not found TX | The total number of GRE (Generic Routing Encapsulation) Key Not Found messages sent by the system, the specified service, or the specified interface.
GRE key not found RX | The total number of GRE Key Not Found messages received by this system, the specified service, or the specified interface.
Reallocation failure TX | The total number of Reallocation Failure messages sent by the system, the specified service, or the specified interface.
Reallocation failure RX | The total number of Reallocation Failure messages received by this system, the specified service, or the specified interface.
Denied in RAT TX | The total number of Denied in RAT (Radio Access Technology) messages sent by the system, the specified service, or the specified interface.
Denied in RAT RX | The total number of Denied in RAT messages received by this system, the specified service, or the specified interface.
Pref. PDN type unsupported TX | The total number of Preferred PDN Type Unsupported messages sent by the system, the specified service, or the specified interface.
Pref. PDN type unsupported RX | The total number of Preferred PDN Type Unsupported messages received by this system, the specified service, or the specified interface.
All dynamic addr occupied TX | The total number of All Dynamic Addresses Occupied messages sent by the system, the specified service, or the specified interface.
All dynamic addr occupied RX | The total number of All Dynamic Addresses Occupied messages received by this system, the specified service, or the specified interface.
UE ctx w/o TFT activated TX | The total number of UE Context without TFT (Traffic Flow Template) Already Activated messages sent by the system, the specified service, or the specified interface.
UE ctx w/o TFT activated RX | The total number of UE Context without TFT Already Activated messages received by this system, the specified service, or the specified interface.
Prot type not supported TX | The total number of Protocol Type Not Supported messages sent by the system, the specified service, or the specified interface.
Prot type not supported RX | The total number of Protocol Type Not Supported messages received by this system, the specified service, or the specified interface.
UE not responding TX | The total number of UE (User Equipment) Not Responding messages sent by the system, the specified service, or the specified interface.
UE not responding RX | The total number of UE Not Responding messages received by this system, the specified service, or the specified interface.
UE refuses TX | The total number of UE Refuses messages sent by the system, the specified service, or the specified interface.
UE refuses RX | The total number of UE Refuses messages received by this system, the specified service, or the specified interface.
Service denied TX | The total number of Service Denied messages sent by the system, the specified service, or the specified interface.
Service denied RX | The total number of Service Denied messages received by this system, the specified service, or the specified interface.
Unable to page UE TX | The total number of Unable to Page UE (User Equipment) messages sent by the system, the specified service, or the specified interface.
Unable to page UE RX | The total number of Unable to Page UE messages received by this system, the specified service, or the specified interface.
No Memory TX | The total number of No Memory messages sent by the system, the specified service, or the specified interface.
No Memory RX | The total number of No Memory messages received by this system, the specified service, or the specified interface.
User Auth Failed TX | The total number of User Authentication Failed messages sent by the system, the specified service, or the specified interface.
User Auth Failed RX | The total number of User Authentication Failed messages received by this system, the specified service, or the specified interface.
Apn Access Denied TX | The total number of APN (Access Point Number) Access Denied messages sent by the system, the specified service, or the specified interface.
Apn Access Denied RX | The total number of APN Access Denied messages received by this system, the specified service, or the specified interface.
Request Rejected TX | The total number of Request Rejected messages sent by the system, the specified service, or the specified interface.
Request Rejected RX | The total number of Request Rejected messages received by this system, the specified service, or the specified interface.
Semantic error in TAD TX | The total number of Semantic Error in TAD (Traffic Aggregate Description) messages sent by the system, the specified service, or the specified interface.
Semantic error in TAD RX | The total number of Semantic Error in TAD messages received by this system, the specified service, or the specified interface.
Syntactic error in TAD TX | The total number of Syntactic Error in TAD messages sent by the system, the specified service, or the specified interface.
Syntactic error in TAD RX | The total number of Syntactic Error in TAD messages received by this system, the specified service, or the specified interface.
Collision with Nw init Req TX | The total number of Collision with Network Initiated Request messages sent by the system, the specified service, or the specified interface.
Collision with Nw init Req RX | The total number of Collision with Network Initiated Request messages received by this system, the specified service, or the specified interface.
UE page unable due to Susp TX | The total number of Unable to Page UE (User Equipment) Due to Suspension messages sent by the system, the specified service, or the specified interface.
UE page unable due to Susp RX | The total number of Unable to Page UE Due to Suspension messages received by this system, the specified service, or the specified interface.
Conditional IE missing TX | The total number of Conditional IE (Information Element) Missing messages sent by the system, the specified service, or the specified interface.
Conditional IE missing RX | The total number of Conditional IE Missing messages received by this system, the specified service, or the specified interface.
Apn Restr Type Incompatible TX | The total number of APN (Access Point Number) Restriction Type Incompatible with Currently Active PDN Connection messages sent by the system, the specified service, or the specified interface.
Apn Restr Type Incompatible RX | The total number of APN Restriction Type Incompatible with Currently Active PDN Connection messages received by this system, the specified service, or the specified interface.
Invalid len Piggybacked msg TX | The total number of Invalid Overall Length of the Triggered Response Message and a Piggybacked Initial Message messages sent by the system, the specified service, or the specified interface.
Invalid len Piggybacked msg RX | The total number of Invalid Overall Length of the Triggered Response Message and a Piggybacked Initial Message messages received by this system, the specified service, or the specified interface.
Invalid remote Peer reply TX | The total number of Invalid Reply from Remote Peer messages sent by the system, the specified service, or the specified interface.
Invalid remote Peer reply RX | The total number of Invalid Reply from Remote Peer messages received by this system, the specified service, or the specified interface.
PTMSI signature mismatch TX | The total number of PTMSI (Packet Temporary Mobile Subscriber Identity) Signature Mismatch messages sent by the system, the specified service, or the specified interface.
PTMSI signature mismatch RX | The total number of PTMSI Signature Mismatch messages received by this system, the specified service, or the specified interface.
IMSI not Known TX | The total number of IMSI (International Mobile Subscriber Identity) Not Known messages sent by the system, the specified service, or the specified interface.
IMSI not Known RX | The total number of IMSI Not Known messages received by this system, the specified service, or the specified interface.
Peer not responding TX | The total number of Remote Peer Not Responding messages sent by the system, the specified service, or the specified interface.
Peer not responding RX | The total number of Remote Peer Not Responding messages received by this system, the specified service, or the specified interface.
Data Fwding not supported TX | The total number of Data Forwarding Not Supported messages sent by the system, the specified service, or the specified interface.
Data Fwding not supported RX | The total number of Data Forwarding Not Supported messages received by this system, the specified service, or the specified interface.
Fallback to GTPV1 TX | The total number of Fallback to GTPv1 messages sent by the system, the specified service, or the specified interface.
Fallback to GTPV1 RX | The total number of Fallback to GTPv1 messages received by this system, the specified service, or the specified interface.
Invalid Peer TX | The total number of Invalid Reply from Remote Peer messages sent by the system, the specified service, or the specified interface.
Invalid Peer RX | The total number of Invalid Reply from Remote Peer messages received by this system, the specified service, or the specified interface.
Temp Rej due to HO in prog TX | The total number of Temporarily Rejected Due to Handover Procedure in Progress messages sent by the system, the specified service, or the specified interface.
Temp Rej due to HO in prog RX | The total number of Temporarily Rejected Due to Handover Procedure in Progress messages received by this system, the specified service, or the specified interface.
Unknown TX | The total number of Unknown (unspecified rejection cause) messages sent by the system, the specified service, or the specified interface.
Unknown RX | The total number of Unknown (unspecified rejection cause) messages received by this system, the specified service, or the specified interface.

SRVCC Messages

The show egtpc statistics verbosecommand includes all of the data provided in the show egtpc statistics command, and appends the detailed rejection statistics as described in the table above as well the following statist is tics for SRVCC (Single Radio Voice Call Continuity) requests and notifications:

- PS to CS Request Denied [RX only]
- PS to CS Complete Notification Denied [TX only]
- PS to CS Cancel Notification Denied [RX only]

Table 5. show egtpc statistics verbose Command Output Descriptions -- SRVCC Messages

Field | Description
--- | ---
PS to CS Request Denied [RX only]
Context not existent RX | The total number of Context Does Not Exist messages received by this system, the specified service, or the specified interface.
Invalid message format RX | The total number of Invalid Message Format messages received by this system, the specified service, or the specified interface.
Version not supported RX | The total number of Version Not Supported messages received by this system, the specified service, or the specified interface.
Invalid length RX | The total number of Invalid Length messages received by this system, the specified service, or the specified interface.
Service not supported | The total number of Service not Supported messages received by this system, the specified service, or the specified interface.
Mandatory IE incorrect RX | The total number of Mandatory IE Incorrect messages received by this system, the specified service, or the specified interface.
Mandatory IE missing RX | The total number of Mandatory IE Missing messages received by this system, the specified service, or the specified interface.
System failure RX | The total number of System Failure messages received by this system, the specified service, or the specified interface.
No resources available RX | The total number of No Resources Available messages received by the system, the specified service, or the specified interface.
Semantic error in TFT RX | The total number of Semantic Error in TFT (Traffic Flow Template) messages received by this system, the specified service, or the specified interface.
Syntactic error in TFT RX | The total number of Syntactic Error in TFT messages received by this system, the specified service, or the specified interface.
Semantic error in Pkt Fltr RX | The total number of Semantic Error in Packet Filtering messages received by this system, the specified service, or the specified interface.
Syntactic error in Pkt Fltr RX | The total number of Syntactic Error in Packet Filtering messages received by this system, the specified service, or the specified interface.
Missing or unknown APN RX | The total number of Missing or Unknown APN (Access Point number) messages received by this system, the specified service, or the specified interface.
GRE key not found RX | The total number of GRE (Generic Routing Encapsulation) Key Not Found messages received by this system, the specified service, or the specified interface.
Reallocation failure RX | The total number of Reallocation Failure messages received by this system, the specified service, or the specified interface.
Denied in RAT RX | The total number of Denied in RAT (Radio Access Technology) messages received by this system, the specified service, or the specified interface.
Pref. PDN type unsupported RX | The total number of Preferred PDN Type Unsupported messages received by this system, the specified service, or the specified interface.
All dynamic addr occupied RX | The total number of All Dynamic Addresses Occupied messages received by this system, the specified service, or the specified interface.
UE ctx w/o TFT activated RX | The total number of UE (User Equipment) Context without TFT Already Activated messages received by this system, the specified service, or the specified interface.
Prot type not supported RX | The total number of Protocol Type Not Supported messages received by this system, the specified service, or the specified interface.
UE not responding RX | The total number of UE (User Equipment) Not Responding messages received by this system, the specified service, or the specified interface.
UE refuses RX | The total number of UE Refuses messages received by this system, the specified service, or the specified interface.
Service denied RX | The total number of Service Denied messages received by this system, the specified service, or the specified interface.
Unable to page UE RX | The total number of Unable to Page UE messages received by this system, the specified service, or the specified interface.
No Memory RX | The total number of No Memory messages received by this system, the specified service, or the specified interface.
User Auth Failed RX | The total number of User Authentication Failed messages received by this system, the specified service, or the specified interface.
Apn Access Denied RX | The total number of APN (Access Point Number) Access Denied messages received by this system, the specified service, or the specified interface.
Request Rejected RX | The total number of Request Rejected messages received by this system, the specified service, or the specified interface.
Semantic error in TAD RX | The total number of Semantic Error in TAD (Traffic Aggregate Description) messages received by this system, the specified service, or the specified interface.
Syntactic error in TAD RX | The total number of Syntactic Error in TAD messages received by this system, the specified service, or the specified interface.
Collision with Nw init Req RX | The total number of Collision with Network Initiated Request messages received by this system, the specified service, or the specified interface.
UE page unable due to Susp RX | The total number of Unable to Page UE Due to Suspension messages received by this system, the specified service, or the specified interface.
Conditional IE missing RX | The total number of Conditional IE Missing messages received by this system, the specified service, or the specified interface.
Apn Restr Type Incompatible RX | The total number of APN (Access Point Name) Restriction Type Incompatible with Currently Active PDN Connection messages sent by the system, the specified service, or the specified interface.
Invalid len Piggybacked msg RX | The total number of Invalid Overall Length of the Triggered Response Message and a Piggybacked Initial Message messages received by this system, the specified service, or the specified interface.
Invalid remote Peer reply RX | The total number of Invalid Reply from Remote Peer messages received by this system, the specified service, or the specified interface.
PTMSI signature mismatch RX | The total number of PTMSI (Packet Temporary Mobile Subscriber Identity) Signature Mismatch messages received by this system, the specified service, or the specified interface.
IMSI not Known RX | The total number of IMSI (International Mobile Subscriber Identity) Not Known messages received by this system, the specified service, or the specified interface.
Peer not responding RX | The total number of Remote Peer Not Responding messages received by this system, the specified service, or the specified interface.
Data Fwding not supported RX | The total number of Data Forwarding Not Supported messages received by this system, the specified service, or the specified interface.
Fallback to GTPV1 RX | The total number of Fallback to GTPv1 messages received by this system, the specified service, or the specified interface.
Invalid Peer RX | The total number of Invalid Reply from Remote Peer messages received by this system, the specified service, or the specified interface.
Temp Rej due to HO in prog RX | The total number of Temporarily Rejected Due to Handover Procedure in Progress messages received by this system, the specified service, or the specified interface.
Unknown RX | The total number of Unknown (unspecified rejection cause) messages received by this system, the specified service, or the specified interface.
PS to CS Complete Notification Denied [TX only]
Context not existent TX | The total number of Context Does Not Exist messages sent by this system, the specified service, or the specified interface.
Invalid message format TX | The total number of Invalid Message Format messages sent by the system, the specified service, or the specified interface.
Version not supported TX | The total number of Version Not Supported messages sent by the system, the specified service, or the specified interface.
Invalid length TX | The total number of Invalid Length messages sent by the system, the specified service, or the specified interface.
Mandatory IE incorrect TX | The total number of Mandatory IE (Information Element) Incorrect messages sent by the system, the specified service, or the specified interface.
Mandatory IE missing TX | The total number of Mandatory IE Missing messages sent by the system, the specified service, or the specified interface.
System failure TX | The total number of System Failure messages sent by the system, the specified service, or the specified interface.
No resources available TX | The total number of No Resources Available messages sent by the system, the specified service, or the specified interface.
Semantic error in TFT TX | The total number of Semantic Error in TFT (Traffic Flow Template) messages sent by the system, the specified service, or the specified interface.
Syntactic error in TFT TX | The total number of Syntactic Error in TFT messages sent by the system, the specified service, or the specified interface.
Semantic error in Pkt Fltr TX | The total number of Semantic Error in Packet Filtering messages sent by the system, the specified service, or the specified interface.
Syntactic error in Pkt Fltr TX | The total number of Syntactic Error in Packet Filtering messages sent by the system, the specified service, or the specified interface.
Missing or unknown APN TX | The total number of Missing or Unknown APN (Access Point number) messages sent by the system, the specified service, or the specified interface.
GRE key not found TX | The total number of GRE (Generic Routing Encapsulation) Key Not Found messages sent by the system, the specified service, or the specified interface.
Reallocation failure TX | The total number of Reallocation Failure messages sent by the system, the specified service, or the specified interface.
Denied in RAT TX | The total number of Denied in RAT (Radio Access Technology) messages sent by the system, the specified service, or the specified interface.
Pref. PDN type unsupported TX | The total number of Preferred PDN Type Unsupported messages sent by the system, the specified service, or the specified interface.
All dynamic addr occupied TX | The total number of All Dynamic Addresses Occupied messages sent by the system, the specified service, or the specified interface.
UE ctx w/o TFT activated TX | The total number of UE Context without TFT (Traffic Flow Template) Already Activated messages sent by the system, the specified service, or the specified interface.
Prot type not supported TX | The total number of Protocol Type Not Supported messages sent by the system, the specified service, or the specified interface.
UE not responding TX | The total number of UE (User Equipment) Not Responding messages sent by the system, the specified service, or the specified interface.
UE refuses TX | The total number of UE Refuses messages sent by the system, the specified service, or the specified interface.
Service denied TX | The total number of Service Denied messages sent by the system, the specified service, or the specified interface.
Unable to page UE TX | The total number of Unable to Page UE (User Equipment) messages sent by the system, the specified service, or the specified interface.
No Memory TX | The total number of No Memory messages sent by the system, the specified service, or the specified interface.
User Auth Failed TX | The total number of User Authentication Failed messages sent by the system, the specified service, or the specified interface.
Apn Access Denied TX | The total number of APN (Access Point Number) Access Denied messages sent by the system, the specified service, or the specified interface.
Request Rejected TX | The total number of Request Rejected messages sent by the system, the specified service, or the specified interface.
Semantic error in TAD TX | The total number of Semantic Error in TAD (Traffic Aggregate Description) messages sent by the system, the specified service, or the specified interface.
Syntactic error in TAD TX | The total number of Syntactic Error in TAD messages sent by the system, the specified service, or the specified interface.
Collision with Nw init Req TX | The total number of Collision with Network Initiated Request messages sent by the system, the specified service, or the specified interface.
UE page unable due to Susp TX | The total number of Unable to Page UE (User Equipment) Due to Suspension messages sent by the system, the specified service, or the specified interface.
Conditional IE missing TX | The total number of Conditional IE (Information Element) Missing messages sent by the system, the specified service, or the specified interface.
Apn Restr Type Incompatible TX | The total number of APN (Access Point Number) Restriction Type Incompatible with Currently Active PDN Connection messages sent by the system, the specified service, or the specified interface.
Invalid len Piggybacked msg TX | The total number of Invalid Overall Length of the Triggered Response Message and a Piggybacked Initial Message messages sent by the system, the specified service, or the specified interface.
Invalid remote Peer reply TX | The total number of Invalid Reply from Remote Peer messages sent by the system, the specified service, or the specified interface.
PTMSI signature mismatch TX | The total number of PTMSI (Packet Temporary Mobile Subscriber Identity) Signature Mismatch messages sent by the system, the specified service, or the specified interface.
IMSI not Known TX | The total number of IMSI (International Mobile Subscriber Identity) Not Known messages sent by the system, the specified service, or the specified interface.
Peer not responding TX | The total number of Remote Peer Not Responding messages sent by the system, the specified service, or the specified interface.
Data Fwding not supported TX | The total number of Data Forwarding Not Supported messages sent by the system, the specified service, or the specified interface.
Fallback to GTPV1 TX | The total number of Fallback to GTPv1 messages sent by the system, the specified service, or the specified interface.
Invalid Peer TX | The total number of Invalid Reply from Remote Peer messages sent by the system, the specified service, or the specified interface.
Temp Rej due to HO in prog TX | The total number of Temporarily Rejected Due to Handover Procedure in Progress messages sent by the system, the specified service, or the specified interface.
Unknown TX | The total number of Unknown (unspecified rejection cause) messages sent by the system, the specified service, or the specified interface.
PS to CS Cancel Notification Denied [RX only]
Context not existent RX | The total number of Context Does Not Exist messages received by this system, the specified service, or the specified interface.
Invalid message format RX | The total number of Invalid Message Format messages received by the system, the specified service, or the specified interface.
Version not supported RX | The total number of Version Not Supported messages received by this system, the specified service, or the specified interface.
Invalid length RX | The total number of Invalid Length messages received by this system, the specified service, or the specified interface.
Mandatory IE incorrect RX | The total number of Mandatory IE (Information Element) Incorrect messages received by this system, the specified service, or the specified interface.
Mandatory IE missing RX | The total number of Mandatory IE Missing messages received by this system, the specified service, or the specified interface.
System failure RX | The total number of System Failure messages received by this system, the specified service, or the specified interface.
No resources available RX | The total number of No Resources Available messages received by the system, the specified service, or the specified interface.
Semantic error in TFT RX | The total number of Semantic Error in TFT (Traffic Flow Template) messages received by this system, the specified service, or the specified interface.
Syntactic error in TFT RX | The total number of Syntactic Error in TFT messages received by this system, the specified service, or the specified interface.
Semantic error in Pkt Fltr RX | The total number of Semantic Error in Packet Filtering messages received by this system, the specified service, or the specified interface.
Syntactic error in Pkt Fltr RX | The total number of Syntactic Error in Packet Filtering messages received by this system, the specified service, or the specified interface.
Missing or unknown APN RX | The total number of Missing or Unknown APN (Access Point Number) messages received by this system, the specified service, or the specified interface.
GRE key not found RX | The total number of GRE Key Not Found messages received by this system, the specified service, or the specified interface.
Reallocation failure RX | The total number of Reallocation Failure messages received by this system, the specified service, or the specified interface.
Denied in RAT RX | The total number of Denied in RAT (Radio Access Technology) messages received by this system, the specified service, or the specified interface.
Pref. PDN type unsupported RX | The total number of Preferred PDN Type Unsupported messages received by this system, the specified service, or the specified interface.
All dynamic addr occupied RX | The total number of All Dynamic Addresses Occupied messages received by this system, the specified service, or the specified interface.
UE ctx w/o TFT activated RX | The total number of UE (User Equipment) Context without TFT Already Activated messages received by this system, the specified service, or the specified interface.
Prot type not supported RX | The total number of Protocol Type Not Supported messages received by this system, the specified service, or the specified interface.
UE not responding RX | The total number of UE Not Responding messages received by this system, the specified service, or the specified interface.
UE refuses RX | The total number of UE Refuses messages received by this system, the specified service, or the specified interface.
Service denied RX | The total number of Service Denied messages received by this system, the specified service, or the specified interface.
Unable to page UE RX | The total number of Unable to Page UE (User Equipment) messages received by this system, the specified service, or the specified interface.
No Memory RX | The total number of No Memory messages received by this system, the specified service, or the specified interface.
User Auth Failed RX | The total number of User Authentication Failed messages received by this system, the specified service, or the specified interface.
Apn Access Denied RX | The total number of APN (Access Point Name) Access Denied messages received by this system, the specified service, or the specified interface.
Request Rejected RX | The total number of Request Rejected messages received by this system, the specified service, or the specified interface.
Semantic error in TAD RX | The total number of Semantic Error in TAD (Traffic Aggregate Description) messages received by this system, the specified service, or the specified interface.
Syntactic error in TAD RX | The total number of Syntactic Error in TAD messages received by this system, the specified service, or the specified interface.
Collision with Nw init Req RX | The total number of Collision with Network Initiated Request messages received by this system, the specified service, or the specified interface.
UE page unable due to Susp RX | The total number of Unable to Page UE Due to Suspension messages received by this system, the specified service, or the specified interface.
Conditional IE missing RX | The total number of Conditional IE Missing messages received by this system, the specified service, or the specified interface.
Apn Restr Type Incompatible RX | The total number of APN Restriction Type Incompatible with Currently Active PDN Connection messages sent by the system, the specified service, or the specified interface.
Invalid len Piggybacked msg RX | The total number of Invalid Overall Length of the Triggered Response Message and a Piggybacked Initial Message messages received by this system, the specified service, or the specified interface.
Invalid remote Peer reply RX | The total number of Invalid Reply from Remote Peer messages received by this system, the specified service, or the specified interface.
PTMSI signature mismatch RX | The total number of PTMSI (Packet Temporary Mobile Subscriber Identity) Signature Mismatch messages received by this system, the specified service, or the specified interface.
IMSI not Known RX | The total number of IMSI (International Mobile Subscriber Identity) Not Known messages received by this system, the specified service, or the specified interface.
Peer not responding RX | The total number of Remote Peer Not Responding messages received by this system, the specified service, or the specified interface.
Data Fwding not supported RX | The total number of Data Forwarding Not Supported messages received by this system, the specified service, or the specified interface.
Fallback to GTPV1 RX | The total number of Fallback to GTPv1 messages received by this system, the specified service, or the specified interface.
Invalid Peer RX | The total number of Invalid Reply from Remote Peer messages received by this system, the specified service, or the specified interface.
Temp Rej due to HO in prog RX | The total number of Temporarily Rejected Due to Handover Procedure in Progress messages received by this system, the specified service, or the specified interface.
Unknown RX | The total number of Unknown (unspecified rejection cause) messages received by this system, the specified service, or the specified interface.

show egtp-service all
Table 6. show egtp service all Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the service configured in the named context.
Service-ID | A system generated ID number applied to the service.
Context | The name of the context where the service is configured.
Interface Type | The type of LTE interface this service is supporting.
Status | The status of the service, i.e., “STARTED”.
Restart Counter |
Message Validation Mode | The type of IE validation to be performed on messages received by this service.
GTPC Retransmission Timeout | The number of seconds between the re-sending of GTP-C echo messages.
GTPC Maximum Request Retransmissions | The number of control packet request message retransmissions that can be sent before an error condition is established.
GTPC IP QOS DSCP value | The IP QoS DSCP per-hop behavior to be marked on the outer header of signalling packets originating from the LTE component.
GTPC Echo | Identifies if GTP-C echo messages will be sent.
GTPC Echo Interval | The duration between the sending of GTP-C echo messages.
GTP-C Bind IPv4 Address | The IPv4 address of the interface to which this service is bound.
GTP-C Bind IPv6 Address | The IPv6 address of the interface to which this service is bound.