# show mbms bearer-service

This chapter includes the show mbms bearer-service command output tables.
show mbms bearer-service full all
Table 1. show mbms bearer-service full all Command Output Descriptions

Field | Description
--- | ---
MBMS Bearer Context ID | Specifies the identifier for bearer context used for MBMs service.
State | Specifies the state of bearer service instance.
Mcast Address | Specifies the IP address of BM-SC (Broadcast Multicast - Service Center) server bind to this instance.
APN | Specifies the name if the APN bind to this bearer instance.
Session Identity | Indicates the identifier for MBMS session active on system.
TMGI | indicates the globally unique Temporary Mobile Group Identity ITMGI) allocated by the BM-SC (Broadcast Multicast - Service Center) per MBMS bearer service.
MBMS Bearer Capabilities | Displays the value to indicate MBMS bearer capabilities in Activate MBMS Context Request message.
Service Area Length | Specifies the length of character string configured to indicate MBMS service area. Service area is the area within which data of a specific MBMS session are sent. Each individual MBMS session of an MBMS Bearer Service may be sent to a different MBMS Service Area.
MBMS 2G/3G indication | Displays the value to indicate type of service networks 2G GPRS network or 3G UMTS in Activate MBMS Context Request message.
Counting Info | Displays the value to indicate counting information for message broadcast in MBMS service area.
Session Repetition Number | Indicates the number or times the MBMS session retransmitted the broadcast message.
MBMS-Session-Identity | Specifies the MBMs session identifier.
MBMS-BMSC-SSM-IP | Indicates the IP address configured in IPv4 format with MBMS service and BM-SC server for interface.
Service Type | Specifies the type of service active for this instance of bearer service. Possible values are: UnicastMulticast
Session Started | Indicates whether MBMs service started or not.
BMSC supported user mode | Indicates the supported user mode on BM-SC for this instance of session. It can be Unicast (Broadcast) and/or Multicast.
GGSN selected user mode | Indicates the user mode selected by GGSN for this instance of session. It can be Ucast (Unicast) and/or Mcast (Multicast).
Time to Xfer | Indicates the time taken to transfer the message from system to UE.
Session Duration | Indicates the time elapsed after MBMS session started.
Num MBMS UEs | Indicates total number of UEs connected for this session.
Num MBMS Bearer | Indicates total number of MBMS bearer session instances active for this session.
Quality Of Service | Indicates the configured or updated QoS parameters for this bearer instance.
Traffic Classl | Specifies the class of traffic of active MBMS session. Possible values are: CoversationalStreaming
Maximum Bit Rate Uplink | Indicates the MBR supported/configured for data flow in uplink (to PDN) direction.
Maximum Bit Rate Downlink | Indicates the MBR supported/configured for data flow in downlink (from PDN) direction.
Guaranteed Bit Rate Uplink | Indicates the GBR supported/configured for data flow in uplink (to PDN) direction.
Guaranteed Bit Rate Downlink | Indicates the GBR supported/configured for data flow in downlink (from PDN) direction.
Total Number of MBMS Bearer Services | Indicates the total number of MBMS bearer instances are active.