> Card Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> Card-level Schema Statistics

> Statistic | Description | Data Type
> card | Chassis slot number between 1 and 16 | Int32
> cpubusy | Total CPU busy (across all CPUs, as percentage) | Float
> cpuidle | Total CPU idle (across all CPUs, as percentage) | Float
> numproc | Total number of processes | Int32
> memused | Total amount of memory used (across all processors) | Int32
> memtotal | Total amount of memory available (across all processors) | Int32
> numcpu | The total number of CPUs | Int32
> cpu0-cpubusy | The percentage of time that CPU 0 was busy | Float
> cpu0-cpuidle | The percentage of time that CPU 0 was idle | Float
> cpu0-numproc | The number of processes running on CPU 0 | Int32
> cpu0-memused | The amount of memory used on CPU 0 | Int32
> cpu0-memtotal | The total amount of memory available for CPU 0 | Int32
> cpu0-name | A string designating the name of CPU 0. | String
> cpu0-cpuused-user | The percentage of resources on CPU 0 used in user session processing. | Float
> cpu0-cpuused-sys | The percentage of resources on CPU 0 used by system tasks. | Float
> cpu0-cpuused-io | The percentage of resources on CPU 0 used by input/output functions. | Float
> cpu0-cpuused-irq | The percentage of resources on CPU 0 used by interrupt requests. | Float
> cpu0-cpuused-idle | The percentage of resources on CPU 0 that are idle. | Float
> cpu1-cpubusy | The percentage of time that CPU 1 was busy | Float
> cpu1-cpuidle | The percentage of time that CPU 1 was idle | Float
> cpu1-numproc | The number of processes running on CPU 1 | Int32
> cpu1-memused | The amount of memory used on CPU 1 | Int32
> cpu1-memtotal | The total amount of memory available for CPU 2 | Int32
> cpu1-name | A string designating the name of CPU 1. | String
> cpu1-cpuused-user | The percentage of resources on CPU 1 used in user session processing. | Float
> cpu1-cpuused-sys | The percentage of resources on CPU 1 used by system tasks. | Float
> cpu1-cpuused-io | The percentage of resources on CPU 1 used by input/output functions. | Float
> cpu1-cpuused-irq | The percentage of resources on CPU 1 used by interrupt requests. | Float
> cpu1-cpuused-idle | The percentage of resources on CPU 1 that are idle. | Float
> cpu2-cpubusy | The percentage of time that CPU 2 was busy | Float
> cpu2-cpuidle | The percentage of time that CPU 2 was idle | Float
> cpu2-numproc | The number of processes running on CPU 2 | Int32
> cpu2-memused | The amount of memory used on CPU 2 | Int32
> cpu2-memtotal | The total amount of memory available for CPU 2 | Int32
> cpu2-name | A string designating the name of CPU 2. | String
> cpu2-cpuused-user | The percentage of resources on CPU 2 used in user session processing. | Float
> cpu2-cpuused-sys | The percentage of resources on CPU 2 used by system tasks. | Float
> cpu2-cpuused-io | The percentage of resources on CPU 2 used by input/output functions. | Float
> cpu2-cpuused-irq | The percentage of resources on CPU 2 used by interrupt requests. | Float
> cpu2-cpuused-idle | The percentage of resources on CPU 2 that are idle. | Float
> cpu3-cpubusy | The percentage of time that CPU 3 was busy | Float
> cpu3-cpuidle | The percentage of time that CPU 3 was idle | Float
> cpu3-numproc | The number of processes running on CPU 3 | Int32
> cpu3-memused | The amount of memory used on CPU 3 | Int32
> cpu3-memtotal | The total amount of memory available for CPU 3 | Int32
> cpu3-name | A string designating the name of CPU 3. | String
> cpu3-cpuused-user | The percentage of resources on CPU 3 used in user session processing. | Float
> cpu3-cpuused-sys | The percentage of resources on CPU 3 used by system tasks. | Float
> cpu3-cpuused-io | The percentage of resources on CPU 3 used by input/output functions. | Float
> cpu3-cpuused-irq | The percentage of resources on CPU 3 used by interrupt requests. | Float
> cpu3-cpuused-idle | The percentage of resources on CPU 3 that are idle. | Float
> 15avg-cpubusy | Average CPU usage across all CPUs on this card over a 15 minute period | Float
> 15peak-cpubusy | Peak CPU usage across all CPUs on this card. This is the peak one minute average over the last 15 minutes. | Float
> 5avg-cpubusy | Average CPU usage across all CPUs on this card over a 5 minute period | Float
> 5peak-cpubusy | Peak CPU usage across all CPUs on this card. This is the peak one minute average over the last 5 minutes. | Float
> 1avg-cpubusy | Average CPU usage across all CPUs on this card over a 1 minute period | Float
> 15avg-memused | Average memory usage across all CPUs on this card over a 15 minute period | Float
> 15peak-memused | Peak memory usage across all CPUs on this card. This is the peak one minute average over the last 15 minutes. | Float
> 5avg-memused | Average memory usage across all CPUs on this card over a 5 minute period | Float
> 5peak-memused | Peak memory usage across all CPUs on this card. This is the peak one minute average over the last 5 minutes. | Float
> 1avg-memused | Average memory usage across all CPUs on this card over a 1 minute period. | Float
> cpu0-15avg-cpubusy | Average CPU usage for CPU 0 on this card over a 15 minute period | Float
> cpu0-15peak-cpubusy | Peak CPU usage for CPU 0. This is the peak one minute average over the last 15 minutes. | Float
> cpu0-5avg-cpubusy | Average CPU usage for CPU 0 on this card over a 5 minute period | Float
> cpu0-5peak-cpubusy | Peak CPU usage for CPU 0. This is the peak one minute average over the last 5 minutes. | Float
> cpu0-1avg-cpubusy | Average CPU usage for CPU 0 on this card over a 1 minute period | Float
> cpu0-15avg-memused | Average memory usage for CPU 0 over a 15 minute period | Float
> cpu0-15peak-memused | Peak memory usage for CPU 0. This is the peak one minute average over the last 15 minutes. | Float
> cpu0-5avg-memused | Average memory usage for CPU 0 over a 5 minute period | Float
> cpu0-5peak-memused | Peak memory usage for CPU 0. This is the peak one minute average over the last 15 minutes. | Float
> cpu0-1avg-memused | Average memory usage for CPU 0 over a 1 minute period | Float
> cpu1-15avg-cpubusy | Average CPU usage for CPU 1on this card over a 15 minute period | Float
> cpu1-15peak-cpubusy | Peak CPU usage for CPU 1. This is the peak one minute average over the last 15 minutes. | Float
> cpu1-5avg-cpubusy | Average CPU usage for CPU 1on this card over a 5 minute period | Float
> cpu1-5peak-cpubusy | Peak CPU usage for CPU 1. This is the peak one minute average over the last 5 minutes. | Float
> cpu1-1avg-cpubusy | Average CPU usage for CPU 1on this card over a 1 minute period | Float
> cpu1-15avg-memused | Average memory usage for CPU 1over a 15 minute period | Float
> cpu1-15peak-memused | Peak memory usage for CPU 1. This is the peak one minute average over the last 15 minutes. | Float
> cpu1-5avg-memused | Average memory usage for CPU 1 over a 5 minute period | Float
> cpu1-5peak-memused | Peak memory usage for CPU 1. This is the peak one minute average over the last 5 minutes. | Float
> cpu1-1avg-memused | Average memory usage for CPU 1over a 1 minute period | Float
> cpu2-15avg-cpubusy | Average CPU usage for CPU 2on this card over a 15 minute period | Float
> cpu2-15peak-cpubusy | Peak CPU usage for CPU 2 This is the peak one minute average over the last 15 minutes. | Float
> cpu2-5avg-cpubusy | Average CPU usage for CPU 2on this card over a 5 minute period | Float
> cpu2-5peak-cpubusy | Peak CPU usage for CPU 2 This is the peak one minute average over the last 5 minutes. | Float
> cpu2-1avg-cpubusy | Average CPU usage for CPU 2on this card over a 1minute period | Float
> cpu2-15avg-memused | Average memory usage for CPU 2 over a 15 minute period | Float
> cpu2-15peak-memused | Peak memory usage for CPU 2. This is the peak one minute average over the last 15 minutes. | Float
> cpu2-5avg-memused | Average memory usage for CPU 2 over a 5 minute period | Float
> cpu2-5peak-memused | Peak memory usage for CPU 2. This is the peak one minute average over the last 5 minutes. | Float
> cpu2-1avg-memused | Average memory usage for CPU 2 over a 1 minute period | Float
> cpu3-15avg-cpubusy | Average CPU usage for CPU 3on this card over a 15 minute period | Float
> cpu3-15peak-cpubusy | Peak CPU usage for CPU 3. This is the peak one minute average over the last 15 minutes. | Float
> cpu3-5avg-cpubusy | Average CPU usage for CPU 3on this card over a 5 minute period | Float
> cpu3-5peak-cpubusy | Peak CPU usage for CPU 3. This is the peak one minute average over the last 5 minutes. | Float
> cpu3-1avg-cpubusy | Average CPU usage for CPU 3on this card over a 1 minute period | Float
> cpu3-15avg-memused | Average memory usage for CPU 3over a 5 minute period | Float
> cpu3-15peak-memused | Peak memory usage for CPU 3. This is the peak one minute average over the last 15 minutes. | Float
> cpu3-5avg-memused | Average memory usage for CPU 3over a 15 minute period | Float
> cpu3-5peak-memused | Peak memory usage for CPU 3. This is the peak one minute average over the last 5 minutes. | Float
> cpu3-1avg-memused | Average memory usage for CPU 3over a 1 minute period | Float
> task-sessmgr-num | Total number of active sessmgr tasks across all CPUs on this card. | Int32
> task-sessmgr-avgcpu | Average percentage of CPU utilization of all active sessmgr tasks across all CPUs on this card. | Float
> task-sessmgr-avgmem | Average percentage of allocated memory utilization of all active sessmgr tasks across all CPUs on this card. | Float
> task-sessmgr-maxcpu | Maximum percentage of CPU utilization of the busiest sessmgr task across all CPUs on this card. | Float
> task-sessmgr-maxmem | Maximum percentage of allocated memory utilization of the peak sessmgr task across all CPUs on this card. | Float
> task-a11mgr-num | Total number of active a11mgr tasks across all CPUs on this card. | Int32
> task-a11mgr-maxcpu | Maximum percentage of CPU utilization of the busiest a11mgr task across all CPUs on this card. | Float
> task-a11mgr-maxmem | Maximum percentage of allocated memory utilization of the peak a11mgr task across all CPUs on this card. | Float
> task-l2tpmgr-num | Total number of active l2tpmgr tasks across all CPUs on this card. | Int32
> task-l2tpmgr-maxcpu | Maximum percentage of CPU utilization of the busiest l2tpmgr task across all CPUs on this card. | Float
> task-l2tpmgr-maxmem | Maximum percentage of allocated memory utilization of the peak l2tpmgr task across all CPUs on this card. | Float
> task-famgr-num | Total number of active famgr tasks across all CPUs on this card. | Int32
> task-famgr-maxcpu | Maximum percentage of CPU utilization of the busiest famgr task across all CPUs on this card. | Float
> task-famgr-maxmem | Maximum percentage of allocated memory utilization of the peak famgr task across all CPUs on this card. | Float
> task-hamgr-num | Total number of active hamgr tasks across all CPUs on this card. | Int32
> task-hamgr-maxcpu | Maximum percentage of CPU utilization of the busiest hamgr task across all CPUs on this card. | Float
> task-hamgr-maxmem | Maximum percentage of allocated memory utilization of the peak hamgr task across all CPUs on this card. | Float
> task-acsmgr-num | Total number of active acsmgr tasks across all CPUs on this card. | Int32
> task-acsmgr-avgcpu | Average percentage of CPU utilization of all active acsmgr tasks across all CPUs on this card. | Float
> task-acsmgr-avgmem | Average percentage of allocated memory utilization of all active acsmgr tasks across all CPUs on this card. | Float
> task-acsmgr-maxcpu | Maximum percentage of CPU utilization of the busiest acsmgr task across all CPUs on this card. | Float
> task-acsmgr-maxmem | Maximum percentage of allocated memory utilization of the peak acsmgr task across all CPUs on this card. | Float
> task-vpnmgr-num | Total number of active vpnmgr tasks across all CPUs on this card. | Int32
> task-vpnmgr-maxcpu | Maximum percentage of CPU utilization of the busiest vpnmgr task across all CPUs on this card. | Float
> task-vpnmgr-maxmem | Maximum percentage of allocated memory utilization of the peak vpnmgr task across all CPUs on this card. | Float
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883