> Content Filtering Thresholds
> Thresholds generate alerts or alarms based on either the total number of Content Filtering calls setup by the system during the specified polling interval, or on the number of currently active calls only.
> Alerts or alarms are triggered for call setups based on the following rules:

> • | Enter condition: Actual number of call setups > or = High Threshold

> • | Clear condition: Actual number of call setups < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Default value is 0, which means there will be no monitoring.
> The polling interval is in seconds and it is an integer between 30 and 60000. Entries will be rounded up to the nearest 30 seconds.
> Configuring Content Filtering Thresholds
> This section describes how to enable and configure Content Filtering thresholds.
> Enabling Thresholds
> To enable thresholds use the following configuration:
> configure
> threshold monitoring content-filtering
> end
> Configuring Threshold Poll Interval
> To configure threshold poll interval use the following configuration:
> configure
> threshold poll contfilt-block interval <interval>
> threshold poll contfilt-rating interval <interval>
> end
> Configuring Thresholds Limits
> To configure threshold limits use the following configuration:
> configure
> threshold contfilt-block <high_thresh> [ clear <low_thresh> ]
> threshold contfilt-rating <high_thresh> [ clear <low_thresh> ]
> end
> Saving Your Configuration
> When you configure thresholds, they are not permanent unless you save the changes. When you have completed configuring thresholds, save your configuration as described in the Verifying and Saving Your Configuration chapter.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883