> LMA Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise described.
> The bulk statistics in the following table are accumulated per LMA service configured on this system.
> LMA Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the LMA service. | String / Static
> vpnid | The identification number of the context configured on the system that is currently facilitating the LMA service. This is an internal reference number. | Gauge / Int32
> servname | Displays the name of the LMA service for which the statistics are displayed. | String / Static
> servid | The identification number of the service configured on the system that is currently facilitating the LMA service. This is an internal reference number. | Gauge / Int32
> sess-cur | The total number of sessions currently established on this system. | Counter / Int32
> mipaaaauth-attempts | The total number of mobile IP AAA authentication attempts made by this service. | Counter / Int32
> mipaaaauth-success | The total number of successful mobile IP AAA authentication attempts made by this service. | Counter / Int32
> mipaaaauth-totalfailures | The total number of failed mobile IP AAA authentication attempts received by this service. | Counter / Int32
> mipaaaauth-actualauthfailures | The total number of mobile IP AAA authentication failures received by this service. | Counter / Int32
> mipaaaauth-miscauthfailures | The total number of miscellaneous mobile IP AAA authentication failures received by this service. | Counter / Int32
> bindupd | The total number of all binding updates received by this system. | Counter / Int32
> bindupd-accept | The total number of all binding updates received and accepted by this system. | Counter / Int32
> bindupd-denied | The total number of all binding updates received and denied by this system. | Counter / Int32
> bindupd-discard | The total number of all binding updates received and discarded by this system. | Counter / Int32
> bindupd-initial | The total number of all initial binding updates received by this system. | Counter / Int32
> bindupd-initialaccept | The total number of initial binding updates received and accepted by this system. | Counter / Int32
> bindupd-initialdenied | The total number of initial binding updates received and denied by this system. | Counter / Int32
> bindupd-refresh | The total number of all refresh binding update requests received by this system. | Counter / Int32
> bindupd-refreshaccept | The total number of refresh binding update requests received and accepted by this system. | Counter / Int32
> bindupd-refreshdenied | The total number of refresh binding update requests received and denied by this system. | Counter / Int32
> bindupd-dereg | The total number of all deregistration request binding updates received by this system. | Counter / Int32
> bindupd-deregaccept | The total number of deregistration request binding updates received and accepted by this system. | Counter / Int32
> bindupd-deregdenied | The total number of deregistration request binding updates received and denied by this system. | Counter / Int32
> bindupd-handoff | The total number of all handoff request binding updates received by this system. | Counter / Int32
> bindupd-handoffaccept | The total number of handoff request binding updates received and accepted by this system. | Counter / Int32
> bindupd-handoffdenied | The total number of handoff request binding updates received and denied by this system. | Counter / Int32
> bindupd-ack | The total number of all binding update acknowledgements sent by this system. | Counter / Int32
> bindupd-ackacceptreg | The total number of accepted registration binding update acknowledgements sent by this system. | Counter / Int32
> bindupd-ackacceptdereg | The total number of accepted deregistration binding update acknowledgements sent by this system. | Counter / Int32
> bindupd-ackdenied | The total number of denied binding update acknowledgements sent by this system. | Counter / Int32
> bindupd-acksenderror | The total number of send error binding update acknowledgements sent by this system. | Counter / Int32
> bindupd-denynoresource | The total number of binding update deny messages, due to insufficient resources, sent by this system. | Counter / Int32
> bindupd-denymisid | The total number of binding update deny messages, due to mismatched IDs, sent by this system. | Counter / Int32
> bindupd-denymnauthfailure | The total number of binding update deny messages, due to a mobile node authentication failure condition, sent by this system. | Counter / Int32
> bindupd-denyadmin | The total number of binding update deny messages, due to an admin prohibited condition, sent by this system. | Counter / Int32
> bindupd-denymsgidreq | The total number of binding update deny messages, due to requiring a message ID, sent by this system. | Counter / Int32
> bindupd-denydadfailed | The total number of binding update deny messages, due to DAD failure, sent by this system. | Counter / Int32
> bindupd-denynothomesub | The total number of binding update deny messages, due to an incorrect home subnet, sent by this system. | Counter / Int32
> bindupd-denyseqoow | The total number of binding update deny messages, due to sequence out of window, sent by this system. | Counter / Int32
> bindupd-denytypchgdis | The total number of binding update deny messages, due to a disallowed registration type change, sent by this system. | Counter / Int32
> bindupd-denyunspec | The total number of binding update deny messages, due to an unspecified reason, sent by this system. | Counter / Int32
> bindupd-denyservauthfailed | The total number of binding update deny messages, due to a service authorization failure, sent by this system. | Counter / Int32
> bindupd-denyproxyreg | The total number of binding update deny messages, due to a proxy registration not enabled error, sent by this system. | Counter / Int32
> bindupd-denytimestamp | The total number of binding update deny messages, due to a timestamp mismatch error, sent by this system. | Counter / Int32
> bindupd-denytimestamplower | The total number of binding update deny messages, due to a timestamp lower than expected reason, sent by this system. | Counter / Int32
> bindupd-denymismnid | The total number of binding update deny messages, due to a missing MN-ID option, sent by this system. | Counter / Int32
> bindupd-denymishnp | The total number of binding update deny messages, due to a missing HNP option, sent by this system. | Counter / Int32
> bindupd-denymisaccesstech | The total number of binding update deny messages, due to a missing access technology option, sent by this system. | Counter / Int32
> bindupd-denymishandoffind | The total number of binding update deny messages, due to a missing handoff indicator option, sent by this system. | Counter / Int32
> bindupd-denynotauthhnp | The total number of binding update deny messages, due to a not authorized for HNP reason, sent by this system. | Counter / Int32
> bindupd-denynotmobile | The total number of binding update deny messages, due to a missing LMA for the MN reason, sent by this system. | Counter / Int32
> bindupd-denynotauthproxyreg | The total number of binding update deny messages, due to a not authorized for proxy registration reason, sent by this system. | Counter / Int32
> bindupd-denybceprefix | The total number of binding update deny messages, due to a BCE prefix not matching, sent by this system. | Counter / Int32
> bindupd-denynoresourcesessmgr | The total number of binding update deny messages, due to insufficient resources - no session manager, sent by this system. | Counter / Int32
> bindupd-denynoresourcememory | The total number of binding update deny messages, due to insufficient resources - no memory, sent by this system. | Counter / Int32
> bindupd-denynoresourcereject | The total number of binding update deny messages, due to insufficient resources - session manager rejected, sent by this system. | Counter / Int32
> bindupd-denynoresourceinputq | The total number of binding update deny messages, due to insufficient resources - input queue exceeded, sent by this system. | Counter / Int32
> bindupd-denynoresourcesimulbind | The total number of binding update deny messages, due to insufficient resources - simultaneous bindings exceeded, sent by this system. | Counter / Int32
> bindupd-denynoresourceaddallocfail | The total number of binding update deny messages, due to insufficient resources - address allocation failed, sent by this system. | Counter / Int32
> bindupd-denyadminprohmnaaaauth | The total number of binding update deny messages, due to an administrator prohibited - MN-AAA auth option missing condition, sent by this system. | Counter / Int32
> bindupd-denyadminprohhbit | The total number of binding update deny messages, due to an administrator prohibited - H-bit not set condition, sent by this system. | Counter / Int32
> bindupd-denyadminprohmnaaaspi | The total number of binding update deny messages, due to an administrator prohibited - invalid MN-AAA option SPI condition, sent by this system. | Counter / Int32
> bindupd-denyadminprohmnhaspi | The total number of binding update deny messages, due to an administrator prohibited - invalid MN-HA option SPI condition, sent by this system. | Counter / Int32
> bindupd-denyadmincong | The total number of binding update deny messages, due to an administrator prohibited - congestion control condition, sent by this system. | Counter / Int32
> bindupd-denyadminpolrej | The total number of binding update deny messages, due to an administrator prohibited - policy rejected condition, sent by this system. | Counter / Int32
> bindupd-denyadminhoa | The total number of binding update deny messages, due to an administrator prohibited - HoA not authorized condition, sent by this system. | Counter / Int32
> bindupd-denyadminperm | The total number of binding update deny messages, due to an administrator prohibited - no permission condition, sent by this system. | Counter / Int32
> bindupd-denyadminbadreq | The total number of binding update deny messages, due to an administrator prohibited - bad request condition, sent by this system. | Counter / Int32
> bindupd-discardcong | The total number of binding update discarded messages, due to congestion, sent by this system. | Counter / Int32
> bindupd-discardchecksum | The total number of binding update discarded messages, due to checksum error(s), sent by this system. | Counter / Int32
> bindupd-discardauthpending | The total number of binding update discarded messages, due to an initial authentication pending condition, sent by this system. | Counter / Int32
> bindupd-discardsessnotfound | The total number of binding update discarded messages, due to a session not found condition, sent by this system. | Counter / Int32
> bindupd-discardhamgrnotready | The total number of binding update discarded messages, due to an HA manager not found condition, sent by this system. | Counter / Int32
> bindupd-discarddecodefail | The total number of binding update discarded messages, due to a decode failure, sent by this system. | Counter / Int32
> bindupd-discardinvbuflen | The total number of binding update discarded messages, due to an invalid buffer length, sent by this system. | Counter / Int32
> bindrev-sent | The total number of binding revocations sent by this system. | Counter / Int32
> bindrev-retriessent | The total number of binding revocation retries sent by this system. | Counter / Int32
> bindrev-ackrcvd | The total number of binding revocation acknowledgements received by this system. | Counter / Int32
> bindrev-notacked | The total number of binding revocations sent, but not acknowledged, by this system. | Counter / Int32
> bindrev-rcvd | The total number of binding revocations received by this system. | Counter / Int32
> bindrev-acksent | The total number of binding revocation acknowledgements sent by this system. | Counter / Int32
> bindrev | The total number of binding revocation acknowledgements received and discarded by this system. | Counter / Int32
> bindrev-discardsessnotfound | The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by this system. | Counter / Int32
> bindrev-discardbadreq | The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by this system. | Counter / Int32
> bindrev-discarddecodeerror | The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by this system. | Counter / Int32
> bindrev-discardchecksumerror | The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by this system. | Counter / Int32
> bindrev-discardinvalidmsgtype | The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by this system. | Counter / Int32
> bindrev-discardhamgrnotready | The total number of binding revocation acknowledgements received and discarded, due to a HAMGR not ready condition, by this system. | Counter / Int32
> bindrev-discardmatchreqnotfound | The total number of binding revocation acknowledgements received and discarded, due to a matching request not found condition, by this system. | Counter / Int32
> bindrev-discardinvalidbuflen | The total number of binding revocation acknowledgements received and discarded, due to a invalid buffer length condition, by this system. | Counter / Int32
> rxpackets | The total number of packets received by this system. | Counter / Int32
> rxpackets-6in6 | The total number of IPv6-in-IPv6 tunnel packets received by this system. | Counter / Int32
> rxpackets-4in6 | The total number of IPv4-in-IPv6 tunnel packets received by this system. | Counter / Int32
> rxpackets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel packets received by this system. | Counter / Int32
> rxpackets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel packets received by this system. | Counter / Int32
> rxoctets | The total number of octets received by this system. | Counter / Int32
> rxoctets-6in6 | The total number of IPv6-in-IPv6 tunnel octets received by this system. | Counter / Int32
> rxoctets-4in6 | The total number of IPv4-in-IPv6 tunnel octets received by this system. | Counter / Int32
> rxoctets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel octets received by this system. | Counter / Int32
> rxoctets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel octets received by this system. | Counter / Int32
> dataerror | The total number of data errors received by this system. | Counter / Int32
> dataerror-proto | The total number of protocol type data errors received by this system. | Counter / Int32
> dataerror-invpktlen | The total number of invalid packet length data errors received by this system. | Counter / Int32
> dataerror-nosess | The total number of no session found data errors received by this system. | Counter / Int32
> txpackets | The total number of packets sent by this system. | Counter / Int32
> txpackets-6in6 | The total number of IPv6-in-IPv6 tunnel packets sent by this system. | Counter / Int32
> txpackets-4in6 | The total number of IPv4-in-IPv6 tunnel packets sent by this system. | Counter / Int32
> txpackets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel packets sent by this system. | Counter / Int32
> txpackets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel packets sent by this system. | Counter / Int32
> txoctets | The total number of octets sent by this system. | Counter / Int32
> txoctets-6in6 | The total number of IPv6-in-IPv6 tunnel octets sent by this system. | Counter / Int32
> txoctets-4in6 | The total number of IPv4-in-IPv6 tunnel octets sent by this system. | Counter / Int32
> txoctets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel octets sent by this system. | Counter / Int32
> txoctets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel octets sent by this system. | Counter / Int32
> icmpv6-pkttoobigrecv | The total number of tunnel ICMP packets - too big received by this system. | Counter / Int32
> icmpv6-pkttoobigdrop | The total number of tunnel ICMP packets - too big dropped by this system. | Counter / Int32
> icmpv6-pkttoobigrelay | The total number of tunnel ICMP packets - too big relayed by this system. | Counter / Int32
> disc | The total number of disconnects initiated by this system. | Counter / Int32
> disclifetime | The total number of disconnects due to lifetime expiry initiated by this system. | Counter / Int32
> discdereg | The total number of disconnects due to deregistrations initiated by this system. | Counter / Int32
> discadmin | The total number of disconnects due to admin drops initiated by this system. | Counter / Int32
> discother | The total number of disconnects due to “other reasons” initiated by this system. | Counter / Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883