> SS7 Routing Domain Schema Statistics
> The SS7RD schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> SS7 Routing Domain Statistics

> Statistics | Description | Data Type
> ss7rd-number | Number identifying the SS7 routing domain | Int32
> ss7rd-asp_instance | The Application Server Process instance in the SS7 Routing domain | Int32
> ss7rd-sctp-init-tx | Total number of SCTP Init chunks sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-init-rtx | Total number of SCTP Init chunks resent per SS7 Routing Domain. | Int32
> ss7rd-sctp-init-rx | Total number of SCTP Init chunks received per SS7 Routing Domain. | Int32
> ss7rd-sctp-init-ack-tx | Total number of number INIT_ACKs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-init-ack-rx | Total number of number INIT_ACKs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-tx | Total number SHUTDOWNs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-rtx | Total number SHUTDOWNs resent per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-rx | Total Number SHUTDOWNs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-ack-tx | Total number of SHUTDOWN_ACKs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-ack-rtx | Total number of SHUTDOWN_ACKSs resent per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-ack-rx | Total number of SHUTDOWN_ACKs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-cookie-tx | Total number of COOKIEs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-cookie-rtx | Total number COOKIEs resent per SS7 Routing Domain. | Int32
> ss7rd-sctp-cookie-rx | Total number of COOKIEs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-cookie-ack-tx | Total number of COOKIE_ACKs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-cookie-ack-rx | Total number COOKIE_ACKs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-data-tx | Total number of DATAs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-data-rtx | Total number of DATAs resent per SS7 Routing Domain. | Int32
> ss7rd-sctp-data-rx | Total number of DATAs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-sack-tx | Total number of SACKs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-sack-rx | Total number of SACKs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-compl-tx | Total number of Shutdown completed sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-shutdown-compl-rx | Total number of Shutdown completed received per SS7 Routing Domain. | Int32
> ss7rd-sctp-heartbeat-tx | Total number of HEARTBEATs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-heartbeat-rx | Total number of HEARTBEATs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-heartbeat-ack-tx | Total number of HBEAT_ACKs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-heartbeat-ack-rx | Total number of HBEAT_ACKs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-abort-tx | Total number of ABORTs sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-abort-rx | Total number of ABORTs received per SS7 Routing Domain. | Int32
> ss7rd-sctp-error-tx | Total number of Errors sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-error-rx | Total number of Errors received per SS7 Routing Domain. | Int32
> ss7rd-sctp-bytes-tx | Total number of bytes sent per SS7 Routing Domain. | Int32
> ss7rd-sctp-bytes-rx | Total number of bytes received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-data-tx | Total number of M3UA DATA messages sent | Int32
> ss7rd-m3ua-duna-tx | Total number of M3UA DUNA messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-dava-tx | Total number of M3UA DAVA messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-daud-tx | Total number of M3UA DAUD messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-scon-tx | Total number of M3UA SCON messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-dupu-tx | Total number of M3UA DUPU messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-drst-tx | Total number of M3UA DRST messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-regreq-tx | Total number of M3UA REG-REQ messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-regrsp-tx | Total number of M3UA REG-RSP messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-deregreq-tx | Total number of M3UA DEREG-REQ messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-deregrsp-tx | Total number of M3UA DEREG-RSP messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspup-tx | Total number of M3UA ASPUP messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspup-ack-tx | Total number of M3UA ASPUP ACK messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspdn-tx | Total number of M3UA ASPDN messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspdn-ack-tx | Total number of M3UA ASPDN ACK messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspac-tx | Total number of M3UA ASPAC messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspac-ack-tx | Total number of M3UA ASPAC ACK messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspia-tx | Total number of M3UA ASPIA messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspia-ack-tx | Total number of M3UA ASPIA ACK messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-hearbeat-tx | Total number of M3UA HBEAT messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-hearbeat-ack-tx | Total number of M3UA HBEAT ACK messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-error-tx | Total number of M3UA ERR messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-notify-tx | Total number of M3UA NTFY messages sent per SS7 Routing Domain. | Int32
> ss7rd-m3ua-data-rx | Total number of M3UA DATA messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-duna-rx | Total number of M3UA DUNA messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-dava-rx | Total number of M3UA DAVA messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-daud-rx | Total number of M3UA DAUD messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-scon-rx | Total number of M3UA SCON messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-dupu-rx | Total number of M3UA DUPU messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-drst-rx | Total number of M3UA DRST messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-regreq-rx | Total number of M3UA REG-REQ messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-regrsp-rx | Total number of M3UA REG-RSP messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-deregreq-rx | Total number of M3UA DEREG-REQ messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-deregrsp-rx | Total number of M3UA DEREG-RSP messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspup-rx | Total number of M3UA ASPUP messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspup-ack-rx | Total number of M3UA ASPUP ACK messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspdn-rx | Total number of M3UA ASPDN messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspdn-ack-rx | Total number of M3UA ASPDN ACK messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspac-rx | Total number of M3UA ASPAC messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspac-ack-rx | Total number of M3UA ASPAC ACK messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspia-rx | Total number of M3UA ASPIA messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-aspia-ack-rx | Total number of M3UA ASPIA ACK messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-hearbeat-rx | Total number of M3UA HBEAT messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-hearbeat-ack-rx | Total number of M3UA HBEAT ACK messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-error-rx | Total number of M3UA ERR messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-notify-rx | Total number of M3UA NTFY messages received per SS7 Routing Domain. | Int32
> ss7rd-m3ua-lower-intf-pdu-tx | Number of per SS7 Routing Domain.DATA PDUs transmitted on lower interface | Int32
> ss7rd-m3ua-lower-intf-pdusize-tx | Size of DATA PDUs transmitted on lower interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-lower-intf-pdu-rx | Number of DATA PDUs received on lower interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-lower-intf-pdusize-rx | Size of DATA PDUs received on lower interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-upper-intf-pdu-tx | Number of DATA PDUs transmitted on upper interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-upper-intf-pdusize-tx | Size of DATA PDUs transmitted on upper interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-upper-intf-pdu-rx | Number of DATA PDUs received on upper interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-upper-intf-pdusize-rx | Size of DATA PDUs received on upper interface per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-no-route-found | Layer Data Error Statistics downward: no route found per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-pc-unvailable | Layer Data Error Statistics downward: point code unavailable per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-pc-congested | Layer Data Error Statistics downward: point code congested per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-no-psp-avail | Layer Data Error Statistics downward: no PSP available per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-no-nsap-avail | Layer Data Error Statistics downward: no NSAP available per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-msg-failed | Layer Data Error Statistics downward: M3UA message failed per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-loadshare-failed | Layer Data Error Statistics downward: load-sharing failed per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-data-conges-q | Layer Data Error Statistics downward: data queued in congested Q per SS7 Routing Domain. | Int32
> ss7rd-m3ua-down-data-as-pend-q | Layer Data Error Statistics downward: data queued in AS pending Q per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-no-route-found | Layer Data Error Statistics upward: no route found per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-pc-unvailable | Layer Data Error Statistics upward: point code unavailable per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-pc-congested | Layer Data Error Statistics upward: point code congested per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-no-psp-avail | Layer Data Error Statistics upward: no PSP available per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-no-nsap-avail | Layer Data Error Statistics upward: no NSAP available per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-msg-failed | Layer Data Error Statistics upward: M3UA message failed per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-loadshare-failed | Layer Data Error Statistics upward: load-sharing failed per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-data-conges-q | Layer Data Error Statistics upward: data queued in congested Q per SS7 Routing Domain. | Int32
> ss7rd-m3ua-up-data-as-pend-q | Layer Data Error Statistics upward: data queued in AS pending Q per SS7 Routing Domain. | Int32
> ss7rd-m3ua-psp-ps-id | Peer Server Identifier | Int32
> ss7rd-m3ua-psp-instance | Peer Server Process Instance | Int32
> ss7rd-m3ua-psp-data-tx | Total number of M3UA PSP DATA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-duna-tx | Total number of M3UA PSP DUNA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-dava-tx | Total number of M3UA PSP DAVA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-daud-tx | Total number of M3UA PSP DAUD messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-scon-tx | Total number of M3UA SCON messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-dupu-tx | Total number of M3UA PSP DUPU messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-drst-tx | Total number of M3UA PSP DRST messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-regreq-tx | Total number of M3UA PSP REG-REQ messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-regrsp-tx | Total number of M3UA PSP REG-RSP messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-deregreq-tx | Total number of M3UA PSP DEREG-REQ messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-deregrsp-tx | Total number of M3UA PSP DEREG-RSP messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspup-tx | Total number of M3UA PSP ASPUP messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspup-ack-tx | Total number of M3UA PSP ASPUP ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspdn-tx | Total number of M3UA PSP ASPDN messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspdn-ack-tx | Total number of M3UA PSP ASPDN ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspac-tx | Total number of M3UA PSP ASPAC messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspac-ack-tx | Total number of M3UA PSP ASPAC ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspia-tx | Total number of M3UA PSP ASPIA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspia-ack-tx | Total number of M3UA PSP ASPIA ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-hearbeat-tx | Total number of M3UA PSP HBEAT messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-hearbeat-ack-tx | Total number of M3UA PSP HBEAT ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-error-tx | Total number of M3UA PSP ERR messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-notify-tx | Total number of M3UA PSP NTFY messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-data-rx | Total number of M3UA PSP DATA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-duna-rx | Total number of M3UA PSP DUNA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-dava-rx | Total number of M3UA PSP DAVA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-daud-rx | Total number of M3UA PSP DAUD messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-scon-rx | Total number of M3UA PSP SCON messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-dupu-rx | Total number of M3UA PSP DUPU messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-drst-rx | Total number of M3UA PSP DRST messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-regreq-rx | Total number of M3UA PSP REG-REQ messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-regrsp-rx | Total number of M3UA PSP REG-RSP messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-deregreq-rx | Total number of M3UA PSP DEREG-REQ messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-deregrsp-rx | Total number of M3UA DEREG-RSP messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspup-rx | Total number of M3UA PSP ASPUP messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspup-ack-rx | Total number of M3UA PSP ASPUP ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspdn-rx | Total number of M3UA PSP ASPDN messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspdn-ack-rx | Total number of M3UA PSP ASPDN ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspac-rx | Total number of M3UA PSP ASPAC messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspac-ack-rx | Total number of M3UA PSP ASPAC ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspia-rx | Total number of M3UA PSP ASPIA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-aspia-ack-rx | Total number of M3UA PSP ASPIA ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-hearbeat-rx | Total number of M3UA PSP HBEAT messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-hearbeat-ack-rx | Total number of M3UA PSP HBEAT ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-error-rx | Total number of M3UA PSP ERR messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-notify-rx | Total number of M3UA PSP NTFY messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-data-pdu-tx | Number of PSP DATA PDUs transmitted per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-data-pdusize-tx | Size of DATA PDUs transmitted per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-data-pdu-rx | Number of DATA PDUs received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-data-pdusize-rx | Size of DATA PDUs received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-no-route-found | Layer Data Error Statistics: no route found per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-pc-unvailable | Layer Data Error Statistics: point code unavailable per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-pc-congested | Layer Data Error Statistics: point code congested per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-no-psp-avail | Layer Data Error Statistics: no PSP available per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-no-nsap-avail | Layer Data Error Statistics: no NSAP available per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-msg-failed | Layer Data Error Statistics: M3UA message failed per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-loadshare-failed | Layer Data Error Statistics: load-sharing failed per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-data-conges-q | Layer Data Error Statistics: data queued in congested Q per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-up-data-as-pend-q | Layer Data Error Statistics: data queued in AS pending Q per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-congestion-count | Congestion count per SS7 Routing Domain, peer server ID, and PSP instance. This statistic value is of Gauge. | Int32
> ss7rd-m3ua-psp-congestion-level1 | Congestion level 1 per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-congestion-level2 | Congestion level 2 per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-congestion-level3 | Congestion level 3 per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-congestion-queue-size | Congestion queue size per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-congestion-queue-hw | Congestion queue Hw per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-congestion-duration | Duration of Congestion per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-unvailable-count | Unavailable count per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-m3ua-psp-unvailable-duration | Unavailable duration per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
> ss7rd-mtp3-user-part-unavail-tx | MTP3 User part unavailable sent per SS7 Routing Domain. | Int32
> ss7rd-mtp3-traffic-restart-allowed-tx | MTP3 Traffic restart allowed sent per SS7 Routing Domain. | Int32
> ss7rd-mtp3-traffic-restart-waiting-tx | MTP3 Traffic restart waiting sent per SS7 Routing Domain. | Int32
> ss7rd-mtp3-user-part-unavail-rx | MTP3 User part unavailable received per SS7 Routing Domain. | Int32
> ss7rd-mtp3-traffic-restart-allowed-rx | MTP3 Traffic restart allowed received per SS7 Routing Domain. | Int32
> ss7rd-mtp3-traffic-restart-waiting-rx | MTP3 Traffic restart waiting received per SS7 Routing Domain. | Int32
> ss7rd-mtp3-msu-dropped-routing-err | MSU dropped due to a routing error per SS7 Routing Domain. | Int32
> ss7-adjacent-point-code | Adjacent Point Code | Int32
> ss7-adjacent-spc-not-accessible | Description: Total number of failures to access the adjacent (directly connected via SS7 link) signaling point code (SPC) element, such as the RNC, HLR, signaling gateway, etc.,. Triggers: Increments when the adjacent SPC goes to unavailable state from available state, possibly due to: - all SS7 links connected to the adjacent SPC are unavailable - the adjacent SPC is made inaccessible by management Availability: per adjacent point code Type: Counter | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883