> Accounting Management
> This section contains additions and changes made to the accounting-related parameters available in Release 9.0. Topics covered in this chapter are:

> l | Bulk Statistic Enhancements in Release 9.0

> l | CDR Enhancements

> l | Command Enhancements

> l | New Commands

> l | RADIUS Attributes in Release 9.0

> l | Diameter Attributes in Release 9.0

> l | Web Element Manager Enhancements

> Bulk Statistic Enhancements in Release 9.0
> This section lists bulk statistic additions and changes in Release 9.0. Detailed information on bulk statistics is located in both the System Administration Guide and in the Statistics and Counters Reference. Bulk statistic changes in this version are divided into the following sections:

> l | New Bulk Statistics

> l | Modified Bulk Statistics

> l | Obsoleted Bulk Statistics

> New Bulk Statistics
> Support for the following bulk statistics were added in Release 9.0.
> APN Schema

> l | inexcd-mbr-pkt-drop

> l | outexcd-mbr-pkt-drop

> l | inexcd-gbr-pkt-drop

> l | outexcd-gbr-pkt-drop

> l | inexcd-ambr-pkt-drop

> l | outexcd-ambr-pkt-drop

> l | inmisc-pkt-drop

> l | outmisc-pkt-drop

> l | inexcd-mbr-byte-drop

> l | outexcd-mbr-byte-drop

> l | inexcd-gbr-byte-drop

> l | outexcd-gbr-byte-drop

> l | inexcd-ambr-byte-drop

> l | outexcd-ambr-byte-drop

> l | inmisc-byte-drop

> l | outmisc-byte-drop

> CSCF Schema

> l | total-roaming-ue-regs

> l | total-roaming-ue-succ-regs

> l | total-roaming-ue-fail-regs

> l | total-roaming-ue-regs-403

> l | total-roaming-ue-re-regs

> l | total-roaming-ue-succ-re-regs

> l | total-roaming-ue-fail-re-regs

> l | total-roaming-ue-re-regs-403

> l | total-roaming-ue-de-regs

> l | total-roaming-ue-succ-de-regs

> l | total-roaming-ue-fail-de-regs

> l | total-roaming-ue-de-regs-403

> l | call-resp-3xxrx

> l | call-resp-3xxtx

> l | call-resp-402rx

> l | call-resp-402tx

> l | call-resp-403rx

> l | call-resp-403tx

> l | call-resp-404rx

> l | call-resp-404tx

> l | call-resp-407rx

> l | call-resp-407tx

> l | call-resp-408rx

> l | call-resp-408tx

> l | call-resp-420rx

> l | call-resp-420tx

> l | call-resp-421rx

> l | call-resp-421tx

> l | call-resp-480rx

> l | call-resp-480tx

> l | call-resp-486rx

> l | call-resp-486tx

> l | call-resp-487rx

> l | call-resp-487tx

> l | call-resp-488rx

> l | call-resp-488tx

> l | call-resp-4xxrx

> l | call-resp-4xxtx

> l | call-resp-500rx

> l | call-resp-500tx

> l | call-resp-503rx

> l | call-resp-503tx

> l | call-resp-5xxrx

> l | call-resp-5xxtx

> l | call-resp-6xxrx

> l | call-resp-6xxtx

> l | migrated-tcp-conn

> l | packet-tcp-rx

> l | packet-tcp-tx

> l | bytes-tcp-rx

> l | bytes-tcp-tx

> l | message-tcp-request-rx

> l | message-tcp-request-tx

> l | message-tcp-response-rx

> l | message-tcp-response-tx

> l | message-tcp-mtu-switch

> l | perf-att-init-reg

> l | perf-att-init-reg-3gpp-geran

> l | perf-att-init-reg-3gpp-utran-fdd

> l | perf-att-init-reg-3gpp2-1x

> l | perf-att-init-reg-ieee-80211a

> l | perf-att-init-reg-ieee-80211b

> l | perf-att-init-reg-other-at

> l | perf-succ-init-reg

> l | perf-succ-init-reg-3gpp-geran

> l | perf-succ-init-reg-3gpp-utran-fdd

> l | perf-succ-init-reg-3gpp2-1x

> l | perf-succ-init-reg-ieee-80211a

> l | perf-succ-init-reg-ieee-80211b

> l | perf-succ-init-reg-other

> l | perf-fail-init-reg

> l | perf-fail-init-reg-401

> l | perf-fail-init-reg-403

> l | perf-fail-init-reg-404

> l | perf-fail-init-reg-420

> l | perf-fail-init-reg-500

> l | perf-fail-init-reg-other

> l | perf-mean-init-reg-setup

> l | perf-att-rereg

> l | perf-att-rereg-3gpp-geran

> l | perf-att-rereg-3gpp-utran-fdd

> l | perf-att-rereg-3gpp2-1x

> l | perf-att-rereg-ieee-80211a

> l | perf-att-rereg-ieee-80211b

> l | perf-att-rereg-other-at

> l | perf-succ-rereg

> l | perf-succ-rereg-3gpp-geran

> l | perf-succ-rereg-3gpp-utran-fdd

> l | perf-succ-rereg-3gpp2-1x

> l | perf-succ-rereg-ieee-80211a

> l | perf-succ-rereg-ieee-80211b

> l | perf-succ-rereg-other

> l | perf-fail-rereg

> l | perf-fail-rereg-401

> l | perf-fail-rereg-403

> l | perf-fail-rereg-404

> l | perf-fail-rereg-420

> l | perf-fail-rereg-500

> l | perf-fail-rereg-other

> l | perf-att-dereg-ue

> l | perf-att-dereg-ue-3gpp-geran

> l | perf-att-dereg-ue-3gpp-utran-fdd

> l | perf-att-dereg-ue-3gpp2-1x

> l | perf-att-dereg-ue-ieee-80211a

> l | perf-att-dereg-ue-ieee-80211b

> l | perf-att-dereg-ue-other-at

> l | perf-succ-dereg-ue

> l | perf-succ-dereg-ue-3gpp-geran

> l | perf-succ-dereg-ue-3gpp-utran-fdd

> l | perf-succ-dereg-ue-3gpp2-1x

> l | perf-succ-dereg-ue-ieee-80211a

> l | perf-succ-dereg-ue-ieee-80211b

> l | perf-succ-dereg-ue-other

> l | perf-fail-dereg-ue

> l | perf-fail-dereg-ue-401

> l | perf-fail-dereg-ue-403

> l | perf-fail-dereg-ue-404

> l | perf-fail-dereg-ue-420

> l | perf-fail-dereg-ue-500

> l | perf-fail-dereg-ue-other

> l | perf-att-dereg-hss

> l | perf-succ-dereg-hss

> l | perf-fail-dereg-hss

> l | perf-fail-dereg-hss-401

> l | perf-fail-dereg-hss-403

> l | perf-fail-dereg-hss-404

> l | perf-fail-dereg-hss-420

> l | perf-fail-dereg-hss-500

> l | perf-fail-dereg-hss-other

> l | perf-att-dereg-serv

> l | perf-succ-dereg-serv

> l | perf-fail-dereg-serv

> l | perf-fail-dereg-serv-401

> l | perf-fail-dereg-serv-403

> l | perf-fail-dereg-serv-404

> l | perf-fail-dereg-serv-420

> l | perf-fail-dereg-serv-500

> l | perf-fail-dereg-serv-other

> l | perf-att-3rdparty-reg

> l | perf-succ-3rdparty-reg

> l | perf-fail-3rdparty-reg

> l | perf-fail-3rdparty-reg-401

> l | perf-fail-3rdparty-reg-403

> l | perf-fail-3rdparty-reg-404

> l | perf-fail-3rdparty-reg-420

> l | perf-fail-3rdparty-reg-500

> l | perf-fail-3rdparty-reg-other

> l | perf-att-uar

> l | perf-succ-uaa

> l | perf-fail-uaa

> l | perf-att-sar

> l | perf-succ-saa

> l | perf-fail-saa

> l | perf-att-session

> l | perf-succ-session-180

> l | perf-succ-session-200

> l | perf-ans-session

> l | perf-fail-session

> l | perf-att-lir

> l | perf-succ-lia

> l | perf-fail-lia

> l | perf-att-session-frm-oth-domain

> l | perf-frbdn-session-frm-oth-domain

> l | perf-att-session-to-oth-domain

> l | perf-frbdn-session-to-oth-domain

> l | perf-att-init-reg-visited

> l | perf-frbdn-init-reg-visited

> l | perf-rmg-users-out

> l | perf-att-mar

> l | perf-succ-maa

> l | perf-fail-maa

> l | perf-att-ppr

> l | perf-succ-ppa

> l | perf-fail-ppa

> l | perf-att-subscribe

> l | perf-succ-subscribe

> l | perf-fail-subscribe

> l | perf-att-notify

> l | perf-succ-notify

> l | perf-fail-notify

> l | de2a-session-init

> l | de2a-session-active

> l | de2a-udr-sent

> l | de2a-uda-received

> l | de2a-uda-err-3xxx

> l | de2a-uda-parse-err

> l | de2a-udr-err

> DCCA Schema
> The DCCA schema was added.

> l | vpnname

> l | vpnid

> l | ipaddr

> l | port

> l | ccr-inisent

> l | cca-inirec

> l | cca-initimeout

> l | ccr-updsent

> l | cca-updrec

> l | cca-updtimeout

> l | ccr-tersent

> l | cca-terrec

> l | cca-tertimeout

> l | reauth-anssent

> l | reauth-reqrec

> DPCA Schema
> The DPCA schema was added.

> l | vpnname

> l | vpnid

> l | ipaddr

> l | port

> l | ccr-inisent

> l | cca-inirec

> l | ccr-initimeout

> l | ccr-updsent

> l | cca-updrec

> l | ccr-updtimeout

> l | ccr-tersent

> l | cca-terrec

> l | ccr-tertimeout

> l | reauth-anssent

> l | reauth-reqrec

> eGTP-C Schema

> l | tun-sent-retransbearrescmd-fail

> l | tun-recv-retransbearrescmd-fail

> GPRS Schema

> l | llc-frame-stats-ui-gea1-ciph-data-frames-rx

> l | llc-frame-stats-ui-gea1-ciph-data-frames-tx

> l | llc-frame-stats-ui-gea1-ciph-data-octets-rx

> l | llc-frame-stats-ui-gea1-ciph-data-octets-tx

> l | llc-frame-stats-ui-gea2-ciph-data-frames-rx

> l | llc-frame-stats-ui-gea2-ciph-data-frames-tx

> l | llc-frame-stats-ui-gea2-ciph-data-octets-rx

> l | llc-frame-stats-ui-gea2-ciph-data-octets-tx

> l | llc-frame-stats-ui-gea3-ciph-data-frames-rx

> l | llc-frame-stats-ui-gea3-ciph-data-frames-tx

> l | llc-frame-stats-ui-gea3-ciph-data-octets-rx

> l | llc-frame-stats-ui-gea3-ciph-data-octets-tx

> l | llc-frame-stats-ui-unciph-rx

> l | llc-frame-stats-ui-unciph-tx

> l | llc-frame-stats-ui-unciph-data-frames-rx

> l | llc-frame-stats-ui-unciph-data-frames-tx

> l | llc-frame-stats-ui-unciph-data-octets-rx

> l | llc-frame-stats-ui-unciph-data-octets-tx

> l | gprs-num-subs-gea0-capable

> l | gprs-num-subs-gea1-capable

> l | gprs-num-subs-gea2-capable

> l | gprs-num-subs-gea3-capable

> l | gprs-num-subs-gea0-negotiated

> l | gprs-num-subs-gea1-negotiated

> l | gprs-num-subs-gea2-negotiated

> l | gprs-num-subs-gea3-negotiated

> MIPv6HA Schema

> l | admprohreason-authoptmiss

> l | admprohreason-hbitnotset

> l | admprohreason-invaaaspi

> l | admprohreason-invhaspi

> l | admprohreason-polrej

> l | admprohreason-notauth

> l | admprohreason-noperm

> l | insufresource-nosessmgr

> l | insufresource-nomem

> l | insufresource-sessmgrrej

> l | insufresource-ipqexc

> l | insufresource-simbindexc

> P-GW Schema
> The P-GW schema was added.
> S-GW Schema
> The S-GW schema was added.
> System Schema

> l | discover-dis-parse-err

> l | request-dis-parse-err

> l | release-dis-parse-err

> l | fng-cursess

> l | fng-curactive

> l | fng-curdormant

> l | fng-ttlsetup

> l | fng-curchildsa

> l | disc-reason-395

> l | disc-reason-396

> l | disc-reason-397

> l | disc-reason-398

> l | disc-reason-399

> l | disc-reason-400

> l | disc-reason-401

> l | disc-reason-402

> l | disc-reason-403

> l | disc-reason-404

> l | disc-reason-405

> l | disc-reason-406

> l | disc-reason-407

> l | disc-reason-408

> l | disc-reason-409

> l | disc-reason-410

> l | disc-reason-411

> SGSN Schema

> l | 3G-service-rej-unknown-cause

> l | 2G-primary-actv-fail

> l | 2G-secondary-actv-fail

> l | 3G-total-attach-fail-all

> l | 2G-total-attach-fail-all

> l | 3G-intra-comb-rau-fail-iu_release

> l | 3G-intra-comb-rau-fail-ongoing-proc

> l | 2G-intra-comb-rau-fail-ongoing-proc

> l | 3G-inter-comb-rau-fail-iu_release

> l | 3G-inter-comb-rau-fail-ongoing-proc

> l | 2G-inter-comb-rau-fail-ongoing-proc

> l | mt-sms-in-queue

> l | relay-prot-err-protocol-error-rx

> l | relay-prot-smma-rx

> Modified Bulk Statistics
> The following bulk statistics were modified in Release 9.0.
> None for this release.
> Obsoleted Bulk Statistics
> The following bulk statistics were obsoleted in Release 9.0.
> SGSN Schema

> l | 2G-service-rej-sem-wrong-msg

> SGTP Schema:

> l | ggsn-address

> Web Element Manager Path
> Click Accounting | Bulk Statistics Configuration.
> CDR Enhancements
> This section lists new custom GTPP dictionaries in Release 9.0. Refer to the AAA Interface Configuration and Reference for details.
> IPv6 Support in S-CDRs in custom11
> IPV6 support is added for the custom11 dictionary in SGSN. With the introduction of this the custom11 now can support either IPV6 or IPV4 served PDP addresses. To support this, PDPType and ServedPDPAddress fields have been changed.

> l | pdpType: IPV6 or IPV4

> l | servedPDPAddress: up to 16 bytes

> SGSN Support for custom17
> custom17 defined CDR fields are now supported in SGSN S-CDRs. A complete listing of the fields is included in the SGSN and Mobility Management Charging Detail Record Field Reference Tables chapter of the AAA Interface and Administration Reference.
> Command Enhancements
> None for this release.
> New Commands
> None for this release.
> RADIUS Attributes in Release 9.0
> This section lists additions and changes to RADIUS AVPs in Release 9.0. Refer to the AAA Interface Configuration and Reference for details.
> New Attributes
> The following RADIUS attributes are new in Release 9.0.

> l | DHCPMSG-Server-IP

> l | DHCP-RK

> l | DHCP-RK-Key-ID

> l | DHCP-RK-Lifetime

> l | hLMA-IPv6-PMIP6

> l | Hotline-Profile-ID

> l | Hotline-Session-Timer

> l | HTTP-Redirection-Rule

> l | IP-Redirection-Rule

> l | NAS-Filter-Rule

> l | PMIP6-RK-KEY

> l | PMIP6-RK-SPI

> l | PMIP6-Service-Info

> l | SN-CF-Call-RoamingInternatnl

> l | SN-Fast-Reauth-Username

> l | SN-QOS-HLR-Profile

> l | WiMAX-Home-HNP-PMIP6

> l | WiMAX-Home-IPv4-HoA-PMIP6

> Modified Attributes
> The following RADIUS attributes were modified in Release 9.0.

> l | 3GPP-PDP-Type

> l | Acct-Termination-Cause

> l | NAS-Port-Type

> l | SN1-Disconnect-Reason

> l | SN1-PPP-Progress-Code

> l | SN1-Service-Type

> l | SN-Disconnect-Reason

> l | SN-PPP-Progress-Code

> l | SN-Service-Type

> l | WiMAX-PPAQ

> Removed Attributes
> The following RADIUS attributes were removed in Release 9.0.
> None for this release.
> Diameter Attributes in Release 9.0
> This section lists additions and changes to Diameter attributes in Release 9.0. Refer to the AAA Interface Reference for details.
> New Attributes
> The following Diameter attributes are new in Release 9.0.

> l | 3GPP-CF-IPv6-Address

> l | 3GPP-SGSN-IPv6-Address

> l | 3GPP2-Allowed-Persistent-TFTS

> l | 3GPP2-BSID

> l | 3GPP2-Correlation-Id

> l | 3GPP2-Information

> l | 3GPP2-Inter-User-Priority

> l | 3GPP2-MEID

> l | 3GPP2-Max-Auth-Aggr-BW-BET

> l | 3GPP2-Max-Inst-Per-Service-Option

> l | 3GPP2-Max-Per-Flow-Priority-User

> l | 3GPP2-Max-Svc-Inst-Link-Flow-Total

> l | 3GPP2-RAT-Type

> l | 3GPP2-RP-Session-ID

> l | 3GPP2-Service-Option

> l | 3GPP2-Service-Option-Profile

> l | 3GPP2-Serving-PCF

> l | 3GPP2-User-Zone

> l | Access-Network-Type

> l | Access Network Type

> l | Access-Restriction-Data

> l | Alert-Reason

> l | Alert Reason.

> l | All-APN-Configurations-Included-Indicator

> l | Allocation-Retention-Priority

> l | AMBR

> l | AN-GW-Address

> l | AN-Trusted

> l | ANID

> l | APN-Aggregate-Max-Bitrate-DL

> l | APN-Aggregate-Max-Bitrate-UL

> l | APN-Authorized

> l | APN-Barring-Type

> l | APN-Configuration

> l | APN-Configuration-Profile

> l | APN-OI-Replacement

> l | ARP

> l | Authentication-Info

> l | Auth-Profile-Id-Bi-Direction

> l | Auth-Profile-Id-Forward

> l | Auth-Profile-Id-Reverse

> l | AUTN

> l | Call-Barring-Info-List

> l | Cancellation-Type

> l | Change-Condition

> l | Change-Time

> l | Chargeable-User-Id

> l | Charging-Rule-Name-LI

> l | Civic-Location

> l | Client-Identity

> l | CoA-Information

> l | CoA-IP-Address

> l | Complete-Data-List-Included-Indicator

> l | Context-Identifier

> l | CSG-Id

> l | CSG-Subscription-Data

> l | Diagnostics

> l | DSA-Flags

> l | DSR-Flags

> l | Dynamic-Address-Flag

> l | EUTRAN-Vector

> l | Event-Report-Indication

> l | Expiration-Date

> l | Extended-QoS-Filter-Rule

> l | External-Client

> l | Feature-List-ID-Resp

> l | Feature-List-Resp

> l | FID

> l | Flow-Information

> l | Flow-Label

> l | Geospatial-Location

> l | GERAN-Vector

> l | GMLC-Address

> l | GMLC-Restriction

> l | GPRS-Subscription-Data

> l | HPLMN-ODB

> l | IDA-Flags

> l | IDR-Flags

> l | IMEI

> l | Item-Number

> l | KASME

> l | KC-Key

> l | LCS-Info

> l | LCS-PrivacyException

> l | Line-Identifier

> l | Local-Sequence-Number

> l | Location-Information

> l | Logical-Access-Id

> l | MEID

> l | MIP-Home-Agent-Address-IETF

> l | MIP-Home-Agent-Host

> l | MIP6-Agent-Info

> l | MIP6-Feature-Vector

> l | MIP6-Home-Link-Prefix

> l | MO-LR

> l | Mobile-Node-Identifier

> l | Node-Id

> l | NOR-Flags

> l | Notification-To-UE-User

> l | OMC-Id

> l | Operator-Determined-Barring

> l | Operator-String

> l | Packet-Filter-Content

> l | Packet-Filter-Identifier

> l | Packet-Filter-Information

> l | Packet-Filter-Operation

> l | PDP-Context

> l | PDP-Type

> l | Physical-Access-Id

> l | PLMN-Client

> l | PMIP-Mobile-Node-Address

> l | Pre-emption-Capability

> l | Pre-emption-Vulnerability

> l | Priority-Level

> l | QoS-Capability

> l | QoS-Negotiation

> l | QoS-Profile-Template

> l | QoS-Resource-Identifier

> l | QoS-Resource-Operation

> l | QoS-Resource-Request

> l | QoS-Resources

> l | QoS-Rule-Definition

> l | QoS-Rule-Install

> l | QoS-Rule-Name

> l | QoS-Rule-Remove

> l | QoS-Rule-Report

> l | QoS-Subscribed

> l | QoS-Upgrade

> l | RACS-Contact-Point

> l | RAND

> l | RAS-Id

> l | RAT-Frequency-Selection-Priority

> l | RAT-Frequency-Selection-Priority.

> l | Re-Synchronization-Info

> l | Regional-Subscription-Zone-Code

> l | Requested-EUTRAN-Authentication-Info

> l | Requested-GERAN-Authentication-Info

> l | Requested-Information

> l | Resource-Allocation-Notification

> l | Roaming-Restricted-Due-To-Unsupported-Feature

> l | Sector-Id

> l | Security-Parameter-Index

> l | Service-Data-Container

> l | Service-Selection

> l | Service-Specific-Info

> l | ServiceTypeIdentity

> l | SGW-Change

> l | Software-Version

> l | Specific-APN-Info

> l | SRES

> l | SS-Code

> l | SS-Status

> l | STN-SR

> l | Subscriber-Priority

> l | Subscriber-Status

> l | Subscription-Data

> l | Supported-Features-Resp

> l | Supported-RAT-Type

> l | Teleservice-List

> l | Terminal-Information

> l | Terminal-Type

> l | Time-First-Usage

> l | Time-Last-Usage

> l | Time-Usage

> l | Traffic-Data-Volumes

> l | TS-Code

> l | Tunnel-Header-Filter

> l | Tunnel-Header-Length

> l | Tunnel-Information

> l | ULA-Flags

> l | ULR-Flags

> l | UMTS-Vector

> l | User-Id

> l | UTRAN-Vector

> l | Vendor-Id-Resp

> l | Vendor-Specific-QoS-Profile-Template

> l | Visited-PLMN-Id

> l | VPLMN-Dynamic-Address-Allowed

> l | XRES

> Modified Attributes
> The following Diameter attributes were modified in Release 9.0.

> l | 3GPP-PDP-Type

> l | Charging-Rule-Install

> l | Event-Trigger

> l | Experimental-Result-Code

> l | Final-Unit-Indication

> l | QoS-Rule-Install

> l | Specific-Action

> l | Trace-Data

> Removed Attributes
> The following Diameter attributes were removed in Release 9.0.
> None for this release.
> Web Element Manager Enhancements
> None for this release.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883