> ASN Paging Controller Configuration Mode Commands
> The ASN Paging Controller Configuration Mode is used to create and manage ASN paging and location register services for WiMAX subscribers within a context.
> asnpc-id
> This command configures the identifier for an ASN Paging Controller for subscribers in this service.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> asnpc-id mac_address
> default asnpc-id
> default
> Sets the ASN paging controller identifier as IP address of system running ASN paging controller and location registry service.
> mac_address
> Specifies the MAC address of the system running ASN paging controller and location registry service.
> mac_address is the MAC address of paging controller in standard (IEEE 802) format in six groups of two hexadecimal digits, separated by hyphens (-) or colons (:).
> Usage
> Use this command to configure the MAC address of paging controller for ASN paging controller service.
> Example
> The following command sets the MAC address of paging controller to 01:23:45:67:89:ab in colon (:) separated format:
> asnpc-id 01:23:45:67:89:ab
> bind
> This command binds the ASN paging controller service to a logical IP interface and configures the maximum number of subscribers allowed within a service.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> bind address ip_address [ max-subscribers max_subs ]
> no bind
> no
> Removes the binding of the service to a specified interface.
> ip_address
> Specifies the IP address of the interface to which the service is being bound.
> ip_address must be expressed in IPv4 dotted decimal or IPv6 colon separated notation.
> max-subscribers max_subs
> Configures the maximum number of subscribers allowed to connect with this ASN Gateway within specific ASN paging controller service.
> max_subs must be an integer between 0 and 1000000 for an ST16 system.
> max_subs must be an integer between 0 and 3000000 for an ASR 5000 system.
> Usage
> Use this command to associated the service with a specific logical IP address and provides the identity of the ASN paging controller as either the domain name of the ASN paging controller service or the IP address. This command also configures the maximum number of subscribers can be allowed with this service.
> Example
> The following command binds the ASN paging controller service to a logical interface with an IP address of 1.2.3.4 with a limit of 250000 subscribers:
> bind address 1.2.3.4 max-subscribers 250000
> end
> This command exits the current mode and returns to the Executive Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Executive mode.
> exit
> This command exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> max-retransmission
> This command configures the maximum number of times that the system attempts retransmission of R6 control packets to communicate with unresponsive BS.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> max-retransmission retry
> default max-retransmission
> default
> Sets the maximum number of retransmission counter to 3 for R6 control packets within specific ASN paging controller service.
> retry
> Default: 3
> Configures the maximum number of retransmission of R6 control packets to BS before marking it as dead/failed. retry must be an integer between 1 and 10.
> Usage
> Use this command to configure number of retransmission of R6 control packets to BS before marking it as fail/dead.
> Example
> The following command configures the system to attempt 2 times to send R6 control packets to BS:
> max-retransmission 2
> paging-announce
> Configures the number of seconds to wait before sending paging announcement messages to MS.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> paging-announce timeout duration
> default paging-announce timeout
> default
> Sets the paging announce timeout duration to 10 seconds for sending paging announce.
> duration
> Default: 10
> Specifies the maximum duration in seconds to wait for sending a paging announce to MS.
> duration is measured in seconds and must be an integer value from 1 through 1,000.
> Usage
> Use this command to configure the ASN paging controller services to send a paging announce if no data communication is happened for specified duration of time.
> Example
> The following command configures the paging announce timeout value of 500 seconds:
> paging-announce timeout 500
> paging-group
> This command creates/removes the Paging-Group Identifier within specific ASN paging controller service.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> paging-group id paging_group_id [ -noconfirm ]
> no paging-group id paging_group_id
> no
> Disables/removes the Paging Group identifier from specific ASN paging controller service.
> id paging_group_id
> Configures the Paging Group identifier to configure paging agent and other parameters within specific ASN paging controller service.
> This is a logical network identifier for the serving BS or other network� entity retaining MS service and operational information and/�or administering paging activity for the MS while in idle mode
> paging_group_id must be an integer from 1 through 65535.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Warning: If this keyword option is used with no paging-group id paging_group_id command the paging group id paging_group_id will be deleted and disabled with all active/inactive configurations in a paging group without prompting any warning or confirmation.
> Usage
> Use this command to enter/enable/disable Paging Group Identifier Configuration mode functionality within specific ASN paging controller service.
> Important: A maximum of 32 paging groups can be configured within a service.
> Example
> The following command configures the paging group identifier as 1234 for the ASN paging controller service:
> paging-group id 1234
> peer-asngw
> This command provides the facility to configure the addresses of trusted anchor ASN GW peers that a specific ASN Paging Controller and Location Registry service will allow R4 control and data path registration with.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> [ no ] peer-asngw address ip_address
> no
> Removes the configured peer anchor ASN GW from a specific ASN PC/LR service’s trusted peer list.
> address ip_address
> Specifies the IP address of the anchor ASN GW which is added as a trusted peer with the ASN PC/LR service.
> ip_address is the IP address of the anchor ASN GW peers expressed in IPv4 dotted decimal or IPv6 colon separated notation.
> Usage
> Use this command to create the trusted peer anchor ASN GWs with a specific ASN PC/LR service to establish R4 control and data path registration.
> On receipt of idle mode entry request message the ASN PC/LR service checks whether the Anchor DPF/Authenticator ASN GW address received in idle mode entry request message is in trusted peer ASN GW list configured with this command. If the Anchor DPF/Authenticator ASN GW address received in idle mode entry request message is not there (or not configured) in peer list the ASN PC/LR service sends idle mode entry response message with Failure Indication TLV with unspecified error code.�
> A maximum of 32 ASN GWs can be configured with this command.
> Example
> The following command adds the anchor ASN GW with an IP address of 1.2.3.4 as a trusted peer within an ASN PC service.
> peer-asngw address 1.2.3.4
> peer-asnpc
> This command configures the peer Anchor Paging Controller(s) in this ASN PC/LR service.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> [ no ] peer-asnpc id mac_address ip-address ip_address
> no
> Removes the configured peer ASN PC/LR MAC address and IP address as trusted peer anchor ASN PC/LR.
> id mac_address
> Specifies the MAC address of the trusted peer system running ASN paging controller and location registry service.
> mac_address is the MAC address of paging controller in standard (IEEE 802) format in six groups of two hexadecimal digits, separated by hyphens (-) or colons (:).
> ip-address ip_address
> Specifies the IP address of the trusted peer system running ASN paging controller and location registry service.
> ip_address is the IP address of paging controller in standard IPv4 format in dotted decimal notation.
> Usage
> Use this command to configure the trusted peer anchor paging controller for ASN paging controller service. This command provides the input for the internal mapping from PC ID to IP address that is needed to forward the Location Update request from new Anchor PC to current Anchor PC during PC relocation.
> Example
> The following command sets the peer AS NPC id to 01:23:45:67:89:ab in colon (:) separated format and the IP address of the paging controller to 1.1.1.1:
> peer-asnpc id 01:23:45:67:89:ab ip-address 1.1.1.1
> policy overload
> Configures traffic overload policy to control congestion in this service.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> policy overload { drop | reject }
> default policy overload
> default
> Sets the traffic overload policy action to reject in this service.
> drop
> Default: disabled
> Specifies that the system is to drop incoming packets containing new session requests.
> reject
> Default: enabled
> Specifies that the system processes new session request messages and responds with a reject message.
> Usage
> Congestion policies at the service-level can be configured for service. When congestion control functionality is enabled at service level, these policies dictate how services respond should the system detect that a congestion condition threshold has been crossed.
> Example
> The following command configures an overload policy of reject for this ASN PC service:
> policy overload reject
> retransmission-timeout
> Configures the amount of time that must pass without any response before the system re-attempts to send R6 control packets to BS.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> default
> Sets the timeout duration to 3 seconds for retransmission of R6 control packets.
> no
> Disables/removes the configured timeout duration for retransmission of R6 control packets.
> duration
> Default: 3
> Specifies the maximum allowable time for the ASN paging controller service to wait for a response from the BS before it a) attempts to communicate with the BS again (if the system is configured to retry the BS) or b) marks the BS as unreachable.
> duration is measured in seconds and can be configured to any integer value between 1 and 1,000.
> Usage
> Use this command in conjunction with the max-retransmission command in order to configure the ASN paging controller services behavior when it does not receive a response from a particular BS.
> Use the no retransmission-timeout command to delete a previously configured timeout value. If after deleting the lifetime setting you desire to return the lifetime parameter to its default setting, use the default retransmission-timeout command.
> The chassis is shipped from the factory with the retransmission timeout set to 3 seconds.
> Example
> The following command configures a retransmission timeout value of 5 seconds:
> retransmission-timeout 5
> The following command deletes a previously configured retransmission-timeout setting:
> setup-timeout
> Configures the total amount of allowable time for the ASN paging controller service to setup a connection with the BS before it marks the BS as unreachable.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> setup-timeout duration
> default setup-timeout
> default
> Sets the total timeout duration to 60 seconds to setup a connection with BS.
> duration
> Default: 60
> Specifies the maximum allowable time for the ASN paging controller service to setup the R6 connection with BS before marks the BS as unreachable.
> duration is measured in seconds and can be configured to any integer value between 1 and 100000.
> Usage
> Use this command to configure the maximum setup timeout duration to setup an R6 connection with BS. This command supersedes the duration set through the max-retransmission and retransmission-timeout commands for R6 connection.
> The chassis is shipped from the factory with the connection setup timeout duration to 60 seconds.
> Example
> The following command configures an ASN paging controller service to mark a BS after waiting for 100 seconds before marks it as dead or unreachable:
> setup-timeout 100

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883