> Configuration Management
> This section contains additions and changes made to the configuration commands available in Release 8.0 unless specifically designated as being in Release 8.1 or higher.
> New Configuration Commands
> Common Commands - New in Release 8.0
> This section provides information on new commands that are common to products in Release 8.0.
> aaa accounting-overload-protection
> This command configures Overload Protection Policy for accounting requests.
> CLI (Global Configuration Mode)
> aaa accounting-overload-protection prioritize-gtpp
> [ default | no ] aaa accounting-overload-protection
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> alarm-disable
> The new command disables the alarm detection for designated sets of alarms on the Channelized line card.
> CLI (Channelized Port Configuration Mode)
> alarm-disable ( all | ds1-e1 | none | sonet-sdh }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> alarm-soak-timer
> This command sets the timer for the duration that a detected alarm will be soaked before the alarm is reported.
> CLI (Channelized Port Configuration Mode)
> alarm-soak-timer seconds
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> card smc upgrade
> This command upgrades programmables on the specified card. Must be followed by a slot number of card to upgrade.
> CAUTION: This command should only be used if instructed by or working with Starent Support.
> CLI (Exec Mode)
> card smc upgrade slot_number
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cdr
> This command configures the CDR file transfer parameters. The following keywords are available with this command:

> l | use-harddisk: Specifies that the hard disk on the SMC be used to store EDR/UDR files. On configuring to use the hard disk for EDR/UDR storage, EDR/UDR files are transferred from RAMFS on the PSC card to the hard disk on the SMC card. Subsequently the files can be offloaded to an external server such as the L-ESS.

> IMPORTANT: The use-harddisk keyword is only available on the ST40 platform.

> l | push-interval value: Specifies the transfer interval, in seconds, to push CDR files.

> l | remove-file-after-transfer: Specifies that the system is to remove an EDR/UDR file as soon as the file is pushed out of the system.

> l | transfer-mode: Specifies the CDR file transfer mode.

> CLI (EDR Module Configuration Mode & UDR Module Configuration Mode)
> cdr [ push-interval value | remove-file-after-transfer | transfer-mode { pull | push primary { encrypted-url enc_url | url url } [ secondary { encrypted-secondary-url enc_sec_url | url sec_url } ] } + | use-harddisk ]
> no cdr [ remove-file-after-transfer | use harddisk ] +
> default cdr [ push-interval | remove-file-after-transfer | transfer-mode | use harddisk ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cdr-push
> This command initiates manual push of CDR files to the configured external storage server.
> On ST16 chassis, this command must be run only from the context where the EDR/UDR module is configured. On ST40 chassis, this command must be run only from the local context. Running in other contexts will fail.
> CLI (Exec Mode)
> cdr-push { all | local-filename file_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> context-timeout
> Ensures that no expired contexts are used for data compression. Default is to 20 seconds.
> Replaces context-cleanup-period which has been obsoleted.
> CLI (ROHC-Profile Decompress-Config Mode)
> [ default ] context-timeout seconds
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter send-ccri
> This command configures sending CCR-I at the first user dcca-enabled-traffic detection, or on receiving Create-PDP-Context-Request.
> CLI (Credit Control Configuration Mode)
> diameter send-ccri { session-start | traffic-start }
> default diameter send-ccri
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow-control
> Flow control is enabled by default on the Quad-Gig-E (QGLC) line card. If flow control is not required, it can be disabled on a per-port basis using the no option.
> CLI (Ethernet Port Config Mode)
> [ no ] flow-control
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> frame-relay
> This command defines the Frame Relay characteristics of the port.
> CLI (Channelized Port Configuration Mode)
> frame-relay path path_id { ds1 connects | e1 connects} [ timeslots | frame-relay [ intf-type intf_type [ lmi_type lmi_type ] ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> header-type
> This command sets the size of the header frame for a Frame Relay-type message emanating from a channelized line card.
> CLI (Card Configuration Mode)
> [ default ] header-type header-size
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> hopath-sdsf
> This command defines the high-order path SDSF bit error rate (BER) threshold.
> CLI (Channelized Port Configuration Mode)
> hopath-sdsf hopath_value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> hopath-sdsf
> This command defines the high-order path SDSF bit error rate (BER) threshold.
> CLI (Channelized Port Configuration Mode)
> hopath-sdsf hopath_value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ingress-mode
> This command toggles between enabling and disabling the port ingress mode.
> CLI (Port Ethernet Configuration Mode)
> ingress-mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> initial-e1-framing
> With this keyword, the user has the option to choose the boot-time framing mode for all the E1s on the line card.
> CLI (Card Configuration Mode Commands)
> initial-e1-framing [ crc4 | standard ]
> default initial-e1-framing
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ipv6 access-list
> A new command mode was added to configure IPv6 ACL commands.
> CLI (Exec Mode Commands)
> ipv6 access-list name
> The following commands are included in this mode:

> l | deny/permit (any)

> l | deny/permit (by host IP address)

> l | deny/permit (by IP packets)

> l | deny/permit (by source ICMP packets)

> l | deny/permit (by source IP address masking)

> l | deny/permit (by TCP/UDP packets)

> l | end

> l | exit

> l | readdress server

> l | redirect context (any)

> l | redirect context (by host IP address)

> l | redirect context (by IP address masking)

> l | redirect context (by IP packets)

> l | redirect context (by source ICMP packets)

> l | redirect context (by TCP/UDP packets

> l | redirect css delivery-sequence (any)

> l | redirect css delivery-sequence (by host IP address)

> l | redirect css delivery-sequence (by IP address masking)

> l | redirect css delivery-sequence (by IP packets)

> l | redirect css delivery-sequence (by source ICMP packets)

> l | redirect css delivery-sequence (by TCP/UDP packets)

> l | redirect css service (any)

> l | redirect css service (by host IP address)

> l | redirect css service (by ICMP packets)

> l | redirect css service (by IP packets)

> l | redirect css service (by source IP address masking)

> l | redirect css service (by TCP/UDP packets)

> l | redirect css service (for downlink, any)

> l | redirect css service (for downlink, by host IP address)

> l | redirect css service (for downlink, by ICMP packets)

> l | redirect css service (for downlink, by IP packets)

> l | redirect css service (for downlink, by source IP address masking)

> l | redirect css service (for downlink, by TCP/UDP packets)

> l | redirect css service (for uplink, any)

> l | redirect css service (for uplink, by host IP address)

> l | redirect css service (for uplink, by ICMP packets)

> l | redirect css service (for uplink, by IP packets)

> l | redirect css service (for uplink, by source IP address masking)

> l | redirect css service (for uplink, by TCP/UDP packets)

> l | redirect nexthop (any)

> l | redirect nexthop (by host IP address)

> l | redirect nexthop (by IP address masking)

> l | redirect nexthop (by IP packets)

> l | redirect nexthop (by source ICMP packets)

> l | redirect nexthop (by TCP/UDP packets)

> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> line-timing
> This command instructs the system to recover the receive timing source from an external device via the optical (ATM) line card attached to the port.
> CLI (ATM Port Configuration Mode)
> line-timing
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> line-timing
> This command instructs the system to recover the receive timing source from an external device via the channelized line card attached to the port.
> CLI (Channelized Port Configuration Mode)
> line-timing
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> link-aggregation
> Link aggregation combines up to four ports on a redundant pair of Quad Gig-E line card so a large file is guaranteed to be sent serially down the same pipe rather than be distributed and be subject to massive packet re-ordering. LACP is the link aggregation control protocol.
> CLI (Ethernet Port Config Mode)
> [ no ] link-aggregation { master | member } | group N }
> [ lacp { active | passive } ] [ rate { slow | fast } ]
> default link-aggregation lacp
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> link-aggregation system-priority
> Configures the link-aggregation system-priority hex value for a system, which comprises a PSC and its associated QGLC(s).
> CLI (Card Config Mode)
> link-aggregation system-priority priority
> default link-aggregation system-priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> loopback
> This command configures various loopback signals to troubleshoot the SDH/SONET physical layers.
> CLI (Channelized Port Configuration Mode)
> loopback { ds1-e1-diag | ds1-e1-line | none | sonet-sdh-diag | sonet-sdh-line }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> lopath-sdsf
> This command defines the low-order path SDSF bit error rate (BER) threshold.
> CLI (Channelized Port Configuration Mode)
> lopath-sdsf lopath_value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nai-construction
> Creates a constructed-nai configuration on a per-APN basis only rather than by per-aaa-group.
> CLI (APN Configuration Mode Commands)
> nai-construction {imsi | msisdn} [ override-null-username ] [ encrypted password string | use-shared-secret-password | password string ]
> no nai-construction
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> port bits
> Using this command enters the BITS port configuration mode which provides configuration for the transmit timing source. The new BITS port configuration mode includes the following commands:

> l | default

> l | end

> l | exit

> l | mode

> l | no

> l | preferred slot

> l | recover

> l | shutdown

> l | snmp trap link-status

> CLI (Global Configuration Mode)
> port bits slot#/port#>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius accounting interim volume
> This command configures the volume of uplink and downlink volume octet counts that triggers RADIUS interim accounting. This command is now available for PDSN and HA services.
> CLI (AAA Server Group Configuration Mode & Context Configuration Mode)
> radius accounting interim volume { downlink bytes uplink bytes | total bytes | uplink bytes downlink bytes }
> no radius accounting interim volume
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius usage-reporting-algorithm
> This command configures the usage reporting algorithm for RADIUS prepaid using DCCA.
> CLI (Global Configuration Mode)
> radius usage-reporting-algorithm { cumulative | relative }
> default radius usage-reporting-algorithm
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> require detailed-rohc-stats
> This command enables/disables detailed ROHC stats
> CLI (Global Config Mode)
> [ no ] require detailed-rohc-stats
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> require diameter-proxy
> This command enables/disables Diameter Proxy mode.
> CLI (Global Configuration Mode)
> require diameter-proxy { multiple | single }
> no require diameter-proxy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show timing
> This command displays the information configured to define a transmit timing source other than the system clock. The display includes related information (such as port status, timing source priority, timing alarms, etc.) for all of the ports configured for either BITS or line timing.
> CLI (Exec Mode)
> show timing
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> toh-sdsf
> This command defines the line SDSF bit error rate (BER) threshold for a port on a Channelized line card.
> CLI (Channelized Port Configuration Mode)
> toh-sdsf toh_value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> use proxy
> This command enables/disables Diameter proxy for the current endpoint.
> CLI (Global Configuration Mode)
> [ no ] use-proxy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - New in Release 8.1
> IMPORTANT: The new commands documented in this section are only available in Release 8.1.
> card lc upgrade
> This command upgrades programmables on the specified card. Must be followed by a slot number of card to upgrade.
> CAUTION: This command should only be used if instructed by or working with Starent Support.
> CLI (Exec Mode)
> card lc upgrade slot_number
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cea-timeout
> This command configures the Capabilities-Exchange-Answer (CEA) message timeout duration for Diameter session.
> CLI (Diameter Endpoint Configuration Mode)
> cea-timeout duration
> default cea-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear ipv6 neighbors
> Clears the given ipv6 address from the neighbor cache.
> CLI (Exec Mode)
> clear ipv6 neighbors ipv6address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clock
> New timezone asia-azerbaijan added for Baku (GMT+4:00; Baku, Azerbaijan) ) to configure system clock on chassis.
> CLI (Global Configuration Mode)
> clock timezone tz [ local ]
> no clock timezone
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter request-timeout
> This command configures the request-timeout setting for Diameter-IMSA Gx interface.
> CLI (Policy Control Configuration Mode)
> diameter request-timeout timeout
> default diameter request-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter sctp
> This command configures Diameter SCTP parameters for all Diameter endpoints within the context.
> CLI (Context Configuration Mode)
> diameter sctp { hearbeat-interval interval | path max-retransmissions retransmissions }
> default diameter sctp { heartbeat-interval | path max-retransmissions }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> dpa-timeout
> This command configures the Disconnect-Peer-Answer (DPA) message timeout duration for Diameter session.
> CLI (Diameter Endpoint Configuration Mode)
> dpa-timeout duration
> default dpa-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow-control
> Flow control is enabled by default on the Quad- Gig-E line card. If flow control is not required, it can be disabled on a per-port basis using the no option.
> CLI (Ethernet Port Config Mode)
> [ no ] flow-control
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> hd raid
> A new command manages the RAID properties on the ST40 SMC hard disks when the hard disk controller task cannot automatically make the correct decisions or admin intervention is required by policy enforcement.
> CLI (Exec Mode)
> hd raid { check | create { local1 | remote1 } | insert { local1 | remote1 } | overwrite { local1 | remote1 } | remove { local1 | remote1 } | select { local1 | remote1 } }
> hd raid
> A new command accesses the HD RAID configuration mode which defines HD RAID management policies with the following commands:
> - end
> - exit
> - overwrite
> - select
> CLI (Global Config Mode)
> hd raid
> Web Element Manager Path
> This functionality is not supported on the Web Element Manager at this time.
> idle-timeout-activity ignore-downlink
> Allows a session idle-timeout to be reset with either uplink-only traffic or both uplink and downlink traffic. The default is no idle-timeout-activity ignore-downlink.
> If idle-timeout-activity ignore-downlink is configured, the downlink traffic will not be used to reset the idle-timeout. Only uplink packets will be able to reset the idle-timeout.
> By default, ignore-downlink is negated by the no command so both uplink and downlink traffic is used to reset the idle-timeout.
> CLI (APN Configuration Mode Commands)
> [ no ] idle-timeout-activity ignore-downlink
> default idle-timeout-activity
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ikev1 disable-phase1-rekey
> New command added to configure the rekeying of Phase1 SA when the Internet Security Association and Key Management Protocol (ISAKMP) lifetime expires in Internet Key Exchange (IKE) v1 protocol. This command replaced the isakmp disable-phase1-rekey command.
> CLI (Context Configuration Mode)
> [ no ] ikev1 disable-phase1-rekey
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ikev1 keepalive dpd
> New command added to configure the ISAKMP IPSec Dead Peer Detection (DPD) message parameters for IKE v1 protocol. This command replaced the isakmp keepalive command.
> CLI (Context Configuration Mode)
> [ no ] ikev1 keepalive dpd interval interval timeout time num-retry retries
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ikev1 policy
> New command added to configure/create an ISAKMP policy with the specified priority and enters ISAKMP Configuration Mode for IKE v1 protocol. This command replaced the isakmp policy command.
> CLI (Context Configuration Mode)
> [ no ] ikev1 policy priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ipms
> This command enables IPMS Client Configuration Mode for Intelligent Packet Monitoring System (IPMS) support on an AGW, configuring IPMS server connectivity in the context.
> IMPORTANT: Currently this external application is available on PDIF service only. Client CLI (Context Configuration Mode)
> [ no ] ipms [-noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ping6
> Support is now provided to ping IPv6 addresses.
> CLI (Exec Mode)
> ping6 { hostname | ipv6 address }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> service-type
> This command configures the type of service (Frame Relay or pwe3-cse) to be employed on the CLC or CLC2 (channelized line cards).
> CLI (Card Configuration Mode)
> service-type { frame-relay | pwe3-cesopsn | unspecified }
> default service-type
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> set control-dont-fragment
> This command controls the don’t fragment (DF) bit in the outer IP header of the IPsec tunnel data packet. It is a new keyword for the set command in the following crypto map configuration modes:

> l | ipsec-isakmp

> l | ipsec-ikev1

> l | ipsec-manual

> l | ipsec-dynamic

> l | ipsec-subscriber

> It is also issued as control-dont-fragment (without the set command) in the crypto template configuration mode.
> CLI (Crypto Map Config Mode)
> set control-dont-fragment { clear-bit | copy-bit | set-bit }
> CLI (Crypto Template Config Mode)
> control-dont-fragment { clear-bit | copy-bit | set-bit }
> Options are:

> l | clear-bit: Clears the DF bit from the outer IP header (sets it to 0).

> l | copy-bit: Copies the DF bit from the inner IP header to the outer IP header. This is the default action.

> l | set-bit: Sets the DF bit in the outer IP header (sets it to 1).

> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> single-port-mode
> New command added in to enable/disable the he L2TP LAC service always to use standard L2TP port 1701 as source port for all L2TP control and data packets originated from LAC node.
> CLI (LAC Service Configuration Mode)
> [no | default] single-port-mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tunnel selection-key
> New command added in to support the creation of L2TP tunnels between LAC service on GGSN and an LNS server on the basis of attribute, “Tunnel-Server-Auth-ID”, value received from AAA server.
> CLI (LAC Service Configuration Mode)
> tunnel selection-key { tunnel-server-auth-id | none }
> [default] tunnel selection-key
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> IMPORTANT: Currently this feature is supported for GGSN only.
> Common Commands - New in Release 8.3
> This section provides information on new commands that are common to products in Release 8.3.
> diameter mscc-per-ccr-update
> This command configures sending single/multiple MSCC AVP (Multiple-Services-Credit-Control) in CCR-U messages.
> CLI (Credit Control Configuration Mode)
> diameter mscc-per-ccr-update { multiple | single }
> default diameter mscc-per-ccr-update
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> failure-action
> This command specifies the action to be taken when communication between ICAP endpoints within a Content Filtering Server Group fails. This command replaces the timeout action command.
> CLI (Content Filtering Server Group Configuration Mode)
> failure-action { allow | content-insertion content_string | discard | redirect-url url | terminate-flow }
> [ default | no ] failure-action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - New in Release 8.1
> IMPORTANT: The new commands documented in this section are only available in Release 8.1.
> content-filtering category match-method
> This command sets the match method to look up URLs in the category-based content filtering database.
> CLI (ACS Configuration Mode)
> content-filtering category match-method { exact | generic }
> default content-filtering category match-method
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> content-filtering flow-any-error
> This command configures allowing/discarding of Content Filtering packets in case of ACS error scenarios.
> CLI (Rulebase Configuration Mode)
> content-filtering flow-any-error { deny | permit }
> default content-filtering flow-any-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> discarded-flow-content-id
> This command is used in the configuration to account for packets discarded as a result of Content Filtering action.
> CLI (Content Filtering Policy Configuration Mode)
> discarded-flow-content-id content_id
> no discarded-flow-content-id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> failure-action
> This command specifies the failure action when the content filtering analysis results are not available to analyze.
> CLI (Content Filtering Policy Configuration Mode)
> failure-action { allow | content-insert content_string | discard | redirect-url url | terminate-flow | www-reply-code-and-terminate-flow reply_code } [ edr edr_format_name ]
> default failure-action [ edr edr_format_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> upgrade url-blacklisting database
> This command upgrades and loads URL Blacklisting database on the ACSMgrs.
> CLI (Exec Mode)
> upgrade url-blacklisting database [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> url-blacklisting action
> This command enables/disables URL Blacklisting functionality for the rulebase, and configures the EDRs to be generated on Blacklisting match and the action to take.
> CLI (Rulebase Configuration Mode)
> url-blacklisting action { discard | redirect-url url | terminate-flow | www-reply-code-and-terminate-flow reply_code } [ edr edr_format_name ]
> [ default | no ] url-blacklisting action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> url-blacklisting database
> This command configures URL Blacklisting database directory parameters.
> CLI (Global Configuration Mode)
> url-blacklisting database { directory path path | max-versions max_versions | override file file_name }
> default url-blacklisting database { directory path | max-versions | override file }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> url-blacklisting match-method
> This command sets the match method to look up URLs in the URL Blacklisting database.
> CLI (ACS Configuration Mode)
> url-blacklisting match-method { exact | generic }
> default url-blacklisting match-method
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> add-ruledef
> This command adds a ruledef to the current Group of Ruledefs.
> CLI (Group of Ruledefs Configuration Mode)
> add-ruledef priority priority ruledef ruledef_name
> no add-ruledef priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> group-of-ruledefs
> This command creates a group of rule definitions, and enters the Group-of-Ruledefs configuration mode.
> CLI (ACS Configuration Mode)
> group-of-ruledefs ruledef_group [ - noconfirm ]
> no group-of-ruledefs ruledef_group
> The Group-of-Ruledefs configuration mode was added. The following commands are available in this mode:

> l | add-ruledef

> l | end

> l | exit

> l | no

> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> host-pool
> This command creates a host pool, and enters the ACS Host Pool Configuration mode.
> CLI (ACS Configuration Mode)
> [ no ] host-pool host_pool [ - noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> http error
> This command defines a rule definition to analyze user traffic for invalid HTTP packets and other errors while parsing HTTP packets.
> CLI (Ruledef Configuration Mode)
> [ no ] http error operator condition
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> idle-timeout
> This command specifies the maximum duration a flow type can remain idle, in seconds, after which the system automatically terminates the flow.
> CLI (ACS Configuration Mode)
> idle-timeout { icmp | tcp | udp } idle_duration
> [ default | no ] idle-timeout { icmp | tcp | udp }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> imsi-pool
> This command creates an IMSI pool, and enters the ACS IMSI Pool Configuration mode.
> CLI (ACS Configuration Mode)
> [ no ] imsi-pool imsi_pool [ - noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip error
> This command defines a rule definition to analyze user traffic for invalid IP packets and other errors while parsing IP packets.
> CLI (Ruledef Configuration Mode)
> [ no ] ip error operator condition
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip max-fragments
> This command limits the maximum number of IP fragments per fragment chain.
> CLI (ACS Configuration Mode)
> ip max-fragments max_fragments
> default ip max-fragments
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip reset-tos
> This command configures the system to be able to reset the IP Type of Service (ToS).
> CLI (Rulebase Configuration Mode)
> ip tos-reset
> default ip tos-reset
> no ip tos-reset
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip vlan
> This command configures the VLAN identifier to be associated with the IP address for the session.
> CLI (Charging Action Configuration Mode)
> ip vlan range
> [ default | no ] ip vlan
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nexthop-forwarding-address
> This command configures the next-hop forwarding address for a charging action.
> CLI (Charging Action Configuration Mode)
> nexthop-forwarding-address ipv4_address
> no nexthop-forwarding-address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> packet-filter
> This command creates an Active Charging Service Packet Filter, and enters the Packet Filter Configuration mode.
> CLI (ACS Configuration Mode)
> packet-filter filter_name [ -noconfirm ]
> no packet-filter filter_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> port-map
> This command creates a port map, and enters the ACS Port Map Configuration mode.
> CLI (ACS Configuration Mode)
> [ no ] port-map port_map [ - noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos-class-identifier
> This command configures the QoS Class Identifier.
> CLI (Charging Action Configuration Mode)
> qos-class-identifier identifier
> no qos-class-identifier
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos-renegotiate traffic-class
> This command configures the QoS traffic class for the charging action for the Layer 7 QoS Renegotiation feature, enabling triggering QoS renegotiation from an active-charging rule. This command is controlled by the dynamic-qos-renegotiation license.
> CLI (Charging Action Configuration Mode)
> qos-renegotiate traffic-class { background | conversational | interactive priority | streaming }
> no qos-renegotiate
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos-renegotiate timeout
> This command configures the timeout setting for the Quality of Service (QoS) Renegotiation feature. This command is controlled by the dynamic-qos-renegotiation license.
> CLI (Rulebase Configuration Mode)
> qos-renegotiate timeout timeout
> no qos-renegotiate timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rtcp uri
> This command defines a rule definition to analyze and charge user traffic using Uniform Resource Identifier (URI) associated with Real-time Transport Control Protocol (RTCP).
> CLI (Ruledef Configuration Mode)
> [ no ] rtp uri [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> tcp check-window-size
> This command enables/disables TCP window-size checking.
> CLI (Rulebase Configuration Mode)
> [ default | no ] tcp check-window-size
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tcp packets-out-of-order
> This command configures the options for out-of-order packets.
> CLI (Rulebase Configuration Mode)
> tcp packets-out-of-order { timeout duration_ms | transmit [ after-reordering | immediately ] }
> default tcp packets-out-of-order { timeout | transmit }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tft packet-filter
> This command configures the packet filter to be sent to the MS.
> CLI (Charging Action Configuration Mode)
> [ no ] tft packet-filter packet_filter
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> url-extraction
> This command enables configuration of ICAP URL extraction behavior.
> CLI (Content Filtering Server Group Configuration Mode)
> url-extraction { after-parsing | raw }
> default url-extraction
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> wtp packets-out-of-order
> This command configures how to process TCP packets that are out of order, while waiting for the earlier packet(s) to arrive.
> CLI (Rulebase Configuration Mode)
> wtp packets-out-of-order { out-of-order-timeout timeout | transmit [ after-reordering | immediately ] }
> default wtp packets-out-of-order { out-of-order-timeout | transmit }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - New in Release 8.1
> This section provides information on new commands available in Release 8.1.
> bearer 3gpp apn
> This command defines a rule definition to analyze and charge user traffic based on APN of the bearer flow.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer 3gpp apn [ case-sensitive ] operator value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer 3gpp imsi
> This command defines a rule definition to analyze and charge user traffic based on the International Mobile Station Identification number (IMSI) in bearer flow.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer 3gpp imsi { operator imsi | { !range | range } imsi-pool imsi_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer 3gpp rat-type
> This command defines a rule definition to analyze and charge user traffic based on the Radio Access Technology (RAT) in bearer flow.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer 3gpp rat-type operator rat
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer 3gpp sgsn-address
> This command defines a rule definition to analyze and charge user traffic based on SGSN address associated in bearer flow. This command replaces the bearer sgsn-address command.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer 3gpp sgsn-address operator address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> edr transaction-complete
> This command configures the generation of an EDR on the completion of a transaction. In this release EDR generation is supported only for HTTP protocol.
> CLI (Rulebase Configuration Mode)
> edr transaction-complete http edr-format edr_format
> { default | no } edr transaction-complete
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> extract-host-from-uri
> If the host field is not present in HTTP/WSP header, this command will extract host from URI, and store it in the host field.
> CLI (Rulebase Configuration Mode)
> extract-host-from-uri { http | wsp + )
> { default | no } extract-host-from-uri
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> http error
> This command defines a rule definition to analyze user traffic for invalid HTTP packets and other errors while parsing HTTP packets.
> CLI (Ruledef Configuration Mode)
> [ no ] http error operator condition
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip error
> This command defines a rule definition to analyze user traffic for invalid IP packets and other errors while parsing IP packets.
> CLI (Ruledef Configuration Mode)
> [ no ] ip error operator condition
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rtp parent-proto
> This command defines a rule definition to analyze and charge user traffic based on the parent protocol of the RTP flow.
> CLI (Ruledef Configuration Mode)
> [ no ] rtp parent-proto operator parent_protocol
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rtcp parent-proto
> This command defines a rule definition to analyze and charge user traffic based on the parent protocol of the RTCP flow.
> CLI (Ruledef Configuration Mode)
> [ no ] rtcp parent-proto operator parent_protocol
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> start
> This command configures timeslots in a timedef.
> CLI (Timedef Configuration Mode)
> [ no ] start day { friday | monday | saturday | sunday | thursday | tuesday | wednesday } time hh mm ss end day { friday | monday | saturday | sunday | thursday | tuesday | wednesday } time hh mm ss
> [ no ] start time hh mm ss end time hh mm ss
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tcp check-window-size
> This command enables/disables TCP window-size checking.
> CLI (Rulebase Configuration Mode)
> [ default | no ] tcp check-window-size
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tcp mss
> This command configures the TCP Maximum Segment Size (MSS) in TCP SYN packets.
> CLI (Rulebase Configuration Mode)
> tcp mss tcp_mss { add-if-not-present | limit-if-present } +
> [ default | no ] tcp mss
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> timedef
> This command enables creating/configuring/deleting an ACS Time Definition (timedef) for the Time-of-Day Activation/Deactivation feature.
> A new configuration mode “Timedef Configuration Mode” was added to configure the timedefs. The following commands are included in this mode:

> l | end

> l | exit

> l | start

> CLI (ACS Configuration Mode)
> timedef timedef_name [ -noconfirm ]
> no timedef timedef_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> url-extraction
> This command enables configuration of ICAP URL extraction behavior.
> CLI (Content Filtering Server Group Configuration Mode)
> url-extraction { after-parsing | raw }
> default url-extraction
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> wsp x-header
> This command defines a rule definition to analyze and charge user traffic based on WSP extension-headers (x-headers).
> CLI (Ruledef Configuration Mode)
> [ no ] wsp x-header name [ case-sensitive ] operator string
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - New in Release 8.3
> This section provides information on new commands available in Release 8.3.
> post-processing priority
> This command configures the post-processing action to be taken for the specified ruledef in the rulebase.
> CLI (Rulebase Configuration Mode)
> post-processing priority priority ruledef ruledef_name charging-action charging_action_name [ description description ]
> no post-processing priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> firewall dos-protection
> This command configures firewall protection from Denial-of-Service (DoS) attacks.
> CLI (ACS Configuration Mode)
> [ no ] firewall dos-protection { all | flooding { icmp | tcp-syn | udp } | ftp-bounce | ip-unaligned-timestamp | mime-flood | seq-number-out-of-range | seq-number-prediction | source-router | teardrop | winnuke }
> default firewall dos-protection
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall flooding
> This command configures firewall protection from packet flooding attacks.
> CLI (ACS Configuration Mode)
> firewall flooding { { protocol { icmp | tcp-syn | udp } packet limit packets } | { sampling-interval interval } }
> default firewall flooding { { protocol { icmp | tcp-syn | udp } packet limit } | { sampling-interval } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall max-ip-packet-size
> This command configures the maximum IP packet size allowed over firewall.
> CLI (ACS Configuration Mode)
> firewall max-ip-packet-size packet_size protocol { icmp | non-icmp }
> default firewall max-ip-packet-size protocol { icmp | non-icmp }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall mime-flood
> This command configures firewall protection from mime-flood attacks.
> CLI (ACS Configuration Mode)
> firewall mime-flood { http-headers-limit max_limit | max-http-header-field-size max_size }
> default firewall mime-flood { http-headers-limit | max-http-header-field-size }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall priority
> This command adds and specifies the priority of a firewall rule definition in the rulebase, and allows to configure a single or range of ports to be allowed on the server for auxiliary/data connections.
> CLI (Rulebase Configuration Mode)
> firewall priority priority firewall-ruledef ruledef_name { { permit [ trigger open-port { aux_port_number | range start_port_number to end_port_number } direction { both | reverse | same } ] } | { deny [ charging-action charging_action ] } }
> no firewall priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall ruledef
> This command creates a Firewall Ruledef, and enters the ACS Firewall Ruledef Configuration Mode.
> CLI (ACS Configuration Mode)
> [ no ] firewall ruledef ruledef_name [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-syn-flood-intercept
> This command enables and configures the TCP intercept parameters to prevent TCP SYN flooding attacks by intercepting and validating TCP connection requests for DoS protection mechanism configured with the dos-protection command.
> CLI (ACS Configuration Mode)
> firewall tcp-syn-flood-intercept { max-attempts max_attempts | mode { none | { intercept | watch } [ aggressive ] } | retransmit-timeout retransmit_timeout | watch-timeout intercept_watch_timeout }
> default firewall tcp-syn-flood-intercept { max-attempts | mode | retransmit-timeout | watch-timeout }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - New in Release 8.1
> IMPORTANT: The new commands documented in this section are only available in Release 8.1.
> bearer username
> This command defines firewall rule definition to analyze user traffic based on user name of the bearer flow.
> CLI (ACS Firewall Ruledef Configuration Mode)
> [ no ] bearer username [ case-sensitive ] operator value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall flow-recovery
> This command configures Firewall flow recovery parameters.
> CLI (ACS Configuration Mode)
> firewall flow-recovery { downlink | uplink } [ timeout timeout ]
> { default | no } firewall flow-recovery { downlink | uplink }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall icmp-destination-unreachable-message-threshold
> This command configures a threshold on the number of ICMP error messages sent by the subscriber for a particular data flow.
> CLI (ACS Configuration Mode)
> firewall icmp-destination-unreachable-message-threshold messages then-block-server
> [ default | no ] firewall icmp-destination-unreachable-message -threshold
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall nat-alg
> This command enables/disables the specified NAT Application Level Gateway (ALG).
> CLI (ACS Configuration Mode)
> [ default | no ] firewall nat-alg { all | ftp | rtsp }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall no-ruledef-matches
> This command configures the default action for packets with no Firewall ruledef matches.
> CLI (ACS Configuration Mode)
> firewall no-ruledef-matches { downlink | uplink } action { deny [ charging-action charging_action ] | permit }
> default firewall no-ruledef-matches { downlink | uplink } action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall policy
> This command enables/disables Stateful Firewall support for all subscribers using the current rulebase. In 8.0, this configuration was present in the Subscriber/APN mode.
> CLI (Rulebase Configuration Mode)
> firewall policy firewall-required
> { default | no } firewall policy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall port-scan
> This command configures port-scan detection parameters.
> CLI (ACS Configuration Mode)
> firewall port-scan { connection-attempt-success-percentage { non-scanner | scanner } percentage | inactivity-timeout inactivity_timeout | protocol { tcp | udp } response-timeout response_timeout | scanner-policy { block inactivity-timeout inactivity_timeout | log-only } }
> default firewall port-scan { connection-attempt-success- percentage { non-scanner | scanner } | inactivity-timeout | protocol { tcp | udp } response-timeout | scanner-policy }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall priority
> This command adds and specifies the priority and type of a firewall rule definition in the rulebase, and allows you to configure a single or range of ports to be allowed on the server for auxiliary/data connections.
> CLI (Rulebase Configuration Mode)
> firewall priority priority [ dynamic-only | static-and-dynamic ] firewall-ruledef ruledef_name { { permit [ trigger open-port { aux_port_number | range start_port_number to end_port_number } direction { both | reverse | same } ] } | { deny [ charging-action charging_action ] } }
> no firewall priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-first-packet-non-syn
> This command configures the action to take on TCP flow starting with a non-syn packet.
> CLI (Rulebase Configuration Mode)
> firewall tcp-first-packet-non-syn { drop | reset }
> default firewall tcp-first-packet-non-syn
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-idle-timeout-action
> This command configures the action to take on TCP idle timeout expiry.
> CLI (Rulebase Configuration Mode)
> firewall tcp-idle-timeout-action { drop | reset }
> default firewall tcp-idle-timeout-action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall track-list
> This command configures the maximum number of server IPs to be tracked that are involved in any kind of DOS attacks.
> CLI (ACS Configuration Mode)
> firewall track-list attacking-servers no_of_servers
> default firewall track-list attacking-servers
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow any-error
> This command configures the accounting action for packets dropped by Firewall due to any error.
> CLI (Rulebase Configuration Mode)
> flow any-error charging-action charging_action
> default flow any-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nat policy
> This command enables/disables Network Address Translation (NAT) processing for all subscribers using this rulebase.
> CLI (Rulebase Configuration Mode)
> nat policy nat-required
> { default | no } nat policy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - New in Release 8.3
> IMPORTANT: The new commands documented in this section are only available in Release 8.3.
> firewall tcp-reset-message-threshold
> This command configures a threshold on the number of TCP reset messages sent by the subscriber for a particular data flow. After this threshold is reached, further downlink traffic to the subscriber on the unwanted flow is blocked.
> CLI (Rulebase Configuration Mode)
> firewall tcp-reset-message-threshold messages then-block-server
> { default | no } firewall tcp-reset-message-threshold
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> bearer-control-mode
> This new command configures the bearer control mode for network controlled QoS (NCQoS) feature.
> CLI (APN Configuration Mode)
> bearer-control-mode [ ms-only | mixed ]
> [ default ] bearer-control-mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpu udp-checksum insert
> Use this command to enable the system to insert UDP checksum in outgoing UDP data packets.
> CLI (GGSN Service Configuration Mode)
> gtpu udp-checksum insert
> default gtpu udp-checksum insert
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nai-construction
> Added new command in APN configuration mode to configure NAI construction for user authentication in GPRS/UMTS networks.
> CLI (APN Configuration Mode)
> nai-construction {imsi | msisdn} [override-null-username]
> default nai-construction
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos negotiate-limit
> This new command configures the traffic shaping and policing related parameters.
> CLI (APN Configuration Mode)
> qos negotiate-limit direction { downlink | uplink } [ class { background | conversational | interactive traffic_priority | streaming } ] [ peak-data-rate bps [ committed-data-rate bps ] | committed-data-rate [ peak-data-rate bps ]]
> no negotiate-limit direction { downlink | uplink } [ class { background | conversational | interactive traffic_priority | streaming }]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos rate-limit
> This new command configures the traffic shaping and policing related parameters.
> CLI (APN Configuration Mode)
> qos rate-limit { downlink | uplink } [ class { background | conversational | interactive traffic_priority | streaming } ] [ burst-size bytes ] [ exceed-action { drop | lower-ip-precedence | transmit }[ violate-action { drop | lower-ip-precedence | shape [transmit-when-buffer-full] | transmit }]]|[ violate-action { drop | lower-ip-precedence | shape [transmit-when-buffer-full] | transmit } [ exceed-action { drop | lower-ip-precedence | transmit }]] +
> no qos rate-limit direction { downlink | uplink } [ class { background | conversational | interactive traffic_priority | streaming } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - New in Release 8.1
> The following commands are new to the GGSN in Release 8.1:
> clear gtpp storage-server local file statistics
> This command clears the statistics for CDRs stored on the local SMC hard disk.
> CLI (Exec Mode)
> clear gtpp storage-server local file statistics [ group name name]
> credit-control-group
> This command configures the Credit Control Group to be used for subscribers configured for a particular APN.
> CLI (APN Configuration Mode)
> credit-control-group cc_group_name
> no credit-control-group
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp compression-process
> This command configures the maximum number of child compression processes that AAAproxy can have. This functionality is a part of the hard disk support processes.
> CLI (Global Configuration Mode)
> gtpp compression-process max_number
> default gtpp compression-process
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp dead-server suppress-cdrs
> New command added to configure the action to be taken on the CDRs generated during communication failure between GGSN and GTPP servers. It also disables the archive of CDRs.
> CLI (GTPP Group Configuration Mode)
> [no | default] gtpp dead-server suppress-cdrs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp ram-disk-limit
> This command configures additional storage space to be allocated for writing files. The memory specified with this command would be added to the existing memory allocated to the AAAproxy only if hard disk storage is enabled.
> CLI (Global Configuration Mode)
> gtpp ram-disk-limit mb mega_bytes
> default gtpp ram-disk-limit
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp secondary-group
> New command added to enable/associate a preconfigured secondary GTPP server group to an APN for CGF accounting functionality. By default it is disabled.
> CLI (APN Configuration Mode)
> gtpp secondary-group group_name [accounting-context actt_ctxt_name]
> [no | default] gtpp secondary-group group_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server local file
> This command configures the parameters for the GTPP files to be stored on the local GTPP storage server. Support for ‘custom6’ has been added to provide 8K block structure for billing CDR files
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server local file { compression { gzip | none } | format { custom1 | custom2 | custom3 | custom4 | custom5 | custom6 } | name prefix prefix | rotation { cdr-count count | time-interval time | volume size } }
> default gtpp storage-server local file { compression | format | name | rotation }
> no gtpp storage-server local file rotation { cdr-count | time-interval }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server mode
> This command specifies where CDRs will be stored -- on an external server of on a hard disk on the SMC in the ST40 chassis.
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server mode { local | remote }
> default gtpp storage-server mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server mode
> New keyword “streaming” added to support backup for streaming CDRs on a hard disk on the SMC in the ST40 chassis.
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server mode { local | remote | streaming }
> default gtpp storage-server mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> IMPORTANT: This is a customer-specific feature.
> gtpp suppress-cdrs zero-volume-and-duration
> This command suppresses the CDRs created by session having zero duration and/or zero volume. By default this mode is ‘disabled’
> CLI (GTPP Group Configuration Mode)
> gtpp suppress-cdrs zero-volume-and-duration { gcdrs [egcdrs] | egcdrs [gcdrs] }
> default gtpp suppress-cdrs zero-volume-and-duration
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp transport-layer
> New command added to provide facility to select the transport layer protocol for Ga interface between AGWs (GSNs) and GTPP servers. By default selected transport layer protocol is UDP.
> CLI (GTPP Group Configuration Mode)
> gtpp transport-layer { tcp | udp }
> default gtpp transport-layer
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - New in Release 8.3
> This section provides information on new commands available in Release 8.3.
> hd raid
> Added requirement to confirm commands.
> CLI (HD RAID Configuration Mode)
> select { newer | none } disk [ -noconfirm ]
> overwrite { invalid | unknown | valid } disk
> [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> wimax-3gpp2 interworking
> New command added in HA Configuration mode to configure the interworking between 3GPP2 and WiMAX technology networks.
> CLI (HA Configuration Mode)
> [no | default] wimax-3gpp2 interworking
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - New in Release 8.1
> This section provides information on new commands available in Release 8.1.
> delay interval
> Configure the delay time, for starting the dead timer, after configuration files are loaded.
> CLI (SRP Configuration Mode)
> hello-interval
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDIF Commands - New in Release 8.0
> PDIF is not supported in Release 8.0.
> PDIF Commands - New in Release 8.1
> certificate
> Apply an X.509 certificate to a crypto template, or remove it, or include or preclude the certificate in the Auth Exchange response payload
> CLI (Crypto Template Config Mode
> [ no | default ] certificate name include-payload
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> certificate
> Create or negate an X.509 trusted certificate.
> CLI (Context Config Mode)
> [ no ] certificate name name pem { data cert_data | url cert_url } private-key pem { [ encrypted ] data private_key_data | url url }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter authentication failure-handling
> This command configures error handling for Diameter EAP requests.
> CLI (AAA Server Group Configuration & Context Configuration Modes)
> [ no ] diameter authentication failure-handling { eap-request | eap-termination-request } { request-timeout action { continue | terminate } } | result-code result_code [ to result_code ] action { continue | retry-and-terminate | terminate } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter disable endpoint
> This command disables a diameter peer without removing the peer’s configuration.
> CLI (Exec Mode)
> diameter disable endpoint endpoint_name peer peer_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter enable endpoint
> This command enables a diameter peer that is disabled.
> CLI (Exec Mode)
> diameter enable endpoint endpoint_name peer peer_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> duplicate-session-detection
> Configured in the PDIF-Service mode, duplicate-session-detection configures the PDIF to check for any attempt to set up a call after a MS comes back into WiFi range using either the IMSI or NAI address from a call lost after the MS initially went out of WiFi AP range. Detection can be based on either the IMSI or NAI (default) address. If NAI is used, it must be the NAI from Stage One authentication.
> CLI (PDIF-Service Config Mode)
> duplicate-session-detection { NAI | IMSI }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> group
> Diffie-Hellman Group 14 has been added to the existing Groups 1, 2 and 5 for IKEv2 security exchanges.
> CLI (IKEv2 Security Association Configuration Mode
> group { 1 | 2 | 5 | 14 }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ignore-rekeying-requests
> Configured in the Crypto Template Payload Config Mode, this is a new command that prevents the creation of a CHILD SA.
> CLI (Crypto Template Payload Config Mode)
> ignore-rekeying-requests
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ikev2-ikesa
> Configured in the Crypto Template Config Mode, the keyword rekey has been added to ikev2-ikesa commands. It specifies if IKESA rekeying should occur before the configured lifetime expires (at approximately 90% of the lifetime interval). Default is no ikev2-ikesa rekey.
> CLI (Crypto Template Config Mode)
> [ no ] ikev2-ikesa [ rekey ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip source-violation
> Source validation requires the source address of received packets to match the IP address assigned to the subscriber. IP source-violation sets parameters for allowing bad packets before terminating the call.
> CLI (PDIF-Service Config Mode)
> ip source-violation { clear-on-valid-packet | drop-limit num | period
> secs }
> no ip source-violation clear-on-valid-packet
> Web Element Manager Path
> Configuration | PDIF Service | Configuration
> ipv6 address
> Enable this ipv6 address when the Service Redundancy Protocol determines this chassis to be active for Session Recovery .
> CLI (loopback-interface-config-mode)
> ipv6 address 2001:268:2008:b::1021/128 srp-activate
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nai
> Configures the NAI parameters to be used for the crypto template IDr. This configured IDr is sent from PDIF to MS in the first IKEv2 AUTH response. The default configuration is no nai. As a result, the default behavior is for the PDIF-service IP address to be sent as the IDr value with the type ID_IP_ADDR.
> CLI (Crypto-Template Config Mode)
> [ default | no ] nai idr name id-type { rfc822-addr | fqdn | ip-addr | key-id }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius accounting pdif trigger-policy
> Configures the policy for dealing with packet overflow.
> CLI (AAA Group Config Mode)
> r adius accounting pdif trigger-policy { counter-rollover | standard }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rekey
> Configured in the Crypto Template Payload Config Mode, the keyword keepalive has been added to the rekey command. If keepalive is configured, a session will be rekeyed even if there has been no data exchanged since the last rekeying operation. By default, rekeying is only performed if there has been data exchanged since the previous rekey.
> CLI (Crypto Template Payload Config Mode)
> [ no ] rekey [ keepalive ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tsi start-address
> Configures the IKEv2 Initiator Traffic Selector (TSI) payload address options.
> CLI (Crypto Template Payload Mode)
> tsi start-address { any { end-address any } | endpoint { end-address endpoint } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> clear credit-control statistics
> This command clears the credit-control statistics.
> CLI (Exec Mode)
> clear credit-control statistics cc-service <name>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ipv6 router advertisement
> New command added in Ethernet Interface Configuration mode to enables or disables the system to send IPv6 router advertisements.
> CLI (Ethernet Interface Configuration Mode)
> [no] ipv6 router advertisement
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> mobile-ipv6
> This new command configures Mobile IPv6 related parameters for a subscriber.
> CLI (Subscriber Configuration Mode)
> [ default | no ] mobile-ipv6 { home-address ipv6_address | home-agent ipv6_address | home-link-prefix ipv6_address | tunnel mtu value }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos traffic-shape
> This new command configures the traffic shaping related parameters.
> CLI (Subscriber Configuration Mode)
> qos traffic-shape direction { downlink | uplink } [ burst-size bytes ] [ committed-data-rate bps ] [ exceed-action { drop | lower-ip-precedence | transmit } ] [ peak-data-rate bps ] [ violate-action { drop | lower-ip-precedence | buffer [transmit-when-buffer-full] | transmit } ] +
> no qos traffic-shape direction { downlink | uplink }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> policy ipv6 tunnel
> Tunnel MTU for IPv6 Tunnel between HA and Mobile Node.
> CLI (Subscriber Config Mode )
> policy ipv6 tunnel mtu exceed { fragment | notify-sender }
> mtu exceed { fragment | notify-sender }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - New in Release 8.1
> This section provides information on new commands available in Release 8.1.
> accounting trigger
> This command configures an accounting trigger policy map to selectively start and terminate accounting sessions based on the categorization of traffic as being interesting or non-interesting to support the QCHAT Billing Suppression feature.
> CLI (Traffic Policy-Map Configuration Mode)
> [ no ] accounting trigger { inactivity-timeout stop | interesting-traffic start }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip routing overlap-pool
> This command provides the ability to advertise overlap-pool addresses into routing
> CLI (config-context mode)
> [ no | default ] ip routing overlap-pool
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Session Control Manager Commands - New in Release 8.0
> Session Control Manager is not supported in Release 8.0.
> Session Control Manager Commands - New in Release 8.1
> This section provides information on new commands available in Release 8.1.
> authorization
> This command configures the policy to allow early bandwidth authorization. Default is disabled.
> CLI (CSCF Policy Rules Configuration Mode)
> [ default | no ] authorization early-bandwidth
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> interface
> This command enables the collection of interface SIP statistics in a CSCF service.
> CLI (CSCF Service Configuration Mode)
> [ no ] interface statistics sip
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nat-policy
> This command configures a NAT (Network Address Translation) policy for the service if the CSCF service is performing one of the following functions:

> l | CSCF services are run in bridging (Back-to-Back User Agent) mode

> l | A-BG is an Application-level Gateway (ALG) for NAT

> CLI (CSCF Service Configuration Mode)
> nat-policy policy_name private-address { address ip_address_mask | default | range start_ip_address end_ip_address }
> no nat-policy policy_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> plmn-id
> This command configures the MCC+MNC pair (plmn-id) used to match location specific emergency/service numbers. Default is disabled.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> plmn-id mcc code mnc code
> no plmn-id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> policy
> This command configures the overload response for this policy. When the P-CSCF/A-BG becomes congested, this overload policy is used to reject subsequent sessions or redirect them to another server.
> CLI (CSCF Policy Rules Configuration Mode)
> policy overload { redirect address1 [ weight weight1 ]
> [ address2 [ weight weight2 ] ] ...
> | reject [ use-reject-code { admin-prohibited | insufficient-resources } ]}
> default policy overload
> no policy overload redirect address1 [ address2 ] ...
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> policy
> This command configures the policy for Served User Routing in this S-CSCF service.
> CLI (CSCF Serving-CSCF Configuration Mode)
> [ default | no ] policy allow p-served-user-routing
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sip-header
> This command enables SIP P-Access-Network-Info (PANI) or P-User-Database (PUD) header insertion for the P-CSCF/A-BG service.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> [ no ] sip-header insert { p-access-network-info | p-user-database }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sip-param
> This command enables the addition of “integrity-protected” parameter in the authorization header of a SIP (REGISTER) message for the P-CSCF/A-BG service.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> [ no ] sip-param insert integrity-protected
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - New in Release 8.0
> This section provides information on new commands available in Release 8.0.
> accept-procedure
> This keyword enables the use of either a new TLLI (temporary logical link identifier) or an old TLLI for attach-accept or RAU-accept messages sent by the SGSN to the MS during related procedures. Default is new-tlli.
> CLI (GPRS Service config mode)
> gmm accept-procedure [ new-tlli | old-tlli ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> accounting
> The new accounting command in the GPRS Service configuration mode enables the configuration of the type of CDRs to be generated and also defines the context in which the CDRs are generated.
> CLI (GPRS Service Configuration Mode)
> accounting ( cdr-types type | context ctxt_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> accounting
> The new command associates an accounting context and optionally a previously defined GTPP group with an SGSN operator policy.
> CLI (SGSN Operator Policy Configuration Mode)
> accounting context ctxt_name [ gtpp group grp_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> associate-service
> This new command specifies which Gs, MAP, and/or SGTP services are to be associated with a GPRS service.
> CLI (GPRS Service Configuration Mode)
> [ no ] associate-service { gs name | map name | sgtp name } [ context ctxt_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bssgp-timer
> The command configures BSS GP timer parameters in Network Service Entity-Frame Relay or IP configuration mode in a 2.5G GPRS frame relay or IP network connection.
> CLI (Network Service Entity Frame Relay Configuration Mode and Network Service Entity - IP Configuration Mode)
> bssgp-timer { T2 time | Th time }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ciphering-algorithm
> This command defines the usage order (priority) for GPRS encryption algorithms for ciphering.
> CLI (GPRS Service Configuration Mode)
> ciphering-algorithm priority priority algorithm
> default ciphering-algorithm priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gmm information-in-messages
> This command is added to provide the configuration to include the information in messages for the GPRS mobility management (GMM) parameters.
> CLI (SGSN Operator Policy Configuration Mode)
> gmm information-in-messages access-type {{gprs |umts } [ network-name {full-text name | short-text name } | [ send-after { attach | rau } ] }
> [ default | no ] gmm { information-in-messages access-type { gprs | umts }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gmm retrieve-equipment-identity
> This command is added to configure the International Mobile Equipment Identity (IMEI) or software version (SV) retrieval and validation procedure for SGSN operator policy.
> CLI (SGSN Operator Policy Configuration Mode)
> gmm retrieve-equipment-identity {imei | imeisv [ unciphered ] [then-imei]} [verify-equipment-identity [ deny-greylisted ]]
> [no | default] gmm retrieve-equipment-identity
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtp send
> This command configures which information this operator policy specifies for sending in a GTP message. This command includes the following send options:

> l | RAT

> l | ULI

> l | IMEISV

> l | MS-timezone

> CLI (SGSN Operator Policy Configuration Mode)
> [ no | remove ] gtp send send_option
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> iu-recovery
> This command enables the IU recovery function to be used whenever sessions are recovered.
> CLI (IuPS Service Configuration Mode)
> [ no ] iu-recovery
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> This command configures the timers that control the data flow for the logical link control (LLC) sub-layer for the GPRS service.
> CLI (GPRS Service Configuration Mode)
> llc { T200-sapi1-timeout time | T200-sapi11-timeout time | T200-sapi3-timeout time | T200-sapi5-timeout time | T200-sapi7-timeout time | T200-sapi9-timeout time } +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> mtp2-lssu-len
> This command sets the length of the link status signal unit (LSSU) which carries link status information used to manage link alignment and indicate the status of the signaling points to each other.
> CLI (Link Configuration Mode)
> mtp2-lssu-len #_octets
> default mtp2-lssu-len
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> network-initiated-pdp-activation
> This command configures the Operator Policy to support activation of network-initiated PDP contexts and defines any desired activation restrictions.
> CLI (SGSN Operator Policy Configuration Mode)
> network-initiated-pdp-activation {allow | primary | restrict | secondary} +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> network-overload-protection
> This new command enables an attach rate throttle mechanism to configure the number of attaches per second and to specific the action to be taken if the limit is exceeded.
> CLI (Global Configuration Mode)
> network-overload-protection sgsn-new-connections-per-second #_attaches action { drop | reject with cause { congestion | network failure } }
> default network-overload-protection sgsn-new-connections-per-second
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> peer-network-service-entity
> The command creates a Peer Network Service Entity instance in the Network Service Entity IP configuration mode to define the peer network service entity.
> CLI (Network Service Entity IP Configuration Mode)
> [ no ] peer-network-service-entity name name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> pool
> This command enables the default SGSN functionality for SGSN (flex) pooling and enables inclusion of the configured count for pool hop-counter in new SGSN context/identify request messages.
> CLI (SGTP Service Configuration Mode)
> pool { default-sgsn | hop-counter count }
> default pool hop-counter
> no pool { default-sgsn | hop-counter }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rab-modify-procedure
> This command configures how the RAB (radio access bearer) assignment procedure will be modified
> CLI (RNC Config Mode)
> rab-modify-procedure { normal-modify | release-and-establish }
> default rab-modify-procedure
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ranap
> This command enables or disables the inclusion of the Signalling Indication IEs in various RANAP messages depending upon circumstances.
> CLI (Radio Network Controller Service Configuration Mode)
> ranap { signalling-indication-ie { rab-assignment-request [ relocation-request ] | relocation-request [ rab-assignment-request ] }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> re-authenticate
> Enables or disables the re-authentication feature.
> CLI (RNC Config Mode)
> re-authenticate [ access-type { gprs | umts }
> remove re-authenticate
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> release-compliance
> Configures data rate management per RNC by defining the 3GPP release compliance (R6 or R7) of the RNC.
> CLI (RNC Config Mode)
> release-compliance { pre-release-7 | release-7 }
> default release-compliance
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> relocation-complete-timeout
> Specifies the maximum time to wait for a relocation completion in the core network.
> CLI (IuPS Service Config Mode)
> relocation-complete-timeout timeout_value
> default relocation-complete-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> reset-resource
> This command enables the operator to control message length by configuring the number of IuConIDs sent in each RANAP Reset Resource message.
> CLI (DNS Client Configuration Mode)
> [ default ] reset-resource max-iuconid-per-msg <number>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> resolver
> This command configures, or resets to default, either of the two parameters for the DNS resolver function: the number of retries or the retransmission timer.
> CLI (DNS Client Configuration Mode)
> [ default ] resolver {number-of-retries retries | retransmission-interval time}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> retries
> The command configures the number of retries for different events in a virtual connection in the Network Service Virtual Connection configuration mode.
> CLI (Network Service Virtual connection Configuration Mode)
> retries { ns-alive-retry num_retries | ns-block-retry num_retries | ns-reset-retry num_retries | ns-unblock-retry num_retries }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> retry-count
> The command configures the retry-count parameters for NS-alive and SNS procedures in the Network Service Entity IP configuration mode.
> CLI (Network Service Entity IP Configuration Mode)
> retry-count { ns-alive max | sns-proc max }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sctp-max-out-strms
> This command sets the maximum number of outbound streams for a specific PSP.
> CLI PSP Configuration Mode)
> sctp-max-out-strms max#_out_streams
> default sctp-max-out-strms
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sctp-suppress-alarm
> This new command is added to enable/disable the suppression of alarms for SCTP path failure between two peer endpoints.
> CLI (PSP Configuration Mode)
> [no] sctp-suppress-alarm path-failure self-end-point-address orig_ipv4_address peer-end-point-address peer_ipv4_address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> setup-timeout
> This new command sets the maximum number of seconds allowed for session setup.
> CLI (GPRS Service Configuration Mode)
> [default] setup-timout seconds
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sgsn-context-request
> This new command tells the system to perform or to skip the PTMSI signature check if the PTMSI signature is not included in the SGSN context request.
> CLI (GPRS Service Configuration Mode)
> [default] sgsn-context-request ptmsi-signature-absence allowed
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sgsn offload
> This command sets or stops the off loading of subscribers, which is part of the SGSN’s Gb flex load redistribution functionality.
> CLI (Exec Mode)
> sgsn offload gprs-service srvc_name { activating | connecting } [ nri-value | stop | t3312-timeout seconds]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sgsn imsimgr
> This command manages the IMSI auditing performed by the IMSIMgr in combination with one or more SessMgr(s).
> CLI (Exec Mode)
> sgsn imsimgr { add-record imsi sessmgr instance sessmgr# | audit-with sessmgr { all | instance sessmgr# } | remove-record imsi }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> short-message-service
> This command enables or disables the SGSN’s SMS service as well as providing access to the SMS Service Configuration Mode and the commands to fine-tune the SMS operation.
> CLI (MAP Service Configuration Mode)
> short-message-service
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sm
> This command configures the SM layer parameter associated with this particular GPRS service context.
> CLI (GPRS Service Configuration Mode)
> sm { activate-max-retransmissions num_retries | deactivate-
> max-retransmissions num_retries | modify-max-retransmissions num_retries | t3385-timeout secs | t3386-timeout secs | t3395-timeout secs }
> default sm { activate-max-retransmissions | deactivate-
> max-retransmissions | modify-max-retransmissions | t3385-timeout | t3386-timeout | t3395-timeout }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sm
> The requested-apn-from-first subrec keyword enables the selection of an APN from the first subscription record as APN(R). If this feature is enabled, the PDP Activation is not rejected during APN Selection; instead, the APN from the first subscription record is used as the requested APN and the SGSN continues with the rest of the APN Selection process.
> CLI (GPRS Service Configuration Mode)
> sm requested-apn-from-first-subrec
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold per-service-gprs-pdp-sessions
> The command configures the thresholds for the total number of PDP contexts for the GPRS sessions per GPRS service.
> CLI (Global Configuration Mode)
> threshold per-service-grps-pdp-sessions high_thresh [ clear low_thresh ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold per-service-gprs-sessions
> The command configures the thresholds for the GPRS sessions per GPRS service.
> CLI (Global Configuration Mode)
> threshold per-service-grps-sessions high_thresh [ clear low_thresh ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold poll per-service-gprs-pdp-sessions interval
> The command configures the polling interval during which thresholds are measured.
> CLI (Global Configuration Mode)
> threshold poll per-service-gprs-pdp-sessions interval time
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold poll total-gprs-pdp-sessions interval
> The command configures the polling interval during which thresholds are measured.
> CLI (Global Configuration Mode)
> threshold poll total-gprs-pdp-sessions interval time
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold poll per-service-gprs-sessions interval
> The command configures the polling interval during which thresholds are measured.
> CLI (Global Configuration Mode)
> threshold poll per-service-gprs-sessions interval time
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold poll total-gprs-sessions interval
> The command configures the polling interval during which thresholds are measured.
> CLI (Global Configuration Mode)
> threshold poll total-gprs-sessions interval time
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold total-gprs-pdp-sessions
> The command configures the thresholds for the total number of PDP contexts for the GPRS sessions in the system.
> CLI (Global Configuration Mode)
> threshold total-gprs-pdp-sessions high_thresh [ clear low_thresh ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold total-gprs-sessions
> The command configures the thresholds for the total number of GPRS sessions in the system.
> CLI (Global Configuration Mode)
> threshold total-gprs-sessions high_thresh [ clear low_thresh ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> timeout
> The command configures the timeout parameter for different events in a virtual connection in the Network Service Virtual Connection configuration mode.
> CLI (Network Service Virtual Connection Configuration Mode)
> timer { ns-alive-timeout duration | ns-block-timeout duration | ns-reset-timeout duration | ns-test-timeout duration }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> timer
> The command configures the timers for SNS-Prov and TNS-Test in the Network Service Entity IP configuration mode.
> CLI (Network Service Entity IP Configuration Mode)
> timer { SNS-Prov-Timeout time | TNS-Test-Timeout time}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> vlan-map
> This command configures a single IPv4 or IPv6 address multiple vlans to use for a single next-hop gateway.
> CLI (Ethernet Interface Configuration Mode and VLAN Configuration Mode)
> vlan-map next-hop ip_address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> weight
> This command configures the signaling and data weight for the network service virtual link (NSVL) for the NSE-IP end-point.
> CLI (NSVL Configuration Mode)
> weight { data data_weight | signaling signaling_weight }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - New in Release 8.1
> The following commands are new to the SGSN in Release 8.1:
> apn-selection-default
> New operator policy command has been added to enable and configure a default APN for use when the normal APN selection process fails.
> CLI (SGSN Operator Policy Configuration Mode)
> apn-selection-default network-identifier <apn_net_id> [ require-subscription-apn network-identifier <apn_net_id>]
> noapn-selection-default
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> check-imei-timeout-action
> This command configures the action to be taken on the Gf interface if a Check-IMEI fails due to a timeout.
> CLI (SGSN or GPRS Service Configuration Modes)
> check-imei-timeout-action [ continue | reject ]
> default check-imei-timeout-action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear gtpp storage-server local file statistics
> This command clears the statistics for CDRs stored on the local SMC hard disk.
> CLI (Exec Mode)
> clear gtpp storage-server local file statistics [ group name name ]
> clock-source
> This command sets the source of the port’s transmit clock.
> CLI (Port Channelized Configuration Mode)
> clock-source { internal-timing | loop-timing }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> dns israu-mcc-mnc-encoding
> This command configures either decimal or hexadecimal format for the MCC and MNC values in the DNS query.
> CLI (GRPS Service Configuration Mode)
> CLI (SGSN Service Configuration Mode)
> dns israu-mcc-mnc-encoding { decimal | hexidecimal }
> default dns israu-mcc-mnc-encoding
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp compression-process
> This command configures the maximum number of child compression processes that AAAproxy can have. This functionality is a part of the hard disk support processes.
> CLI (Global Configuration Mode)
> gtpp compression-process max_number
> default gtpp compression-process
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp dead-server suppress-cdrs
> New command defines the action the SGSN will take on the CDRs generated during a communication failure between the SGSN and the GTPP servers.
> CLI (GTPP Group Configuration Mode)
> [no | default] gtpp dead-server suppress-cdrs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp ram-disk-limit
> This command configures additional storage space to be allocated for writing files. The memory specified with this command would be added to the existing memory allocated to the AAAproxy only if hard disk storage is enabled.
> CLI (Global Configuration Mode)
> gtpp ram-disk-limit mb mega_bytes
> default gtpp ram-disk-limit
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server local file
> This command configures the parameters for the GTPP files to be stored on the local GTPP storage server. Support for ‘custom6’ has been added to provide 8K block structure for billing CDR files.
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server local file { compression { gzip | none } | format { custom1 | custom2 | custom3 | custom4 | custom5 | custom6} | name prefix prefix | rotation { cdr-count count | time-interval time | volume size } }
> default gtpp storage-server local file { compression | format | name | rotation }
> no gtpp storage-server local file rotation { cdr-count | time-interval }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server mode
> This command specifies where CDRs will be stored -- on an external server of on a hard disk on the SMC in the ST40 chassis.
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server mode { local | remote }
> default gtpp storage-server mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp suppress-cdrs zero-volume-and-duration
> This command suppresses the CDRs created by sessions having zero duration and/or zero volume. By default this mode is ‘disabled’
> CLI (GTPP Group Configuration Mode)
> gtpp suppress-cdrs zero-volume-and-duration { gcdrs [egcdrs] | egcdrs [gcdrs] }
> default gtpp suppress-cdrs zero-volume-and-duration
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp transport-layer
> A new keyword has been added to configure either UDP or TCP as the Ga interface transport layer between SGSN and GTPP servers. By default, UPD protocol is enabled for transport layer.
> CLI (GTPP Group Configuration Mode)
> gtpp transport-layer { tcp | udp }
> default gtpp transport-layer
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> inbound-asp-identifier validate
> This command enables or disables the validation of ASP identifiers inbound to the SGSN via routes defined with the SS7 routing domain.
> CLI (SS7 Routing Domain Configuration Mode)
> inbound-asp-identifier validate
> [ default | no ] inbound-asp-identifier validate
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> link-type
> This keyword is not yet functional - the feature is still in development. This keyword will only be applicable to releases 8.1 and higher.
> Identifies the signalling type for this link.
> CLI (SGSN Linkset Configuration Mode)
> link id id [ link-type [ atm-broadband | highspeed-narrowband | lowspeed-narrowband ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> network-sharing cs-ps-coordination
> This command enables/disables the SGSN service to perform a CS-PS coordination check.
> CLI (SGSN Service Configuration Mode)
> network-sharing cs-ps-coordination
> default network-sharing cs-ps-coordination
> no network-sharing cs-ps-coordination
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ranap
> This command enables or disables the inclusion of the paging cause IEs and the modification of paging sources in various RANAP messages .
> CLI (RNC Service Configuration Mode)
> ranap { paging-cause-ie { all | background-data <value> | conversational-data <value> | gmm-signalling <value>| gs-signalling <value> | interactive-data <value> | sm-signalling <value> | sms-signalling <value> | streaming-data <value> } | { signalling-indication-ie { rab-assignment-request [ relocation-request ] | relocation-request [ rab-assignment-request ] } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ranap
> This command enables or disables the inclusion of the Signalling Indication IEs in various RANAP messages depending upon circumstances.
> CLI (RNC Service Configuration Mode)
> ranap { signalling-indication-ie { rab-assignment-request [ relocation-request ] | relocation-request [ rab-assignment-request ] }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> reset-resource
> This command enables the operator to control message length by configuring the number of IuConIDs sent in each RANAP Reset Resource message.
> CLI (DNS Client Configuration Mode)
> [ default ] reset-resource max-iuconid-per-msg <number>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> routing-context
> This command sets the routing context instructions included in the M3UA messages.
> CLI (SGSN PSP Configuration Mode)
> routing-context { discard-inbound | process-inbound } { insert-outbound | suppress-outbound }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sgsn-number
> This command defines the SGSN’s E.164 number to associate with the Gs Service.
> CLI (Gs Service Configuration Mode)
> sgsn-number <E.164_number>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> super-charger
> This command enables/disables the SGSN to work with a super-charged network.
> CLI (SGSN Operator Policy Configuration Mode)
> super-charger
> remove super-charger
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Modified Configuration Commands
> Common Commands - Modified in Release 8.0
> This section provides information on commands modified for Release 8.0.
> cca quota-state
> This command specifies the quota state of a subscriber for prepaid credit control service. The lower-bandwidth keyword was added to this command. When configured, this state matches the lower-bandwidth quota state of a rating group.
> CLI (Ruledef Configuration Mode)
> [ no ] cca quota-state operator { limit-reached | lower-bandwidth }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear subscriber sgsn-service
> New sgsn-service keyword clears all PDP contexts associated with a specific SGSN service. This keyword can be used with filtering keywords that are part of the clear subscriber command set. Using this command can trigger a network-initiated service request (paging) procedure.
> CLI (Exec Mode)
> clear subscriber sgsn-service name [filter_keyword]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clock
> Added following new time zones to this command:

> l | newzealand-auckland (GMT +12:00; Auckland, Wellington)

> l | newzealand-chatham (GMT +12:45; Chatham)

> CLI (Global Configuration Mode)
> clock timezone tz [ local ]
> no clock timezone
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> congestion-control policy
> The following congestion-control policies were added:

> l | mipv6ha-service

> l | pdif-service

> l | sgsn-service

> CLI (Global Configuration Mode)
> congestion-control policy {asngw-service | asnpc-service | cscf-service | ggsn-service | ha-service | lns-service | mipv6ha-service | pdif-service | pdsn-service | sgsn-service } action
> { drop | none | redirect | reject }
> Web Element Manager Path
> Click Monitoring | Congestion Control to view the pdif-service congestion control policy. The other policies are not supported at this time.
> diameter accounting
> The dictionary keyword was added to the diameter accounting command.
> CLI (AAA Server Group and Context Configuration Mode)
> diameter accounting { dictionary { aaa-custom1 | aaa-custom10 | aaa-custom2 | aaa-custom3 | aaa-custom4 | aaa-custom5 | aaa-custom6 | aaa-custom7 | aaa-custom8 | aaa-custom9 | nasreq | rf-plus } | endpoint endpoint_name | max-retries tries | max-transmissions transmissions | request-timeout duration | server host_name priority priority }
> [ no ] diameter accounting { endpoint | max-retries | max-transmissions | server host_name }
> [ default ] diameter accounting { dictionary | max-retries | max-transmissions | request-timeout }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter authentication
> The dictionary keyword was added to the diameter authentication command.
> CLI (AAA Server Group and Context Configuration Modes)
> diameter authentication { dictionary { aaa-custom1 | aaa-custom10 | aaa-custom2 | aaa-custom3 | aaa-custom4 | aaa-custom5 | aaa-custom6 | aaa-custom7 | aaa-custom8 | aaa-custom9 | nasreq } | endpoint endpoint_name | max-retries tries | max-transmissions transmissions | request-timeout duration | server host_name priority priority }
> [ no ] diameter authentication { endpoint | max-retries | max-transmissions | server host_name }
> [ default ] diameter authentication { dictionary | max-retries | max-transmissions | request-timeout }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter pending-timeout
> The after-expiry-try-secondary-host keyword was removed from the diameter pending-timeout command. This feature can now be managed using the retry-after-tx-expiry and go-offline-after-tx-expiry keywords available in the failure-handling command.
> CLI (Credit Control Configuration Mode)
> diameter pending-timeout duration
> default diameter pending-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> failure-handling
> The following keywords were added to this command:

> l | initial-request

> l | terminate-request

> l | update-request

> l | retry-after-tx-expiry

> l | go-offline-after-tx-expiry

> CLI (Credit Control Configuration Mode)
> failure-handling { initial-request | terminate-request | update-request } { continue [ go-offline-after-tx-expiry | retry-after-tx-expiry ] | retry-and-terminate [ retry-after-tx-expiry ] | terminate }
> default failure-handling [ initial-request | terminate-request | update-request ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> failure-handling
> This command configures the failure handling behavior for flow or protocol in Enhanced-Policy Decision Function (E-PDF). The any-error keyword was added to this command. This enables configuring failure handling behavior for those result-codes for which failure-handling behavior has not been specified.
> CLI (Policy Control Configuration Mode)
> failure-handling { continue | retry-and-terminate | terminate | diameter-result-code { any-error | integer result_code } ccfh { continue | retry-and-terminate | terminate } [ cc-request-type { initial-request | terminate-request | update-request } ] }
> no failure-handling diameter-result-code { any-error | integer result_code } [ cc-request-type { initial-request | terminate-request | update-request } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> file
> This command configures EDR file parameters. The following changes have been made to this command:

> l | The file-sequence-number rulebase-seq-num keyword was added to the command. This keyword enables generating file sequence numbers on a per rulebase basis with the rulebase name and format name.

> l | The num-records option was added to the file rotation keyword. This option enables limiting the file size by number of records.

> l | On ST40 chassis, the maximum amount of space available for storage of EDR/UDR files configured using the storage-limit keyword has changed.

> On ST40 chassis, the total storage limit is 536870912 bytes (512 MB). On ST16 chassis, the total storage limit is 268435456 bytes (256 MB). This limit is for UDR and EDR files combined.
> CLI (EDR Module Configuration Mode)
> file [ charging-service-name { include | omit } ] [ compression { gzip | none } ] [ current-prefix string ] [ delete-timeout seconds ] [ directory dir_name ] [ edr-format-name ] [ exclude-checksum-record ] [ field-separator { hyphen | omit | underscore } ] [ file-sequence-number rulebase-seq-num ] [ headers ] [ name file_name ] [ reset-indicator ] [ rotation [ num-records number | time seconds | volume bytes ] ] [ sequence-number { omit | padded | padded-six-length | unpadded } ] [ storage-limit limit ] [ time-stamp { expanded-format | rotated-format | unix-format } ] [ trailing-text string ] [ trap-on-file-delete ] [ xor-final-record ] +
> default file [ charging-service-name ] [ compression ] [ current-prefix ] [ delete-timeout ] [ directory ] [ edr-format-name ] [ field-separator ] [ file-sequence-number ] [ headers ] [ name ] [ reset-indicator ] [ rotation { num-records | time | volume } ] [ sequence-number ] [ storage-limit ] [ time-stamp ] [ trailing-text ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> file
> This command configures UDR file parameters. The following changes were made to this command:

> l | The file-sequence-number rulebase-seq-num keyword was added to the command. This keyword enables generating file sequence numbers on a per rulebase basis with the rulebase name and format name.

> l | The num-records option was added to the file rotation keyword. This option enables limiting the file size by number of records.

> l | On ST40 chassis, the maximum amount of space available for storage of EDR/UDR files configured using the storage-limit keyword has changed.

> On ST40 chassis, the total storage limit is 536870912 bytes (512 MB). On ST16 chassis, the total storage limit is 268435456 bytes (256 MB). This limit is for UDR and EDR files combined.
> CLI (UDR Module Configuration Mode)
> file [ charging-service-name { include | omit } ] [ compression { gzip | none } ] [ current-prefix string ] [ delete-timeout seconds ] [ directory dir_name ] [ exclude-checksum-record ] [ field-separator { hyphen | omit | underscore } ] [ file-sequence-number rulebase-seq-num ] [ headers ] [ name file_name ] [ reset-indicator ] [ rotation [ num-records number | time seconds | volume bytes ] ] [ sequence-number { omit | padded | padded-six-length | unpadded } ] [ storage-limit limit ] [ time-stamp { expanded-format | rotated-format | unix-format } ] [ trailing-text string ] [ trap-on-file-delete ] [ udr-seq-num ] [ xor-final-record ] +
> default file [ charging-service-name ] [ compression ] [ current-prefix ] [ delete-timeout ] [ directory ] [ field-separator ] [ file-sequence-number ] [ headers ] [ name ] [ reset-indicator ] [ rotation { num-records | time | volume } ] [ sequence-number ] [ storage-limit ] [ time-stamp ] [ trailing-text ] [ udr-seq-num ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> frame-relay
> This command defines the Frame Relay characteristics of the port - the word ‘channel’ was removed from the command.
> CLI (Channelized Port Configuration Mode)
> frame-relay path path_id { ds1 connects | e1 connects} [ timeslots | frame-relay [ intf-type intf_type [ lmi_type lmi_type ] ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> lawful-intercept
> Added new keyword all for this command to use with no keyword to clear all warrant information in one single command no lawful-intercept all:
> CLI (Exec Mode)
> no lawful-intercept [ all ] { [ imei imei_value ] [ imsi imsi_value ] [ ip-addr intercept_ip_addr ] [ msid ms_id ] [ msisdn msisdn_value ] [ username subscriber_name ] + } [ calltype call_type ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> logging filter runtime facility
> Additional facility options have been added to the logging filter command in the Global Configuration Mode. Those with an * (asterisk) are for the SGSN.

> l | *bssap+: Bssap+ logging facility

> l | *bssgp: BSSGP Protocol logging facility

> l | *cap: CAP Protocol logging facility

> l | chatconf: Voice Chat/Conference logging facility

> l | credit-control: Credit Control facility

> l | demuxmgr: Demux Manager API facility

> l | dgmbmgr: Diameter Gmb Application Manager logging facility

> l | dhcpv6: DHCPV6

> l | ds3mgr: DS3 Manager logging facility

> l | eap-ipsec: EAP

> l | ecs-css: ACSMGR <-> Session Manager Signalling Interface Logging facility

> l | * gmm: GMM Protocol logging facility

> l | * gprs-ns: GPRS-NS Protocol logging facility

> l | hdctrl: HD Controller logging facility

> l | igmp: IGMP

> l | ikev2: IKEv2

> l | ims-sh: HSS SH Service facility

> l | imsimgr: SGSN IMSI Manager facility

> l | ipsg: IP Service Gateway interface logging facility

> l | kvstore: KV Store facility

> l | * linkmgr: SGSN/SS7 Links Manager facility

> l | * llc: LLC Protocol logging facility

> l | * m3ua: M3UA Protocol logging facility

> l | * map: MAP Protocol logging facility

> l | megadiammgr: Megadiameter Manager (SLF Service)

> l | mmgr: Master Manager logging facility

> l | mobile-ipv6: Mobile IPv6 control logging facility

> l | * mtp3: MTP3 Protocol logging facility

> l | pdif: PDIF logging facility

> l | pmm-app: PMM application logging facility

> l | ptt: Voice push-to-talk logging facility

> l | push: VPNMGR CDR push logging facility

> l | * ranap: RANAP Protocol logging facility

> l | * sccp: SCCP Protocol logging facility

> l | * sctp: SCTP Protocol logging facility

> l | * sgsn-app: SGSN-APP interface logging facility

> l | * sgsn-gtpc: SGSNs GTP-C Protocol logging facility

> l | * sgsn-gtpu: SGSNs GTP-U Protocol logging facility

> l | * sgsn-misc: SGSN miscellaneous logging facility

> l | * sgsn-system: SGSNs System Components logging facility

> l | * sgsn-test: SGSN Tests logging facility

> l | * sgtpcmgr: SGSN GTPC Manager facility

> l | * sm-app: SM Protocol logging facility

> l | * sms: SMS Service logging facility

> l | * sndcp: SNDCP Protocol logging facility

> l | * sscfnni: SSCFNNI Protocol logging facility

> l | * sscop: SSCOP Protocol logging facility

> l | * taclcp: TAC Local Call Processing logging facility

> l | * tcap: TCAP Protocol logging facility

> l | ttg: TTG logging facility

> l | tucl: TUCL logging facility

> l | vim: Voice Instant Messaging logging facility

> l | vinfo: Voice Information logging facility

> l | vmgctrl: Virtual Media Gateway Controller logging facility

> l | vmgctxmgr: VMG Context Manager logging facility

> newcall policy
> The mipv6ha-service keyword was added to the syntax.
> CLI (Exec Mode)
> newcall policy mipv6ha-service { all | name service_name } reject
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ping
> The broadcast keyword was added to the syntax.
> CLI (Exec Mode)
> ping hostname broadcast
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bind
> Added new license-enabled keywords to configure traffic from the specified DHCP service bind address to use the MPLS labels. This support also provides the configuration to define nexthop gateway address:
> CLI (DHCP Service Configuration Mode)
> bind address ip_address [ nexthop-forwarding-address nexthop_ip_address
> [ mpls-label input in_mpls_label_value output out_mpls_label_value1
> [ out_mpls_label_value2 ]]]
> no bind address ip_address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - Modified in Release 8.1
> IMPORTANT: The commands documented in this section are only available in Release 8.1.
> accounting trigger
> New option “default” is added and the “start” and “stop” stop keywords have been deprecated (removed).
> CLI (Traffic Policy-Map Configuration Mode Commands)
> [ no | default ] accounting trigger { inactivity-timeout |
> interesting-traffic | intra-service-handoff }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> attribute
> This command specifies the order of fields to appear within an EDR. The following attributes were added to this command:

> l | sn-parent-protocol: Parent protocol of flow.

> l | sn-subscriber-nat-flow-ip: NAT IP address of NAT-enabled subscriber.

> l | sn-subscriber-nat-flow-port: NAT port number of NAT-enabled subscriber.

> CLI (EDR Format Configuration Mode)
> attribute attribute { [ format { MM/DD/YY-HH:MM:SS | MM/DD/YYYY-HH:MM:SS | YYYY/MM/DD-HH:MM:SS | YYYYMMDDHHMMSS | seconds } ] [ localtime ] | [ { ip | tcp } { bytes | pkts } { downlink | uplink } ] priority priority }
> no attribute attribute [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> attribute
> This command specifies the order of fields to appear within an UDR. The following attribute was added to this command:

> l | sn-subscriber-nat-flow-ip: NAT IP address of NAT-enabled subscriber.

> CLI (UDR Format Configuration Mode)
> attribute attribute { [ format { MM/DD/YY-HH:MM:SS | MM/DD/YYYY-HH:MM:SS | YYYY/MM/DD-HH:MM:SS | YYYYMMDDHHMMSS | seconds } [ localtime ] | [ { bytes | pkts } { downlink | uplink } ] ] priority priority }
> no attribute attribute [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bcmcs
> This command has been modified by adding the optional keyword encrypted so the password grppasswd can be sent either encrypted or clear.
> CLI (PDSN-Service Config Mode)
> [ encrypted ] grppasswd group_passwd
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cdr
> This command configures the CDR file transfer parameters. The transfer-mode keyword was enhanced to support EDR/UDR push via SPIO. Previously, the push was support only via LC.
> CLI (EDR Module Configuration Mode & UDR Module Configuration Mode)
> cdr [ [ push-interval value ] [ remove-file-after-transfer ] [ transfer-mode { pull | push primary { encrypted-url enc_url | url url } [ via local-context ] [ secondary { encrypted-secondary-url enc_sec_url | url sec_url } ] } ] + | use-harddisk ]
> no cdr [ remove-file-after-transfer | use harddisk ] +
> default cdr [ push-interval | remove-file-after-transfer | transfer-mode [ push via ] | use harddisk ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear crypto
> This command has been modified to clear all IKEv2 statistics for the current context, or to clear statistics based on service ip address or service name.
> CLI (Exec Mode)
> clear crypto statistics { ikev2 [ service-ip-address ip-address | service-name name ] }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> framing
> The ability to identify the path-type (either E1 or DS1/T1) has been added to the framing command for use with the CLC2 SONET or SDH configuration.
> CLI (Channelized Port Configuration Mode)
> framing { ethernet | sdh [ ds1 | e1 ] | sonet [ ds1 | e1 ] | unspecified } [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> iiop port
> The no keyword has been added to the iiop port command.
> CLI (ORBEM Config mode)
> no iiop port
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip access-list
> This command enables creating/configuring/deleting an IP Access List in the current context. The access list name to be specified has been restricted to be an alpha and/or numeric string of 1 through 47 characters in length. In StarOS 8.0, it can be an alpha and/or numeric string of 1 through 79 characters in length.
> CLI (Context Configuration Mode)
> ip access-list name
> [ default | no ] ip access-list name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip pool
> The nat-realm keyword was added to this command. This enables to designate an IP address pool as a Firewall Network Address Translation (NAT) realm pool.
> CLI (Context Configuration Mode)
> ip pool name { ip_address subnet_mask | ip_addr_mask_combo |
> range start_address end_address } [ private [ priority ] |
> public [ priority ] | static ] [ tag { none | pdif-setup-addr } ] [ address-hold-timer seconds | alert-threshold [ group-available | pool-free | pool-hold | pool-release | pool-used ] low_thresh [ clear high_thresh ] ] [ group-name group_name ] [ include-nw-bcast ] [ nat priority ] [ nat-realm users-per-nat-ip-address users [ on-demand [ address-hold-timer address_hold_timer ] ] ] [ nexthop-forwarding-address ip_address [ overlap vlanid vlan_id ] [ nw-reachability server server_name ] [ respond-icmp-echo ip_address ] [ resource ] [ send-icmp-dest-unreachable ] [ explicit-route-advertise ] [ srp-activate ] [ suppress-switchover-arp ] [ unicast-gratuitous-arp-address ip_address ] [ policy allow-static-allocation ]
> no ip pool name [ tag { none | pdif-setup-addr } ] [ address-hold-timer | alert-threshold [ group-available | pool-free | pool-hold | pool-release | pool-used ] ] [ group-name ] [ include-nw-bcast ] [ nexthop-forwarding-address ] [ nw-reachability server ] [respond-icmp-echo ip_address ] [ send-icmp-dest-unreachable ] [ explicit-route-advertise ] [ srp-activate ] [ suppress-switchover-arps ] [ unicast-gratuitous-arp-address ] [ policy allow-static-allocation ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> mobile-ip send
> This command includes two new options for the send keyword:

> l | accounting-correlation-info

> l | imsi

> CLI (Subscriber Config Mode)
> [ no ] mobile-ip send { accounting-correlation-info | dns-address | imsi | terminal-verification }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> port-switch-on-l3-fail
> This command has been extended to support ipv6 addresses
> CLI (Ethernet Interface Config Mode)
> port-switch-on-L3-fail address { ip_address | ipv6_address }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius accounting max-outstanding
> The maximum number of outstanding messages a single AAA manager instance will queue has been set to 4000.
> CLI (AAA Group Config Mode & Context Config Mode)
> radius accounting max-outstanding msgs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius charging accounting server
> The maximum number of outstanding messages that may be allowed to the server has been set to 4000.
> CLI (AAA Group Config Mode & Context Config Mode)
> radius charging accounting server ip_address [ encrypted ] key string max msgs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius charging max-outstanding
> The maximum number of outstanding messages a single AAA manager instance will queue has been set to 4000.
> CLI (AAA Group Config Mode & Context Config Mode)
> radius charging max-outstanding msgs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius charging server
> The maximum number of outstanding messages that may be allowed to the server has been set to 4000.
> CLI (AAA Group Config Mode & Context Config Mode)
> radius charging server ip_address [ encrypted ] key string max msgs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius max-outstanding
> The maximum number of outstanding messages a single AAA manager instance will queue has been set to 4000.
> CLI (AAA Group Config Mode & Context Config Mode)
> radius max-outstanding msgs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius server
> The maximum number of outstanding messages that may be allowed to the server has been set to 4000.
> CLI (AAA Group Config Mode & Context Config Mode)
> radius server ip_address [ encrypted ] key string max msgs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> service-type
> This command configures the type of service (Frame Relay or pwe3-cse) to be employed on the CLC or CLC2 (channelized line cards).
> CLI (Card Configuration Mode)
> service-type { frame-relay | pwe3-cesopsn | unspecified }
> default service-type
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show srp
> New option “call-loss statistics” is added to show history of calls lost during switchover.
> CLI (Excec Mode Commands)
> show srp { call-loss statistics | checkpoint statistics [verbose ] | info | statistics } | [ grep grep_options | more ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Common Commands - Modified in Release 8.3
> IMPORTANT: This section provides information on commands modified in Release 8.3.
> attribute
> This command specifies the order of fields to appear within an EDR. The following attributes were added to this command:

> l | sn-nat-binding-timer: Port chunk hold timer.

> l | sn-nat-gmt-offset: GMT offset of the node generating NAT bind record.

> l | sn-nat-ip: NAT IP address of the port chunk.

> l | sn-nat-last-activity-time-gmt: The time when the last flow in a specific NAT set of flows was seen.

> l | sn-nat-port-block-end: Last port number of the port chunk.

> l | sn-nat-port-block-start: Starting port number of the port chunk.

> l | sn-nat-port-chunk-alloc-dealloc-flag: Indicates whether the port chunk is allocated or released.

> l | sn-nat-port-chunk-alloc-time-gmt: Indicates when the port chunk was allocated.

> l | sn-nat-port-chunk-dealloc-time-gmt: Indicates when the port chunk was released.

> l | sn-nat-realm-name: Name of the NAT realm.

> l | sn-nat-subscribers-per-ip-address: Subscriber(s) per NAT IP address.

> CLI (EDR Format Configuration Mode)
> attribute attribute { [ format { MM/DD/YY-HH:MM:SS | MM/DD/YYYY-HH:MM:SS | YYYY/MM/DD-HH:MM:SS | YYYYMMDDHHMMSS | seconds } ] [ localtime ] | [ { ip | tcp } { bytes | pkts } { downlink | uplink } ] priority priority }
> no attribute attribute [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip pool
> This command enables adding, updating, or deleting an IP address pool in the current context. The following keywords and several options were added to this command:

> l | nat-one-to-one: This keyword enables configuring one-to-one NAT realm pool.

> l | napt-users-per-ip-address: This keyword enables configuring the number of users sharing a single NAT IP address for a many-to-one NAT realm.

> The following keyword was removed from this command:

> l | nat-realm

> CLI (Context Configuration Mode)
> ip pool name { ip_address subnet_mask | ip_addr_mask_combo | range start_ip_address end_ip_address } [ private [ priority ] | public [ priority ] | static ] [ tag { none | pdif-setup-addr } ] [ address-hold-timer seconds | alert-threshold [ group-available | pool-free | pool-hold | pool-release | pool-used ] low_thresh [ clear high_thresh ] ] [ group-name group_name ] [ include-nw-bcast ] [ nat priority ] [ nexthop-forwarding-address ip_address [ overlap vlanid vlan_id ] [ nw-reachability server server_name ] [ respond-icmp-echo ip_address ] [ resource ] [ send-icmp-dest-unreachable ] [ explicit-route-advertise ] [ srp-activate ] [ suppress-switchover-arp ] [ unicast-gratuitous-arp-address ip_address ] [ policy allow-static-allocation ] [ nat-one-to-one [ [ alert-threshold [ { pool-free | pool-hold | pool-release | pool-used } low_thresh [ clear high_thresh ] + ] [ nat-binding-timer binding_timer ] [ on-demand ] [ send-nat-binding-update ] + ] | napt-users-per-ip-address users [ [ alert-threshold [ { pool-free | pool-hold | pool-release | pool-used } low_thresh [ clear high_thresh ] + ] [ max-chunks-per-user chunks ] [ nat-binding-timer timer ] [ on-demand ] [ port-chunk-size size ] [ port-chunk-threshold chunk_threshold ] [ send-nat-binding-update ] + ]
> no ip pool name [ tag { none | pdif-setup-addr } ] [ address-hold-timer | alert-threshold [ group-available | pool-free | pool-hold | pool-release | pool-used ] ] [ group-name ] [ include-nw-bcast ] [ nexthop-forwarding-address ] [ nw-reachability server ] [ respond-icmp-echo ip_address ] [ send-icmp-dest-unreachable ] [ explicit-route-advertise ] [ send-nat-binding-update ] [ srp-activate ] [ suppress-switchover-arps ] [ unicast-gratuitous-arp-address ] [ policy allow-static-allocation ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> readdress server commands in inbound IPv4 ACLs
> Prior to Release 8.3, for packets received from the packet data network destined for a subscriber's UE, the system applied logic to reset the source address of a packet to the original destination address of the input packet before applying the outbound ACL (access control list). In Release 8.3 and higher, the system reverses the order and applies the outbound ACL before resetting the source address. This change impacts all current readdress server rules in inbound IPv4 ACLs.
> After upgrading to Release 8.3, for every readdress server rule in an inbound IPv4 ACL, customers must now add a permit rule to an outbound ACL that explicitly permits packets from the readdress rule's redirect address and port number. If customers omit this permit rule, the system will reject all packets destined for the subscriber's UE from the readdress rule's redirect address and port number.
> deny/permit (by TCP/UDP packets)
> This command was modified to include the range option for PDIF Release 8.3.
> CLI (Access Control List Configuration Mode)
> permit { tcp | udp } [ range start_port end_port ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold cpu-orbs-warn
> The default is changed for this command. The default is now 50.
> CLI (Global Config Mode Commands)
> threshold cpu-orbs-warn high_thresh [ clear low_thresh ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> threshold cpu-orbs-crit
> The default is changed for this command. The default is now 60.
> CLI (Global Config Mode Commands)
> threshold cpu-orbs-crit high_thresh [ clear low_thresh ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - Modified in Release 8.0
> This section provides information on CF commands modified in Release 8.0.
> analyze
> The cat_string variable in category keyword in this command is now changed to provide explicit category name to configure analysis priority.
> CLI (CFP Configuration Mode)
> analyze priority priority { all | category cat_string } action { allow | content-insertion content_string | discard | redirect-url url | terminate-flow }
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Services
> analyze
> This command specifies the action to take for the indicated result after content filtering analysis. An optional keyword “edr edr_format_name” was added to this command for EDR generation based on content category and action.
> CLI (CFP Configuration Mode)
> analyze priority priority { all | category cat_string } action { allow | content-insertion content_string | discard | redirect-url url | terminate-flow } [edr edr_format_name]
> edr_format_name is the name of a pre-defined EDR file format name in the EDR Format Configuration Mode.
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Services
> CF Commands - Modified in Release 8.1
> This section provides information on CF commands modified in Release 8.1.
> analyze
> This command specifies the action to take for the indicated result after content filtering analysis. The following keywords were added to this command:

> l | www-reply-code-and-terminate-flow

> l | x-category

> The following category options were added to the category keyword:

> l | ENERGY

> l | STREAM

> l | VOIP

> The following category options were removed from the category keyword:

> l | ADV

> l | AUCT

> l | CLEAN

> l | CPORN

> l | P2P

> l | PHISH

> l | RADIO

> l | SFTWRE

> l | SPYWRE

> l | SUSP

> CLI (Content Filtering Policy Configuration Mode)
> analyze priority priority { all | category cat_string | x-category string } action { allow | content-insert content_string | discard | redirect-url url | terminate-flow | www-reply-code-and-terminate-flow reply_code } [ edr edr_format_name ]
> no analyze priority priority
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Services
> content-filtering
> This command enables/disables the Category Policy Identifier for Content Filtering support, and enters the Content Filtering Policy Configuration Mode. The description option allows the operator to provide a description for the CF Category Policy ID. Both the description keyword and the argument desc_string are now optional. This enables adding and removing the descriptions.
> CLI (ACS Configuration Mode)
> content-filtering category policy-id cf_policy_id [ description [ desc_string ] ] [ -noconfirm ]
> no content-filtering category policy-id cf_policy_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> content-filtering category policy-id
> This command configures the Content Filtering Category Policy Identifier for Policy-based Content Filtering support in a rulebase. Now, while removing the configured category policy from the rulebase, optionally the policy ID can be specified. If the specified policy ID is invalid, or is not configured in the rulebase, an error message is displayed. If no policy ID is specified, whatever policy is configured, if any, is removed from the rulebase.
> CLI (Rulebase Configuration Mode)
> content-filtering category policy-id cf_policy_id
> no content-filtering category policy-id [ cf_policy_id ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> timeout action
> This command specifies the actions when the content filtering analysis results are not available to analyze. The www-reply-code-and-terminate-flow keyword was added to this command.
> CLI (Content Filtering Policy Configuration Mode)
> timeout action { allow | content-insert content_string | discard | redirect-url url | terminate-flow | www-reply-code-and-terminate-flow reply_code } [ edr edr_format_name ]
> default timeout action [ edr edr_format_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 8.0
> This section provides information on ECS commands in Release 8.0.
> action
> This command assigns an action priority to a rule definition. The group-of-ruledefs keyword was added to this command. This enables assigning a group of rule definitions to the rulebase.
> CLI (Rulebase Configuration Mode)
> action priority action_priority { [ dynamic-only | static-and-dynamic ] { ruledef name | group-of-ruledefs name } charging-action name [ description desc ] }
> no action-priority action_priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer imsi
> This command defines a rule definition to analyze and charge user traffic using an International Mobile Station Identification number (IMSI) in bearer flow. The { !range | range } imsi-pool imsi_pool } option was added to this command. This enables the IMSI number to be selected from a range configured in an IMSI pool.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer imsi { operator msid | { !range | range } imsi-pool imsi_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> charge-volume
> This command configures the volume counter for eG-CDR and DCCA charging calculation. The packet-length keyword was added to this command. This enables to configure charge volume for packet length.
> CLI (Charging Action Configuration Mode)
> charge-volume { protocol { bytes | packet-length | packets } [ downlink | uplink ] | constant value }
> [ no | default ] charge-volume
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> charging-rule-optimization
> This command configures the amount of internal optimization for improved performance when evaluating each instance of the action CLI command. There is no external change to this command, only that now “www url =” kind of rules under the ambit of charging-rule-optimization in rulebase. Until now, setting “charging-rule-optimization” to “medium” or “high” would only optimize the “starts-with” and “contains” rules, not the “=” rules. Now the “=” rules are also optimized.
> CLI (Rulebase Configuration Mode)
> charging-rule-optimization { low | medium | high }
> default charging-rule-optimization
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> dictionary
> This command specifies the dictionary to use for requests to the server(s) in a Content Filtering Server Group. The custom2 keyword was added to this command.
> CLI (Content Filtering Server Group Configuration Mode)
> dictionary { custom1 | custom2 | standard }
> [ default | no ] dictionary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow action
> This command specifies the actions for packets that match a rule definition. The following changes were made to this command:

> l | The discard keyword now includes the downlink and uplink options. This enables selecting specific packets.

> l | The readdress keyword was added to this command. This enables specifying a re-address server for the charging action.

> CLI (Charging Action Configuration Mode)
> flow action { conditional user-agent end-token end_token_name | discard [ downlink | uplink ] | readdress { server ip_address [ port port_number ] | port port_number } | redirect-url url [ clear-quota-retry-timer ] | terminate-flow }
> no flow action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow limit-across-applications
> The non-tcp limit and tcp limit keywords were added to this command. This command can now also be used to limit the total number of flows per Subscriber/APN sent to a rulebase based on the protocol type.
> CLI (Rulebase Configuration Mode)
> flow limit-across-applications { limit | non-tcp limit | tcp limit }
> [ no ] flow limit-across-applications [ non-tcp | tcp ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow limit-for-bandwidth
> This command enables and configures bandwidth limits for Session Control functionality to the subscriber. The exceed-action keyword is now optional.
> CLI (Charging Action Configuration Mode)
> [ no | default ] flow limit-for-bandwidth direction { downlink | uplink } peak-data-rate bps peak-burst-size bytes violate-action { discard | lower-ip-precedence } [ committed-data-rate bps committed-burst-size bytes [ exceed-action { discard | lower-ip-precedence } ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip dst-address
> This command defines rule definition to analyze and charge user traffic based on Internet Protocol (IP) destination address. The “{ !range | range } host-pool host_pool” option was added to this command. This enables the IP destination address to be selected from a range configured in a host pool.
> CLI (Ruledef Configuration Mode)
> [ no ] ip dst-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip server-ip-address
> This command defines rule definition to analyze and charge user traffic matching the Internet Protocol (IP) address of the destination, i.e. from the subscriber, of the connection. The { !range | range } host-pool host_pool option was added to this command. This enables the IP address to be selected from a range configured in a host pool.
> CLI (Ruledef Configuration Mode)
> [ no ] ip server-ip-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip src-address
> This command defines rule definition to analyze and charge user traffic based on Internet Protocol (IP) source address. The { !range | range } host-pool host_pool option was added to this command. This enables the IP source address to be selected from a range configured in a host pool.
> CLI (Ruledef Configuration Mode)
> [ no ] ip src-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip subscriber-ip-address
> This command defines rule definition to analyze and charge user traffic matching the Internet Protocol (IP) address of the subscriber (either source address or destination address). The { !range | range } host-pool host_pool option was added to this command. This enables the IP address to be selected from a range configured in a host pool.
> CLI (Ruledef Configuration Mode)
> [ no ] ip subscriber-ip-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip tos
> This command sets the IP Type of Service (ToS) octets being used in the charging action. The option to allow the IP TOS to be set using a numeric value was added to this command.
> CLI (Charging Action Configuration Mode)
> ip tos { tos_value | af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef } [ uplink | downlink ]
> no ip tos [ uplink | downlink ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> mms bcc
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms bcc [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms cc
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms cc [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms content location
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms content location[ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms content type
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms content type [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms from
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms from [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms message-id
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms message-id [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms subject
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms subject [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> mms to
> The “case-sensitive” keyword was added to this command.
> CLI (Ruledef Configuration Mode)
> [ no ] mms to [ case-sensitive ] operator string
> Web Element Manager Path
> Click Configuration | Active Charging | Active Charging Service and click Add or Modify.
> p2p protocol
> This command configures the system to detect specific P2P protocols for charging purposes. The following P2P protocol options have been added to this command:

> l | applejuice

> l | ares

> l | directconnect

> l | feidian

> l | filetopia

> l | gadugadu

> l | imesh

> l | manolito

> l | mute

> l | pando

> l | pplive

> l | ppstream

> l | qq

> l | qqlive

> l | skinny

> l | sopcast

> l | soulseek

> l | zatoo

> CLI (Ruledef Configuration Mode)
> [ no ] p2p protocol = { applejuice | ares | bittorrent | directconnect | edonkey | fasttrack | feidian | filetopia | gadugadu | gnutella | imesh | jabber | manolito | msn | mute | orb | pando | pplive | ppstream | qq | qqlive | skinny | skype | slingbox | sopcast | soulseek | winny | yahoo | zattoo }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> p2p detection-protocol
> This command configures the system to detect specific peer-to-peer (P2P) protocols. The following P2P protocol options have been added to this command:

> l | applejuice

> l | ares

> l | directconnect

> l | feidian

> l | filetopia

> l | gadugadu

> l | imesh

> l | manolito

> l | mute

> l | pando

> l | pplive

> l | ppstream

> l | qq

> l | qqlive

> l | skinny

> l | sopcast

> l | soulseek

> l | zatoo

> CLI (Active Charging Configuration Mode)
> [ no ] p2p-detection protocol [ all | applejuice | ares | bittorrent | directconnect | edonkey | fasttrack | feidian | filetopia | gadugadu | gnutella | imesh | jabber | manolito | msn | mute | orb | pando | pplive | ppstream | qq | qqlive | skinny | skype | slingbox | sopcast | soulseek | winny | yahoo | zattoo ]+
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ruledef
> This command creates a rule definition for the Active Charging Service, and enters ACS Ruledef Configuration Mode. The “description string” keyword was removed from this command.
> CLI (ACS Configuration Mode)
> [ no ] ruledef ruledef_name [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rule-variable
> This command configures the event rule variable for EDR file format attribute. The following rules were added to this command:

> l | http protocol: user-agent

> l | bearer protocol: ggsn-address

> CLI (EDR Format Configuration Mode)
> rule-variable protocol rule priority priority [ in-quotes ]
> no rule-variable protocol rule [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tcp either-port
> This command defines rule definition to analyze and charge user traffic using either (destination or source) TCP port. The { !range | range } port-map port_map option was added to this command. This enables the port number to be selected from a range configured in a port map.
> CLI (Ruledef Configuration Mode)
> [ no ] tcp either-port { operator port_number | { !range | range } { start_range to end_range | port-map port_map } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tcp dst-port
> This command defines rule definition to analyze and charge user traffic based on destination Transmission Control Protocol (TCP) port. The { !range | range } port-map port_map option was added to this command. This enables the port number to be selected from a range configured in a port map.
> CLI (Ruledef Configuration Mode)
> [ no ] tcp dst-port { operator port_number | { !range | range } { start_range to end_range | port-map port_map } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tcp src-port
> This command defines rule definition to analyze and charge user traffic based on source Transmission Control Protocol (TCP) port. The { !range | range } port-map port_map option was added to this command. This enables the port number to be selected from a range configured in a port map.
> CLI (Ruledef Configuration Mode)
> [ no ] tcp src-port { operator port_number | { !range | range } { start_range to end_range | port-map port_map } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> udp dst-port
> This command defines rule definition to analyze and charge user traffic based on destination User Datagram Protocol (UDP) port number. The { !range | range } port-map port_map option was added to this command. This enables the port number to be selected from a range configured in a port map.
> CLI (Ruledef Configuration Mode)
> [ no ] udp dst-port { operator port_number | { !range | range } { start_range to end_range | port-map port_map } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> udp either-port
> This command defines rule definition to analyze and charge user traffic using either (destination or source) User Datagram Protocol (UDP) port. The { !range | range } port-map port_map option was added to this command. This enables the port number to be selected from a range configured in a port map.
> CLI (Ruledef Configuration Mode)
> [ no ] udp either-port { operator port_number | { !range | range } { start_range to end_range | port-map port_map } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> udp src-port
> This command defines rule definition to analyze and charge user traffic based on source User Datagram Protocol (UDP) port number. The { !range | range } port-map port_map option was added to this command. This enables the port number to be selected from a range configured in a port map.
> CLI (Ruledef Configuration Mode)
> [ no ] udp src-port { operator port_number | { !range | range } { start_range to end_range | port-map port_map } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> license
> Configures the session license key.
> CLI (Global Configuration Mode Commands)
> license key key_value [ -force ] session-limit
> no license key key_value [ -force ] session-limit
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 8.1
> IMPORTANT: The commands documented in this section have all been modified for Release 8.1.
> action priority
> This command configures the action priority for a ruledef/group-of-ruledefs in the rulebase. The following keywords were added to this command:

> l | timedef timedef_name: Associates the specified time definition with the ruledef/group-of-ruledefs. Timedefs enable activation/deactivation of ruledefs/groups-of-ruledefs such that they are available for rule matching only when they are active.

> CLI (Rulebase Configuration Mode)
> action priority action_priority { [ dynamic-only | static-and-dynamic | timedef timedef_name ] { group-of-ruledefs group_name | ruledef ruledef_name } charging-action charging_action_name [ monitoring-key monitoring_key ] [ description description ] }
> no action priority action_priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> attribute
> This command specifies the order of fields to appear within an EDR. The following new attributes were added to this command:

> l | transaction-downlink-bytes

> l | transaction-downlink-packets

> l | transaction-uplink-bytes

> l | transaction-uplink-packets

> Also, a new closure reason for EDRs has been added: “ACS_EDR_TRANSACTION_COMPLETE_EVENT”. So “attribute sn-closure-reason” in EDRs will populate value 12 (corresponding to closure-reason “ACS_EDR_TRANSACTION_COMPLETE_EVENT”) in EDRs.
> CLI (Rulebase Configuration Mode)
> attribute attribute { [ format { MM/DD/YY-HH:MM:SS | MM/DD/YYYY-HH:MM:SS | YYYY/MM/DD-HH:MM:SS | YYYYMMDDHHMMSS | seconds } ] [ localtime ] | [ { ip | tcp } { bytes | pkts } { downlink | uplink } ] priority priority }
> no attribute attribute [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> credit-control
> This command enables/disables Prepaid Credit Control Configuration mode. The group keyword was added to this command. This enables configuring credit control groups. This enables applying different credit control configurations (DCCA dictionary, failure-handling, session-failover, Diameter endpoint selection, etc.) to different subscribers on the same system.
> CLI (Active Charging Configuration Mode)
> [ no ] credit-control [ group group_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow action
> This command specifies the actions for packets that match a rule definition. The terminate-session keyword was added to this command. This enables specifying the flow action to terminate session. When a rule pointing to a charging action configured with the terminate-session keyword is hit, then the corresponding session will be terminated.
> CLI (Charging Action Configuration Mode)
> flow action { conditional user-agent end-token end_token_name | discard [ downlink | uplink ] | readdress { server ip_address [ port port_number ] | port port_number } | redirect-url url [ clear-quota-retry-timer ] | terminate-flow | terminate-session }
> no flow action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow action redirect-url
> This command specifies the redirection of URL for packets that matches a rule definition. This command also specifies the redirect-URL action on packet and flow for Session Control functionality. This CLI can now be used to redirect SIP requests as well.
> CLI (Charging Action Configuration Mode)
> flow action redirect-url url/%3furl=dynamic_field [ clear-quota-retry-timer ]
> { default | no } flow action redirect-url
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> flow limit-for-bandwidth
> This command enables and configures bandwidth limits for Session Control functionality to the subscriber. Uplink and downlink limits are configured separately. The id keyword was added to this command. This enables configuring identifier for bandwidth limiting.
> CLI (Charging Action Configuration Mode)
> flow limit-for-bandwidth { { direction { downlink | uplink } peak-data-rate bps peak-burst-size bytes violate-action { discard | lower-ip-precedence } [ committed-data-rate bps committed-burst-size bytes [ exceed-action { discard | lower-ip-precedence } ] ] } | { id id } }
> { default | no } flow limit-for-bandwidth { direction { downlink | uplink } | id }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> icap server
> This command adds an Internet Content Adaptation Protocol (ICAP) server configuration to a Content Filtering Server Group. The priority keyword was added to this command. This enables specifying the priority of an ICAP server in a Content Filtering Server Group.
> IMPORTANT: The maximum outstanding request per ICAP connection configured using the optional max <max_msgs> keyword is limited to one. Therefore, other values configured using the max keyword will be ignored.
> CLI (Content Filtering Server Group Configuration Mode)
> icap server ip_address [ port port_number ] [ max msgs ] [ priority priority ]
> no icap server ip_address [ port port_number ] [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> insert
> This command configures the x-header fields to be inserted in HTTP GET and POST request packets.
> The following keywords were added to this command:

> l | customer-id

> l | charging-characteristics

> l | imei

> The following keywords were moved from under “insert xheader_field_name variable bearer” to under “insert xheader_field_name variable bearer 3gpp”:

> l | imsi

> l | sgsn-address

> CLI (x-header Format Configuration Mode)
> insert xheader_field_name { string-constant xheader_field_value | variable { bearer { 3gpp { charging-characteristics | charging-id | imei | imsi | sgsn-address } | customer-id | ggsn-address | radius-calling-station-id | sn-rulebase | subscriber-ip-address } | http { host | url } }
> no insert xheader_field_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip protocol
> This command defines a rule definition to analyze user traffic based on the protocol being transported by IP packets. The following keywords were added to this command:

> l | protocol: Enables specifying a protocol by its name.

> l | operator protocol_assignment: Enables specifying a protocol lesser than or equal to, or greater than or equal to a protocol assignment number.

> CLI (Ruledef Configuration Mode)
> [ no ] ip protocol { { operator { protocol | protocol_assignment } } | { operator protocol_assignment } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip tos
> This command sets the IP Type of Service (ToS) octets being used in the charging action. The keyword to set IP ToS using a numeric value was modified to lower-bits tos_value.
> CLI (Charging Action Configuration Mode)
> ip tos { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef | lower-bits tos_value } [ uplink | downlink ]
> no ip tos [ uplink | downlink ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ping6
> This command configures IPv6 ping options. A new keyword interface name has been added that specifies the originating source interface name.
> CLI (Exec Mode Commands)
> ping6 interface name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> p2p protocol
> This command configures the system to detect specific P2P protocols for charging purposes. The following P2P protocol options have been added to this command in Release 8.1:

> l | ddlink

> l | halflife2

> l | hamachivpn

> l | irc

> l | oscar

> l | popo

> l | steam

> l | tvants

> l | tvuplayer

> l | uusee

> l | vpnx

> l | vtun

> l | winmx

> l | wofwarcraft

> l | xbox

> CLI (Ruledef Configuration Mode)
> [ no ] p2p protocol = { applejuice | ares | bittorrent | ddlink | directconnect | edonkey | fasttrack | feidian | filetopia | gadugadu | gnutella | halflife2 | hamachivpn | imesh | irc | jabber | manolito | msn | mute | orb | oscar | pando | popo | pplive | ppstream | qq | qqlive | skinny | skype | slingbox | sopcast | soulseek | steam | tvants | tvuplayer | uusee | vpnx | vtun | winmx | winny | wofwarcraft | xbox | yahoo | zattoo }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> p2p detection-protocol
> This command configures the system to detect specific peer-to-peer (P2P) protocols. The following P2P protocol options have been added to this command in Release 8.1:

> l | ddlink

> l | halflife2

> l | hamachivpn

> l | irc

> l | oscar

> l | popo

> l | steam

> l | tvants

> l | tvuplayer

> l | uusee

> l | vpnx

> l | vtun

> l | winmx

> l | wofwarcraft

> l | xbox

> CLI (Active Charging Configuration Mode)
> [ no ] p2p-detection protocol [ all | applejuice | ares | bittorrent | ddlink | directconnect | edonkey | fasttrack | feidian | filetopia | gadugadu | gnutella | halflife2 | hamachivpn | imesh | irc | jabber | manolito | msn | mute | orb | oscar | pando | popo | pplive | ppstream | qq | qqlive | skinny | skype | slingbox | sopcast | soulseek | steam | tvants | tvuplayer | uusee | vpnx | vtun | winmx | winny | wofwarcraft | xbox | yahoo | zattoo ]+
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> require active-charging
> This command enables/disables Enhanced Charging Service with or without Category-based Content Filtering application. The following changes were made to this command:

> l | The optimized-mode keyword was added to this command. This enables ECS in Optimized mode, wherein enhanced charging facilities run as part of the SessMgr.

> IMPORTANT: In Release 8.1, Enhanced Charging Service must be enabled in Optimized mode.
> IMPORTANT: By default, on installing Release 8.1, the system comes up with ECS in non-optimized mode. To change to the optimized mode, the require active-charging optimized-mode command must be saved to the configuration from the CLI, and the system rebooted for the change to take effect.
> If the enhanced-charging mode is changed from the default (non-optimized) mode to the Optimized mode, or vice-versa, the system must be rebooted for the change to take effect.

> l | The isolated-mode keyword was removed from this command. This keyword is still supported on Release 8.0 and earlier, wherein it enables ECS, and separates ECS-related resources from other sub-system resource sharing.

> CLI (Global Configuration Mode)
> require active-charging [ content-filtering category ] [ optimized-mode ]
> no require active-charging
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rule-variable
> This command configures the event rule variable for EDR file format attribute. The following fields were added under “bearer 3gpp” rule:

> l | imei

> l | rat-type

> l | sgsn-address

> l | user-location-information

> CLI (EDR Format Configuration Mode)
> rule-variable protocol rule priority priority [ in-quotes ]
> no rule-variable protocol rule [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 8.3
> IMPORTANT: The commands documented in this section have all been modified for Release 8.3.
> file sequence-number
> This command configures EDR file parameters. The length option was added to the sequence-number keyword, this enables to specify the file sequence number length.
> CLI (EDR Module Configuration Mode)
> file [ charging-service-name { include | omit } ] [ compression { gzip | none } ] [ current-prefix string ] [ delete-timeout seconds ] [ directory dir_name ] [ edr-format-name ] [ exclude-checksum-record ] [ field-separator { hyphen | omit | underscore } ] [ file-sequence-number rulebase-seq-num ] [ headers ] [ name file_name ] [ reset-indicator ] [ rotation [ num-records number | time seconds | volume bytes ] ] [ sequence-number { length length | omit | padded | padded-six-length | unpadded } ] [ storage-limit limit ][ time-stamp { expanded-format | rotated-format | unix-format } ] [ trailing-text string ] [ trap-on-file-delete ] [ xor-final-record ] +
> default file [ charging-service-name ] [ compression ] [ current-prefix ] [ delete-timeout ] [ directory ] [ edr-format-name ] [ field-separator ] [ file-sequence-number ] [ headers ] [ name ] [ reset-indicator ] [ rotation { num-records | time | volume } ] [ sequence-number ] [ storage-limit ][ time-stamp ] [ trailing-text ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> require active-charging
> This command enables/disables Enhanced Charging Service with or without Category-based Content Filtering application. The optimized-mode keyword was obsoleted. With or without this keyword ECS is always enabled in Optimized mode.
> CLI (Global Configuration Mode)
> require active-charging [ content-filtering category ] [ optimized-mode ]
> no require active-charging
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rule-application
> This command specifies the application rule for a rule definition. The post-processing keyword was added to this command, this enables to specify rule definitions for post-processing purposes.
> CLI (Ruledef Configuration Mode)
> rule-application { charging | post-processing | routing }
> no rule-application
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Modified in Release 8.0
> This section provides information on commands modified for Release 8.0.
> firewall policy
> This command enables/disables Stateful Firewall support for the subscriber.
> CLI (APN Configuration Mode)
> firewall policy firewall-required
> [ default | no ] firewall policy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall policy
> This command enables/disables Stateful Firewall support for the APN.
> CLI (Subscriber Configuration Mode)
> firewall policy firewall-required
> [ default | no ] firewall policy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Modified in Release 8.1
> IMPORTANT: The commands documented in this section have been modified in Release 8.1.
> firewall dos-protection
> This command configures firewall protection from Denial-of-Service (DoS) attacks. In 8.0 this command was available in the Active Charging Service Configuration mode. In 8.1 it was moved to the Rulebase Configuration mode. Also, in 8.1, the port-scan option was added to this command.
> CLI (Rulebase Configuration Mode)
> [ no ] firewall dos-protection { all | flooding { icmp | tcp-syn | udp } | ftp-bounce | ip-unaligned-timestamp | mime-flood | port-scan | seq-number-out-of-range | seq-number-prediction | source-router | teardrop | winnuke }
> default firewall dos-protection
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall flooding
> This command configures firewall protection from packet flooding attacks. In 8.0 this command was available in the Active Charging Service Configuration mode. In 8.1 it is moved to the Rulebase Configuration mode.
> CLI (Rulebase Configuration Mode)
> firewall flooding { { protocol { icmp | tcp-syn | udp } packet limit packets } | { sampling-interval interval } }
> default firewall flooding { { protocol { icmp | tcp-syn | udp } packet limit } | { sampling-interval } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall icmp-destination-unreachable-message-threshold
> This command configures a threshold on the number of ICMP error messages sent by the subscriber for a particular data flow. In 8.0 this command was available in the Active Charging Service Configuration mode. In 8.1 it is moved to the Rulebase Configuration mode.
> CLI (Rulebase Configuration Mode)
> firewall icmp-destination-unreachable-message-threshold messages then-block-server
> [ default | no ] firewall icmp-destination-unreachable-message -threshold
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall max-ip-packet-size
> This command configures the maximum IP packet size allowed over firewall. In 8.0 this command was available in the Active Charging Service Configuration mode. In 8.1 it is moved to the Rulebase Configuration mode.
> CLI (Rulebase Configuration Mode)
> firewall max-ip-packet-size packet_size protocol { icmp | non-icmp }
> default firewall max-ip-packet-size protocol { icmp | non-icmp }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall mime-flood
> This command configures firewall protection from MIME Flooding attacks. In 8.0 this command was available in the Active Charging Service Configuration mode. In 8.1 it was moved to the Rulebase Configuration mode.
> CLI (Rulebase Configuration Mode)
> firewall mime-flood { http-headers-limit max_limit | max-http-header-field-size max_size }
> default firewall mime-flood { http-headers-limit | max-http-header-field-size }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall no-ruledef-matches
> This command configures the default action for packets when no Firewall ruledef matches.
> In 8.0 this command was available in the Active Charging Service Configuration mode. In 8.1 it is moved to the Rulebase Configuration mode.
> The nat-realm keyword was added to this command. This enables to optionally specify a NAT realm to be used for performing NAT on subscriber packets.
> CLI (Rulebase Configuration Mode)
> firewall no-ruledef-matches { downlink | uplink } action { deny [ charging-action charging_action ] | permit [ nat-realm nat_realm ] }
> default firewall no-ruledef-matches { downlink | uplink } action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall priority
> This command adds and specifies the priority and type of a firewall rule definition in the rulebase, and allows to configure a single or range of ports to be allowed on the server for auxiliary/data connections.
> The nat-realm keyword was added to this command. This enables to optionally specify a NAT realm to be used for performing NAT on subscriber packets matching the firewall ruledef.
> CLI (Rulebase Configuration Mode)
> firewall priority priority [ dynamic-only | static-and-dynamic ] firewall-ruledef firewall_ruledef { { deny [ charging-action charging_action ] } | { permit [ nat-realm nat_realm | trigger open-port { aux_port_number | range start_port_number to end_port_number } direction { both | reverse | same } ] } }
> no firewall priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-syn-flood-intercept
> This command enables and configures the TCP intercept parameters to prevent TCP SYN flooding attacks by intercepting and validating TCP connection requests for DoS protection mechanism configured with the dos-protection command. In v8.0 this command was available in the Active Charging Service Configuration mode. In v8.1 it is moved to the Rulebase Configuration mode.
> CLI (Rulebase Configuration Mode)
> firewall tcp-syn-flood-intercept { max-attempts max_attempts | mode { none | { intercept | watch } [ aggressive ] } | retransmit-timeout retransmit_timeout | watch-timeout intercept_watch_timeout }
> default firewall tcp-syn-flood-intercept { max-attempts | mode | retransmit-timeout | watch-timeout }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip protocol
> This command defines a firewall rule definition to analyze user traffic based on the protocol being transported by IP packets. The following keywords were added to this command:

> l | protocol: Enables specifying a protocol by its name.

> l | operator protocol_assignment: Enables specifying a protocol lesser than or equal to, or greater than or equal to a protocol assignment number.

> CLI (Firewall Ruledef Configuration Mode)
> [ no ] ip protocol { { operator { protocol | protocol_assignment } } | { operator protocol_assignment } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Modified in Release 8.3
> IMPORTANT: The commands documented in this section have been modified in Release 8.3.
> firewall no-ruledef-matches
> This command configures the default action for packets when no Firewall Ruledef matches. The optional keyword bypass-nat was added to this command. This enables to configure packets permitted to pass to bypass Network Address Translation (NAT).
> CLI (Rulebase Configuration Mode)
> firewall no-ruledef-matches { downlink | uplink } action { deny [ charging-action charging_action ] | permit [ bypass-nat | nat-realm nat_realm ] }
> default firewall no-ruledef-matches { downlink | uplink } action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall priority
> This command adds and specifies the priority and type of a firewall rule definition in the rulebase, and allows to configure a single or range of ports to be allowed on the server for auxiliary/data connections.
> The optional keyword bypass-nat was added to this command. This enables to configure packets to bypass NAT.
> CLI (Rulebase Configuration Mode)
> firewall priority priority [ dynamic-only | static-and-dynamic ] firewall-ruledef firewall_ruledef { { deny [ charging-action charging_action ] } | { permit [ nat-realm nat_realm | [ byass-nat ] [ trigger open-port { aux_port_number | range start_port_number to end_port_number } direction { both | reverse | same } ] ] } }
> no firewall priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Modified in Release 8.0
> This section provides information on GGSN commands modified in Release 8.0.
> allow aaa-assigned-hostname
> Existing command now modified to accommodate new keyword to configure the system to allow different attributes in the LAC Hostname AVP and Called-Number AVP for L2TP messages exchanged between LAC and LNS.
> CLI (LAC Service Configuration Mode)
> allow {aaa-assigned-hostname | called-number value apn}
> [ no | defualt ] allow {aaa-assigned-hostname | called-number value apn}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer-control-mode
> New keyword none added to exclude the bearer control mode information elements and BCM information in PCO IE in GTP messages in a network where unknown information elements are not ignored by AGWs or firewall results in message drop/reject.
> CLI (APN Configuration Mode)
> bearer-control-mode [ ms-only | mixed | none ]
> [ default ] bearer-control-mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cc profile
> This command includes additional tariff timers.
> CLI (GGSN Service Configuration Mode)
> cc profile 10 tariff time1 0 7 time2 30 19 time3 0 7 time4 30 19 time5 30 26 time4 0 7
> Web Element Manager Path
> Click Configuration | GGSN | GGSN Service.
> gtpp dictionary
> This command designates specific dictionary used by GTPP for specific context. New dictionaries were added to this command.
> CLI (Context Configuration and GTPP Server Group Configuration Modes)
> gtpp dictionary { custom1 | custom10 | custom11 | custom12 | custom13 | custom14 | custom15 | custom16 | custom17 | custom18 | custom19 | custom2 | custom20 | custom3 | custom4 | custom5 | custom6 | custom7 | custom8 | custom9 | standard }
> default gtpp dictionary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp error-response
> This command determines whether the GGSN retries sending a DRT request after receiving an error response message.
> CLI (GTPP Group Configuration Mode)
> gtpp error-response { discard-cdr | retry-request }
> default gtpp error-response
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp interim now
> This command check points current GTPP accounting messages and identifies which types of interim CDRs are to be generated and sent to the external charging/storage servers (e.g., a CFG or a GSS). The impact of this command is immediate. Two new keywords have been added to assist with fine tuning the GTPP messages: callid and dhcp-server.
> CLI (Exec Mode)
> gtpp interim now [ active-charging egcdr | apn apn_name | callid call_id | cdr-types { mcdr | scdr } | dhcp-server ip_address | gprs-service svc_name | ggsn-service svc_name | imsi imsi [ ip-address sub_address [ username name ] now | nsapi nsapi [ ip-address sub-address [ username name ] | username name ] ] | ip-address sub_address [ username name ] | ip-pool pool_name | mcc mcc_number mnc mnc_numbe r | msisdn msisdn_num | sgsn-address ip_address | sgsn-service svc_name | username name ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp max-cdrs
> TP PR 4360 ST16 PR 70569
> The default keyword was added to the syntax.
> CLI (GTPP Group Configuration Mode)
> [ default ] gtpp max-cdrs number [ wait-time seconds ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sgsn-address
> New keywords GAN and HSPA added to support Generic Access Network and High Speed Packet Access type of radio access technology with SGSN address in GGSN service configuration mode.
> CLI (GGSN Service Configuration Mode)
> sgsn address {{ip_address [ subnetmask netmask ]} | ip_address/netmask}[plmn-foreign [ reject-foreign-subscriber ]
> | mcc mcc_code mnc mnc_code [ reject-foreign-subscriber ] ] [ rat-type { GAN | GERAN | HSPA | UTRAN | WLAN }] [ description description ]
> [ disable-gtpc-echo ]
> no sgsn { address ip_address [ subnetmask netmask ] }
> [ no ] sgsn multiple-address-group grp_name [ disable-gtpc-echo ]
> [ mcc mcc_code mnc mnc_code [ reject-foreign-subscriber ] ]
> [ plmn-foreign [ reject-foreign-subscriber ] [ rat-type { GAN | GERAN | HSPA | UTRAN | WLAN }] [ description description ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Modified in Release 8.1
> The following commands have been modified in Release 8.1.
> gtpp dictionary
> New dictionaries are available for selection - custom 21 - custom30. The new dictionaries have a default behavior of gtpp dictionary ‘standard’.
> CLI (Context Configuration and GTPP Server Group Configuration Modes)
> gtpp dictionary {custom1 | custom10 | custom11 | custom12 | custom13 | custom14 | custom15 | custom16 | custom17 | custom18 | custom19 | custom20 | custom21 | custom22 | custom23 | custom24 | custom25 | custom26 | custom27 | custom28 | custom29 | custom3 | custom30 | custom4 | custom5 | custom6 | custom7 | custom8 | custom9 | standard }
> default gtpp dictionary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp egcdr
> This command configures the parameters and triggers for eG-CDRs. This command has a new keyword set - final-record, with multiple options - to fine-tune the configuration of the final eG-CDRs.
> CLI (GTPP Group Configuration Mode)
> gtpp egcdr { final-record [ closing-cause [ same-in-all-partials | unique ] | include-content-ids [ all | only-with-traffic ] ] | losdv-max-containers number | lotdv-max-containers number | service-data-flow threshold [ interval seconds | volume { downlink | total | uplink } bytes ] | service-idle-timeout seconds }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpu udp-checksum insert
> New keyword default added to this command and now system sends UDP checksum in outgoing UPD packets by default.
> CLI (GGSN Service Configuration Mode)
> [ no | default } gtpu udp-checksum insert
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server local file
> New keyword purge-processed-files added in this command to configure the periodic deletion of local processed (*.p) CDR files from the Hard disk on SMC card. This keyword deletes the processed CDR files in every 4 minutes.
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server local file { compression { gzip | none } | format { custom1 | custom2 | custom3 | custom4 | custom5 } | name prefix prefix | purge-processed-files | rotation { cdr-count count | time-interval time | volume size } }
> default gtpp storage-server local file { compression | format | name | purge-processed-files | rotation }
> no gtpp storage-server local file rotation { cdr-count | purge-processed-files | time-interval }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos rate-limit { downlink | uplink }
> New keyword auto-readjust [ duration dur ] added in this command to configure the burst size dynamically. It also provides different burst size for Peak and Committed data rate-limiting through an APN.
> CLI (APN Configuration Mode)
> qos rate-limit { downlink | uplink } [ class { background | conversational | interactive traffic_priority | streaming } ] [ burst-size { bytes | auto-readjust [ duration dur ] } ] [ exceed-action { drop | lower-ip-precedence | transmit } [ violate-action { drop | lower-ip-precedence | shape [transmit-when-buffer-full] | transmit }]] | [ violate-action { drop | lower-ip-precedence | shape [transmit-when-buffer-full] | transmit } [ exceed-action { drop | lower-ip-precedence | transmit }]] +
> no qos rate-limit direction { downlink | uplink } [ class { background | conversational | interactive traffic_priority | streaming } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ipv6 pool
> The dup-addr-detection option has been added to the policy keyword. This configuration allows an IPv6 shared pool prefix to be shared in multiple call sessions with different interface IDs for an IPv6 address, and duplicate interface IDs are detected.
> CLI (Ethernet Port Configuration Mode)
> ipv6 pool name prefix ip_address/len shared policy dup-addr-detection
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tunnel l2tp
> New keyword local-hostname hostname added to this command to configures the LAC-Hostname AVP to be used for the communication with the LNS peer for an APN.
> CLI (APN Configuration Mode)
> tunnel l2tp [peer-address lns-address [[encrypted] secret l2tp_secret] [preference num] [tunnel-context name] [local-address ip-address] [crypto-map map_name {[encrypted] isakmp-secret crypto_secret}] [local-hostname hostname]
> no tunnel [peer-address lns-address]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - Modified in Release 8.0
> This section provides information on HA commands modified in Release 8.0.
> authentication aaa-distributed-mip-keys
> New keyword added to authentication command in HA Configuration mode to configure the usage of AAA distributed MIP keys for authenticating RRQ for WiMax HA calls.
> CLI (HA Configuration Mode)
> authentication {aaa-distributed-mip-keys [disabled | optional | required]| imsi-auth | mn-aaa {allow-noauth | always | dereg-noauth | noauth | renew-reg-noauth | renew-and-dereg-noauth} | mn-ha {allow-noauth | always}}
> no authentication {aaa-distributed-mip-keys required | imsi-auth}
> default authentication [aaa-distributed-mip-keys | imsi-auth | mn-aaa | mn-ha]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - Modified in Release 8.1
> This section provides information on HA commands modified in Release 8.1.
> redirect
> This command identifies DNS IP addresses from foreign networks that are to be redirected to the home DNS. A maximum of 16 intercept rules (either redirect or pass-thru) are allow for each intercept list.
> Since this command is configured in the source context, the destination context containing the path to the home network DNS is identified using the Context Configuration Mode command ip dns-proxy source-address.
> CLI (HA Configuration Mode)
> [ no ] redirect any [ primary-dns ip_address [ secondary-dns
> ip_address ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> NAT Commands - Modified in Release 8.3
> This section provides information on NAT commands modified in Release 8.3.
> nat policy
> This command enables/disables Network Address Translation (NAT) processing for all subscribers using this rulebase. The optional keyword default-nat-realm was added to this command. This enables to configure the default NAT realm to be used if one is not already configured.
> CLI (Rulebase Configuration Mode)
> nat policy nat-required [ default-nat-realm realm_name ]
> { default | no } nat policy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDIF Commands - Modified in Release 8.0
> PDIF is not supported in Release 8.0.
> PDIF Commands - Modified in Release 8.1
> The PDIF commands documented in this section are only available in Release 8.1.
> aaa attribute
> PDIF decides the radius attributes values and inclusion/exclusion criteria normally through configured radius dictionaries. However, generation of each new dictionary requires a new ST40 PDIF image. The above command is an exception for specifying the required values for the attribute without building a new software image. 3gpp2-serving-pcf is an addition to the existing aaa attribute CLI under PDIF-service config mode.
> CLI (Config PDIF Service Config Mode)
> [ no ] aaa attribute 3gpp2-serving-pcf <ip-address>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> aaa authentication
> Sets the aaa authentication for first and second phase authentication when multiple authentication is configured on the system. Two phase-authentication happens in IKEv2 setup for setting up the IPSec session. The first authentication uses Diameter AAA EAP method and second authentication uses RADIUS AAA authentication. The same AAA context may be used for both authentications. PDIF service allows you to specify only a single AAA group, which could normally be used for the first authentication method.
> A given AAA group only supports either Diameter or RADIUS authentication. If the NAI in the first authentication is different from NAI in the second authentication each NAI can point to a different domain profile in the PDIF. Each domain profile may be configured with each AAA group, one for Diameter and the other for RADIUS.
> CLI (PDIF Service Config Mode)
> aaa authentication { { first-phase | second-phase } |
> { context-name name aaa-group name } }
> no aaa authentication [ first-phase | second-phase ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> authentication
> The authentication command has a new keyword gateway to configure the pre-shared gateway key. The key is either encrypted or clear.
> There is also a new keyword second-phase eap-profile for installations using multiple authentication and need to configure a second EAP profile
> CLI (Crypto Template Config Mode
> gateway { encrypted key value | key value }
> authentication eap-profile name [ second-phase eap-profile name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> group
> PDIF now supports encryption at Diffie-Hellman Group level 14. Selecting any group automatically enables Perfect Forward Secrecy. Selecting the new keyword none disables PFS. none is the default setting.
> CLI (IPsec Transform-set Config Mode)
> group 14
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> hmac
> The NULL encryption algorithm represents the optional use of applying encryption within ESP. ESP can then be used to provide authentication and integrity without confidentiality.
> CLI (IPsec Transform-Set Config Mode)
> hmac null
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> IKEv2-IKESA policy error notification
> This modified command in the Crypto-Template config mode generates errors for packets with invalid syntax or invalid message ids.
> CLI (Crypto Template Configuration Mode
> i kev2-ikesa { keepalive-user-activity | max-retransmissions number | retransmission-timeout msec |
> policy error-notification [ invalid-message-id | invalid-syntax ] | setup-timer sec | transform-set list name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> peer
> The peer command has been amended so the user can administratively enable and disable a Diameter peer. If the peer is disabled, it still retains its configuration. The default option is to Enable.
> CLI (Diameter Endpoint Config Mode)
> peer peer_name admin-status { enable | disable }
> default peer peer_name admin-status
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> proxy-mip
> Proxy-MIP command has been extended to include PDIF.
> CLI (Subscriber Config Mode)
> proxy-mip required
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> server
> The start port range for this command has been changed to 45001.
> CLI (IPMS Client Config Mode)
> server address ip_address start-port 45001 end-port 45005
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - Modified for Release 8.0
> This section provides information on PDSN commands modified in Release 8.0.
> file
> New keywords have been added to this command in version 8.0 so unique file sequence numbers can be generated for different rulebase-format-name combinations.
> CLI (EDR Configuration Mode/UDR Configuration Mode)
> [ default ] file-sequence-number rulebase-seq-num
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - Modified for Release 8.1
> This section provides information on PDSN commands modified in Release 8.1.
> ipv6 pool
> The dup-addr-detection option has been added to the policy keyword. This configuration allows an IPv6 shared pool prefix to be shared in multiple call sessions with different interface IDs for an IPv6 address, and duplicate interface IDs are detected.
> CLI (Ethernet Port Configuration Mode)
> ipv6 pool name prefix ip_address/len shared policy dup-addr-detection
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ink aggregation
> The auto option has been added to the rate keyword. This configuration allows the rate to be set by the peer.
> CLI (Ethernet Port Configuration Mode)
> link aggregation { master | member | group N }
> [ lacp { active | passive } ] [ rate { auto | slow | fast } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear snmp trap
> The cli “clear snmp trap” is updated with new option “statistics”
> CLI (Exec Mode Commands)
> clear snmp trap { history | statistics }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - Modified for Release 8.3
> This section provides information on PDSN commands modified in Release 8.3.
> bcmcs
> This command is modified to include new keywords to support ppt.
> CLI (PDSN Service Mode Commands)
> bcmcs custom ptt {destination-context dest_name | disconnect-dscp-label dscp-label_value| mtu | rohc-profile-name profile_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Session Control Manager Commands - Modified for Release 8.0
> Session Control Manager is not supported in Release 8.0.
> Session Control Manager Commands - Modified for Release 8.1
> The following commands have been modified in Release 8.1.
> access-type
> This ue-ip-address-range has been added to specify a UE IP address/range for a specific access type.
> CLI (CSCF Service Configuration Mode)
> access-type { 3gpp-geran | 3gpp-utran-fdd | 3gpp-utran-tdd | 3gpp2-1x | 3gpp2-1x-hrpd | 3gpp2-umb | adsl | adsl2 | adsl2p | docsis | gshdsl | hdsl | hdsl2 | idsl | ieee-80211 | ieee-80211a | ieee-80211b | ieee-80211g | ieee-80216e | radsl | sdsl | vdsl } access-profile { default | name access_profile_name } | ue-ip-address-range name ue_ip_name { address ip_address_mask | range start_ip_address end_ip_address }
> no access-type { 3gpp-geran | 3gpp-utran-fdd | 3gpp-utran-tdd | 3gpp2-1x | 3gpp2-1x-hrpd | 3gpp2-umb | adsl | adsl2 | adsl2p | docsis | gshdsl | hdsl | hdsl2 | idsl | ieee-80211 | ieee-80211a | ieee-80211b | ieee-80211g | ieee-80216e | radsl | sdsl | vdsl } [ access-profile | ue-ip-address-range [ name ue_ip_name ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cnsa-media-profile
> The content-type keyword has been added.
> CLI (CSCF Service Configuration Mode)
> [ no ] cnsa-media-profile profile_id cscf-service-policy policy_name content-type { application-3gpp-ims-xml | application-pidf-diff-xml | application-pidf-partial-xml | application-pidf-xml | application-reginfo-xml | application-sdp | application-xml | message-sipfrag | multipart-mixed | multipart-related | text-plain }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter
> The location-info keyword has been added to specify the E2-interface for location-information.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> diameter location-info { dictionary { e2custom01 | e2custom02 | e2custom03 | e2custom04 | e2custom05 | e2custom06 | e2custom07 | e2custom08 | e2custom09 | e2standard } | origin endpoint endpoint_name | peer-select peer peer_name [ peer-realm realm_name ] [ secondary-peer peer_name
> [ sec-peer-realm realm_name ] ] }
> diameter policy-control { dictionary { Gq-custom | Gq-standard | Rx-standard | Tx-standard | custom01 | custom02 | custom03 | custom04 | custom05 | custom06 | custom07 | custom08 | custom09 } | origin endpoint endpoint_name | peer-select peer peer_name [ peer-realm realm_name ]
> [ secondary-peer peer_name [ sec-peer-realm realm_name ] ] }
> default diameter { location-info | policy-control } dictionary
> no diameter { location-info | policy-control } [ origin endpoint | peer-select ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> policy
> The threshold congestion-control keyword has been added to configure the congestion control threshold values that are to be monitored on this CSCF service.
> CLI (CSCF Service Configuration Mode)
> policy { allow-early-media | threshold congestion-control
> [ system-cpu-utilization percent ] [ tolerance percent ] }
> [ default | no ] policy { allow-early-media | threshold congestion-control tolerance }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> trusted-domain-entity
> The foreign-network keyword has been added to specify that an entity belongs to a Foreign Network.
> CLI (CSCF Service Configuration Mode)
> trusted-domain-entity address [ foreign-network ]
> no trusted-domain-entity address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - Modified for Release 8.0
> The following commands have been modified in Release 8.0
> accounting
> The gtpp group keyword has been added to this command to associate a defined GTPP group with the SGSN operator policy for accounting (CDR) purposes.
> CLI (SGSN Operator Policy Configuration Mode)
> accounting context ctxt_name [ gtpp group grp_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager
> accounting
> This modified command in the SGSN Service configuration mode provides support for the generation of SMS-types of CDRs for the defined context.
> CLI (SGSN Service Configuration Mode)
> accounting ( cdr-types { s-cdr | m-cdr | sms-mo-cdr | sms-mt-cdr } + | context ctxt_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager
> application-context-name
> Three new timer options have been added for configuration of the MAP application contexts.
> - mo-fwd-sm
> - mt-fwd-sm
> - ready-for-sm
> CLI (MAP Service Configuration Mode)
> application-context-name application operation-timer value
> default application-context-name application operation-timer
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager
> authenticate all-event
> The all-event keyword has been added to the authenticate command that all procedures - attaches, service requests, RAUs, detaches, and activations - are to be authenticated for a specific SGSN operator policy.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate { activate | all-events | attach | detach | rau | service-request }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> authenticate attach
> The attach keyword has been modified and the inter-rat keyword has been included to enable or disable (default) authentication for Inter-RAT Attaches.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate { attach [ inter-rat [ access-type gprs | umts ] ] }
> default authenticate attach inter-rat [ access-type gprs | umts ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> authenticate frequency
> The frequency keyword has been added to the authenticate command to enable the configuration of 1-in-N selective authentication of subscriber events such as attach, RAU, service request, detach, activate primary PDP context requests.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate { activate | all-events | attach | detach | rau | service-request } [ frequency frequency ] [ access-type gprs | umts ]
> default authenticate { activate | all-events | attach | detach | rau | service-request } [ frequency ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> authenticate rau update-type
> The authentica rau update-type command has been enhanced to include the with inter-rat-local-ptmsi qualifier to enable or disable (default) authentication for Inter-RAT RAUs.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate rau update-type { ra-update with inter-rat-local-ptmsi | combined-update with inter-rat-local-ptmsi | imsi-combined-update with inter-rat-local-ptmsi }
> default authenticate rau update-type { ra-update | combined-update | imsi-combined-update }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bind link
> For this command, the nsei keyword has been changed to be peer-nsei
> CLI (Port Channelized Configuration Mode)
> bind link peer-nsei nse_id 245 ns-vci ns-vc_id 5555
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager
> cc profile
> This modified command defines an instance of the CC profile with the charging triggers, configured with modified keywords, the SGSN will use to generate various types of CDRs for the SGSN service.
> CLI (GPRS Service Configuration Mode)
> cc profile profile_bits [ buckets number | interval time | tariff time1 mins hours [ time2 mins hours ] [ time3 mins hours ] [ time4 mins hours ] | volume { downlink down_vol uplink up_vol | total total_vol } ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ciphering-algorithm
> Default value has been changed so that the user has more control over when ciphering is performed. The new default value is gea0, no ciphering.
> CLI (GPRS Service Configuration Mode)
> default ciphering-algorithm priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear subscriber
> New filter keyword nsapi added to this existing command to clear the subscriber and session information on the basis of network service access point identifier (NSAPI).
> CLI (Exec Mode)
> clear subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more}]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> equipment-identity-register
> New filter keyword check-imei-every-n-events added to this existing command to set the frequency (1-in-N) of sending ‘check IMEI’ messages to the EIR. This reduces EIR-SGSN traffic.
> CLI (MAP Service Configuration Mode)
> equipment-identity-register { isdn E.164_num | point code pt_code }
> [ source-ssn ssn | check-imei-every-n-events times ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> frame-relay
> This command configures the parameters for the Frame Relay connection, including the fractional channel.
> CLI (Channelized Port Configuration Mode)
> frame-relay path path_id { ds1 connects | e1 connects }
> timeslots slot# [ intf-type intf_type ] [ lmi_type lmi_type ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gmm
> In this command, new timers have been added:

> l | mobile-reachable-timeout - range 4 to 1440 minutes, default 58 minutes

> l | purge-timeout - range 1 to 20160, default 10080 minutes

> In this command, timers have been given default values:

> l | t3302-timeout - default 12 minutes

> l | t3312-timeout - default 54 minutes

> l | t3313-timeout - default 5 seconds

> l | t3314-timeout - default 44 seconds

> l | t3350-timeout - default 6 seconds

> l | t3360-timeout - default 6 seconds

> l | t3370-timeout - default 6 seconds

> In this command, some timers have been modified:

> l | ‘t3314-negotiate-timeout’ is now ‘negotiate-t3314-timeout’

> l | ‘llc pdu-lifetime’ timer has been moved to the llc command

> In this command, some timers have been removed:

> l | t3322-timeout

> l | implicit-detach-timeout

> l | max-auth-retransmission

> l | max-identity-retransmission

> l | max-page-retransmission

> l | perform-identity-on-auth-failure

> l | ptmsi-reallocate

> CLI (GPRS Service Configuration Mode)
> [ default ] gmm { mobile-reachable-timeout mins | negotiate-t3314-timeout secs | purge-timeout mins | T3302-timeout mins | T3312-timeout mins | T3313-timeout secs | T3350-timeout secs | T3360-timeout secs | T3370-timeout secs } +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gmm
> TP PR 7549; ST16 PR 110911
> The negotiate-t3314-timeout keyword has been modified in two way:

> l | the maximum value for this timer has increased to 11160.

> l | the behavior of this timer has changed when it is disabled, so that by disabling negotiation of the T3314-timeout value, if the MS sends the requested value of the ready timer in the Att/RAU Request, then the SGSN sends the T3314-timeout value in the Att/RAU Accept.

> CLI (GPRS Service Configuration Mode)
> [ no | default ] gmm negotiate-t3314-timeout [<0-11160> seconds ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp
> This existing command is now available for SGSN service in Context configuration mode for mentioned variants to configure Ga interface for accounting in SGSN service.
> CLI (Context Configuration Mode)
> gtpp charging-agent address
> gtpp duplicate-hold-time minutes
> gtpp echo-interval
> gtpp max-cdrs
> gtpp max-pdu-size
> gtpp max-retries
> gtpp redirection-allowed
> gtpp server
> gtpp storage-server
> gtpp timeout
> Web Element Manager Path
> Configuration of these features is not yet supported by the Web Element Manager.
> gtpp dictionary
> This command designates specific dictionary used by GTPP for specific context. New dictionaries were added to this command.
> CLI (Context Configuration and GTPP Server Group Configuration Modes)
> gtpp dictionary { custom1 | custom10 | custom11 | custom12 | custom13 | custom14 | custom15 | custom16 | custom17 | custom18 | custom19 | custom2 | custom20 | custom3 | custom4 | custom5 | custom6 | custom7 | custom8 | custom9 | standard }
> default gtpp dictionary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp interim now
> This command check points current GTPP accounting messages and identifies which types of interim CDRs are to be generated and sent to the external charging/storage servers (e.g., a CFG or a GSS). The impact of this command is immediate. The following keywords have been added to assist with fine tuning the GTPP messages:

> l | callid

> l | cdr-types

> l | dhcp-server

> l | gprs-service

> l | mcc/mnc

> l | msisdn

> l | sgsn-service

> CLI (Exec Mode)
> gtpp interim now [ active-charging egcdr | apn apn_name | callid call_id | cdr-types { mcdr | scdr } | dhcp-server ip_address | gprs-service svc_name | ggsn-service svc_name | imsi imsi [ ip-address sub_address [ username name ] now | nsapi nsapi [ ip-address sub-address [ username name ] | username name ] ] | ip-address sub_address [ username name ] | ip-pool pool_name | mcc mcc_number mnc mnc_numbe r | msisdn msisdn_num | sgsn-address ip_address | sgsn-service svc_name | username name ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp max-cdrs
> TP PR 4360 ST16 PR 70569
> The default keyword was added to the syntax.
> CLI (GTPP Group Configuration Mode)
> [ default ] gtpp max-cdrs number [ wait-time seconds ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp trigger
> The plmn-id-change keyword has been added to this command to enable the PLMN-ID-change trigger for S-CDRs if the dictionary specified in the gtpp dictionary configuration supports the PLMN-ID change. If enabled, the SGSN generates a partial S-CDR when the MS changes the PLMN while under the same 2G SGSN. Currently, custom18 dictionary supports this trigger.
> CLI (GTPP Group Configuration Mode)
> [ no ] gtpp trigger plmn-id-change
> default gtpp trigger
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> lawful-intercept
> Two new keywords, interception-point-policy ( sms-mt or sms-mo) and reprovision-target-policy resend-pdp-context-active-iri have been added to the lawful-intercept command for use with an SGSN license to support interception of SMS messages.
> CLI (Global Configuration Mode)
> lawful-intercept { acked-udp [ num-retry number ] [ timeout time ] | hand-off-policy send-start-intercept-with-pdp-active-iri | interception-point-policy { { sms-mo | sms-mt } { message-delivered | request-received } } | reprovision-target-policy resend-pdp-context-active-iri | src-ip-addr ip_address | tcp tcp_option | unack-format use-service-address }
> Web Element Manager Path
> Configuration of these features is not yet supported by the Web Element Manager.
> lawful-intercept
> A new keyword, hand-off-policy send-start-intercept-with-pdp-active-iri, has been added to the lawful-intercept command for use with an SGSN license to enable/disable configuration to send ‘start intercept’ messages in the event of an ISRAU.
> CLI (Global Configuration Mode)
> lawful-intercept { acked-udp [ num-retry number ] [ timeout time ] | hand-off-policy send-start-intercept-with-pdp-active-iri | interception-point-policy { { sms-mo | sms-mt } { message-delivered | request-received } } | reprovision-target-policy resend-pdp-context-active-iri | src-ip-addr ip_address | tcp tcp_option | unack-format use-service-address }
> Web Element Manager Path
> Configuration of these features is not yet supported by the Web Element Manager.lawful-intercept
> A new keyword, tcp, has been added to the lawful-intercept command for use with an SGSN license to enable use of the TCP interface in place of the UPD interface. The new keyword includes timer and addressing options.
> CLI (Global Configuration Mode)
> lawful-intercept { acked-udp [ num-retry number ] [ timeout time ] | hand-off-policy send-start-intercept-with-pdp-active-iri | interception-point-policy { { sms-mo | sms-mt } { message-delivered | request-received } } | reprovision-target-policy resend-pdp-context-active-iri | src-ip-addr ip_address | tcp
> { [ application-heartbeat-messages timeout time ] | [ connection-retry-timer time ] | [ content-delivery { dest-addr ipv4_add dest-port port } ]
> [ event-delivery { dest-addr ipv4_add dest-port port } ]
> | unack-format use-service-address }
> Web Element Manager Path
> Configuration of these features is not yet supported by the Web Element Manager.
> llc
> The pdu-lifetime parameter has been moved from the gmm command in the GPRS Service Configuration Mode to the llc command in the same mode and the parameter’s default has been changed from 60 seconds to 6 seconds. As well, all the t200 timer names have been simplified.
> CLI (GPRS Service Configuration Mode)
> llc { pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> The iov-ui-in-xid-reset keyword has been added to the llc command to allow the operator to configure whether or not the SGSN sends IOV-UI in XID-RESET messages. The SGSN sends the IOV-UI by default.
> CLI (GPRS Service Configuration Mode)
> llc { iov-ui-in-xid-reset | pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> The n201u-max keyword has been added to the llc command to allow the operator to set the maximum size that can be negotiated for the downlink data packet (information field length for U/UI frames.
> CLI (GPRS Service Configuration Mode)
> llc { iov-ui-in-xid-reset | n201u-max | pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> The uplink-pdu-len-validation keyword has been added to the llc command to provide the operator the ability to validate or ignore the negotiated uplink N201_U packet size.
> CLI (GPRS Service Configuration Mode)
> llc { iov-ui-in-xid-reset | n201u-max | pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time | uplink-pdu-len-validation }
> no llc uplink-pdu-len-validation
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> map
> This existing command is now enhanced with new keyword imeisv to include the International Mobile Equipment Identity-Software Version (IMEI-SV) information to include in GPRS Location Update (GLU) request message.
> CLI (SGSN Operator Policy Configuration Mode)
> [remove] map message update-gprs-location [private-extension access-type | imeisv]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> network-service-entity ip
> This command has been modified. See network-service-entity
> network-service-entity
> The network-service-entity frame-relay and network-service-entity ip commands have been combined under this new command name - network-service entity.
> This command has two keyword options:
> ip-local - to create an NSE instance within an IP environment and enter NSE-IP configuration mode, a sub-mode of the Global Configuration Mode . The Network Service Entity - IP mode enables you to configure the management functionality for the Gb interface between a BSS and an SGSN over a 2.5G GPRS IP network connection. This configuration mode includes the following commands.

> l | max-ns-retransmissions

> l | ns-timer

> l | nsvc-failure-action

> l | nsvl

> peer-nsei - to create an NSE instance within a Frame Relay environment and enter the NSE-FR configuration mode, a sub-mode of the Global Configuration mode. The NSE-FR configuration mode enables you to define and manage the functionality for the Gb interface between a BSS and an SGSN over a 2.5G GPRS frame relay network connection. This configuration mode includes the following command:

> l | nsvc to create a network service virtual connection instance and enter the NSVC configuration mode.

> CLI (Global Configuration Mode)
> [ no ] network-service-entity ( ip-local | peer-nsei peer-nsei frame-relay}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> network-service-entity ip-local
> A new keyword - all-nsvc-failure-action - has been added to this command to configure how the SGSN handles the NSE when NSVC, connected to the BSC, go down. Options include:

> l | clear-nse which instructs the SGSN to SGSN to clear NSE if all NSVC to the BSC are down.

> l | default which means the NSE is not cleared if all NSVC go down.

> CLI (Network Service Entity IP Local Configuration Mode)
> all-nsvc-failure-action clear-nse
> default all-nsvc-failure-action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nri
> Two new keywords - null-nri-value and non-broadcast lac/rac - have been added to this command to facilitate the SGSN off loading procedure which is part of Gb flex (SGSN) pooling.
> CLI (GPRS Service Configuration Mode)
> nri length length null-nri-value null_nri_value non-broadcast lac lac_id rac rac_id nri-value nri_value
> no nri
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ns-timer
> The default value of the test keyword for the ns-timer command has been increased from 5 to 30 seconds:
> CLI (Network Service Entity IP Local Configuration Mode)
> ns-timer test <time>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ns-vc
> The command creates Network Service Virtual Connection Configuration sub-mode in the Network Service Entity Frame Relay configuration mode to define the management functionality for a specific network service virtual connection of the Gb interface between a BSS and an SGSN in a 2.5G GPRS frame relay network connection.

> l | retries - command has been deprecated

> l | timer - command has been deprecated

> CLI (Network Service Entity - Peer NSEI Configuration Mode)
> [ no ] ns-vc instance nsvc_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nsvl
> This command name has been modified - it was originally ns-vl - it is now nsvl. Nothing else about this command has changed.
> The command creates Network Service Virtual Link Configuration sub-mode in the Network Service Entity IP configuration mode to define the management functionality for a specific network service virtual link in a 2.5G GPRS IP network connection.
> CLI (Network Service Entity - IP Configuration Mode)
> [ no ] nsvl instance nsvl_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nsvl-address
> The following keywords in this command have been deprecated and the functionality has been moved into a separate command in this configuration mode, command weight.
> - signaling weight
> - data weight
> CLI (NSVL Configuration Mode)
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> paging-policy
> The command name has changed from paging-scheme to paging policy but it still configures the paging parameters for the GPRS service. Keywords (parameters) have been modified and combined to enhance efficiency:
> CLI (GPRS Service Configuration Mode)
> paging-policy { last-known-area { all | bsc | cell | location-area | routing-area } | max-retransmissions retran_num }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> paging-policy
> With the addition of the zero (‘0’) to the value range for the max-retransmissions keyword, it is now possible to disable retransmissions for paging policy so only a single 2G PS-paging request will be sent to the BSC.
> CLI (GPRS Service Configuration Mode)
> paging-policy { last-known-area { all | bsc | cell | location-area | routing-area } | max-retransmissions < 0 to 5 >}
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> partial-apn-match
> New keyword (partial-apn-match) has been added to the sm command to optimize radio resource usage by managing signaling between the MS and the SGSN. Specifically, this keyword enables partial matching of a requested APN during APN selection.
> CLI (GPRS Service Configuration Mode)
> sm { activate-max-retransmissions num_retries | deactivate-max-
> retransmissions num_retries | ignore-pco-decode-error | modify-max-retransmissions num_retries | partial-apn-match | requested-apn-from-first-subrec | t3385-timeout secs | t3386-timeout secs | t3395-timeout secs | trim-trailing-spaces-in-apn }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> peer-nsei
> This command was the nsei command in the GPRS service configuration mode. The command now has a new name.
> This command has a new keyword - pooled - which enables pooling with non-pooled BSCs within the pool area.
> CLI (GPRS Service Configuration Mode)
> peer-nsei nse_id { lac lac_id rac rac_id | pooled }
> [ no ] peer-nsei nse_id { lac lac_id rac rac_id | pooled }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos class
> The MBR and GBR downlink rates, part of the qualifying options configuration, for all four QoS classes have been increased to 256000 kbps.
> CLI (SGSN APN Configuration Mode)
> qos class { background | conversational | interactive | streaming } [ qualif_option ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos class
> Existing CLIs keywords value options have been modified to support the HSUPA+ in the SGSN.
> CLI (SGSN APN Configuration Mode)
> qos class background mbr-up <1…256000kbps>
> qos class conversational mbr-up <1…256000kbps>
> qos class conversational gbr-up <1…256000kbps>
> qos class interactive mbr-up <1…256000kbps>
> qos class streaming mbr-up <1…256000kbps>
> qos class streaming gbr-up <1…256000kbps>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos prefer-as-cap
> The qos command, in the SGSN operator policy's APN policy configuration mode, has been modified to support capping of the local QoS bit rate when the subscribed QoS provided by the HLR is lower than the locally configured value.
> CLI (IuPS Service Configuration Mode)
> qos { class | prefer-as-cap { hlr-subscription | local | both-hlr-and-local } | rate-limit }
> remove qos prefer-as-cap
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> rau-inter
> This new CLI keyword enables the operator to configure the GMM cause code that will be included in the Routing Area Update Reject message sent to the MS when the peer SGSN address resolution process fails during Inter SGSN RAU.
> CLI (SGSN Operator Policy Configuration Mode)
> rau-inter peer-sgsn-addr-resolution-failure failure-code { 9 | 10 }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> requested-apn-from-first-subrec
> This new keyword for the sm command enables use of a ‘requested APN’ from the first subscription record.
> CLI (GPRS Service Configuration Mode)
> [ default | no ] sm requested-apn-from-first-subrec
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sgsn-context-request
> The word 'allowed' has been removed from the default form of this command.
> CLI (GPRS Service Configuration Mode)
> default sgsn-context-request ptmsi-signature-absence
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show session
> The words gprs-only and sgsn-only have been added to various show session commands to limit output to MM and PDP context information.
> CLI (Exec Configuration Mode)
> show session disconnect-reasons [ gprs-only | sgsn-only ]
> show session duration [ gprs-only | sgsn-only ]
> show session setuptime [ gprs-only | sgsn-only ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sm
> A new keyword has been added to the sm command, ignore-pco-decode-error. This option enables the SGSN to ignore received decode errors that are due to incorrectly encoded PCO IE length in SM Requests.
> CLI (GPRS Service Configuration Mode)
> sm ignore-pco-decode-error
> default sm ignore-pco-decode-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> trim-trailing-spaces-in-apn
> New keyword (trim-trailing-spaces-in-apn) has been added to the sm command to optimize radio resource usage by managing signaling between the MS and the SGSN. Specifically, this keyword enables the SGSN to strip off any trailing space(s) in the requested APN.
> CLI (GPRS Service Configuration Mode)
> sm { activate-max-retransmissions num_retries | deactivate-max-
> retransmissions num_retries | ignore-pco-decode-error | modify-max-retransmissions num_retries | partial-apn-match | requested-apn-from-first-subrec | t3385-timeout secs | t3386-timeout secs | t3395-timeout secs | trim-trailing-spaces-in-apn }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - Modified for Release 8.1
> The following commands have been modified in Release 8.1
> apn/apn-selection-default/wildcard-apn
> To meet 3GPP TS23.003, the maximum length for the network-identifier for all APN definitions has been reduced from 63 characters to 62.
> CLI (SGSN Operator Policy Configuration Mode)
> apn { network-identifier apn_net_id | operator-identifier apn_op_id }
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> authenticate rau update-type
> The authentica rau update-type command has been enhanced to include the with inter-rat-local-ptmsi qualifier to enable or disable (default) authentication for Inter-RAT RAUs.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate rau update-type { ra-update with inter-rat-local-ptmsi | combined-update with inter-rat-local-ptmsi | imsi-combined-update with inter-rat-local-ptmsi }
> default authenticate rau update-type { ra-update | combined-update | imsi-combined-update }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> frame-relay
> This command configures the parameters for the Frame Relay connection, including the fractional channel.
> CLI (Channelized Port Configuration Mode)
> frame-relay path path_id { ds1 connects | e1 connects }
> timeslot slot# [ intf-type intf_type ] [ lmi_type lmi_type ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp storage-server local file
> New keyword purge-processed-files added in this command to configure the periodic, every 4 minutes, deletion of local processed (*.p) CDR files from the hard disk on SMC card.
> CLI (GTPP Group Configuration Mode)
> gtpp storage-server local file { compression { gzip | none } | format { custom1 | custom2 | custom3 | custom4 | custom5 } | name prefix prefix | purge-processed-files | rotation { cdr-count count | time-interval time | volume size } }
> default gtpp storage-server local file { compression | format | name | purge-processed-files | rotation }
> no gtpp storage-server local file rotation { cdr-count | purge-processed-files | time-interval }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpc
> Keyword ignore response-port-validation has been added to this command to instruct the SGSN to ignore the response port validation.
> CLI (SGTP Service Configuration Mode)
> gtpc ignore response-port-validation
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> imsi
> The keyword imsi has been added to the imsi command to enable the IMSI (E.212 address) to be used as the destination address in the HLR configuration.
> CLI (HLR Configuration Mode)
> imsi { any | starts-with prefix_number } { imsi [ sgsn-source-address-format point-code-ssn [ source-ssn ssn ] | isdn isdn_number | mobile-global-title mgt_number | point-code pt-code } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> imsi
> The functionality of this keyword has been modified so that it enables configurable default behavior for routing.

> l | Entering imsi with the any keyword preserves the default behavior and the E.212 address is used as a destination address and the MAP request will be sent towards the HLR.

> l | If this keyword is not used with the any keyword, then the MAP request will be rejected.

> CLI (HLR Configuration Mode)
> imsi { any | starts-with prefix_number } { imsi [ sgsn-source-address-format point-code-ssn [ source-ssn ssn ] | isdn isdn_number | mobile-global-title mgt_number | point-code pt-code } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> The n201u-max keyword has been added to the llc command to allow the operator to set the maximum size that can be negotiated for the downlink data packet (information field length for U/UI frames.
> CLI (GPRS Service Configuration Mode)
> llc { iov-ui-in-xid-reset | n201u-max | pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nri length
> The non-broadcast keyword in this command has been modified to include the values of the PLMN’s MCC and MNC to enable support for multiple IuPS Services when Iu-Flex is utilized.
> CLI (SGSN APN Configuration Mode)
> nri length nri_length { nri-value nri_value | null-nri-value null_nri_value non-broadcast mcc mcc mnc mnc lac lac_id rac rac_id [ nri-value value }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> qos prefer-as-cap
> The qos command, in the SGSN operator policy's APN policy configuration mode, has been modified to support capping of the local QoS bit rate when the subscribed QoS provided by the HLR is lower than the locally configured value.
> CLI (IuPS Service Configuration Mode)
> qos { class | prefer-as-cap { hlr-subscription | local | both-hlr-and-local } | rate-limit }
> remove qos prefer-as-cap
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> qos rate-limit
> Keyword auto-readjust and keyword duration have been added as options to the burst-size keyword to expand functionality and provide dynamic burst-size calculation support for traffic policing.

> l | readjust : This keyword enables dynamic burst-size calculation support for traffic policing.

> l | duration <seconds> : Must be an integer from 1 to 30. This keyword sets the number of seconds that the dynamic burst-size calculation will last.

> CLI (SGSN APN Configuration Mode)
> qos rate-limit direction { downlink | uplink } [ burst-size { auto-readjust [ duration <seconds> ] | <bytes> } ]
> qos rate-limit direction { downlink | uplink } class <traffic-class> [burst-size { auto-readjust [ duration <seconds> ] | <bytes> } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radio-network-controller
> The radio-network-controller command has been changed to make it easier for the operator to enter the command. The new command to create an RNC configuration instance is rnc. Identification of the MCC and MNC are no longer associated with the configuration instance.
> CLI (IuPS Service Configuration Mode)
> rnc rnc_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ranap allocation-retention-priority-ie
> This command configures the parameters for the allocation-retention-priority (ARP) IE inserted in the RAB assignment request message.
> CLI (SGSN APN Configuration Mode)
> ranap allocation-retention-priority-ie subscription-priority priority class { { background | conversational | interactive | streaming } { not-pre-emptable | priority | queuing-disallowed | shall-not-trigger-pre-emptable } + }
> [ default | remove | no ] ranap allocation-retention-priority-ie [ subscription-priority priority class { background | conversational | interactive | streaming } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> routing-context
> For releases 8.1 and higher, the range of values for this keyword has been increased from maximum of 65535 to 4294967295 in accordance with RFC 4666.
> CLI (SS7 Routing Domain Configuration Mode)
> routing-context < 1 - 4294967295>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Obsoleted Commands
> Common Commands - Obsoleted in Release 8.0
> This section provides information on commands that are common to all products that were obsoleted in Release 8.0.
> context-cleanup-period
> Removed and replaced in functionality by context-timeout seconds
> CLI (ROHC-Profile Decompress-Config Mode
> context-cleanup-period variable
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter dictionary
> This command is deprecated. The Diameter dictionaries for accounting and authentication can now be configured using the diameter accounting dictionary and diameter authentication dictionary commands.
> CLI (AAA Server Group and Context Configuration Modes)
> diameter dictionary { aaa-custom1 | aaa-custom10 | aaa-custom2 | aaa-custom3 | aaa-custom4 | aaa-custom5 | aaa-custom6 | aaa-custom7 | aaa-custom8 | aaa-custom9 | nasreq | rf-plus }
> [ default ] diameter dictionary
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> fragment-size
> The fragment-size command has been removed from DLCI Configuration Mode.
> CLI (DLCI Configuration Mode Commands)
> [default] fragment-size number
> header-type
> The header-type command has been removed from DLCI Configuration Mode.
> CLI (DLCI Configuration Mode Commands)
> header-type { 2byte | 4byte }
> [ default ] header-type
> service-type
> The pwe3-cseopsn keyword has been obsoleted and replaced with the mtp2 keyword.
> CLI (Card Configuration Mode)
> service-type { frame-relay | pwe3-cesopsn | mtp2 | unspecified }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tx-priority
> The tx-priority command has been removed from DLCI Configuration Mode.
> CLI (DLCI Configuration Mode Commands)
> tx-priority priority
> [ default ] tx-priority
> vc-mapping
> The vc-mapping command has been deprecated and removed from the Channelized Port Configuration Mode. Frame mapping is now completely standards compliant and done through path command configuration explained in the Channelized Port Configuration Mode chapter in the Command Line Interface Reference.
> CLI (Channelized Port Mode Commands)
> vc-mapping { g.707 | interleaved }
> { deny | permit } [ log ] { tcp | udp }
> Removed “treatment { conversational | streaming | background | interactive-1 | interactive-2 | interactive-3}” keyword from this command:
> CLI (ACL Configuration Mode and IPv6 ACL Configuration Mode)
> { deny | permit } [ log ] { tcp | udp } { { source_address source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address dest_wildcard | any |
> host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] | treatment { conversational | streaming | background | interactive-1 | interactive-2 | interactive-3}}
> Common Commands - Obsoleted in Release 8.1
> This section provides information on commands that are common to all products that were obsoleted in Release 8.1.
> enable/disable super-charger
> This command has been deprecated and replaced with the super-charger command in the SGSN Operator Policy configuration mode.
> CLI (SGSN Service Configuration Mode)
> enable | disable super-charger
> isakmp disable-phase1-rekey
> This command deprecated and replaced with ikev1 disable-phase1-rekey command.
> CLI (Context Configuration Mode)
> [ no ] isakmp disable-phase1-rekey
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> isakmp keepalive
> This command deprecated and replaced with ikev1 keepalive dpd command.
> CLI (Context Configuration Mode)
> [ no ] isakmp keepalive dpd interval interval timeout time num-retry retries
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> isakmp policy
> This command deprecated and replaced with ikev1 policy command.
> CLI (Context Configuration Mode)
> [ no ] isakmp policy priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - Obsoleted in Release 8.0
> This section provides information on CF commands that were obsoleted in Release 8.0.
> timeout action
> This command is deprecated and replaced with the failure-action command.
> CLI (Content Filtering Server Group Configuration Mode)
> timeout action { allow | content-insertion content_string | discard | redirect-url url | terminate-flow }
> default timeout action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> CF Commands - Obsoleted in Release 8.1
> timeout action
> This command is deprecated and replaced by the failure-action command.
> CLI (Content Filtering Policy Configuration Mode)
> timeout action { allow | content-insert content_string | discard | redirect-url url | terminate-flow | www-reply-code-and-terminate-flow reply_code } [ edr edr_format_name ]
> default timeout action [ edr edr_format_name ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Obsoleted in Release 8.0
> This section provides information on ECS commands that were obsoleted in Release 8.0.
> tcp out-of-order-timeout
> This command is deprecated and replaced with the tcp packets-out-of-order command.
> CLI (Rulebase Configuration Mode)
> tcp out-of-order-timeout timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> wtp out-of-order-timeout
> This command is deprecated and replaced with the wtp packets-out-of-order command.
> CLI (Rulebase Configuration Mode)
> wtp out-of-order-timeout duration_ms
> default wtp out-of-order-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Obsoleted in Release 8.1
> This section provides information on ECS commands that were obsoleted in Release 8.1.
> bearer apn
> This command defines a rule definition to analyze and charge user traffic based on APN bearer. In StarOS 8.1 and later, this command is deprecated and is replaced by the bearer 3gpp apn command.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer apn [ case-sensitive ] operator value
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer imsi
> This command defines a rule definition to analyze and charge user traffic based on International Mobile Station Identification number (IMSI) in bearer flow. In StarOS 8.1 and later, this command is deprecated and is replaced by the bearer 3gpp imsi command.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer imsi { operator imsi | { !range | range } imsi-pool imsi_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer rat-type
> This command defines a rule definition to analyze and charge user traffic based on the Radio Access Technology (RAT) in bearer flow. In StarOS 8.1 and later, this command is deprecated and is replaced by the bearer 3gpp rat-type command.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer rat-type operator rat
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> bearer sgsn-address
> This command defines a rule definition to analyze and charge user traffic based on SGSN address associated in bearer flow. This command is deprecated and replaced by the bearer 3gpp sgsn-address command.
> CLI (Ruledef Configuration Mode)
> [ no ] bearer sgsn-address operator address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Obsoleted in Release 8.0
> No Firewall commands were obsoleted from Release 8.0.
> Firewall Commands - Obsoleted in Release 8.1
> This section provides information on Firewall commands that were obsoleted in Release 8.1.
> firewall policy
> This command enables/disables Stateful Firewall support for subscriber/APN. This configuration is now available in the Rulebase Configuration mode.
> CLI (APN and Subscriber Configuration Modes)
> firewall policy firewall-required
> { default | no } firewall policy
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Obsoleted in Release 8.0
> This section provides information on GGSN commands that were obsoleted in Release 8.0.
> qos traffic-policing
> This command is deprecated and replaced with traffic shaping related commands:

> l | qos negotiate-limit

> l | qos rate-limit

> qos-renegotiation
> This command is deprecated for GGSN service from APN configuration mode and Subscriber Configuration Mode. Dynamic QoS renegotiation support is now in Enhanced Charging Service configuration.
> CLI (APN Configuration Mode and Subscriber Configuration Mode)
> [no | default] qos-renegotiate
> timeout
> Keyword qos-renegotiate time is removed from this command for GGSN service from APN configuration mode and Subscriber Configuration Mode. Dynamic QoS renegotiation support is now in Enhanced Charging Service configuration.
> CLI (APN Configuration Mode and Subscriber Configuration Mode)
> [no | default] timeout qos-renegotiate time
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Obsoleted in Release 8.1
> No GGSN commands were obsoleted from Release 8.1.
> HA Commands - Obsoleted in Release 8.0
> No HA commands were obsoleted from Release 8.0.
> HA Commands - Obsoleted in Release 8.1
> No HA commands were obsoleted from Release 8.1.
> PDSN Commands - Obsoleted in Release 8.0
> No PDSN commands were obsoleted from Release 8.0.
> PDSN Commands - Obsoleted in Release 8.1
> No PDSN commands were obsoleted from Release 8.1.
> Session Control Manager Commands - Obsoleted in Release 8.0
> Session Control Manager is not supported in Release 8.0.
> Session Control Manager Commands - Obsoleted in Release 8.1
> This section provides information on SCM commands that were obsoleted in Release 8.1.
> access-network
> This command configures the location specific mobile network identifiers used to match location specific emergency/service numbers.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> access-network mcc code mnc code
> no access-network
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - Obsoleted in Release 8.0
> The following commands have been obsoleted during the development cycle of Release 8.0
> Gs Service Configuration Mode
> The following commands have been removed from this configuration mode:
> CLI (Gs Service Configuration Mode)
> - T10-timeout
> - T12-1-timeout
> - T12-2-timeout
> - T6-1-timeout
> - T8-timeout
> - T9-timeout
> - access-protocol
> - location-area-code-list
> - max-N10-retransmission
> - max-N12-retransmission
> - max-N8-retransmission
> - max-N9-retransmission
> - vlr-hash
> NSE-FR Configuration Mode
> The following command has been obsoleted:
> - bssgp-timer
> NSE-IP Configuration Mode
> The following commands have been obsoleted or replaced:
> - peer-network-service-entity
> - retry-count
> - timer
> Replacement commands have been documented in the NSE-IP Configuration Mode chapter of the CLI Reference Guide.
> SGSN Operator Policy Configuration Mode
> The following command has been obsoleted:
> - charging context
> Replacement commands have been documented in the CLI Reference Guide.
> SGSN Service Configuration Mode
> The following commands have been removed from this configuration mode:
> CLI (SGSN Service Configuration Mode)
> - page-timer
> - path-failure
> - periodic-ra-upd-timer
> - plmn
> - purge-timer
> SGSN Commands - Obsoleted in Release 8.1
> No SGSN commands were obsoleted from Release 8.1.
> GTPP Storage Server (GSS)
> This section documents additions and modifications to the GSS.
> GSS Changes in Release 8.0
> None for this release.
> GSS Changes in Release 8.1
> None for this release.
> Web Element Manager Changes
> This section documents additions and modifications to the Web Element Manager.
> No changes were made for this release.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883