> CSCFINTF Schema Statistics
> The CSCFINTF schema provides the following types of service-level statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> CSCFINTF Schema Statistics

> Statistic | Description | Data Type
> vpnname | VPN Name | String (Fixed Value)
> vpnid | VPN ID | Int32 (Fixed Value)
> svcname | Service Name | String (Fixed Value)
> svcid | Service ID | Int32 (Fixed Value)
> peer-ipaddr | Peer Ip-address | String (Fixed Value)
> peer-domain | Peer Domain Name | String (Fixed Value)
> regreqrx | Total number of Register requests received. | Int64
> regreqtx | Total number of Register requests transmitted. | Int64
> invreqrx | Total number of Invite requests received. | Int64
> invreqtx | Total number of Invite requests transmitted. | Int64
> ackreqrx | Total number of ACK requests received. | Int64
> ackreqtx | Total number of ACK requests transmitted. | Int64
> byereqrx | Total number of Bye requests received. | Int64
> byereqtx | Total number of Bye requests transmitted. | Int64
> cancreqrx | Total number of Cancel requests received. | Int64
> cancreqtx | Total number of Cancel requests transmitted. | Int64
> optreqrx | Total number of Options requests received. | Int64
> optreqtx | Total number of Options requests transmitted. | Int64
> prackreqrx | Total number of PRACK requests received. | Int64
> prackreqtx | Total number of PRACK requests transmitted. | Int64
> subreqrx | Total number of Subscribe requests received. | Int64
> subreqtx | Total number of Subscribe requests transmitted. | Int64
> notreqrx | Total number of Notify requests received. | Int64
> notreqtx | Total number of Notify requests transmitted. | Int64
> refreqrx | Total number of Refer requests received. | Int64
> refreqtx | Total number of Refer requests transmitted. | Int64
> inforeqrx | Total number of Info requests received. | Int64
> inforeqtx | Total number of Info requests transmitted. | Int64
> updreqrx | Total number of Update requests received. | Int64
> updreqtx | Total number of Update requests transmitted. | Int64
> msgreqrx | Total number of Message requests received. | Int64
> msgreqtx | Total number of Message requests transmitted. | Int64
> pubreqrx | Total number of Publish requests received. | Int64
> pubreqtx | Total number of Publish requests transmitted. | Int64
> tryrsprx | Total number of Trying responses received. | Int64
> tryrsptx | Total number of Trying responses transmitted. | Int64
> rngrsprx | Total number of Ringing responses received. | Int64
> rngrsptx | Total number of Ringing responses transmitted. | Int64
> fwdrsprx | Total number of Forwarded responses received. | Int64
> fwdrsptx | Total number of Forwarded responses transmitted. | Int64
> quersprx | Total number of Queued responses received. | Int64
> quersptx | Total number of Queued responses transmitted. | Int64
> prgrsprx | Total number of Progress responses received. | Int64
> prgrsptx | Total number of Progress responses transmitted. | Int64
> 200-rsprx | Total number of 200 OK responses received. | Int64
> 200-rsptx | Total number of 200 OK responses transmitted. | Int64
> 202-rsprx | Total number of 202 Accepted responses received. | Int64
> 202-rsptx | Total number of 202 Accepted responses transmitted. | Int64
> mchrsprx | Total number of Multiple Choices responses received. | Int64
> mchrsptx | Total number of Multiple Choices responses transmitted. | Int64
> mpersprx | Total number of Moved Permanently responses received. | Int64
> mpersptx | Total number of Moved Permanently responses transmitted. | Int64
> mtersprx | Total number of Moved Temporarily responses received. | Int64
> mtersptx | Total number of Moved Temporarily responses transmitted. | Int64
> upxrsprx | Total number of Use Proxy responses received. | Int64
> upxrsptx | Total number of Use Proxy responses transmitted. | Int64
> altrsprx | Total number of Alternative Service responses received. | Int64
> altrsptx | Total number of Alternative Service responses transmitted. | Int64
> brqerrrx | Total number of BadRequest errors received. | Int64
> brqerrtx | Total number of BadRequest errors transmitted. | Int64
> uauerrrx | Total number of UnAuthorized errors received. | Int64
> uauerrtx | Total number of UnAuthorized errors transmitted. | Int64
> prerrrx | Total number of Payment Required Errors received. | Int64
> prerrtx | Total number of Payment Required Errors transmitted. | Int64
> forerrrx | Total number of Forbidden errors received. | Int64
> forerrtx | Total number of Forbidden errors transmitted. | Int64
> nfderrrx | Total number of NotFound errors received. | Int64
> nfderrtx | Total number of NotFound errors transmitted. | Int64
> mnaerrrx | Total number of MethodNotAllowed errors received. | Int64
> mnaerrtx | Total number of MethodNotAllowed errors transmitted. | Int64
> nac406errrx | Total number of NotAcceptable(406) errors received. | Int64
> nac406errtx | Total number of NotAcceptable(406) errors transmitted. | Int64
> parerrrx | Total number of ProxyAuthRequired errors received. | Int64
> parerrtx | Total number of ProxyAuthRequired errors transmitted. | Int64
> rtoerrrx | Total number of RequestTimeout errors received. | Int64
> rtoerrtx | Total number of RequestTimeout errors transmitted. | Int64
> conferrrx | Total number of Conflict Errors received. | Int64
> conferrtx | Total number of Conflict Errors transmitted. | Int64
> lrerrrx | Total number of Length Required Errors received. | Int64
> lrerrtx | Total number of Length Required Errors transmitted. | Int64
> gonerrrx | Total number of Gone errors received. | Int64
> gonerrtx | Total number of Gone errors transmitted. | Int64
> crferrrx | Total number of ConditionalRequestFail errors received. | Int64
> crferrtx | Total number of ConditionalRequestFail errors transmitted. | Int64
> relerrrx | Total number of RequestEntityTooLarge errors received. | Int64
> relerrtx | Total number of RequestEntityTooLarge errors transmitted. | Int64
> rulerrrx | Total number of RequestURITooLong errors received. | Int64
> rulerrtx | Total number of RequestURITooLong errors transmitted. | Int64
> umterrrx | Total number of UnsupportedMediaType errors received. | Int64
> umterrtx | Total number of UnsupportedMediaType errors transmitted. | Int64
> uuserrrx | Total number of Unsupported URI Scheme errors received. | Int64
> uuserrtx | Total number of Unsupported URI Scheme errors transmitted. | Int64
> bexerrrx | Total number of BadExtension errors received. | Int64
> bexerrtx | Total number of BadExtension errors transmitted. | Int64
> exrerrrx | Total number of Extension Required errors received. | Int64
> exrerrtx | Total number of Extension Required errors transmitted. | Int64
> sitserrrx | Total number of Session Interval Too Small errors received. | Int64
> sitserrtx | Total number of Session Interval Too Small errors transmitted. | Int64
> itberrrx | Total number of Interval Too Brief errors received. | Int64
> itberrtx | Total number of Interval Too Brief errors transmitted. | Int64
> blierrrx | Total number of Bad Location Information errors received. | Int64
> blierrtx | Total number of Bad Location Information errors transmitted. | Int64
> tnaerrrx | Total number of TempNotAvailable errors received. | Int64
> tnaerrtx | Total number of TempNotAvailable errors transmitted. | Int64
> tdnerrrx | Total number of Transaction Does Not Exist errors received. | Int64
> tdnerrtx | Total number of Transaction Does Not Exist errors transmitted. | Int64
> ldterrrx | Total number of LoopDetected errors received. | Int64
> ldterrtx | Total number of LoopDetected errors transmitted. | Int64
> tmherrrx | Total number of TooManyHops errors received. | Int64
> tmherrtx | Total number of TooManyHops errors transmitted. | Int64
> adierrrx | Total number of AddrIncomplete errors received. | Int64
> adierrtx | Total number of AddrIncomplete errors transmitted. | Int64
> amberrrx | Total number of Ambiguous errors received. | Int64
> amberrtx | Total number of Ambiguous errors transmitted. | Int64
> bhrerrrx | Total number of BusyHere errors received. | Int64
> bhrerrtx | Total number of BusyHere errors transmitted. | Int64
> rqcerrrx | Total number of RequestCancel errors received. | Int64
> rqcerrtx | Total number of RequestCancel errors transmitted. | Int64
> namerrrx | Total number of NotAcceptableMedia errors received. | Int64
> namerrtx | Total number of NotAcceptableMedia errors transmitted. | Int64
> beerrrx | Total number of BusyEverywhere errors received. | Int64
> beerrtx | Total number of BusyEverywhere errors transmitted. | Int64
> trperrrx | Total number of Request Pending errors received. | Int64
> trperrtx | Total number of Request Pending errors transmitted. | Int64
> udperrrx | Total number of Undecipherable errors received. | Int64
> udperrtx | Total number of Undecipherable errors transmitted. | Int64
> sarerrrx | Total number of sec-agree Required errors received. | Int64
> sarerrtx | Total number of Sec-agree Required errors transmitted. | Int64
> ineerrrx | Total number of InternalError errors received. | Int64
> ineerrtx | Total number of InternalError errors transmitted. | Int64
> nimerrrx | Total number of NotImplemented errors received. | Int64
> nimerrtx | Total number of NotImplemented errors transmitted. | Int64
> bgterrrx | Total number of BadGateway errors received. | Int64
> bgterrtx | Total number of BadGateway errors transmitted. | Int64
> suaerrrx | Total number of ServiceUnavailable errors received. | Int64
> suaerrtx | Total number of ServiceUnavailable errors transmitted. | Int64
> gtterrrx | Total number of GatewayTimeout errors received. | Int64
> gtterrtx | Total number of GatewayTimeout errors transmitted. | Int64
> bsverrrx | Total number of BadSipVersion errors received. | Int64
> bsverrtx | Total number of BadSipVersion errors transmitted. | Int64
> mtlerrrx | Total number of Message Too Large errors received. | Int64
> mtlerrtx | Total number of Message Too Large errors transmitted. | Int64
> pcferrrx | Total number of Precondition Failure errors received. | Int64
> pcferrtx | Total number of Precondition Failure errors transmitted. | Int64
> bewerrrx | Total number of BusyEverywhere errors received. | Int64
> bewerrtx | Total number of BusyEverywhere errors transmitted. | Int64
> decerrrx | Total number of Decline errors received. | Int64
> decerrtx | Total number of Decline errors transmitted. | Int64
> neaerrrx | Total number of NotExistAnywhere errors received. | Int64
> neaerrtx | Total number of NotExistAnywhere errors transmitted. | Int64
> nac606errrx | Total number of NotAcceptable(606) errors received. | Int64
> nac606errtx | Total number of NotAcceptable(606) errors transmitted. | Int64
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883