> HA Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> The following variables are supported:
> HA Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the HA service. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the HA service. This is an internal reference number. | Int32
> servname | Displays the name of the HA service for which the statistics are displayed. | String
> disconnects | The total number of sessions that were disconnected. | Int32
> num-sessions | The current total number of Mobile IP HA sessions. | Int32
> revoc-sent | The total number of HA registration revocations sent. | Int32
> revoc-retry-sent | The total number of HA registration revocation messages the system attempted to re-send. | Int32
> revoc-ack-recv | The total number of HA registration revocation acknowledgement messages received. | Int32
> revoc-timeout | The total number of timeouts that occurred during HA registration revocations. | Int32
> revoc-recv | The total number of HA registration revocations received | Int32
> revoc-ack-sent | The total number of The total number of HA registration revocation acknowledgement messages sent. | Int32
> expiry | The total number of sessions that were disconnected due to the expiration of their lifetime setting. | Int32
> dereg | The total number of sessions that were disconnected due to de-registrations. | Int32
> admindrop | The total number of sessions that were disconnected due to an administrative clearing of calls (i.e. executing the clear subscriber command). | Int32
> miscerror | The total number of sessions that were disconnected due to miscellaneous errors. | Int32
> farevocation | The total number of FA revocations that occurred. | Int32
> auth-attempt | The total number of authentication attempts made. | Int32
> auth-failure | The total number of authentication attempts that were unsuccessful. | Int32
> auth-success | The total number of authentication attempts that were successful. | Int32
> auth-real-failure | The total number of authentication attempts that were unsuccessful due to the receipt of an access reject message from the AAA server. | Int32
> auth-misc-failure | The total number of authentication attempts that were unsuccessful due to occurrences other than the receipt of an access reject messages (i.e. AAA server timeout or internal errors). | Int32
> recv-total | The total number of registration requests received. | Int32
> recv-initial | The total number of initial registration requests received. | Int32
> recv-renew | The total number of renewal registration requests received. | Int32
> recv-dereg | The total number of requests for de-registration received. | Int32
> recv-ho | The total number of handoff requests received | Int32
> recv-ho-3g3g | 3GPP2 to 3GPP2 Handoff Requests received | Int32
> recv-ho-3gwi | 3GPP2 to WiMax Handoff Requests received | Int32
> recv-ho-wi3g | Wimax to 3GPP2 Handoff Requests Received | Int32
> recv-ho-wiwi | Wimax to Wimax Handoff Requests Received | Int32
> accept-total | The total number of registration requests accepted. | Int32
> accept-reg | The total number of initial registration requests accepted. | Int32
> accept-renew | The total number of renewal registration requests accepted. | Int32
> accept-dereg | The total number of requests for de-registration accepted. | Int32
> accept-ho | The total number of handoff registration requests accepted. | Int32
> accept-ho-3g3g | 3GPP2 to 3GPP2 Handoff Requests accepted | Int32
> accept-ho-3gwi | 3GPP2 to WiMax Handoff Requests accepted | Int32
> accept-ho-wi3g | Wimax to 3GPP2 Handoff Requests accepted | Int32
> accept-ho-wiwi | Wimax to Wimax Handoff Requests accepted | Int32
> denied-total | The total number of registration requests that were denied. | Int32
> denied-initial | The total number of initial registration requests denied. | Int32
> denied-renew | The total number of renewal registration requests denied. | Int32
> denied-dereg | The total number of requests for de-registration denied. | Int32
> denied-ho | The total number of handoff registration requests denied. | Int32
> denied-ho-3g3g | 3GPP2 to 3GPP2 Handoff Requests denied | Int32
> denied-ho-3gwi | 3GPP2 to WiMax Handoff Requests denied | Int32
> denied-ho-wi3g | Wimax to 3GPP2 Handoff Requests denied | Int32
> denied-ho-wiwi | Wimax to Wimax Handoff Requests denied | Int32
> discard-total | The total number of registration requests that were discarded. | Int32
> reply-total | The total number of registration replies sent. | Int32
> reply-acceptreg | The total number of successful registration replies sent. | Int32
> reply-acceptdereg | The total number of successful de-registration replies sent. | Int32
> reply-denied | The total number of denied registration replies sent. | Int32
> reply-badreq | The total number of denied registration replies that were sent with a reply code of 86H (Registration Denied - poorly formed request). | Int32
> reply-mismatchid | The total number of denied registration replies that were sent with a reply code of 85H (Registration Denied - registration identification mismatch). | Int32
> reply-adminprohib | The total number of denied registration replies that were sent with a reply code of 81H (Registration Denied - administratively prohibited). | Int32
> reply-unspecerr | The total number of denied registration replies that were sent with a reply code of 80H (Registration Denied - reason unspecified). | Int32
> reply-noresource | The total number of denied registration replies that were sent with a reply code of 82H (Registration Denied - insufficient resources). | Int32
> reply-mnauthfail | The total number of denied registration replies that were sent with a reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
> reply-faauthfail | The total number of denied registration replies that were sent with a reply code of 84H (Registration Denied - home agent failed authentication). | Int32
> reply-simulbind | The total number of denied registration replies that were sent with a reply code of 87H (Registration Denied - too many simultaneous mobility bindings). | Int32
> reply-unknownha | The total number of denied registration replies that were sent with a reply code of 88H (Registration Denied - unknown home agent address). | Int32
> reply-revtununavail | The total number of denied registration replies that were sent with a reply code of 89H (Registration Denied - reverse tunneling unavailable). | Int32
> reply-revtunmand | The total number of denied registration replies that were sent with a reply code of 8AH (Registration Denied - reverse tunneling mandatory). | Int32
> reply-encapunavail | The total number of denied registration replies that were sent with a reply code of 8BH (Registration Denied - reverse tunneling encapsulation style unavailable). | Int32
> reply-senderror | The total number of errors that occurred while sending replies. | Int32
> reply-unknowncvse | The total number of denied registration replies that were sent with a reply code of 8DH (Registration Denied - unsupported Vendor-ID or unable to interpret Vendor-CVSE-Type.). | Int32
> reply-udp-encapunavail | The total number of denied registration replies that were sent with a reply code of 8EH (Registration Denied - ERROR_HA_UDP-ENCAP_UNAVAIL). | Int32
> reply-error | The total number of reply errors that occurred. | Int32
> reply-cong-drop | The total number of registration replies discarded due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> reply-cong-adminprohib | The total number of denied registration replies that were sent with a reply code of 81H (Registration Denied - administratively prohibited) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> reply-cong-unknownha | The total number of denied registration replies that were sent with a reply code of 88H (Registration Denied - unknown home agent address) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> ttlprepaid | The total number of Prepaid calls facilitated by the service. | Int32
> curprepaid | The total number of Prepaid calls currently being facilitated by the service. | Int32
> ttlonlineauthsucc | The total number of successful Online Authentications for the service. | Int32
> ttlonlineauthfail | TThe total number of successful Online Authentications for the service. | Int32
> paaa-query-total | The total number of Binding Context requests received from the proxy-AAA server. | Ctr32
> paaa-query-accept | The total number of Binding Context requests received from the proxy-AAA server that were accepted. | Ctr32
> paaa-query-denied | The total number of Binding Context requests from the proxy-AAA server that were denied. | Ctr32
> paaa-resp-sent | The total number of Binding Context responses that were sent to the proxy-AAA server. | Ctr32
> paaa-resp-found | The total number of Binding Context responses that were sent to the proxy-AAA server that indicated that the requested binding context was found. | Ctr32
> paaa-resp-notfound | The total number of Binding Context responses that were sent to the proxy-AAA server that indicated that the requested binding context was not found. | Ctr32
> paaa-resp-poolover | The total number of Binding Context responses that were sent to the proxy-AAA server that indicated that there is an IP Pool overflow condition for the requested binding context. | Ctr32
> paaa-resp-misc | The total number of Binding Context responses that were sent to the proxy-AAA server that indicated other miscellaneous errors for the requested binding context. | Ctr32
> ipsec-esp-txpackets | The total number of ESP Encode packets transmitted over IPSec. | Int64
> ipsec-esp-txbytes | The total number of ESP Encode Bytes transmitted over IPSec. | Int64
> ipsec-ah-txpackets | The total number of AH Encode packets transmitted over IPSec. | Int64
> ipsec-ah-txbytes | The total number of AH Encode Bytes transmitted over IPSec. | Int64
> ipsec-error-txpackets | The total number of Encode Error packets transmitted over IPSec. | Int64
> ipsec-error-txbytes | The total number of Transmit Encode Error Bytes transmitted over IPSec. | Int64
> ipsec-esp-rxpackets | The total number of ESP Decode packets received over IPSec. | Int64
> ipsec-esp-rxbytes | The total number of ESP Decode Bytes received over IPSec. | Int64
> ipsec-ah-rxpackets | The total number of AH Decode packets received over IPSec. | Int64
> ipsec-ah-rxbytes | The total number of AH Decode Bytes received over IPSec. | Int64
> ipsec-error-packets | The total number of Error packets received over IPSec. | Int64
> ipsec-error-bytes | The total number of Error Bytes received over IPSec. | Int64
> ipsec-replay-packets | The total number of Error Replay packets received over IPSec. | Int64
> ipsec-replay-bytes | The total number of Error Replay Bytes received over IPSec. | Int64
> ipsec-decode-packets | The total number of Error Decode packets received over IPSec. | Int64
> ipsec-decode-bytes | The total number of Error Decode Bytes received over IPSec. | Int64
> ipsec-auth-packets | The total number of Error Authentication packets received over IPSec. | Int64
> ipsec-auth-bytes | The total number of Error Authentication Bytes received over IPSec. | Int64
> ipsec-tooshort-packets | The total number of Error Too Short packets received over IPSec. | Int64
> ipsec-tooshort-bytes | The total number of Receive Error Too Short Bytes received over IPSec. | Int64
> ipsec-dpdreq-sent | The total number of DPD requests sent | Int32
> ipsec-dpdreq-recv | The total number of DPD requests received | Int32
> ipsec-dpdreply-sent | The total number of DPD replies sent | Int32
> ipsec-dpdreply-recv | The total number of DPD replies received | Int32
> ipsec-dpdtimeout | The total number of DPD timeouts (retransmissions) | Int32
> ipsec-dpddisconn | The total number of DPD disconnects | Int32
> ipsec-dpdrekey | The total number of DPD phase1 rekeys | Int32
> ipsec-nattkeepalive-sent | The total number of NATT keepalives sent | Int32
> ipsec-nattkeepalive-recv | The total number of NATT keepalives received | Int32
> ipsec-ike-udpflows | The total number of current IKE UDP flows | Int32
> ipsec-ike-cookieflows | The total number of current IKE cookie flows | Int32
> ipsec-ike-txpackets | The total number of IKE packets transmitted | Int64
> ipsec-ike-rxpackets | The total number of IKE packets received | Int64
> ipsec-ike-reqrecv | The total number of IKE requests received | Int64
> ipsec-ike-udpflowpackets | The total number of IKE UDP flow packets received | Int64
> ipsec-ike-cookieflowpackets | The total number of IKE cookie flow packets received | Int64
> ipsec-cur-tun | The total current number of IPSEC tunnels | Int32
> ipsec-cur-tunestablished | The total number of currently established IPSEC tunnels | Int32
> ipsec-ike-fails | The total number of IKE failures | Int32
> ipsec-ttl-tun | The total number of tunnels setup | Int32
> ipsec-ttl-tunestablished | The total number of tunnels that were established | Int32
> ipsec-call-req-rej | The total number of call requests that were rejected | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883