> ASN QoS Descriptor Configuration Mode Commands
> The ASN QoS Descriptor Configuration Mode is used to create and manage Quality of Service Descriptor table for the ASN GW service subscribers within the current source context.
> end
> This command exits the current mode and returns to the Executive Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Executive mode.
> exit
> This command exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> global-service-class-name
> This command configures the global service class name within specific QoS descriptor table.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> global-service-class-name svc_class_name
> no global-service-class-name
> no
> Removes/deletes the configured global service class name from this QoS descriptor table.
> svc_class_name
> Specifies the global service class name in QoS descriptor table.
> svc_class_name must be an ASCII string of 6 characters in length.
> Usage
> Use this command to specify global service class name as per IEEE 802.16e standard within specific QoS descriptor table for an ASN GW service.
> Global Service Class Name is similar in function to the Service Class Name except that (1) Global Service Class Name use may not be modified by a BS, (2) Global Service Class Name remains consistent among all BS, and 3) Global Service Class Names are a rules-based naming system and contains referential QoS parameter codes.
> Example
> The following command specifies the global service class name g_svc1 in an ASN QoS descriptor table:
> global-service-class-name g_svc1
> schedule-type
> This command configures the type of data delivery service identifier/type for specific ASN GW service.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> schedule-type be [ max-sustained-traffic-rate max_sust_traffic_rate | traffic-priority priority_value ] +
> schedule-type ert-vr min-reserved-traffic-rate min_resd_traffic_rate max-latency dur_ms unsolicited-grant-interval dur_ms [ max-sustained-traffic-rate max_sust_traffic_rate | max-traffic-burst burst_size | tolerated-jitter dur_ms | traffic-priority priority_value ] +
> schedule-type nrt-vr min-reserved-traffic-rate min_resd_traffic_rate [ max-sustained-traffic-rate max_sust_traffic_rate | max-traffic-burst burst_size | traffic-priority priority_value ] +
> schedule-type rt-vr min-reserved-traffic-rate min_resd_traffic_rate max-latency dur_ms unsolicited-polling-interval dur_ms [ max-sustained-traffic-rate max_sust_traffic_rate | max-traffic-burst burst_size | traffic-priority priority_value ] +
> schedule-type ugs min-reserved-traffic-rate min_resd_traffic_rate max-latency dur_ms unsolicited-grant-interval dur_ms [ sdu-size sdu_size | tolerated-jitter dur_ms | traffic-priority priority_value] +
> default schedule-type
> default
> Configures the data delivery service type to Best Efforts (BE) service for specific ASN GW service.
> be
> Configures the data delivery service type to Best Efforts (BE) service for specific ASN GW service.
> ert-vr
> Configures the data delivery service type to Extended Real-Time Variable Rate (ERT-VR) service for specific ASN GW service.
> nrt-vr
> Configures the data delivery service type to Non-Real-Time Variable Rate (NRT-VR) service for specific ASN GW service.
> rt-vr
> Configures the data delivery service type to Real-Time Variable Rate (RT-VR) service for specific ASN GW service.
> ugs
> Configures the data delivery service type to Unsolicited Grant Service (UGS) for specific ASN GW service.
> max-latency dur_ms
> Specifies the maximum interval in milliseconds between the reception of a packet to BS or SS on its network interface/Convergence Sublayer (CS) and the arrival of packet to its RF interface or the peer device. This value represents a service commitment.
> dur_ms must be any integer value between 0 and 65535. Maximum latency set to zero means no commitment available for this service flow.
> min-reserved-traffic-rate min_resd_traffic_rate
> Default: 0 (disabled)
> Specifies the minimum traffic rates in bits per second, reserved for a service flow.
> min_resd_traffic_rate must be any integer value between 0 and 65535. Minimum reserved traffic rate set to zero means no minimum traffic rate reservation is required for this service flow.
> max-sustained-traffic-rate max_sust_traffic_rate
> Configures the maximum sustained traffic rate in bits per second for traffic schedule.
> traffic_rate must be an integer between 1 and 65535.
> max-traffic-burst burst_size
> Default: 0 (disabled)
> Specifies the maximum burst size in bits that must be maintained for the service.
> burst_size must be any integer value between 0 and 65535. Maximum traffic burst set to zero means no maximum traffic burst reservation is required for this service flow.
> sdu-size sdu_size
> Default: 49
> Specifies the length of the Service Data Unit (SDU) in bytes for a fixed-length SDU service flow.
> sdu_size must be any integer value between 1 and 65535.
> Important: This parameter is used only if packing is on and the service flow is indicated as carrying fixed-length SDUs.
> tolerated-jitter dur_ms
> Specifies the maximum delay variation (jitter) allowed for the connection.
> dur_ms must be any integer value between 1 and 65535.
> traffic-priority priority_value
> Default: 0 (disabled)
> This optional keyword specifies the traffic priority.
> priority_value must be an integer from 0 to 7.
> unsolicited-grant-interval dur_ms
> Specifies the nominal interval in millisecond between successive data grant opportunities for this service flow.
> dur_ms must be an integer value between 1 and 65535.
> unsolicited-polling-interval dur_ms
> Specifies the maximum nominal interval in millisecond between successive polling grants opportunities for this service flow.
> dur_ms must be any integer value between 1 and 65535.
> Usage
> Use this command to configure type of data delivery service identifier within ASN GW service.
> Important: Only one data delivery service type between be, et-vr, rt-vr, nrt-vr, or ugs is allowed within an ASN GW service.
> Example
> The following command configures the data delivery service type to Best Efforts (BE) service for an ASN GW service:
> default schedule-type
> service-class-name
> This command configures the Service Class Name name within specific QoS descriptor table.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> service-class-name svc_class_name
> no service-class-name
> no
> Removes/deletes the configured global service class name from this QoS descriptor table.
> svc_class_name
> Specifies the service class name in QoS descriptor table.
> svc_class_name must be an ASCII string of 2 through 128 characters.
> Usage
> A Service Class Name is a group of QoS parameters defined at the BS and can be referenced by a service flow to apply certain QoS parameters. Use this command to specify Service Class Name as per IEEE 802.16 standard within specific QoS descriptor table for ASN GW service
> Example
> The following command specifies the service class name ASN_Serv_class1 in a ASN QoS descriptor table:
> service-class-name ASN_Serv_class1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883