> IPMS Application MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the IPMS application.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1).
> starentIPMSMIB(102)
> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102).
> starIPMSMIBObjects(1)

> Object: | starIPMSTimeTicks

> Object ID: | enterprises.8164.1.102.1.1

> Description: | This object indicates the time when this notification was generated.

> Syntax: | TimeStamp

> Access: | Read-Only

> Object: | starIPMSComponentName

> Object ID: | enterprises.8164.1.102.1.2

> Description: | This object indicates the name of the IPMS application component.

> Syntax: | DisplayString

> Access: | Read-Only

> Object: | starIPMSTaskInfo

> Object ID: | enterprises.8164.1.102.1.3

> Description: | This object indicates the IPMS process facility name and instance id of the IPMS application.

> Syntax: | DisplayString

> Access: | Read-Only

> Object: | starIPMSProcessMaxRestartCnt

> Object ID: | enterprises.8164.1.102.1.4

> Description: | This object indicates the maximum restart counts for IPMS processes.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starIPMSProcessRestartWaitTime

> Object ID: | enterprises.8164.1.102.1.5

> Description: | This object indicates the waiting period in seconds to restart IPMS processes.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starIPMSPacketLossCnt

> Object ID: | enterprises.8164.1.102.1.6

> Description: | This object indicates the number of packets detected as lost in the current IPMS process.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starIPMSTotalPacketLossCnt

> Object ID: | enterprises.8164.1.102.1.7

> Description: | This object indicates the total number of packets detected as lost since IPMS process started.

> Syntax: | Unsigned32

> Access: | Read-only

> Object: | starIPMSDPIFailureReason

> Object ID: | enterprises.8164.1.102.1.8

> Description: | This object indicates the deep packet inspection (DPI) failure reasons with packet monitoring attributes.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | attributenotpresent(1) valuenotidentical(2) valuefunctionfailed(3)

> Object: | starIPMSDPIDetails

> Object ID: | enterprises.8164.1.102.1.9

> Description: | This object indicates the details of the deep packet inspection information of packets with packet monitoring attributes.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSEventSource

> Object ID: | enterprises.8164.1.102.1.10

> Description: | This object indicates the name of the event source of IPMS processes.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSAttribute

> Object ID: | enterprises.8164.1.102.1.11

> Description: | This object indicates the name of the IPMS attributes.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSResourceType

> Object ID: | enterprises.8164.1.102.1.12

> Description: | This object indicates the type of resource facilitate available/used for IPMS application processes.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | serverhbd(1) servmgr(2) serverevtlog(3) qryproc(4) evtproc0(5) evtproc1(6) evtproc2(7) evtproc3(8) evtproc4(9) queryhbd(10) qsmgr(11) eventlog(12) reqmgr(13) ctrlhbd(14) ctrlmgr(15) ctrlevtlog(16) totalcpu(17) swapmemory(18) export(19) log(20) data(21) crash(22) disk(23) invalid(24)

> Object: | starIPMSResourceInfoState

> Object ID: | enterprises.8164.1.102.1.13

> Description: | This object indicates the information of resource status for IPMS application processes.

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | available(1) notavailable(2) unknown(3) invalid(4)

> Object: | starIPMSResourceCurrentValue

> Object ID: | enterprises.8164.1.102.1.14

> Description: | This object indicates the current value/status of IPMS process resources like CPU, memory, disk space etc.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSResourceConfThreshold

> Object ID: | enterprises.8164.1.102.1.15

> Description: | This object indicates the configured threshold values of IPMS process resources like CPU, memory, disk space etc. The value is in Float so mapped to string.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSPeerName

> Object ID: | enterprises.8164.1.102.1.16

> Description: | This object indicates the name of the IPMS peer server.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSPeerIP

> Object ID: | enterprises.8164.1.102.1.17

> Description: | This object indicates the IP address of the IPMS peer server.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSPeerPort

> Object ID: | enterprises.8164.1.102.1.18

> Description: | This object indicates the port number of the IPMS server peer.

> Syntax: | DisplayString

> Access: | Read-only

> Object: | starIPMSICMPState

> Object ID: | enterprises.8164.1.102.1.19

> Description: | This object indicates the status of the Internet Control Message Protocol (ICMP) link between IPMS components and AGW. Possible state is either Up (1) or Down (2).

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | icmpstateup(1) icmpstatedown(2)

> Object: | starIPMSCORBAState

> Object ID: | enterprises.8164.1.102.1.20

> Description: | This object indicates the status of the Common Object Request Broker Architecture (CORBA) link between IPMS components and AGW. Possible state is either Up (1) or Down (2).

> Syntax: | Integer

> Access: | Read-only

> Enumeration: | corbasateup(1) corbastatedown(2)

> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102)
> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102).
> starIPMSMIBTraps(2).

> Object: | starIPMSComponentStart

> Object ID: | enterprises.8164.1.102.2.1

> Description: | This notification generated when an IPMS component started successfully.

> Objects: | starIPMSComponentName

> Object: | starIPMSComponentStop

> Object ID: | enterprises.8164.1.102.2.2

> Description: | This notification generated when an IPMS component stopped or going for shutting down.

> Objects: | starIPMSComponentName

> Object: | starIPMSProcessStart

> Object ID: | enterprises.8164.1.102.2.3

> Description: | This notification generated when an IPMS process started/restarted successfully.

> Objects: | starIPMSTaskInfo

> Object: | starIPMSProcessStartFail

> Object ID: | enterprises.8164.1.102.2.4

> Description: | This notification generated when an IPMS process failed to start/restart.

> Objects: | starIPMSComponentName starIPMSProcessMaxRestartCnt starIPMSTaskInfo starIPMSProcessRestartWaitTime

> Object: | starIPMSPacketLossThreshold

> Object ID: | enterprises.8164.1.102.2.5

> Description: | This notification generated when maximum packet loss count from event source reached the threshold limit.

> Objects: | starIPMSTaskInfo starIPMSEventSource starIPMSPacketLossCnt starIPMSTotalPacketLossCnt

> Object: | starIPMSDPIFail

> Object ID: | enterprises.8164.1.102.2.6

> Description: | This notification generated when deep packet inspection (DPI) has been detected.

> Objects: | starIPMSTaskInfo starIPMSEventSource starIPMSAttribute starIPMSDPIFailureReason starIPMSDPIDetails

> Object: | starIPMSThresholdExceed

> Object ID: | enterprises.8164.1.102.2.7

> Description: | This notification generated when system exceeds the configured threshold value for IPMS components, resource, processes.

> Objects: | starIPMSComponentName starIPMSResourceType starIPMSResourceInfoState starIPMSResourceCurrentValue starIPMSResourceConfThreshold

> Object: | starIPMSThresholdClear

> Object ID: | enterprises.8164.1.102.2.8

> Description: | This notification generated when system clears the threshold exceed condition for IPMS components, resource, processes.

> Objects: | starIPMSComponentName starIPMSResourceType starIPMSResourceInfoState starIPMSResourceCurrentValue starIPMSResourceConfThreshold

> Object: | starIPMSPeerStateChange

> Object ID: | enterprises.8164.1.102.2.9

> Description: | This notification generated when IPMS Server/Query Server peer changes its state.

> Objects: | starIPMSComponentName starIPMSPeerName starIPMSPeerIP starIPMSPeerPort starIPMSICMPState starIPMSCORBAState

> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102).
> starIPMSMIBConformances(3).starIPMSMIBCompliances(1)

> Object: | starIPMSMIBCompliance

> Object ID: | enterprises.8164.1.102.3.1.1

> Description: | The compliance statements for entities which implement the STARENT IPMS MIB.

> Objects: | starIPMSObjectGroup starIPMSNotifGroup

> starentMIB(8164).starentMIBObjects(1).starentIPMSMIB(102).
> starIPMSMIBConformances(3).starIPMSMIBGroups(2)

> Object: | starIPMSObjectGroup

> Object ID: | enterprises.8164.1.102.3.2.1

> Description: | This group is a collection of objects related with notification management on IPMS.

> Objects: | starIPMSTimeTicks starIPMSComponentName starIPMSTaskInfo starIPMSProcessMaxRestartCnt starIPMSProcessRestartWaitTime starIPMSPacketLossCnt starIPMSTotalPacketLossCnt starIPMSDPIFailureReason starIPMSDPIDetails starIPMSEventSource starIPMSAttribute starIPMSResourceType starIPMSResourceInfoState starIPMSResourceCurrentValue starIPMSResourceConfThreshold starIPMSPeerName starIPMSPeerIP starIPMSPeerPort starIPMSICMPState starIPMSCORBAState

> Object: | starIPMSNotifGroup

> Object ID: | enterprises.8164.1.102.3.2.2

> Description: | This group is a collection of notifications for IPMS management.

> Objects: | starIPMSComponentStart starIPMSComponentStop starIPMSProcessStart starIPMSProcessStartFail starIPMSPacketLossThreshold starIPMSDPIFail starIPMSThresholdExceed starIPMSThresholdClear starIPMSPeerStateChange

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883