> show lma-service
> This chapter describes the outputs of the ahow lma-service command.
> show lma-service statistics
> show lma-service statistics Command Output Descriptions

> Field | Description
> MIP AAA Authentication
> Attempts | The total number of MIP AAA authentication attempts made by this system or the specified service.
> Success | The total number of MIP AAA authentication attempts that were successful made by this system or the specified service.
> Total Failures | The total number of MIP AAA authentication attempts that failed made by this system or the specified service.
> Actual Auth Failures | The total number of actual MIP AAA authentication failures received by this system or the specified service.
> Failures | The total number of failures received by this system or the specified service.
> Misc Auth Failures | The total number of miscellaneous MIP AAA authentication failures received this system or the specified service.
> Binding Updates Received
> Total Received | The total number of all binding updates received by this system or the specified service.
> Total Accepted | The total number of all binding updates received and accepted by this system or the specified service.
> Total Denied | The total number of all binding updates received and denied by this system or the specified service.
> Total Discarded | The total number of all binding updates received and discarded by this
> Initial Binding Update Requests
> Received | The total number of all initial binding updates received by this system or the specified service.
> Accepted | The total number of initial binding updates received and accepted by this system or the specified service.
> Denied | The total number of initial binding updates received and denied by this system or the specified service.
> Refresh Binding Update Requests
> Received | The total number of all refresh binding updates received by this system or the specified service.
> Accepted | The total number of refresh binding update requests received and accepted by this system or the specified service.
> Denied | The total number of refresh binding update requests received and denied by this system or the specified service.
> DeReg Requests
> Received | The total number of all deregistration request binding updates received by this system or the specified service.
> Accepted | The total number of deregistration request binding updates received and accepted by this system or the specified service.
> Denied | The total number of deregistration request binding updates received and denied by this system or the specified service.
> Handoff Requests
> Received | The total number of all handoff request binding updates received by this system or the specified service.
> Accepted | The total number of handoff request binding updates received and accepted by this system or the specified service.
> Denied | The total number of handoff request binding updates received and denied by this system or the specified service.
> Binding Acknowledgements Sent
> Total | The total number of all binding update acknowledgements sent by this system or the specified service.
> Accepted Reg | The total number of accepted registration binding update acknowledgements sent by this system or the specified service.
> Accepted DeReg | The total number of accepted deregistration binding update acknowledgements sent by this system or the specified service.
> Denied | The total number of denied binding update acknowledgements sent by this system or the specified service.
> Send Error | The total number of send error binding update acknowledgements sent by this system or the specified service.
> Binding Update Deny Reasons
> Insufficient Resources | The total number of binding update deny messages, due to insufficient resources, sent by this system or the specified service.
> Mismatched ID | The total number of binding update deny messages, due to mismatched IDs, sent by this system or the specified service.
> MN Auth Failure | The total number of binding update deny messages, due to a mobile node authentication failure condition, sent by this system or the specified service.
> Admin Prohibited | The total number of binding update deny messages, due to requiring a message ID, sent by this system or the specified service.
> Msg ID Required | The total number of binding update deny messages, due to requiring a message ID, sent by this system or the specified service.
> DAD Failed | The total number of binding update deny messages, due to DAD failure, sent by this system or the specified service.
> Not Home Subnet | The total number of binding update deny messages, due to an incorrect home subnet, sent by this system or the specified service.
> Sequence Out Of Window | The total number of binding update deny messages, due to sequence out of window, sent by this system or the specified service.
> Reg Type Change Disallowed | The total number of binding update deny messages, due to a disallowed registration type change, sent by this system or the specified service.
> Unspecified Reason | The total number of binding update deny messages, due to an unspecified reason, sent by this system or the specified service.
> Service-Authorization Failed | The total number of binding update deny messages, due to a service authorization failure, sent by this system or the specified service.
> Proxy Reg Not Enabled | The total number of binding update deny messages, due to a proxy registration not enabled error, sent by this system or the specified service.
> Timestamp Mismatch | The total number of binding update deny messages, due to a timestamp mismatch error, sent by this system or the specified service.
> Timestamp Lower Than Expected | The total number of binding update deny messages, due to a timestamp lower than expected reason, sent by this system or the specified service.
> Missing MN-ID Option | The total number of binding update deny messages, due to a missing MN-ID option, sent by this system or the specified service.
> Missing HNP Option | The total number of binding update deny messages, due to a missing HNP option, sent by this system or the specified service.
> Missing Access Tech Option | The total number of binding update deny messages, due to a missing access technology option, sent by this system or the specified service.
> Missing Handoff Ind Option | The total number of binding update deny messages, due to a missing handoff indicator option, sent by this system or the specified service.
> Not Authorized For HNP | The total number of binding update deny messages, due to a not authorized for HNP reason, sent by this system or the specified service.
> Not LMA For Mobile | The total number of binding update deny messages, due to a missing LMA for the MN reason, sent by this system or the specified service.
> Not Authorized For Proxy Reg | The total number of binding update deny messages, due to a not authorized for proxy registration reason, sent by this system or the specified service.
> BCE Prefix Do Not Match | The total number of binding update deny messages, due to a BCE prefix not matching, sent by this system or the specified service.
> Update Denied - Insufficient Resource Reasons
> No Session Manager | The total number of binding update deny messages, due to insufficient resources - no session manager, sent by this system or the specified service.
> No Memory | The total number of binding update deny messages, due to insufficient resources - no memory, sent by this system or the specified service.
> Session Manager Rejected | The total number of binding update deny messages, due to insufficient resources - session manager rejected, sent by this system or the specified service.
> Input-Q Exceeded | The total number of binding update deny messages, due to insufficient resources - input queue exceeded, sent by this system or the specified service.
> Simul Bindings Exceeded | The total number of binding update deny messages, due to insufficient resources - simultaneous bindings exceeded, sent by this system or the specified service.
> Address Alloc Failed | The total number of binding update deny messages, due to insufficient resources - address allocation failed, sent by this system or the specified service.
> Update Denied - Admin Prohibited Reasons
> MN-AAA Auth Option Missing | The total number of binding update deny messages, due to an administrator prohibited - MN-AAA auth option missing condition, sent by this system or the specified service.
> H-bit Not Set | The total number of binding update deny messages, due to an administrator prohibited - H-bit not set condition, sent by this system or the specified service.
> Invalid MN-AAA Option SPI | The total number of binding update deny messages, due to an administrator prohibited - invalid MN-AAA option SPI condition, sent by this system or the specified service.
> Invalid MN-HA Option SPI | The total number of binding update deny messages, due to an administrator prohibited - invalid MN-HA option SPI condition, sent by this system or the specified service.
> Congestion Control Denied | The total number of binding update deny messages, due to an administrator prohibited - congestion control denied condition, sent by this system or the specified service.
> Policy Rejected | The total number of binding update deny messages, due to an administrator prohibited - policy rejected condition, sent by this system or the specified service.
> HoA Not Authorized | The total number of binding update deny messages, due to an administrator prohibited - HoA not authorized condition, sent by this system or the specified service.
> No Permission | The total number of binding update deny messages, due to an administrator prohibited - no permission condition, sent by this system or the specified service.
> Bad Request | The total number of binding update deny messages, due to an administrator prohibited - bad request condition, sent by this system or the specified service.
> Binding Updates Discard Reasons
> Congestion Discarded | The total number of binding update discarded messages, due to congestion, sent by this system or the specified service.
> Checksum Error | The total number of binding update discarded messages, due to checksum error(s), sent by this system or the specified service.
> Initial Auth Pending | The total number of binding update discarded messages, due to an initial authentication pending condition, sent by this system or the specified service.
> Session Not Found | The total number of binding update discarded messages, due to a session not found condition, sent by this system or the specified service.
> HAMGR Not Ready | The total number of binding update discarded messages, due to an HA manager not found condition, sent by this system or the specified service.
> Decode Failure | The total number of binding update discarded messages, due to a decode failure, sent by this system or the specified service.
> Invalid Buffer Length | The total number of binding update discarded messages, due to an invalid buffer length, sent by this system or the specified service.
> Revocation Pending | The total number of binding update discarded messages, due to pending revocations, sent by this system or the specified service.
> Binding Revocation
> Sent | The total number of binding revocations sent by this system or the specified service.
> Retries Sent | The total number of binding revocation retries sent by this system or the specified service.
> Ack Rcvd | The total number of binding revocation acknowledgements received by this system or the specified service.
> Not Acknowledged | The total number of binding revocations sent, but not acknowledged, by this system or the specified service.
> Rcvd | The total number of binding revocations received by this system or the specified service.
> Ack Sent | The total number of binding revocation acknowledgements sent by this system or the specified service.
> Sent Revocation Trigger Reasons
> Reserved | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “Reserved” revocation trigger reason.
> Unspecified | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Unspecified” revocation trigger reason.
> Administrative Reason | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Administrative Reason” revocation trigger reason.
> Inter-MAG Handoff-Same ATT | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Inter-MAG Handoff-Same ATT” revocation trigger reason.
> Inter-MAG - Unknown Handoff | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Inter-MAG - Unknown Handoff” revocation trigger reason.
> Inter-MAG Handoff-Diff ATT | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Inter-MAG Handoff-Diff ATT” revocation trigger reason.
> Per-Peer Policy | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “Per-Peer Policy” revocation trigger reason.
> Revoking Node Local Policy | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “Revoking Node Local Policy” revocation trigger reason.
> User Initiated Session Term | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “User Initiated Session Term” revocation trigger reason.
> Access Network Session Term | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Access Network Session Term” revocation trigger reason.
> IPv4 HoA Binding Only | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “IPv4 HoA Binding Only” revocation trigger reason.
> Out-of Sync BCE State | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Out-of Sync BCE State” revocation trigger reason.
> Unknown | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Unknown” revocation trigger reason.
> Received Revocation ACK Status
> Success | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Success” status.
> Partial-Success | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Partial-Success” status.
> Binding-Does-Not-Exist | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Binding-Does-Not-Exist” status.
> No IPv4-HoA-Bind | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “No IPv4-HoA-Bind” status.
> Global-Revoc-Not-Authorized | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Global-Revoc-Not-Authorized” status.
> Cannot-Identify-Binding | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Cannot-Identify-Binding” status.
> Revoc-Failed-MN-Attached | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Revoc-Failed-MN-Attached” status.
> Unknown | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with an “Unknown” status.
> Binding Revocation ACK Discarded
> Total | The total number of binding revocation acknowledgements received and discarded by this system or the specified service.
> Session Not Found | The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by this system or the specified service.
> Badly Formed Request | The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by this system or the specified service.
> Decode Error | The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by this system or the specified service.
> Checksum Error | The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by this system or the specified service.
> Invalid Message Type | The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by this system or the specified service.
> HAMGR Not Ready | The total number of binding revocation acknowledgements received and discarded, due to a HAMGR not ready condition, by this system or the specified service.
> Matching Request Not Found | The total number of binding revocation acknowledgements received and discarded, due to a matching request not found condition, by this system or the specified service.
> Invalid Buffer Length | The total number of binding revocation acknowledgements received and discarded, due to a invalid buffer length condition, by this system or the specified service.
> Tunnel Data Received
> Total Packets | The total number of tunnel packets received by this system or the specified service.
> 6in6 | The total number of IPv6-in-IPv6 tunnel packets received by this system or the specified service.
> 4in6 | The total number of IPv4-in-IPv6 tunnel packets received by this system or the specified service.
> IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel packets received by this system or the specified service.
> IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel packets received by this system or the specified service.
> Total Bytes | The total number of tunnel bytes received by this system or the specified service.
> 6in6 | The total number of IPv6-in-IPv6 tunnel bytes received by this system or the specified service.
> 4in6 | The total number of IPv4-in-IPv6 tunnel bytes received by this system or the specified service.
> IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel bytes received by this system or the specified service.
> IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel bytes received by this system or the specified service.
> Errors
> Protocol Type Error | The total number of protocol type data errors received by this system or the specified service.
> Invalid Pkt Length | The total number of invalid packet length data errors received by this system or the specified service.
> No Session Found | The total number of no session found data errors received by this system or the specified service.
> Tunnel Data Sent
> Total Packets | The total number of tunnel packets sent by this system or the specified service.
> 6in6 | The total number of IPv6-in-IPv6 tunnel packets sent by this system or the specified service.
> 4in6 | The total number of IPv4-in-IPv6 tunnel packets sent by this system or the specified service.
> IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel packets sent by this system or the specified service.
> IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel packets sent by this system or the specified service.
> Total Bytes | The total number of tunnel bytes sent by this system or the specified service.
> 6in6 | The total number of IPv6-in-IPv6 tunnel bytes sent by this system or the specified service.
> 4in6 | The total number of IPv4-in-IPv6 tunnel bytes sent by this system or the specified service.
> IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel bytes sent by this system or the specified service.
> IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel bytes sent by this system or the specified service.
> Tunnel ICMPV6 Packets
> Packet Too Big Rcvd | The total number of tunnel ICMP packets - too big received by this system or the specified service.
> Packet Too Big Dropped | The total number of tunnel ICMP packets - too big dropped by this system or the specified service.
> Packet Too Big Relayed | The total number of tunnel ICMP packets - too big relayed by this system or the specified service.
> Total Disconnects
> Lifetime expiry | The total number of disconnects due to lifetime expiry initiated by this system or the specified service.
> Deregistrations | The total number of disconnects due to deregistrations initiated by this system or the specified service.
> Admin Drops | The total number of disconnects due to admin drops initiated by this system or the specified service.
> Other Reasons | The total number of disconnects due to “other reasons” initiated by this system or the specified service.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883