> Crypto Map IKEv1 Configuration Mode Commands
> The Crypto Map IKEv1 Configuration Mode is used to configure properties for IPSec tunnels that will be created using the Internet Key Exchange (IKE) that operates within the framework of the Internet Key Exchange version 1 (IKEv1).
> Modification(s) to an existing IKEv1 crypto map configuration will not take effect until the related security association has been cleared. Refer to the clear crypto security-association command located in the Exec Mode Commands chapter of the Command Line Interface Reference for more information.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the context configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the context configuration mode.
> match address
> Matches or associates the crypto map to an access control list (ACL) configured in the same context.
> Product
> PDSN, HA, GGSN, SCM
> Privilege
> Security Administrator, Administrator
> Syntax
> match address acl_namepriority
> no match address
> no
> Removes a previously matched ACL.
> acl_name
> The name of the ACL that the crypto map is to be matched with.
> acl_name can be from 1 to 79 alpha and/or numeric characters and is case sensitive.
> priority
> Default: 0
> Specifies the preference of the ACL. The ACL preference is factored when a single packet matches the criteria of more than one ACL.
> The preference can be configured to any integer value from 0 to 4294967295. “0” is the highest priority.
> Important: The priorities are only compared for ACLs matched to other crypto maps or to policy ACLs (those applied to the entire context).
> Usage
> ACLs matched to crypto maps are referred to as crypto ACLs. Crypto ACLs define the criteria that must be met in order for a subscriber data packet to routed over an IPSec tunnel.
> Prior to routing, the system examines the properties of each subscriber data packet. If the packet properties match the criteria specified in the crypto ACL, the system will initiate the IPSec policy dictated by the crypto map.
> Example
> The following command sets the crypto map ACL to the ACL named ACLlist1 and sets the crypto maps priority to the highest level.
> match address ACLlist1 0
> match crypto group
> Matches or associates the crypto map a crypto group configured in the same context.
> Product
> PDSN, HA, GGSN, SCM
> Privilege
> Security Administrator, Administrator
> Syntax
> match crypto group group_name { primary | secondary }
> no match crypto group group_name
> no
> Deletes a previously configured crypto group association.
> group_name
> The name of the crypto group and can consist of from 1 to 127 alpha and/or numeric characters in length and is case sensitive.
> primary
> Specifies that the policies configured as part of this crypto map will be used for the primary tunnel in the Redundant IPSec Tunnel Failover feature.
> secondary
> Specifies that the policies configured as part of this crypto map will be used for the secondary tunnel in the Redundant IPSec Tunnel Failover feature.
> Usage
> Use this command to dictate the primary and secondary tunnel policies used for the Redundant IPSec Tunnel Failover feature.
> At least two policies must be configured to use this feature. One policy must be configured as the primary, the other as the secondary.
> Example
> The following command associates the crypto map to a crypto group called group1 and dictates that it will serve as the primary tunnel policy:
> match crypto group group1 primary
> match ip pool
> Matches the specified IP pool to the current IKEv1 crypto map. This command can be used multiple times to change more than one IP pool.
> Product
> PDSN, HA, GGSN, SCM
> Privilege
> Security Administrator, Administrator
> Syntax
> match ip pool pool-name pool_name
> no match ip pool pool-name pool_name
> no
> Delete the matching statement for the specified IP pool from the crypto map.
> pool_name
> The name of an existing IP pool that should be matched.
> Usage
> Use this command to set the names of IP pools that should be matched in the current crypto map.
> Important: If an IP address pool that is matched to a IKEv1 crypto map is resized, removed, or added, the corresponding security association must be cleared in order for the change to take effect. Refer to the clear crypto command in the Exec mode for information on clearing security associations.
> Example
> The following command sets a rule for the current crypto map that will match an IP pool named ippool1:
> match ip pool pool-name ippool1
> set
> Configures parameters for the dynamic crypto map.
> Product
> PDSN, HA, GGSN, SCM
> Privilege
> Security Administrator, Administrator
> Syntax
> set { control-dont-fragment { clear-bit | copy-bit | set-bit } | ikev1 natt [ keepalive time ] | pfs { group1 | group2 | group5 } | phase1-idtype { id-key-id | ipv4-address [ mode { aggressive | main } ] | phase2-idtype { ipv4-address | ipv4-address-subnet } | security-association lifetime { disable-phase2-rekey | keepalive | kilo-bytes kbytes | seconds secs } transform-set transform_name [ transform-set transform_name2 ... transform-set transform_name6 ]
> no set { ikev1 natt | pfs | phase1-idtype | phase2-idtype | security-association lifetime { disable-phase2-rekey | keepalive | kilo-bytes | seconds } | transform-set transform_name [ transform-set transform_name2 ... transform-set transform_name6 ]
> control-dont-fragment { clear-bit | copy-bit | set-bit }
> Controls the don’t fragment (DF) bit in the outer IP header of the IPsec tunnel data packet. Options are:

> • | clear-bit: Clears the DF bit from the outer IP header (sets it to 0).

> • | copy-bit: Copies the DF bit from the inner IP header to the outer IP header. This is the default action.

> • | set-bit : Sets the DF bit in the outer IP header (sets it to 1).

> ikev1 natt [ keepalive time ]
> Specifies IKE parameters.
> natt: Enables IPSec NAT Traversal.
> keepalive time: The time to keep the NAT connection alive in seconds. time must be an integer of from 1 through 3600 seconds.
> pfs { group1 | group2 | group5 }
> Specifies the modp Oakley group (also known as the Diffie-Hellman (D-H ) group) that is used to determine the length of the base prime numbers that are used for Perfect Forward Secrecy (PFS).

> • | group1 : Diffie-Hellman Group1 (768-bit modp)

> • | group2 :- Diffie-Hellman Group2 (1024-bit modp)

> • | group5 :- Diffie-Hellman Group5 (1536-bit modp)

> phase1-idtype { id-key-id | ipv4-address [ mode { aggressive | main } ]
> Sets the IKE negotiations Phase 1 payload identifier. Default: id-key-id
> id-key-id: ID KEY ID
> ipv4-address: ID IPV4 Address

> • | mode: Configures IKE mode

> • | aggressive: IKE negotiation mode: AGGRESSIVE

> • | main: IKE negotiation mode: MAIN

> phase2-idtype { ipv4-address | ipv4-address-subnet }
> Sets the IKE negotiations Phase 2 payload identifier. Default: ipv4-address-subnet
> ipv4-address: Use IPV4_ADDR as the Phase 2 payload identifier.
> ipv4-address-subnet: Use IPV4_ADDR_SUBNET as the Phase 2 payload identifier.
> security-association lifetime { disable-phase2-rekey | keepalive | kilo-bytes kbytes | seconds secs }
> Defaults:

> • | disable-phase2-rekey: Rekeying is enabled by default

> • | keepalive: Disabled

> • | kilo-bytes: 4608000 kbytes

> • | seconds: 28800 seconds

> This keyword specifies the parameters that determine the length of time an IKE Security Association (SA) is active when no data is passing through a tunnel. When the lifetime expires, the tunnel is torn down. Whichever parameter is reached first expires the SA lifetime.

> • | disable-phase2-rekey : If this keyword is specified, when the lifetime expires, the Phase2 SA is not rekeyed.

> • | keepalive : The SA lifetime expires only when a keepalive message is not responded to by the far end.

> • | kilo-bytes kbytes : This specifies the amount of data in kilobytes to allow through the tunnel before the SA lifetime expires. kbytes must be an integer from 2560 through 4294967294.

> • | seconds secs : The number of seconds to wait before the SA lifetime expires. secs must be an integer from 1200 through 86400.

> Important: If the dynamic crypto map is being used in conjunction with Mobile IP and the Mobile IP renewal timer is less than the crypto map’s SA lifetime (either in terms of kilobytes or seconds), then the keepalive parameter must be configured.
> transform-set transform_name [ transform-set transform_name2 ... transform-set transform_name6 ]
> This keyword specifies the name of a transform set configured in the same context that will be associated with the crypto map. Refer to the command crypto ipsec transform-set for information on creating transform sets.
> You can repeat this keyword up to 6 times on the command line to specify multiple transform sets.
> transform_name is the name of the transform set and must be an alpha and/or numeric string from 1 to 127 characters and is case sensitive.
> no
> Deletes the specified parameter or resets the specified parameter to the default value.
> Usage
> Use this command to set parameters for a dynamic crypto map.
> Example
> The following command sets the PFS group to Group1:
> set pfs group1
> The following command sets the SA lifetime to 50000 KB:
> set security-association lifetime kilo-bytes 50000
> The following command sets the SA lifetime to 10000 seconds:
> set security-association lifetime seconds 10000
> The following command enables the SA to re-key when the tunnel lifetime expires:
> set security-association lifetime keepalive
> The following command defines transform sets tset1 and tset2.
> set transform-set tset1 transform-set tset2

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883