> show srp
> This chapter describes the outputs of the show srp command.
> show srp info
> show srp info Command Output Descriptions

> Field | Description
> Context | Displays the srp context configured for service redundancy protocol. Only one context may be configured with this service.
> Local Address | Displays the local address of the chassis.
> Chassis State | Displays the chassis state (standby or active).
> Chassis Mode | Displays the chassis mode (primary or backup).
> Chassis Priority | Displays the chassis priority. The chassis priority is an integer that determines which chassis is in the active state. The lower number has a higher priority. The priority must be an integer from 1 through 255. Default is 125.
> Local Tiebreaker | Displays the MAC address which is used to determine priority when both chassis have the same priority and route modifier. The lower MAC address has the higher priority.
> Route-Modifier | Displays the modifier which is used to determine which chassis has priority. The lower the number the higher the priority.
> Peer Remote Address | Displays the IP address of the remote peer.
> Peer State | Displays whether the peer is in the active or standby state.
> Peer Mode | Displays the peer mode (standby or active).
> Peer Priority | Displays the peer priority (primary or backup).
> Peer Tiebreaker | Displays the peer MAC address.
> Peer Route-Modifier | Displays the peer’s BGP route modifier.
> Last Hello Message received | Displays a time stamp for the most recent hello message that was received.
> Peer Configuration Validation | Displays the peer configuration validation.
> Last Peer Configuration Error | Displays the most recent error that was received when the chassis was no able to validate its peer configuration.
> Connection State | Displays the status of the redundancy link between the two chassis.

> ‌
> show srp checkpoint statistics
> show srp checkpoint statistics Command Output Descriptions

> Field | Description
> Number of Sessmgrs | Displays the total number of session managers
> Sessmgrs in Active-Connected state | Displays the number of session managers in the active-connected state.
> Sessmgrs in Standby-Connected state | Displays the number of session managers in the standby-connected state.
> Sessmgrs in Pending-Active state | Displays the number of sessions managers in the pending-active state.
> Current Call Recovery Records (CRRs) | Displays the number of current call recovery records.
> Current pre-allocated calls | Displays the number of pre-allocated calls.
> Total id-mapping checkpoint rcvd | Displays the number of id-mapping checkpoints received by the chassis.
> Total APN id-mapping chkpnt rcvd | Displays the number of APN id-mapping checkpoints received by the chassis.
> Total full session checkpoint sent | Displays the number of full session checkpoints sent by the chassis.
> Total micro session checkpoint sent | Displays the number of micro session checkpoints sent by the chassis.
> total inv-crr micro-chkpnt sent | Displays the total number of invalid CRR micro checkpoints sent.
> total call-stats micro-chkpnt sent | Displays the total call statistics micro checkpoints sent.
> Standby call pre-alloc failures | Displays the number of standby call pre allocation failures.
> table-id mapping failures | Displays the number of table id mapping failures.
> aaa session failures | Displays the number of aaa session failures.
> recovery record alloc failures | Displays the number of recovery record allocation failures.
> Standby micro-checkpoint failures | Displays the number of standby micro checkpoint failures.
> recovery record not found | Displays the number of recovery records not found.

> ‌
> show srp statistics
> show srp statistics Command Output Descriptions

> Field | Description
> Peer Remote Address | The IP address for the redundant peer chassis.
> Hello Messages Sent | The number of hello messages that were sent to the peer chassis.
> Hello Message Received | The number of hello messages received from the peer chassis.
> Configuration Validation Messages Sent | The number of configuration validation messages sent to the peer.
> Configuration Validation Message Received | The number of configuration validation messages received from the peer chassis.
> Resource Messages Sent | The number of resource messages sent to the peer chassis.
> Resource Messages Received | The number of resource messages received from the peer chassis.
> Resource Messages Discarded | The number of discarded resource messages.
> Switchover Events | The number of switchover events, where one chassis went from active to inactive and the other chassis went from inactive to active.

> ‌
> show srp monitor
> show srp monitor Command Output Descriptions

> Field | Description
> probe monitor state | Displays the authentication probe monitor state (e.g., success).
> probe monitors up | Displays the number of authentication probe monitors in the active state.
> probe monitors down | Displays the number of authentication probe monitors in the inactive state.
> probe monitors init | Displays the number of authentication probe monitors in the initialized state.
> BGP monitor state | Displays the BGP monitor state (e.g., success).
> BGP monitors up | Displays the number of BGP monitors in the active state.
> BGP monitors down | Displays the number of BGP monitors in the inactive state.
> BGP monitors init | Displays the number of BGP monitors in the initialized state.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883