> MIPv6HA Schema Statistics
> The MIPv6HA schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> MIPv6 HA Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the LAC service. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the LAC service. This is an internal reference number. | Int32
> servname | Displays the name of the LAC service for which the statistics are displayed. | String
> servid | The identification number of the MIPv6 HA service for which the statistics are displayed. | Int32
> num-subscriber | The current total number of MIPv6 HA sessions. | Int32
> aaa-attempt | The number of authentication requests attempted on receiving a bind update request. | Ctr32
> aaa-success | The number of successful authorization attempts. | Ctr32
> aaa-totfail | The number of failed authorization attempts. | Ctr32
> aaa-actauthfail | The authorization attempt failure count due to access rejects from AAA. | Ctr32
> aaa-misauthfail | The authorization attempt failure s due to other reasons like internal error or AAA response timeout. | Ctr32
> bindupdrec-totrec | The total number of MIPv6 bind update requests received. | Ctr32
> bindupdrec-totacc | The total number of MIPv6 bind update requests accepted. | Ctr32
> bindupdrec-totdeny | The total number of MIPv6 bind update requests denied. | Ctr32
> bindupdrec-totdisc | The total number of MIPv6 bind update requests discarded. | Ctr32
> bindupdrec-totcongdiscreq | The total number of MIPv6 bind update requests discarded because of congestion. | Ctr32
> ibindupdreq-receive | The total number of initial bind update requests received. | Ctr32
> ibindupdreq- accept | The total number of initial bind update requests accepted. | Ctr32
> ibindupdreq-deny | The total number of initial bind update requests denied. | Ctr32
> rbindupdreq- receive | The total number of renew bind update requests received. | Ctr32
> rbindupdreq-accept | The total number of renew bind update requests accepted. | Ctr32
> rbindupdreq-deny | The total number of renew bind update requests denied. | Ctr32
> deregreq-receive | The total number of dereg bind update requests received. | Ctr32
> deregreq-accept | The total number of dereg bind update requests accepted. | Ctr32
> deregreq-deny | The total number of dereg bind update requests denied. | Ctr32
> horeq-receive | The total number of handoff bind update requests received. A handoff bind update request is a bind update request received for the same session (NAI/HA/HoA) with a new CoA. | Ctr32
> horeq-accept | The total number of handoff requests accepted. | Ctr32
> horeq-deny | The total number of handoff requests denied. | Ctr32
> bindacksent-total | The total number of MIPv6 binding acknowledgement messages sent. | Ctr32
> bindacksent-acceptreg | The total number of MIPv6 binding acknowledgement replies sent. | Ctr32
> bindacksent-acceptdereg | The total number of MIPv6 dereg replies sent (bind acknowledgement with a lifetime of zero). | Ctr32
> bindacksent-deny | The total number of denied bind acknowledgement replies sent. | Ctr32
> denyreason -badreq | The total number of bind updates denied with status code 81H due to poorly formed bind update request. | Ctr32
> denyreason -mismatchid | The total number of bind update denied with status code 90H (mismatched id). | Ctr32
> denyreason-mnauthfail | The total number of bind update denied with status code 92H (mobile auth failure). | Ctr32
> denyreason-admprohibit | The total number of bind update denied with status code 81H (Admin prohibited). | Ctr32
> denyreason-noresource | The total number of bind update denied with status code 82H (Insufficient resources). | Ctr32
> denyreason-simbindexceed | The total number of bind update denied with status code 82H because simultaneous binding limit is exceeded. | Ctr32
> denyreason-unspereason | The total number of bind update denied with status code 80H (Reason Unspecified). | Ctr32
> denyreason-msgidrequire | The total number of bind update denied with status code 91H (Mesg-Id-Required). | Ctr32
> denyreason-dadfail | The total number of bind update denied with status code 86H (Duplicate Address Detection failed). | Ctr32
> denyreason-nothomesubnet | The total number of bind update denied with status code 84H (Not Home Subnet). | Ctr32
> denyreason-seqoutwindow | The total number of bind update denied with status code 87H (Sequence number Out of Window). | Ctr32
> denyreason-regchadisallow | The total number of bind update denied with status code 8BH (Registration Type change disallowed). | Ctr32
> datareceive-totpkt | The total number of tunneled data packets received. | Ctr32
> datareceive-totpkt6in6 | The total number of ipv6-ipv6 tunneled data packets received. | Ctr32
> datareceive-totbyte | The total byte count of the tunnel data received | Ctr32
> datareceive-totbyte6in6 | The total byte count of ipv6-ipv6 tunneled data received | Ctr32
> datareceive-errorprotocol | The total number of packets received with protocol type error. | Ctr32
> datareceive-errorinvpkt | The total number of invalid data packets received | Ctr32
> datareceive-errornosess | The total number of data packets received for which session was not found. | Ctr32
> datasent- totpkt | The total number of tunnel data packet sent | Ctr32
> datasent- totpkt6in6 | The total number of ipv6-ipv6 tunneled data packets sent | Ctr32
> datasent-totbyte | The total byte count of tunneled data sent | Ctr32
> datasent- totbyte6in6 | The total byte count for ipv6-ipv6 tunneled data sent | Ctr32
> disconnect-lifetimeexp | The total number of session disconnected due to lifetime expiry | Ctr32
> disconnect-deregistration | The total number of disconnects due to deregistration from MN. | Ctr32
> disconnect-admdrop | The total number of sessions disconnected administratively. | Ctr32
> disconnect-othreason | The total number of sessions disconnects due to other reasons. | Ctr32
> icmpv6-toobigreceive | The total number of ICMPv6 Packet too big received for tunneled packets originating within tunnel. | Ctr32
> icmpv6-toobigforward | The total number of ICMPv6 packet too big forwarded messages | Ctr32
> total-subscriber |  | Ctr32
> admprohreason-badreq | Number of updates denied for an Admin prohibited reason: bad request | Ctr32
> insufresource-badreq | Number of binding updates denied | Ctr32
> bindacksent-senderror | The total number of binding acknowledgements sent with a send error | Ctr32
> admprohreason-congcondenied | Number of updates denied for an Admin prohibited reason: congestion control denied | Ctr32
> icmpv6-toobigdrop | Number of ICMPv6 packets dropped because they are too big and need to be fragmented. | Ctr32
> bindupddiscard-congdisc | Number of binding updates discarded because HAMGR is configured to drop packets on congestion | Ctr32
> bindupddiscard-chkerror | Number of bind updates discarded because of a checksum error on binding update. | Ctr32
> bindupddiscard-iniauthpend | Number of bind updates discarded because initialization authorization is pending when retry binding updates are received | Ctr32
> bindupddiscard-sessnotfound | Number of bind updates discarded because hamgr forwards RRQ for existing session but session not found in Sessmgr | Ctr32
> bindupddiscard-hamgrnotrea | Number of bind updates discarded because HAMGR is not yet ready and packet buffering limit is exceeded | Ctr32
> bindupddiscard-decfail | Number of binding updates discarded because the binding update packet decoding has failed in HAMGR. | Ctr32
> bindupddiscard-invbuflen | Number of bind updates discarded because there is mismatch in the binding update packet buffer length and expected length. | Ctr32
> admprohreason-authoptmiss | Number of bind updates denied because there are Admin Prohibited Reasons-MN-AAA Auth Option Missing. | String
> admprohreason-hbitnotset | Number of bind updates denied because there are Admin Prohibited Reasons-H-bit Not Set. | String
> admprohreason-invaaaspi | Number of bind updates denied because there are Admin Prohibited Reasons-Invalid MN-AAA Option SPI. | String
> admprohreason-invhaspi | Number of bind updates denied because there are Admin Prohibited Reasons-Invalid MN-HA Option SPI. | String
> admprohreason-polrej | Number of bind updates denied because there are Admin Prohibited Reasons-Policy Rejected. | String
> admprohreason-notauth | Number of bind updates denied because there are Admin Prohibited Reasons-HoA Not Authorized. | String
> admprohreason-noperm | Number of bind updates denied because there are Admin Prohibited Reasons-No Permission. | String
> insufresource-nosessmgr | Number of bind updates denied because there are Insufficient Resource Reasons-No Session Manager. | String
> insufresource-nomem | Number of bind updates denied because there are Insufficient Resource Reasons-No Memory. | String
> insufresource-sessmgrrej | Number of bind updates denied because there are Insufficient Resource Reasons-Session Manager Rejected. | String
> insufresource-ipqexc | Number of bind updates denied because there are Insufficient Resource Reasons-Input-Q Exceeded. | String
> insufresource-simbindexc | Number of bind updates denied because there are Insufficient Resource Reasons-Simul Bindings Exceeded. | String
> tun-conn-attempt | The total number of tunnel connection attempts. | Int32
> tun-conn-success | The total number of successful tunnel connections. | Int32
> tun-conn-fail | The total number of failed tunnel connections. | Int32
> tun-conn-curactive | The total number of currently active tunnel connections. | Int32
> sess-attempts | The total number of session connection attempts. | Int32
> sess-successful | The total number of successful session connections. | Int32
> sess-failed | The total number of failed session connections. | Int32
> sess-curactive | The total number of currently active session connections. | Int32
> sess-intrapdsnho-attempt | The total number of Intra-PDSN Hand-Offs connection attempts. | Int32
> sess-intrapdsnho-success | The total number of successful Intra-PDSN Hand-Offs connections. | Int32
> sess-intrapdsnho-failed | The total number of failed Intra-PDSN Hand-Offs connections. | Int32
> sess-interpdsnho-attempt | The total number of Inter-PDSN Hand-Offs connection attempts. | Int32
> recv-err-malformed | The total number of Tunnel Receive Control Packet errors experienced due to malformed packets . | Int32
> recv-err-ctrlfield | The total number of Tunnel Receive Control Packet errors experienced due to control field errors. | Int32
> recv-err-pktlen | The total number of Tunnel Receive Control Packet errors experienced due to packet length errors. | Int32
> recv-err-avplen | The total number of Tunnel Receive Control Packet errors experienced due to AVP length errors. | Int32
> recv-err-protover | The total number of Tunnel Receive Control Packet errors experienced due to protocol version errors. | Int32
> recv-err-md5 | The total number of Tunnel Receive Control Packet errors experienced due to MD5 errors. | Int32
> recv-err-invattr | The total number of Tunnel Receive Control Packet errors experienced due to invalid attribute errors. | Int32
> recv-err-unkattr | The total number of Tunnel Receive Control Packet errors experienced due to unknown attribute errors. | Int32
> recv-err-invsessid | The total number of Tunnel Receive Control Packet errors experienced due to invalid session ID errors. | Int32
> recv-err-invstate | The total number of Tunnel Receive Control Packet errors experienced due to invalid state errors. | Int32
> recv-err-unkmsg | The total number of Tunnel Receive Control Packet errors experienced due to unknown message errors. | Int32
> recv-err-unmatchpktlen | The total number of Tunnel Receive Control Packet errors experienced due to unmatched packet length errors. | Int32
> recv-err-invtunid | The total number of Tunnel Receive Control Packet errors experienced due to invalid tunnel length errors. | Int32
> tun-genclear | The total number of tunnels cleared normally. | Int32
> tun-ctrlconnexists | The total number of tunnel disconnects/failures experienced due to a pre-existing control connection. | Int32
> tun-unauth | The total number of tunnel disconnects/failures experienced due to unauthorized errors. | Int32
> tun-badproto | The total number of tunnel disconnects/failures experienced due to bad protocol errors. | Int32
> tun-reqshutdown | The total number of tunnel disconnects experienced due to requester shutdown. | Int32
> tun-statemacherr | The total number of tunnel disconnects/failures experienced due to state machine errors. | Int32
> tun-badlen | The total number of tunnel disconnects/failures experienced due to wrong length errors. | Int32
> tun-oor | The total number of tunnel disconnects/failures experienced due to out-of-range errors. | Int32
> tun-noresource | The total number of tunnel disconnects/failures experienced due to insufficient resources. | Int32
> tun-vendspec | The total number of tunnel disconnects/failures experienced due to vendor-specific errors. | Int32
> tun-tryanotherlns | The total number of tunnel disconnects/failures experienced resulting in “Try Another LNS” message generation. | Int32
> tun-unkavp | The total number of tunnel disconnects/failures experienced due to unknown AVP with M-bit errors. | Int32
> tun-ipsecdisc | The total number of tunnel disconnects experienced due to IPSEC. | Int32
> tun-ipsecfail | The total number of tunnel failures experienced due to IPSEC. | Int32
> tun-license | The total number of tunnel disconnects/failures experienced due to license exceeded errors. | Int32
> tun-newcallpoldisc | The total number of tunnel disconnects experienced due to new call policies. | Int32
> tun-maxretry | The total number of tunnel disconnects/failures experienced due to the maximum number of retries being exceeded. | Int32
> tun-syslimit | The total number of tunnel disconnects/failures experienced due to reaching the system tunnel limit. | Int32
> tun-miscerr | The total number of tunnel disconnects/failures experienced due to miscellaneous errors. | Int32
> sess-nogeneral | The total number of sessions for which there were no general errors experienced. | Int32
> sess-admin | The total number of session disconnects/failures experienced due to administrative reasons. | Int32
> sess-lossofcarr | The total number of session disconnects/failures experienced due to loss of carrier. | Int32
> sess-remoteadmin | The total number of session disconnects/failures experienced due to remote administrative reasons. | Int32
> sess-nofactemp | The total number of session disconnects/failures experienced due to temporary no facility available errors. | Int32
> sess-nofacperm | The total number of session disconnects/failures experienced due to permanent no facility available errors. | Int32
> sess-invdest | The total number of session disconnects/failures experienced due to invalid destination errors. | Int32
> sess-nocarrier | The total number of session disconnects/failures experienced due no carrier being detected. | Int32
> sess-busysig | The total number of session disconnects/failures experienced due to receipt of a busy signal. | Int32
> sess-nodialtime | The total number of session disconnects/failures experienced due to receipt of no dial tone. | Int32
> sess-lactimeout | The total number of session disconnects/failures experienced due to LAC timeout. | Int32
> sess-noframing | The total number of session disconnects/failures experienced due to no appropriate framing. | Int32
> sess-noctrlconn | The total number of session disconnects/failures experienced due to no control connection existing. | Int32
> sess-badlen | The total number of session disconnects/failures experienced due to wrong length errors. | Int32
> sess-oor | The total number of session disconnects/failures experienced due to out-of-range errors. | Int32
> sess-noresource | The total number of session disconnects/failures experienced due to insufficient resources. | Int32
> sess-invsessid | The total number of session disconnects/failures experienced due to an invalid session ID. | Int32
> sess-vendspec | The total number of session disconnects/failures experienced due to vendor specific errors. | Int32
> sess-tryanotherlns | The total number of session disconnects/failures experienced resulting in “Try Another LNS” message generation. | Int32
> sess-unkavp | The total number of session disconnects/failures experienced due to unknown AVP with M-bit errors. | Int32
> sess-maxtunnel | The total number of session disconnects/failures experienced due to reaching the maximum tunnel limit. | Int32
> sess-ipsecfail | The total number of session failures experienced due to IPSEC. | Int32
> sess-ipsecdisc | The total number of session disconnects experienced due to IPSEC. | Int32
> sess-newcallpoldisc | The total number of session disconnects experienced due to new call policies. | Int32
> sess-license | The total number of session disconnects/failures experienced due to license exceeded errors. | Int32
> sess-servmismatch | The total number of session disconnects/failures experienced due to service mismatch errors. | Int32
> sess-miscerr | The total number of session disconnects/failures experienced due to miscellaneous errors. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883