> Content Filtering Application MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the Content Filtering service applications.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfCommonMIB(1)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfCommonMIB(1).starCfCommonMIBObjects(1)

> Object: | starCfNotifRaisedTime

> Object ID: | enterprises.8164.1.100.1.1.1

> Description: | This object indicates the time when this notification was generated.

> Syntax: | TimeStamp

> Access: | read-only

> Object: | starCfthresholdConfigured

> Object ID: | enterprises.8164.1.100.1.1.2

> Description: | This object indicates the current configured threshold value of process monitoring.

> Syntax: | DisplayString (SIZE (1..10))

> Access: | read-only

> Object: | starCfthresholdMeasured

> Object ID: | enterprises.8164.1.100.1.1.3

> Description: | This object indicates the current measured threshold value of process monitoring.

> Syntax: | DisplayString (SIZE (1..10))

> Access: | read-only

> Object: | starCfIPAddr

> Object ID: | enterprises.8164.1.100.1.1.4

> Description: | This object indicates the IP address of IMG.

> Syntax: | InetAddress

> Access: | read-only

> Object: | starCfNotifInfo

> Object ID: | enterprises.8164.1.100.1.1.5

> Description: | This object contains a textual description of notification with additional information besides alarm types. If the test of the message exceeds 64 bytes, the messages will be truncated to 63 bytes with a ‘*’ character appended to indicate the messages is truncated.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | read-only

> Object: | starCfEmsMcrdbsHostAddress

> Object ID: | enterprises.8164.1.100.1.1.6

> Description: | The object indicates the IP address of MCRDBS.

> Syntax: | InetAddress

> Access: | read-only

> Object: | starCfEmsDbType

> Object ID: | 8164.1.100.1.1.7

> Description: |

> Syntax: | INTEGER

> Access: | read-only

> Objects: | sfmdb(1) sfmdbinc(2) optcmdb(6) optcmdbinc(7)

> Object: | starCfEmsSourceDbFileName

> Object ID: | 8164.1.100.1.1.8

> Description: | This object indicates name of the file whose SFTP/Conversion is failed.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | read-only

> Object: | starCfEmsCdpHostAddress

> Object ID: | 8164.1.100.1.1.9

> Description: | The object indicates the IP address of CDP.

> Objects: | sfmdb(1) sfmdbinc(2)

> Object: | starCfEmsToDbType

> Object ID: | 8164.1.100.1.1.10

> Description: |

> Objects: | optcmdb(6) optcmdbinc(7)

> Object Group: | starCfEmsDestDbFileName

> Object ID: | 8164.1.100.1.1.11

> Description: | his object indicates name of the destination file, this used to specify destination file created after conversion.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | read-only

> Object: | starCfEmsFtpHostInfo

> Object ID: | 8164.1.100.1.1.12

> Description: | The object indicates the IP address of Host used for FTP.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | read-only

> Object: | starCfEmsServerProcStart

> Object ID: | 8164.1.100.1.1.13

> Description: | This notification is generated by CFEMS when CFEMS server process comes up.

> Object: | starCfEmsServerProcStop

> Object ID: | 8164.1.100.1.1.14

> Description: | This notification is generated by CFEMS when CFEMS server process goes down.

> Object: | starCfEmsDbImportFailed

> Object ID: | 8164.1.100.1.1.15

> Description: | This notification is generated by CFEMS when failed to Import Database file.

> Objects: | starCfNotifRaisedTime starCfEmsMcrdbsHostAddress starCfEmsDbType starCfEmsSourceDbFileName

> Object Group: | starCfEmsDbImportSucceeded

> Object ID: | 8164.1.100.1.1.16

> Description: | This notification is generated by CFEMS Database file is imported successfully.

> Objects: | starCfNotifRaisedTime starCfEmsMcrdbsHostAddress starCfEmsDbType starCfEmsSourceDbFileName

> Object Group: | starCfEmsDbExportFailed

> Object ID: | 8164.1.100.1.1.17

> Description: | This notification is generated by CFEMS when failed to Export Database file.

> Objects: | starCfNotifRaisedTime starCfEmsCdpHostAddress starCfEmsDbType

> Object Group: | starCfEmsDbConversionFailed

> Object ID: | 8164.1.100.1.1.18

> Description: | This notification is generated by CFEMS when Database conversion fails.

> Objects: | starCfNotifRaisedTime starCfEmsFromDbType starCfEmsToDbType starCfEmsSourceDbFileName starCfEmsDestDbFileName

> Object Group: | starCfEmsDbConversionSucceeded

> Object ID: | 8164.1.100.1.1.19

> Description: | This notification is generated by CFEMS when Database conversion done successfully.

> Objects: | starCfNotifRaisedTime starCfEmsFromDbType starCfEmsToDbType starCfEmsSourceDbFileName starCfEmsDestDbFileName

> Object Group: | starCfEmsFtpConnetionFailed

> Object ID: | 8164.1.100.1.1.20

> Description: | This notification is generated by CFEMS when FTP connection fails.

> Objects: | starCfNotifRaisedTime starCfEmsFtpHostInfo

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCOMMONMIB(1).starCFCOMMONMIBTraps(2)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCOMMONMIB(1)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3).
> starCFCOMMONMIBCompliances(1)

> Object: | starCFCOMMONMIBCompliance

> Object ID: | enterprises.8164.1.100.1.3.1.1

> Description: | The compliance statements for entities which implement the STARENT CF MIB.

> Objects: | starCFCOMMONNotifMgmtGroup

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCOMMONMIB(1).starCFCOMMONMIBConformances(3).
> starCFCOMMONMIBGroup(2)

> Object Group: | starCFCOMMONNotifMgmtGroup

> Object ID: | enterprises.8164.1.100.1.3.2.1

> Description: | A collection of objects related with notification management on CF-Common.

> Objects: | starCfNotifRaisedTime starCfThresholdConfigured starCfThresholdMeasured starCfIPAddr starCfNotifInfo

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCDPMIB(2)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCDPMIB(2).starCFCDPMIBTraps(2)

> Object: | starCfCdpStart

> Object ID: | enterprises.8164.1.100.2.2.1

> Description: | This notification is generated when CDP server starts and CF-CDP server process comes up.

> Objects: | starCfNotifRaisedTime starCfNotifInfo

> Object: | starCfCdpStop

> Object ID: | enterprises.8164.1.100.2.2.2

> Description: | This notification is generated when CDP server stops and CF-CDP server process goes down.

> Objects: | starCfNotifRaisedTime starCfNotifInfo

> Object: | starCfCdpRestart

> Object ID: | enterprises.8164.1.100.2.2.3

> Description: | This notification is generated when CDP server restarts and CF-CDP server process again comes up.

> Objects: | starCfNotifRaisedTime starCfNotifInfo

> Object: | starCfCdpProcApiOpFailed

> Object ID: | enterprises.8164.1.100.2.2.4

> Description: | This notification is generated by CF-CDP when the CFLIB API Operation fails.

> Objects: | starCfNotifRaisedTime starCfParseFileName starCfNotifInfo

> Object: | starCfCdpApiVerError

> Object ID: | enterprises.8164.1.100.2.2.5

> Description: | Notification generated by CF-CDP when the CFLIB DB Version Error occurs.

> Objects: | starCfNotifRaisedTime starCfParseFileName starCfNotifInfo

> Object: | starCfCdpThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.2.2.6

> Description: | This notification is generated by CF-System when the CDP process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current CDP process’s CPU usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfCdpClearThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.2.2.7

> Description: | This notification is generated by CF-System when the CDP process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current CDP process’s CPU usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfCdpThreshDiskUtilization

> Object ID: | enterprises.8164.1.100.2.2.8

> Description: | This notification is generated by CF-System when the CDP process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current CDP process’s disk usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfCdpClearThreshDiskUtilization

> Object ID: | enterprises.8164.1.100.2.2.9

> Description: | This notification is generated by CF-System when the CDP process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current CDP process’s disk usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfCdpThreshSwapUtilization

> Object ID: | enterprises.8164.1.100.2.2.10

> Description: | This notification is generated by CF-System when the CDP process’s swap usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current CDP process’s swap usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfCdpClearThreshSwapUtilization

> Object ID: | enterprises.8164.1.100.2.2.11

> Description: | This notification is generated by CF-System when the CDP process’s swap usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current CDP process’s swap usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfCdpProcReportErrWithMsg

> Object ID: | enterprises.8164.1.100.2.2.12

> Description: | This notification is generated by CF-CDP when any system error is generated by CFLIB API.

> Objects: | starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo

> Object: | StarCfCdpProcApiCfdcmErrWithMsg

> Object ID: | enterprises.8164.1.100.2.2.13

> Description: | This notification is generated by CFDCM Library when any error other than system error occurs.

> Objects: | starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCDPMIB(2).starCFCDPMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCDPMIB(2).starCFCDPMIBConformances(3).
> starCFCDPMIBCompliances(1)

> Object: | starCFCDPMIBCompliance

> Object ID: | enterprises.8164.1.100.2.3.1.1

> Description: | The compliance statements for entities which implement the STARENT CF-CDP MIB.

> Objects: | starCFCDPNotifMgmtGroup starCFCDPNotifGroup

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCDPMIB(2).starCFCDPMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCDPMIB(2).starCFCDPMIBConformances(3).
> starCFCDPMIBGroup(2)

> Object Group: | starCFCDPNotifMgmtGroup

> Object ID: | enterprises.8164.1.100.2.3.2.1

> Description: | A collection of objects related with notification management on CF-CDP.

> Objects: | starCfParseFileName

> Object Group: | starCFCDPNotifGroup

> Object ID: | enterprises.8164.1.100.2.3.2.2

> Description: | A collection of CF-CDP notifications.

> Objects: | starCfCdpStart starCfCdpStop starCfCdpRestart starCfCDPApiOpFailed starCfCdpApiVerError starCfCdpThreshCPUUtilization starCfCdpClearThreshCPUUtilization starCfCdpThreshDiskUtilization starCfCdpClearThreshDiskUtilization starCfCdpThreshSwapUtilization starCfCdpClearThreshSwapUtilization starCfCdpProcReportErrWithMsg, StarCfCdpProcApiCfdcmErrWithMsg starCfCdpProcApiPermissionDenied starCfCdpProcApiInvalidAgrs

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFREMIB(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFREMIB(3).starCFREMIBObjects(1)

> Object: | starCfParseFileName

> Object ID: | enterprises.8164.1.100.3.1.1

> Description: | This object indicates name of the file getting parsed by the Report Engine.

> Syntax: | DisplayString (SIZE (1..64))

> Access: | read-only

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFREMIB(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFREMIB(3).starCFREMIBTraps(2)

> Object: | starCfReStart

> Object ID: | enterprises.8164.1.100.3.2.1

> Description: | This notification is generated when Report Engine starts and CF-RE process comes up.

> Objects: | starCfNotifRaisedTime

> Object: | starCfReStop

> Object ID: | enterprises.8164.1.100.3.2.2

> Description: | This notification is generated when Report Engine stops and CF-RE process goes down.

> Objects: | starCfNotifRaisedTime

> Object: | starCfReRestart

> Object ID: | enterprises.8164.1.100.3.2.3

> Description: | This notification is generated when Report Engine restarts and CF-RE process restart is detected.

> Objects: | starCfNotifRaisedTime

> Object: | starCfReFileParsingAborted

> Object ID: | enterprises.8164.1.100.3.2.4

> Description: | This notification is generated by CF-RE when Report Engine fails to parse EDR.

> Objects: | starCfNotifRaisedTime starCfParseFileName

> Object: | starCfReThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.3.2.5

> Description: | This notification is generated by CF-System when the Report Engine process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Report Engine process’s CPU usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfReClearThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.3.2.6

> Description: | This notification is generated by CF-System when the Report Engine process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Report Engine process’s CPU usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfReThreshDiskUtilization

> Object ID: | enterprises.8164.1.100.3.2.7

> Description: | This notification is generated by CF-System when the Report Engine process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Report Engine process’s disk usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfReClearThreshDiskUtilization

> Object ID: | enterprises.8164.1.100.3.2.8

> Description: | This notification is generated by CF-System when the Report Engine process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Report Engine process’s disk usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfDbThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.3.2.9

> Description: | This notification is generated by CF-System when the Postgres process’s CPU usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Postgres process’s CPU usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfDbClearThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.3.2.10

> Description: | This notification is generated by CF-System when the Postgres process’s CPU usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Postgres process’s CPU usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfDbThreshDiskUtilization

> Object ID: | enterprises.8164.1.100.3.2.11

> Description: | This notification is generated by CF-System when the Postgres process’s disk usage threshold exceeds the configured limit. The starCfThresholdMeasured indicates the current Postgres process’s disk usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> Object: | starCfDbClearThreshDiskUtilization

> Object ID: | enterprises.8164.1.100.3.2.12

> Description: | This notification is generated by CF-System when the Postgres process’s disk usage comes back to below the threshold limit. The starCfThresholdMeasured indicates the current Postgres process’s disk usage in percentage.

> Objects: | starCfNotifRaisedTime starCfThresholdMeasured

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFREMIB(3).starCFREMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFREMIB(3).starCFREMIBConformances(3).
> starCFREMIBCompliances(1)

> Object: | starCFEMSMIBCompliance

> Object ID: | enterprises.8164.1.100.3.3.1.1

> Description: | The compliance statements for entities which implement the STARENT CF MIB.

> Objects: | starCFEMSNotifMgmtGroup starCFEMSNotifGroup

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfReMIB(3).starCfReMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfReMIB(3).starCfReMIBConformances(3).starCfReMIBGroup(2)

> Object Group: | starCFEMSNotifMgmtGroup

> Object ID: | enterprises.8164.1.100.3.3.2.1

> Description: | A collection of objects related with notification management on CF Report Engine.

> Objects: | starCfEmsMcrdbsHostAddress starCfEmsDbType starCfEmsSourceDbFileName starCfEmsCdpHostAddress starCfEmsFromDbType starCfEmsToDbType starCfEmsDestDbFileName

> Object Group: | starCFRENotifGroup

> Object ID: | enterprises.8164.1.100.3.3.2.2

> Description: | A collection of CF-CDP notifications.

> Objects: | starCfReStart starCfReStop starCfReRestart starCfReFileParsingAborted starCfReThreshCPUUtilization starCfReClearThreshCPUUtilization starCfReThreshDiskUtilization starCfReClearThreshDiskUtilization starCfDbThreshCPUUtilization starCfDbClearThreshCPUUtilization starCfDbThreshDiskUtilization starCfDbClearThreshDiskUtilization

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCCIMIB(4).starCFCCIMIBObjects(1)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCCIMIB(4).starCFCCIMIBTraps(2)

> Object: | starCfCciApplicationStart

> Object ID: | enterprises.8164.1.100.4.2.1

> Description: | This notification is generated when Customer Care Interface application starts.

> Objects: | starCfNotifRaisedTime starCfIPAddr starCfNotifInfo

> Object: | starCfCciApplicationStop

> Object ID: | enterprises.8164.1.100.4.2.2

> Description: | This notification is generated when Customer Care Interface application stops.

> Objects: | starCfNotifRaisedTime starCfIPAddr starCfNotifInfo

> Object: | starCfCciCdpServerReachable

> Object ID: | enterprises.8164.1.100.4.2.3

> Description: | This notification is generated when CDP server is reachable for Customer Care Interface application. This can be the result of a server startup or a previously unreachable server is now reachable.

> Objects: | starCfNotifRaisedTime starCfIPAddr starCfNotifInfo

> Object: | starCfCciCdpServerUnreachable

> Object ID: | enterprises.8164.1.100.4.2.4

> Description: | This notification is generated when Customer Care Interface application is unable to communicate with a CDP server.

> Objects: | starCfNotifRaisedTime starCfIPAddr starCfNotifInfo

> Object: | starCfCciThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.4.2.5

> Description: | This notification is generated by CF-System when the overall CPU usage of CCI application exceeds the configured limit for the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm model, a starCfCciClearThreshCPUUtilization notification is generated when the measured value falls below the threshold.

> Objects: | starCfNotifRaisedTime starCfThresholdConfigured starCfThresholdMeasured starCfNotifInfo

> Object: | starCfCciClearThreshCPUUtilization

> Object ID: | enterprises.8164.1.100.4.2.6

> Description: | This notification is generated when CPU utilization threshold is clear.

> Syntax: | starCfNotifRaisedTime starCfThresholdConfigured starCfThresholdMeasured starCfNotifInfo

> Object: | starCfCciThreshMemoryUtilization

> Object ID: | enterprises.8164.1.100.4.2.7

> Description: | This notification is generated by CF-System when the overall memory usage of CCI application exceeds the configured limit for the current monitoring period. Probable Cause: This is a user-configurable threshold. Condition Clear Alarm: If the thresholding subsystem is configured to run in an 'alarm' model, a starCfCciClearThreshmemoryUtilization notification will be generated when the measured value falls below the threshold.

> Objects: | starCfNotifRaisedTime starCfThresholdConfigured starCfThresholdMeasured starCfNotifInfo

> Object: | starCfCciClearThreshMemoryUtilization

> Object ID: | enterprises.8164.1.100.4.2.8

> Description: | This notification is generated when memory utilization threshold is clear.

> Syntax: | starCfNotifRaisedTime starCfThresholdConfigured starCfThresholdMeasured starCfNotifInfo

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfCciMIB(4).starCfCciMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfCciMIB(4).starCfCciMIBConformances(3).
> starCfCciMIBCompliances(1)

> Object: | starCFCCIMIBCompliance

> Object ID: | enterprises.8164.1.100.4.3.1.1

> Description: | The compliance statements for entities which implement the STARENT CF-CCI MIB.

> Objects: | starCFCCINotifGroup

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFCCIMIB(4)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfCciMIB(4).starCfCciMIBConformances(3).starCfCciMIBGroup(2)

> Object Group: | starCFEMSNotifGroup

> Object ID: | enterprises.8164.1.100.4.3.2.1

> Description: | A collection of CF-CDP notifications.

> Objects: | starCfEmsServerProcStart starCfEmsServerProcStop starCfEmsDbImportFailed starCfEmsDbImportSucceeded starCfEmsDbExportFailed starCFEMSDbExportSucceeded starCfEmsDbConversionFailed starCfEmsDbConversionSucceeded starCfEmsFtpConnetionFailed

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6).starCFMCRDBSMIBObjects(1)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6).starCFMCRDBSMIBTraps(2)

> Object: | starCfMdbProcStart

> Object ID: | enterprises.8164.1.100.6.2.1

> Description: | This notification is generated when MCRDBS server starts and CF-MCRDBS server process comes up.

> Objects: | starCfNotifRaisedTime starCfNotifInfo

> Object: | starCfMdbProcStop

> Object ID: | enterprises.8164.1.100.6.2.2

> Description: | This notification is generated when MCRDBS server stops and CF-MCRDBS server process goes down.

> Objects: | starCfNotifRaisedTime starCfNotifInfo

> Object: | starCfMdbProcDbAbsent

> Object ID: | enterprises.8164.1.100.6.2.3

> Description: | This notification is generated by CF-MCRDBS when the required database for conversion is absent.

> Objects: | starCfNotifRaisedTime starCfParseFileName starCfNotifInfo

> Object: | starCfMdbProcApiOpFailed

> Object ID: | enterprises.8164.1.100.6.2.4

> Description: | This notification is generated by CF-MCRDBS when the CFLIB API Operation fails.

> Objects: | starCfNotifRaisedTime starCfParseFileName starCfNotifInfo

> Object: | starCfMdbProcDbParseError

> Object ID: | enterprises.8164.1.100.6.2.5

> Description: | This notification is generated by CF-MCRDBS when the database merging fails due to the parse error.

> Objects: | starCfNotifRaisedTime starCfParseFileName starCfNotifInfo

> Object: | starCfMdbProcMemUsageOverLimit

> Object ID: | enterprises.8164.1.100.6.2.6

> Description: | Notification generated by CF when memory usage threshold for MCRDBS process is exceeded. The starCFThresholdMeasured varbind indicates process memory usage as a percentage.

> Objects: | starCfNotifRaisedTime starCfNotifInfo starCfThresholdMeasured

> Object: | starCfMdbProcMemUsageNormal

> Object ID: | enterprises.8164.1.100.6.2.7

> Description: | Notification generated by CF when memory usage threshold for MCRDBS process is normal. The starCFThresholdMeasured varbind indicates process memory usage as a percentage.

> Objects: | starCfNotifRaisedTime starCfNotifInfo starCfThresholdMeasured

> Object: | starCfMdbProcCpuUsageOverLimit

> Object ID: | enterprises.8164.1.100.6.2.8

> Description: | Notification generated by CF when processor cpu threshold for MCRDBS process is exceeded. The starCFThresholdMeasured varbind indicates process cpu usage as a percentage.

> Objects: | starCfNotifRaisedTime starCfNotifInfo starCfThresholdMeasured

> Object: | starCfMdbProcCpuUsageNormal

> Object ID: | enterprises.8164.1.100.6.2.9

> Description: | Notification generated by CF when processor cpu threshold for MCRDBS process is normal. The starCFThresholdMeasured varbind indicates process cpu usage as a percentage.

> Objects: | starCfNotifRaisedTime starCfNotifInfo starCfThresholdMeasured

> Object: | starCfMdbProcDiskUsageOverLimit

> Object ID: | enterprises.8164.1.100.6.2.10

> Description: | Notification generated by CF when disk usage threshold for MCRDBS process is exceeded. The starCFThresholdMeasured varbind indicates process disk usage as a percentage.

> Objects: | starCfNotifRaisedTime starCfNotifInfo starCfThresholdMeasured

> Object: | starCfMdbProcDiskUsageNormal

> Object ID: | enterprises.8164.1.100.6.2.11

> Description: | Notification generated by CF when disk usage threshold for MCRDBS process is normal. The starCFThresholdMeasured varbind indicates process disk usage as a percentage.

> Objects: | starCfNotifRaisedTime starCfNotifInfo starCfThresholdMeasured

> Object: | starCfMdbProcInvalidFileName

> Object ID: | enterprises.8164.1.100.6.2.12

> Description: | This notification is generated by the CF-MCRDBS if it finds a Database having an Invalid name.

> Objects: | starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo

> Object: | starCfMdbProcReportErrWithMsg

> Object ID: | enterprises.8164.1.100.6.2.13

> Description: | This notification is generated by CF-MCRDBS when any system error is generated.

> Objects: | starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo

> Object: | starCfMdbProcCfdcmErrWithMsg

> Object ID: | enterprises.8164.1.100.6.2.14

> Description: | This notification is generated by CF-MCRDBS when any CF-LIB error is generated.

> Objects: | starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo

> Object: | starCfMdbProcMcrdbsErrWithMsg

> Object ID: | enterprises.8164.1.100.6.2.15

> Description: | This notification is generated by CF-MCRDBS when MCRDBS-specific errors are generated.

> Objects: | starCfNotifRaisedTime, starCfParseFileName, starCfNotifInfo

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).starCfMcrdbsMIB(6).starCfMcrdbsMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCfMcrdbsMIB(6).starCfMcrdbsMIBConformances(3).
> starCfMcrdbsMIBCompliances(1)

> Object: | starCFMCRDBSMIBCompliance

> Object ID: | enterprises.8164.1.100.6.3.1.1

> Description: | The compliance statements for entities which implement the STARENT CF-MCRDBS MIB.

> Objects: | starCFMDBNotifMgmtGroup starCFMDBNotifGroup

> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6).starCFMCRDBSMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentCFMIB(100).
> starCFMCRDBSMIB(6).starCFMCRDBSMIBConformances(3).
> starCFMCRDBSMIBGroup(2)

> Object Group: | starCFMDBNotifMgmtGroup

> Object ID: | enterprises.8164.1.100.6.3.2.1

> Description: | A collection of objects related with notification management on CF-MCRDBS.

> Objects: | starCfParseFileName

> Object Group: | starCFMDBNotifGroup

> Object ID: | enterprises.8164.1.100.6.3.2.2

> Description: | A collection of CF-MCRDBS notifications.

> Objects: | starCfMdbProcStart starCfMdbProcStop starCfMdbProcDbAbsent starCfMdbProcApiOpFailed starCfMdbProcDbParseErrot starCfMdbProcMemUsageOverLimit starCfMdbProcmemUsageNormal starCfMdbProcCpuUsageOverLimit starCfMdbProcCpuUsageNormal starCfMdbProcDiskUsageOverLimit starCfMdbProcDiskUsageNormalstarCfMdbProcInvalidFileName starCfMdbProcReportErrWithMsg starCfMdbProcCfdcmErrWithMsg starCfMdbProcMcrdbsErrWithMsg

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883