> Configuration Management
> This section contains additions and changes made to the configuration commands available in Release 9.0. Topics covered in this chapter are:

> l | New Configuration Commands

> l | Modified Configuration Commands

> l | Obsoleted Commands

> l | GTPP Storage Server (GSS)

> l | Web Element Manager Changes

> New Configuration Commands
> This section contains configuration commands that are new in Release 9.0. New commands in this version are divided into the following sections:

> l | Common Commands - New in Release 9.0

> l | ASN GW Commands - New in Release 9.0

> l | Content Filtering Commands - New in Release 9.0

> l | ECS Commands - New in Release 9.0

> l | Firewall Commands - New in Release 9.0

> l | GGSN Commands - New in Release 9.0

> l | HA Commands - New in Release 9.0

> l | NAT Commands - New in Release 9.0

> l | PDIF Commands - New in Release 9.0

> l | PDSN Commands - New in Release 9.0

> l | Peer-to-Peer - New in Release 9.0

> l | Session Control Manager Commands - New in Release 9.0

> l | SGSN Commands - New in Release 9.0

> Common Commands - New in Release 9.0
> This section provides information on new commands that are common to products in Release 9.0.
> apn-name-to-be-included
> This command configures the APN name to be included in CCR Gx messages.
> CLI (Policy Control Configuration Mode)
> apn-name-to-be-included { gn | virtual }
> default apn-name-to-be-included
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> cdr-multi-mode
> This command enables multiple instances of CDRMOD.
> CLI (Global Configuration Mode)
> [ default ] cdr-multi-mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip vrf
> New command added to create new configuration mode named IP VRF Context Configuration Mode to configure the parameters for GRE tunnel interface support. This command configures Virtual Routing and Forwarding (VRF) parameters and also creates IP VRF Context instance for GRE tunnel interface configuration. For more information, refer IP VRF Context Configuration Mode Commands chapter in Command Line Interface Reference.
> CLI (Context Configuration Mode)
> ip vrf vrf_name
> no ip vrf
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip vrf
> New command added to create new configuration mode named OSPF VRF Configuration Mode to configure the virtual routing and forwarding (VRF) context instances for OSPF routing protocol. This mode includes commands that configure VRF instance for OSPF routing parameters. For more information, refer OSPF VRF Context Configuration Mode Commands chapter in Command Line Interface Reference.
> CLI (OSPF Configuration Mode)
> ip vrf vrf_name
> no ip vrf
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip vrf forwarding
> New command added to configure the parameters for GRE tunnel interface support. This command configures the IP VRF forwarding and associates preconfigured VRF context with the current interface for GRE tunnel interface configuration.
> CLI (Tunnel Interface Configuration Mode)
> ip vrf forwarding vrf_name
> no ip vrf forwarding
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius ip vrf
> New command added to configure the parameters for GRE tunnel interface support. This command associates the Virtual Routing and Forwarding (VRF) Context instance for GRE tunnel interface configuration with specific AAA group.
> CLI (AAA Group Configuration Mode)
> radius ip vrf vrf_name
> no radius ip vrf
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius ip vrf
> New command added to configure the parameters for GRE tunnel interface support. This command associates the Virtual Routing and Forwarding (VRF) Context instance for GRE tunnel interface configuration with default AAA group.
> CLI (Context Configuration Mode)
> ip radius vrf vrf_name
> no radius ip vrf
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius accounting billing-version
> This command configures the billing-system version of RADIUS accounting servers.
> CLI (AAA Group & Context Configuration Modes)
> radius accounting billing-version version
> default radius accounting billing-version
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius attribute
> New optional keyword added to configure the RADIUS client to sent VLAN ID with nexthop forwarding address to system when running in single nexthop gateway mode.
> IMPORTANT: This option is available only when nexthop-forwarding gateway is also configured with nexthop-forwarding-address nexthop_address keyword and aaa-large configuration is enabled at Global Configuration level.
> CLI (AAA Server Group Configuration Mode)
> [ no ] radius attribute nas-ip-address address primary_address [ nexthop-forwarding-address nexthop_address [ vlan vlan_id ] ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ASN GW Commands - New in Release 9.0
> This section provides information on new ASN GW commands available in Release 9.0.
> None for this release.
> Content Filtering Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> None for this release.
> ECS Commands - New in Release 9.0
> This section provides information on new ECS commands available in Release 9.0.
> edr voip-call-end
> This command enables generating Event Data Record (EDR) on the completion of voice calls.
> CLI (Rulebase Configuration Mode)
> edr voip-call-end edr-format edr_format_name
> { default | no } edr voip-call-end
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> group-of-prefixed-urls
> This command enables creating/configuring/deleting a group-of-prefixed-URLs.
> CLI (Active Charging Service Configuration Mode)
> group-of-prefixed-urls group_name [ -noconfirm ]
> no group-of-prefixed-urls group_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> group-of-ruledefs-application
> This command specifies the purpose of setting up a group-of-ruledefs as either for charging or for post processing.
> CLI (Group-of-Ruledefs Configuration Mode)
> group-of-ruledefs-application { charging | post-processing }
> no group-of-ruledefs-application
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> icmp req-threshold
> This command configures the maximum number of outstanding ICMP requests to store for ICMP reply matching. This command will be available to all products using Enhanced Charging Service.
> CLI (Ruledef Configuration Mode)
> icmp req-threshold threshold
> default icmp req-threshold
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> icmpv6 any-match
> This command defines a rule definition to analyze and charge user traffic based on any match (catch-all) expression for Internet Control Message Protocol Version 6 (ICMPv6).
> CLI (Ruledef Configuration Mode)
> [ no ] icmpv6 any-match operator condition
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> icmpv6 code
> This command defines a rule definition to analyze and charge user traffic based on the ICMPv6 code.
> CLI (Ruledef Configuration Mode)
> [ no ] icmpv6 code operator code
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> icmpv6 type
> This command defines a rule definition to analyze and charge user traffic based on the ICMPv6 type.
> CLI (Ruledef Configuration Mode)
> [ no ] icmpv6 type operator type
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip version
> This command specifies a rule definition to analyze and charge user traffic based on the IP version—ipv4 or ipv6.
> CLI (Ruledef Configuration Mode)
> [ no ] ip version operator ip_version
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> system-limit
> This command configures the system-wide Layer 4 flow limit.
> CLI (ACS Configuration Mode)
> system-limit l4-flows limit
> { default | no } system-limit l4-flows
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> policy-control burst-size
> This command configures the burst size for bandwidth limiting per dynamic-rule or per bearer.
> CLI (ACS Configuration Mode)
> policy-control burst-size { auto-readjust [ duration duration ] | bytes bytes }
> { default | no } policy-control burst-size
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> post-processing dynamic
> This command configures specified ruledefs/group-of-ruledefs as dynamic post-processing ruledefs/group-of-ruledefs enabling to differentiate between normal post-processing rules from pre-configured ones.
> CLI (Rulebase Configuration Mode)
> post-processing dynamic { group-of-ruledefs group_name | ruledef ruledef_name } charging-action charging_action [ description description ]
> no post-processing dynamic { group-of-ruledefs group_name | ruledef ruledef_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> prefixed-url
> This command adds URLs to be filtered to a group-of-prefixed-URLs. This command used for the URL Filtering feature, and is available in the new ACS Group-of-Prefixed-URLs Configuration Mode.
> CLI (Group-of-Prefixed-URLs Configuration Mode)
> [ no ] prefixed-url url
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> url-preprocessing
> This command enables/disables a group-of-prefixed-urls for preprocessing.
> CLI (Rulebase Configuration Mode)
> [ no ] url-preprocessing bypass group-of-prefixed-urls group_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> firewall icmp-checksum-error
> This command configures Stateful Firewall action on packets with ICMP Checksum errors.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall icmp-checksum-error { drop | permit }
> default firewall icmp-checksum-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall icmp-fsm
> This command enables/disables Stateful Firewall’s ICMP Finite State Machine (FSM).
> CLI (Firewall-and-NAT Policy Configuration Mode)
> [ default | no ] firewall icmp-fsm
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall ip-reassembly-failure
> This command configures Stateful Firewall action on packets involved in IP Reassembly Failure scenarios.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall ip-reassembly-failure { drop | permit }
> default firewall ip-reassembly-failure
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall malformed-packets
> This command configures Stateful Firewall action on malformed packets.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall malformed-packets { drop | permit }
> default firewall malformed-packets
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-checksum-error
> This command configures Stateful Firewall action on packets with TCP Checksum errors.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall tcp-checksum-error { drop | permit }
> default firewall tcp-checksum-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-fsm
> This command enables/disables Stateful Firewall’s TCP Finite State Machine (FSM).
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall tcp-fsm [ first-packet-non-syn { drop | permit | send-reset } ]
> { default | no } firewall tcp-fsm
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-options-error
> This command configures Stateful Firewall action on packets with TCP Option errors.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall tcp-options-error { drop | permit }
> default firewall tcp-options-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall tcp-syn-with-ecn-cwr
> This command configures Stateful Firewall action on TCP SYN packets with either ECN or CWR flag set.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall tcp-syn-with-ecn-cwr { drop | permit }
> default firewall tcp-syn-with-ecn-cwr
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall udp-checksum-error
> This command configures Stateful Firewall action on packets with UDP Checksum errors.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall udp-checksum-error { drop | permit }
> default firewall udp-checksum-error
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> firewall validate-ip-options
> This command enables / disables the Stateful Firewall validation of IP options for errors. When enabled, Stateful Firewall will drop packets with IP option errors.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> [ default | no ] firewall validate-ip-options
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> gtpc nsapi-in-create-pdp-response
> New command added to configure the inclusion/exclusion of optional IE NSAPI in “Create PDP Context Response” message in GTP-C.
> CLI (GGSN Service Configuration Mode)
> [default | no] gtpc nsapi-in-create-pdp-response
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpc ran-procedure-ready-delay
> New command added to configure the GGSN to enable the RAN Procedure Ready feature for the particular GGSN service and specify the timeout period for RAN procedure timer in GGSN which is started on arrival of every secondary Create PDP Context request.
> Once a “Create PDP Context Request” is received by GGSN from SGSN, a timer will be started at GGSN and GGSN will wait till the Radio Access Bearer setup is completed and “Update PDP Context Request” is sent by SGSN. If any downlink data is received before arrival of “Update PDP Context Request” or before timer expire, that downlink packets will be queued or buffered.
> To support this feature each sub-session uses a common flag ‘ran procedure ready state’, whenever a “Create PDP Context Request” is received for secondary PDP context and sub-session is allocated, this flag will be set to TRUE by default. This common flag is checked while sending downlink traffic, if this flag is FALSE then GGSN permit flow of downlink data but, if it is TRUE, GGSN will queue the downlink packets.
> In case if the buffer becomes full (total buffer limit is of 1024 packets) then, all the newly coming packets will be dropped.
> If “Update PDP Context Request” is received by GGSN with RAN Procedure flag set or if timer expires the ‘ran-procedure ready state’ flag in sub-session will be reset and hence GGSN will start sending queued packets in ‘first-in first-out’ manner and buffering will be disabled for further downlink traffic.
> IMPORTANT: This feature make no effect on Enhanced Charging Service or DPI as the buffering of downlink data is done before sending it to ACSMgr.
> IMPORTANT: During SGSN handoff scenario all packets will be processed in a normal way and the downlink packets buffered till the timer expires.
> CLI (GGSN Service Configuration Mode)
> gtpc ran-procedure-ready-delay [timeout dur]
> [default | no] gtpc ran-procedure-ready-delay
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpc private-extension
> New keyword added to configure the overcharging protection when radio coverage lost for a subscriber in a GGSN service.
> CLI (GGSN Service Configuration Mode)
> gtpc private-extension {{{focs | odb} access-list acl_name in disconnect-on-violation }| ggsn-preservation-mode | insk | loss-of-radio-coverage | none}
> no gtpc private-extension [ focs | insk | preservation-mode | loss-of-radio-coverage]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> None for this release.
> NAT Commands - New in Release 9.0
> This section provides information on new NAT commands available in Release 9.0.
> firewall tcp-idle-timeout-action
> This command configures action to take on TCP idle timeout expiry. In this release, this CLI configuration is also available to NAT with the “[600-00-7805] NAT/PAT With DPI” license.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> firewall tcp-idle-timeout-action { drop | reset }
> { default | no } firewall tcp-idle-timeout-action
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> nat private-ip-flow-timeout
> This command configures the Private IP NPU Flow Timeout setting. By default, for NAT-enabled calls the downlink private IP NPU flow will not be installed at call setup for a subscriber session. The flow will only be installed on demand. When there is no traffic on the private flow, the private IP flow will be removed after the configurable timeout period.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> nat private-ip-flow-timeout timeout
> { default | no } nat private-ip-flow-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> secondary ip pool
> This command specifies a secondary IP pool to be used as backup pool for NAT.
> IMPORTANT: This command is license dependent, requiring the [600-00-7871] NAT Bypass license. For more information, please contact your local sales representative.
> CLI (APN Configuration Mode)
> secondary ip pool pool_name
> no secondary ip pool
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDIF Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> None for this release.
> PDSN Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> l2tp send accounting-correlation-info
> New command added to enable the L2TP LAC to send accounting correlation information (Correlation-Id, NAS-IP-Address and NAS-ID) in L2TP control message (ICRQ) during session setup to LNS. LNS can be configured to include this information in ECS billing records, so that billing servers can easily correlate accounting records from PDSN/LAC and LNS.
> CLI (Subscriber Configuration Mode)
> [no | default] l2tp send accounting-correlation-info
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Peer-to-Peer - New in Release 9.0
> This section provides information on new Peer-to-Peer commands in Release 9.0.
> p2p-dynamic-rules
> This command enables/disables the P2P Dynamic Signature Updates feature.
> CLI (ACS Configuration Mode)
> p2p-dynamic-rules { { file location [ force ] } | { protocol [ all | bittorrent | directconnect | edonkey | gnutella | skype | yahoo + ] } }
> default p2p-dynamic-rules file
> no p2p-dynamic-rules { file | protocol [ all | bittorrent | directconnect | edonkey | gnutella | skype | yahoo + ] }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Session Control Manager Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> ipv4-ipv6-interworking
> This command allows the IPv4-IPv6 interworking functionality. Default is disabled.
> CLI (CSCF Service Configuration Mode)
> [ no ] ipv4-ipv6-interworking
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> sip-request
> This command configures SIP Request-related configuration in a S-CSCF service.
> CLI (CSCF Serving-CSCF Configuration Mode)
> sip-request re-route { response-code code | max-attempts attempts }
> default sip-request re-route max-attempts
> no sip-request re-route response-code code
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - New in Release 9.0
> This section provides information on new commands available in Release 9.0.
> apn-selection-default
> New operator policy command has been added to enable and configure a default APN for use when the normal APN selection process fails.
> CLI (SGSN Operator Policy Configuration Mode)
> apn-selection-default network-identifier <apn_net_id> [ require-subscription-apn network-identifier <apn_net_id>]
> noapn-selection-default
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtp
> New command to enable/disable the GTPC private extension in cases of loss of radio coverage (LORC). This is one of the two commands required to enable the overcharging protection feature.
> CLI (SGSN APN Policy Configuration Mode)
> gtp private-extension loss-of-radio-coverage send-to-ggsn [send-to-peer-sgsn]
> remove gtp private-extension loss-of-radio-coverage
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp trigger rat-change
> SGSN support for this command has been added. This command configures whether or not the RAT change interim CDR is generated for the inter-service handoff
> CLI (GTPP Server Group Configuration Mode)
> [ no ] gtpp trigger rat-change
> default gtpp trigger
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> override-arp-with-ggsn-arp
> New CLI has been added to enable configuration of the SGSN to negotiate or change or "not" to negotiate or change the value of the ARP received from the GGSN. This configuration of the SGSN will allow the ARP sent by GGSN in CPCR / UPCR / UPCQ to be applicable as an overriding value.
> CLI (SGSN Operator Policy Configuration Mode)
> [ remove] override-arp-with-ggsn-arp
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ranap
> This command enables or disables the inclusion of the paging cause IEs and the modification of paging sources in various RANAP messages.
> CLI (RNC Service Configuration Mode)
> ranap { paging-cause-ie { all | background-data <value> | conversational-data <value> | gmm-signalling <value>| gs-signalling <value> | interactive-data <value> | sm-signalling <value> | sms-signalling <value> | streaming-data <value> } | { signalling-indication-ie { rab-assignment-request [ relocation-request ] | relocation-request [ rab-assignment-request ] } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> loss-of-radio-coverage ranap-cause
> New command to include the detection cause for loss of radio coverage in the Iu Release message. This is one of the two commands required to enable the overcharging protection feature.
> CLI (IuPS Service Configuration Mode)
> loss-of-radio-coverage ranap-cause cause#
> default loss-of-radio-coverage ranap-causee
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ranap
> This command enables or disables the inclusion of the Signalling Indication IEs in various RANAP messages depending upon circumstances.
> CLI (RNC Service Configuration Mode)
> ranap { signalling-indication-ie { rab-assignment-request [ relocation-request ] | relocation-request [ rab-assignment-request ] }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> reset-resource
> This command enables the operator to control message length by configuring the number of IuConIDs sent in each RANAP Reset Resource message.
> CLI (DNS Client Configuration Mode)
> [ default ] reset-resource max-iuconid-per-msg <number>
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> gtpp dead-server suppress-cdrs
> New command defines the action the SGSN will take on the CDRs generated during a communication failure between the SGSN and the GTPP servers.
> CLI (GTPP Group Configuration Mode)
> [no | default] gtpp dead-server suppress-cdrs
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> inbound-asp-identifier validate
> This command enables or disables the validation of ASP identifiers inbound to the SGSN via routes defined with the SS7 routing domain.
> CLI (SS7 Routing Domain Configuration Mode)
> inbound-asp-identifier validate
> [ default | no ] inbound-asp-identifier validate
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Modified Configuration Commands
> This section contains configuration commands that have been modified in Release 9.0. Modified commands in this version are divided into the following sections:

> l | Common Commands - Modified in Release 9.0

> l | Content Filtering Commands - Modified in Release 9.0

> l | ECS Commands - Modified in Release 9.0

> l | Firewall Commands - Modified in Release 9.0

> l | GGSN Commands - Modified in Release 9.0

> l | HA Commands - Modified in Release 9.0

> l | NAT Commands - Modified in Release 9.0

> l | PDIF Commands - Modified in Release 9.0

> l | PDSN Commands - Modified for Release 9.0

> l | Peer-to-Peer - Modified for Release 9.0

> l | Session Control Manager Commands - Modified for Release 9.0

> l | SGSN Commands - Modified for Release 9.0

> Common Commands - Modified in Release 9.0
> This section provides information on common commands modified for Release 9.0.
> configure hd raid
> Configures the disk preference when both hard disks on the ST40 have valid RAID information.
> CLI (HD Raid Configuration Mode
> [ default ] select { newer | none } disk [ -noconfirm ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter peer-select
> This command specifies the Diameter Credit Control primary and secondary host for credit control. This command now enables specifying IMSI prefix or suffix, or IMSI prefix or suffix ranges for peer selection. In this release, this change is only available to UMTS networks.
> CLI (Credit Control Configuration Mode)
> diameter peer-select peer peer_name [realm realm_name] [secondary-peer sec_peer_name [ realm realm_name ] ] [ imsi-based { [ prefix | suffix ] imsi/prefix/suffix_start_value } [ to imsi/prefix/suffix_end_value ]]
> no diameter peer-select [ imsi-based { [ prefix | suffix ] imsi/prefix/suffix_start_value } [ to imsi/prefix/suffix_end_value ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip arp
> New optional keyword added to associate a Virtual Routing and Forwarding (VRF) context with specific static ARP entry for GRE tunnel interface support.
> CLI (Context Configuration Mode)
> ip arp ip_address mac_address [vrf vrf_name]
> no ip arp ip_address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip route
> New optional keyword added to associate a Virtual Routing and Forwarding (VRF) context with specific static route configuration for GRE tunnel interface support.
> CLI (Context Configuration Mode)
> [ no ] ip route {ip_address/ip_mask | ip_address ip_mask}
> { gateway_ip_address | next-hop next_hop_ip_address | point-to-point | tunnel} egress_intrfc_name [ cost cost ]
> [ precedence precedence ] [vrf vrf_name] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ospf graceful-restart
> Support for OSPF graceful restart has been added to the existing command.
> CLI (Global Configuration Mode)
> ospf graceful-restart { grace-period grace_period | helper { never | policy { only-reload | only-upgrade } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> policy-control charging-rule-base-name
> This command configures interpretation of Charging-Rule-Base-Name AVP from PCRF either as active-charging rulebase or active-charging group-of-ruledefs. The optional keyword ignore-when-removed was added to this command.
> When Charging-Rule-Base-Name AVP is interpreted as active-charging rulebase, if PCRF requests the removal of a Charging-Rule-Base-Name, which is the same as the rulebase used for that PDP context, the PDP context is terminated. This is because after removal of the rulebase, the PDP context will have no rulebase. This is the default behavior.
> When the ignore-when-removed option is configured, PCRF request for removal of Charging-Rule-Base-Name is ignored and no action is taken.
> CLI (Active Charging Service Configuration Mode)
> policy-control charging-rule-base-name { active-charging-group-of-ruledefs | active-charging-rulebase [ ignore-when-removed ] }
> default policy-control charging-rule-base-name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> require active-charging
> This command enables/disables Active Charging Service (ACS) with or without Category-based Content Filtering application. The static-and-dynamic keyword was added to this command, which for Dynamic Content Filtering support, specifies that the Dynamic Rater Package (model and feature files) must be distributed to rating modules on startup, recovery, etc.
> CLI (Global Configuration Mode)
> require active-charging [ isolated-mode ] [ content-filtering category [ static-and-dynamic ] ] [ optimized-mode ]
> no require active-charging
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> radius accounting
> This command configures the current context’s RADIUS accounting function options. The stop-only keyword was added to this command, which specifies archiving of STOP accounting messages only.
> CLI (AAA Group & Context Configuration Modes)
> radius accounting { archive [ stop-only ] | deadtime dead_minutes | detect-dead-server { consecutive-failures count | keepalive | response-timeout seconds } | interim interval seconds | max-outstanding msgs | max-pdu-size octets | max-retries tries | max-transmissions trans | timeout idle_seconds | unestablished-sessions }
> no radius accounting { archive | detect-dead-server | interim interval | max-transmissions | unestablished-sessions }
> default radius accounting { deadtime | detect-dead-server | interim interval seconds | max-outstanding | max-pdu-size | max-retries | max-transmissions | timeout }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> snmp target
> A new security level, priv-auth, has been added to the snmp target command to support SNMPv3 notifications. When the security level is set to priv-auth, both authentication and encryption are enabled.
> CLI (Global Configuration Mode)
> snmp target name ip_address [ port number ] [ non-default ] [ security-name string ] [ version { 1 | 2c | 3| view ] [security-level { noauth | { auth | priv-auth privacy [encrypted] des } authentication [encrypted] { md5 | sha } } } [ informs | traps ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> tunnel-mode
> New configuration keyword added to create new configuration mode named GRE Tunnel Interface Configuration Mode for GRE interface configuration. Refer GRE Tunnel Interface Configuration Mode Commands chapter in Command Line Interface Reference.
> CLI (Context Configuration Mode)
> tunnel-mode {gre | ipv6ip}
> defualt tunnel-mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Content Filtering Commands - Modified in Release 9.0
> This section provides information on Content Filtering commands modified in Release 9.0.
> content-filtering mode
> This command enables the specified Content Filtering mode within a rulebase. In this release, specifying the static-and-dynamic mode enables dynamic rating in the rulebase after static rating fails.
> CLI (Rulebase Configuration Mode)
> content-filtering mode { category { static-only | static-and-dynamic } | server-group cf_server_group }
> no content-filtering mode
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> upgrade content-filtering category rater-pkg
> This command upgrades the Static Rating Database (SRDB) for Category-based Content Filtering application. The rater-pkg option was added to this command. This enables manual upgrades of the Dynamic Content-Filtering Rater Package (rater.pkg file). The rater.pkg file contains the models and feature counters that are used to return the dynamic content rating. The upgrade will trigger distribution of the rater.pkg to all the SRDBs.
> CLI (Exec Mode)
> upgrade content-filtering category { database | rater-pkg }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 9.0
> This section provides information on ECS commands modified in Release 9.0.
> billing-records
> This command configures the type of billing to be performed for subscriber sessions. The rf keyword was added to this command. This keywords enables Rf accounting. Rf accounting is applicable only for dynamic and predefined rules that are marked for it. Dynamic rules have a field offline-enabled to indicate this. To mark a predefined rule as offline-enabled, use this keyword and the billing-action CLI in the Charging Action Configuration Mode.
> CLI (Rulebase Configuration Mode)
> billing-records { egcdr | radius | rf | udr udr-format udr_format_name } +
> no billing-records
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ftp command id
> This command defines a rule definition to analyze and charge user traffic based on FTP command ID. This release onwards, the command identifier for a rule definition can be specified as an integer from 0 through 18.
> CLI (Ruledef Configuration Mode)
> [ no ] ftp command id operator command_id
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ftp command name
> This command defines a rule definition to analyze and charge user traffic based on FTP command name. This release onwards, the following options are supported for FTP analyzer:

> l | eprt: eprt command

> l | epsv: epsv command

> CLI (Ruledef Configuration Mode)
> [ no ] ftp command name operator command_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip dst-address
> This command defines a rule definition to analyze and charge user traffic based on IP destination address. This command now accepts IPv6 addresses.
> CLI (Ruledef Configuration Mode)
> [ no ] ip dst-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip protocol
> This command configures the IP protocol setting for a packet filter. The range keyword option to select a range of protocols is now obsoleted.
> CLI (Packet Filter Configuration Mode)
> ip protocol = protocol_number
> no ip protocol
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip protocol
> This command defines a rule definition to analyze and charge user traffic based on the protocol being transported by IP packets. This command now accepts icmpv6 protocol option.
> CLI (Ruledef Configuration Mode)
> [ no ] ip protocol operator { protocol_assignment | ah | esp | gre | icmp | icmpv6 | tcp | udp }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip remote-address
> This command configures IP remote address setting for a packet filter. The range keyword option to select a range of IP addresses is now obsoleted.
> CLI (Packet Filter Configuration Mode)
> ip remote-address = { ip_address | ip_address/mask }
> no ip remote-address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip server-ip-address
> This command defines a rule definition to analyze and charge user traffic matching the IP address of the destination, i.e. from the subscriber, of the connection. This command now accepts IPv6 addresses.
> CLI (Ruledef Configuration Mode)
> [ no ] ip server-ip-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip src-address
> This command defines a rule definition to analyze and charge user traffic based on IP source address. This command now accepts IPv6 addresses.
> CLI (Ruledef Configuration Mode)
> [ no ] ip src-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip subscriber-ip-address
> This command defines a rule definition to analyze and charge user traffic matching the IP address of the subscriber (either source address or destination address). This command now accepts IPv6 addresses.
> CLI (Ruledef Configuration Mode)
> [ no ] ip subscriber-ip-address { operator { ip_address | ip_address/mask } | { !range | range } host-pool host_pool }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> post-processing priority
> This command configures the post-processing action to be taken on the specified ruledef in the rulebase. The group-of-ruledefs keyword was added to the command. This enables assigning the specified group-of-ruledefs to the rulebase.
> CLI (Rulebase Configuration Mode)
> post-processing priority priority { group-of-ruledefs group_name | ruledef ruledef_name } charging-action charging_action_name [ description description ]
> no post-processing priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rule-variable
> This command specifies the event rule variable for EDR file format attribute. The following new rule variable options were added to this command:

> l | ip:

> l | version

> l | icmpv6:

> l | code

> l | type

> l | traffic-type

> l | voip-duration

> CLI (EDR Format Configuration Mode)
> rule-variable protocol rule priority priority [ in-quotes ]
> no rule-variable protocol rule [ priority priority ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Modified in Release 9.0
> This section provides information on commands modified for Release 9.0.
> None for this release.
> GGSN Commands - Modified in Release 9.0
> This section provides information on GGSN commands modified in Release 9.0.
> gtpp storage-server local file
> New keyword custom8 added to define customized CDR file format It uses node-id-suffix_date_time_fixed-length-seq-num.u format for file naming where:

> l | date is date in MMDDYYYYY (01312010) for mat

> l | time is time in HHMMSS (023508) format

> l | fixed-length-seq-num is the fixed length of sequence number for specific file having 6 digit counter starting from 000001 and end to 999999. Once file sequence reached to 999999 the sequence will be reset to 000001.

> CLI (GTPP Server Group Configuration Mode)
> gtpp storage-server local file { compression { gzip | none } | format { custom1 | custom2 | custom3 | custom4 | custom5 | custom6 | custom7 | custom8 } | name prefix prefix | purge-processed-files [ purge-interval purge_dur ] | rotation { cdr-count count | time-interval time | volume size} }
> default gtpp storage-server local file { compression | format | name prefix | purge-processed-files | rotation { cdr-count | time-interval | volume } }
> no gtpp storage-server local file rotation { purge-processed-files | rotation { cdr-count | time-interval } }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> authentication
> New optional keywords username-strip-apn and password-use-pco added to configure support for AAA Auth user name as MSISDN/IMSI and password as PCO received password for APN.
> CLI (APN Configuration Mode)
> authentication {[ msid-auth | imsi-auth [username-strip-apn] [password-use-pco] | msisdn-auth [username-strip-apn] [password-use-pco]]| [ allow-noauth ][ chap preference ][ mschap preference ] [ pap preference ]}
> default authentication
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - Modified in Release 9.0
> This section provides information on HA commands modified in Release 9.0.
> None for this release.
> NAT Commands - Modified in Release 9.0
> This section provides information on NAT commands modified in Release 9.0.
> access-rule
> With the NAT-only license [600-00-7805] NAT/PAT With DPI, the trigger open-port keyword is no longer available with this command. In the earlier releases, for NAT this keyword was not functional.
> CLI (Firewall-and-NAT Policy Configuration Mode)
> access-rule { no-ruledef-matches { downlink | uplink } action { deny [ charging-action charging_action ] | permit [ bypass-nat | nat-realm nat_realm ] } | priority priority { [ dynamic-only | static-and-dynamic ] access-ruledef ruledef_name { deny [ charging-action charging_action ] | permit [ bypass-nat | nat-realm nat_realm ] } } }
> default access-rule no-ruledef-matches { downlink | uplink } action
> no access-rule priority priority
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ip pool
> IMPORTANT: This change is applicable to UMTS deployments in StarOS 9.0, and for CDMA deployments in StarOS 8.3.
> This command enables adding, modifying, and deleting an IP address pool in the current context. The following keywords and associated options were added to this command for the Network Address Translation (NAT) feature:

> l | nat-one-to-one: This keyword and associated options enable configuring one-to-one NAT realms.

> l | napt-users-per-ip-address: This keyword and associated options enable configuring many-to-one NAT realms.

> The following keyword and associated options were removed from this command:

> l | nat-realm

> IMPORTANT: On upgrading from StarOS 8.1 to StarOS 9.0, all NAT realms configured in StarOS 8.1 using the nat-realm keyword must in StarOS 9.0 be reconfigured using one of the following keywords:
> - nat-one-to-one
> - napt-users-per-ip-address
> For example, the following command in StarOS 8.1 configuration:
> ip pool pool1 range 11.22.33.44 55.66.77.88 nat-realm ...
> must in StarOS 9.0 be reconfigured to one of the following:
> ip pool pool1 range 11.22.33.44 55.66.77.88 nat-one-to-one ...
> ip pool pool1 range 11.22.33.44 55.66.77.88 napt-users-per-ip-address ...
> CLI (Context Configuration Mode)
> ip pool name { ip_address subnet_mask | ip_addr_mask_combo | range start_ip_address end_ip_address } [ private [ priority ] | public [ priority ] | static ] [ tag { none | pdif-setup-addr } ] [ address-hold-timer seconds | alert-threshold [ group-available | pool-free | pool-hold | pool-release | pool-used ] low_thresh [ clear high_thresh ] ] [ group-name group_name ] [ include-nw-bcast ] [ nat priority ] [ nexthop-forwarding-address ip_address [ overlap vlanid vlan_id ] [ nw-reachability server server_name ] [ respond-icmp-echo ip_address ] [ resource ] [ send-icmp-dest-unreachable ] [ explicit-route-advertise ] [ srp-activate ] [ suppress-switchover-arp ] [ unicast-gratuitous-arp-address ip_address ] [ policy allow-static-allocation ] [ nat-one-to-one [ [ alert-threshold [ { pool-free | pool-hold | pool-release | pool-used } low_thresh [ clear high_thresh ] + ] [ nat-binding-timer binding_timer ] [ on-demand ] [ send-nat-binding-update ] + ] | napt-users-per-ip-address users [ [ alert-threshold [ { pool-free | pool-hold | pool-release | pool-used } low_thresh [ clear high_thresh ] + ] [ max-chunks-per-user chunks ] [ nat-binding-timer timer ] [ on-demand ] [ port-chunk-size size ] [ port-chunk-threshold chunk_threshold ] [ send-nat-binding-update ] + ]
> no ip pool name [ tag { none | pdif-setup-addr } ] [ address-hold-timer | alert-threshold [ group-available | pool-free | pool-hold | pool-release | pool-used ] ] [ group-name ] [ include-nw-bcast ] [ nexthop-forwarding-address ] [ nw-reachability server ] [ respond-icmp-echo ip_address ] [ send-icmp-dest-unreachable ] [ explicit-route-advertise ] [ send-nat-binding-update ] [ srp-activate ] [ suppress-switchover-arps ] [ unicast-gratuitous-arp-address ] [ policy allow-static-allocation ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDIF Commands - Modified in Release 9.0
> This section provides information on PDIF commands modified in Release 9.0.
> control-dont-fragment
> This command controls the don’t fragment (DF) bit in the outer IP header of the IPsec tunnel data packet.
> CLI (Crypto Map Manuel Configuration Mode)
> default set control-dont-fragment { clear-bit | copy-bit | set-bit }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> PDSN Commands - Modified for Release 9.0
> This section provides information on PDSN commands modified in Release 9.0.
> None for this release.
> Peer-to-Peer - Modified for Release 9.0
> This section provides information on Peer-to-Peer commands modified in Release 9.0.
> p2p-detection protocol
> This command configures the system to detect peer-to-peer (P2P) protocols. The following keywords were added to this command:

> l | gtalk

> l | oovoo

> CLI (ACS Configuration Mode)
> [ no ] p2p-detection protocol [ all | applejuice | ares | bittorrent | ddlink | directconnect | edonkey | fasttrack | feidian | filetopia | fring | gadugadu | gnutella | gtalk | halflife2 | hamachivpn | imesh | irc | iskoot | jabber | manolito | msn | mute | oovoo | orb | oscar | pando | popo | pplive | ppstream | qq | qqlive | skinny | skype | slingbox | sopcast | soulseek | steam | tvants | tvuplayer | uusee | vpnx | vtun | winmx | winny | wofwarcraft | xbox | yahoo | zattoo ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> p2p-detection protocol
> This command configures the system to detect peer-to-peer (P2P) protocols. The following keywords were added to this command:

> l | freenet

> l | aimini

> l | battlefld

> l | openft

> l | qqgame

> l | quake

> l | secondlife

> l | actsync

> l | nimbuzz

> l | iax

> l | paltalk

> l | warcft3

> l | rdp

> l | iptv

> l | pandora

> CLI (ACS Configuration Mode)
> [ no ] p2p-detection protocol [ all | applejuice | ares | bittorrent | ddlink | directconnect | edonkey | fasttrack | feidian | filetopia | fring | gadugadu | gnutella | gtalk | halflife2 | hamachivpn | imesh | irc | iskoot | jabber | manolito | msn | mute | oovoo | orb | oscar | pando | popo | pplive | ppstream | qq | qqlive | skinny | skype | slingbox | sopcast | soulseek | steam | tvants | tvuplayer | uusee | vpnx | vtun | winmx | winny | wofwarcraft | xbox | yahoo | zattoo | freenet | aimini | battlefld | openft | qqgame | quake | secondlife | actsync | nimbuzz | iax | paltalk | warcft3 | rdp | iptv | pandora ] +
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging analyzer statistics
> This command displays the statistics for protocol analyzers. The following new protocols were added to this command:

> l | freenet

> l | aimini

> l | battlefld

> l | openft

> l | qqgame

> l | quake

> l | secondlife

> l | actsync

> l | nimbuzz

> l | iax

> l | paltalk

> l | warcft3

> l | rdp

> l | iptv

> l | pandora

> CLI (Exec Mode)
> show active-charging analyzer statistics [ name protocol [ verbose ] ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging flows
> This command displays information for active charging flows. The following new protocols were added to this command for the type keyword:

> l | freenet

> l | aimini

> l | battlefld

> l | openft

> l | qqgame

> l | quake

> l | secondlife

> l | actsync

> l | nimbuzz

> l | iax

> l | paltalk

> l | warcft3

> l | rdp

> l | iptv

> l | pandora

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ]
> [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-tha n ] number ]
> [ rx-packets [ < | > | greater-than | less-tha n ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions
> This command displays the statistics for specific active charging service sessions. The following new protocols were added to this command for the type keyword:

> l | freenet

> l | aimini

> l | battlefld

> l | openft

> l | qqgame

> l | quake

> l | secondlife

> l | actsync

> l | nimbuzz

> l | iax

> l | paltalk

> l | warcft3

> l | rdp

> l | iptv

> l | pandora

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> p2p protocol
> This command configures the system to detect specific P2P protocols for charging purposes. The following new protocols were added to this command:

> l | freenet

> l | aimini

> l | battlefld

> l | openft

> l | qqgame

> l | quake

> l | secondlife

> l | actsync

> l | nimbuzz

> l | iax

> l | paltalk

> l | warcft3

> l | rdp

> l | iptv

> l | pandora

> CLI (Exec Mode)
> [ no ] p2p protocol operator protocol
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Session Control Manager Commands - Modified for Release 9.0
> The following commands have been modified in Release 9.0.
> bind
> The use-serviceport-towards-network keyword has been added.
> CLI (CSCF Service Configuration Mode)
> bind address ip_address [ access-ipsec-crypto-template template ]
> [ cscf-hostname host_name ] [ max-sessions max# ] [ port number ]
> [ reserved-call-capacity percentage] [ transport tcp ] [ use-serviceport-towards-network ]
> no bind address
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> diameter
> The request-timeout sec, Rq-custom, and Rx-rel8 keywords have been added.
> CLI (CSCF Proxy-CSCF Configuration Mode)
> diameter location-info { dictionary { e2custom01 | e2custom02 | e2custom03 | e2custom04 | e2custom05 | e2custom06 | e2custom07 | e2custom08 | e2custom09 | e2standard } | origin endpoint endpoint_name | peer-select peer peer_name [ peer-realm realm_name ] [ secondary-peer peer_name
> [ sec-peer-realm realm_name ] ] | request-timeout sec }
> diameter policy-control { dictionary { Gq-custom | Gq-standard | Rq-custom| Rx-rel8 | Rx-standard | Tx-standard | custom01 | custom02 | custom03 | custom04 | custom05 | custom06 | custom07 | custom08 | custom09 } |
> origin endpoint endpoint_name | peer-select peer peer_name [ peer-realm realm_name ] [ secondary-peer peer_name [ sec-peer-realm realm_name ] ] | request-timeout sec }
> default diameter { location-info | policy-control } { dictionary | request-timeout }
> no diameter { location-info | policy-control } [ origin endpoint | peer-select ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - Modified for Release 9.0
> The following commands have been modified in Release 9.0.
> gmm
> The Inter-SGSN RAU TRAU timer is now configurable for both 2G and 3G SGSNs with a range of 5 to 60 seconds.
> CLI (GPRS Service Configuration Mode)
> gmm trau-timeout seconds
> default gmm trau-timeout
> CLI (SGSN Service Configuration Mode)
> gmm trau-timeout seconds
> default gmm trau-timeout
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> The n201u-max keyword has been added to the llc command to allow the operator to set the maximum size that can be negotiated for the downlink data packet (information field length for U/UI frames.
> CLI (GPRS Service Configuration Mode)
> llc { iov-ui-in-xid-reset | n201u-max | pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> llc
> The uplink-pdu-len-validation keyword has been added to the llc command to provide the operator the ability to validate or ignore the negotiated uplink N201_U packet size.
> CLI (GPRS Service Configuration Mode)
> llc { iov-ui-in-xid-reset | n201u-max | pdu-lifetime secs | T200 sapi1 time | T200 sapi11 t time | T200 sapi3 time | T200 sapi5 time | T200 sapi7 time | T200 sapi9 time | uplink-pdu-len-validation }
> no llc uplink-pdu-len-validation
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> rnc id
> The SGSN now supports the Extended RNC Id IE from Release 7. The maximum range was 4095 and has now been increased to 65535.
> CLI (IuPS Service Configuration Mode)
> rnc id <0 - 65535>
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> qos prefer-as-cap
> The qos command, in the SGSN operator policy's APN policy configuration mode, has been modified to support capping of the local QoS bit rate when the subscribed QoS provided by the HLR is lower than the locally configured value.
> CLI (IuPS Service Configuration Mode)
> qos { class | prefer-as-cap { hlr-subscription | local | both-hlr-and-local } | rate-limit }
> remove qos prefer-as-cap
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> apn/apn-selection-default/wildcard-apn
> To meet 3GPP TS23.003, the maximum length for the network-identifier for all APN definitions has been reduced from 63 characters to 62.
> CLI (SGSN Operator Policy Configuration Mode)
> apn { network-identifier apn_net_id | operator-identifier apn_op_id }
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> application-context-name
> The range for the Gf 1-in-N IMEI check event timer has been expanded to 1 -30 seconds from 15 - 30 seconds; keeping 15 seconds as the default.
> CLI (SGSN Operator Policy Configuration Mode)
> application-context-name application operator timer time
> Web Element Manager Path
> This expansion is not supported at this time on the Web Element Manager.
> Obsoleted Commands
> This section contains configuration commands that have been obsoleted in Release 9.0. Obsoleted commands in this version are divided into the following sections:

> l | Common Commands - Obsoleted in Release 9.0

> l | Content Filtering Commands - Obsoleted in Release 9.0

> l | ECS Commands - Obsoleted in Release 9.0

> l | Firewall Commands - Obsoleted in Release 9.0

> l | GGSN Commands - Obsoleted in Release 9.0

> l | HA Commands - Obsoleted in Release 9.0

> l | PDSN Commands - Obsoleted in Release 9.0

> l | SGSN Commands - Obsoleted in Release 9.0

> Common Commands - Obsoleted in Release 9.0
> This section provides information on commands that are common to all products that were obsoleted in Release 9.0.
> css acsmgr-selection-attempts
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Global Configuration Mode)
> [ default ] css acsmgr-selection-attempts num_attempts
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> css delivery-sequence
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Global Configuration Mode)
> css delivery-sequence name [ -noconfirm ]
> no css delivery-sequence name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> css service
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Global Configuration Mode)
> css service name [ -noconfirm ]
> no css service name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> css server
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Context Configuration Mode)
> css server name keepalive [ interval seconds ] [ local-address localIP ] [ num-retry number ] [ protocol { icmp | tcp } ] [ remote-address remIP ] [ timeout seconds ]
> no css server name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> redirect css delivery-sequence
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (ACL Configuration Mode)
> redirect css delivery-sequence sequence_name { options }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> redirect css delivery-sequence
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (IPv6 ACL Configuration Mode)
> redirect css delivery-sequence sequence_name { options }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Content Filtering Commands - Obsoleted in Release 9.0
> This section provides information on CF commands that were obsoleted in Release 9.0.
> None for this release.
> ECS Commands - Obsoleted in Release 9.0
> This section provides information on ECS commands that were obsoleted in Release 9.0.
> None for this release.
> Firewall Commands - Obsoleted in Release 9.0
> This section provides information on Firewall commands that were obsoleted in Release 9.0.
> firewall tcp-first-packet-non-syn
> This command configures the action to take on TCP flows starting with a non-syn packet. In StarOS 9.0, this command is deprecated. This configuration is now available as the “firewall tcp-fsm [ first-packet-non-syn { drop | permit | send-reset } ]” command.
> CLI (Firewall-and-NAT Configuration Mode)
> firewall tcp-first-packet-non-syn { drop | reset }
> default firewall tcp-first-packet-non-syn
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Obsoleted in Release 9.0
> This section provides information on GGSN commands that were obsoleted in Release 9.0.
> None for this release.
> HA Commands - Obsoleted in Release 9.0
> This section provides information on HA commands that were obsoleted in Release 9.0.
> None for this release.
> PDSN Commands - Obsoleted in Release 9.0
> This section provides information on PDSN commands that were obsoleted in Release 9.0.
> None for this release.
> SGSN Commands - Obsoleted in Release 9.0
> This section provides information on SGSN commands that were obsoleted in Release 9.0.
> authenticate attach
> The attach keyword has been modified and the inter-rat keyword has been included to enable or disable (default) authentication for Inter-RAT Attaches.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate { attach [ inter-rat [ access-type gprs | umts ] ] }
> default authenticate attach inter-rat [ access-type gprs | umts ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> authenticate rau update-type
> The authentica rau update-type command has been enhanced to include the with inter-rat-local-ptmsi qualifier to enable or disable (default) authentication for Inter-RAT RAUs.
> CLI (SGSN Operator Policy Configuration Mode)
> authenticate rau update-type { ra-update with inter-rat-local-ptmsi | combined-update with inter-rat-local-ptmsi | imsi-combined-update with inter-rat-local-ptmsi }
> default authenticate rau update-type { ra-update | combined-update | imsi-combined-update }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GTPP Storage Server (GSS)
> This section provides information on GSS changes in Release 9.0.
> GSS Changes in Release 9.0
> This section provides information on GSS changes in Release 9.0.
> None for this release.
> Web Element Manager Changes
> This section provides information on Web Element Manager changes in Release 9.0.
> None for this release.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883