> SGSN Multiple Address Group Configuration Mode Commands
> This configuration mode defines the IP addresses for the current SGSN Multiple Address Group.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> address
> This command specifies and IP address to include in the current SGSN Multiple Address Group.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> address ip_address[/mask]
> no
> Delete the specified IP address or IP address and netmask from the current SGSN Multiple Address Group.
> ip_address[/mask ]
> Specifies the IP address or IP address and netmask to include in the current SGSN Multiple Address Group.
> ip_address is an IPv4 address in dotted-decimal notation and mask is the number of subnet bits, representing a subnet mask in shorthand. These must be entered in the dotted-decimal notation/subnet bits format (1.1.1.1/24).
> Usage
> Use this command to specify an IP address or IP address and netmask to include in the current SGSN Multiple Address Group.
> Example
> The following command adds the IP address 10.1.2.250 to the current SGSN Multiple Address Group:
> address 10.1.2.250
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the context configuration mode.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the GGSN Service configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883