> SMS Service Configuration Mode Commands
> The SMS (short message service) Service configuration mode is used to configure properties of the SMS Service component. The SGSN uses the SMS Service component to communicate via the Gd interface with a gateway message service controller (GMSC) to send short text messages (up to 140 octets in length) to a mobile (SMS-MT) and/or receive messages from a mobile (SMS-MO) .
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> cp-data
> Enables the SGSN to send and/or receive cp-data (text messages).
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> cp-data max-retransmission retries_num
> default cp-data max-retransmissions
> default
> This keyword resets the SGSN’s max-retransmission to the default number of retries.
> max-retransmission retries_num
> retries_num: enter an integer from 1 to 3.
> Usage
> Use this command to configure the number of times the SGSN will attempt to retransmit a message.
> Example
> cp-data max-retransmission 2
> mo-message-forwarding-destination
> This command defines the SGSN’s handling policy for MO (mobile originating) message.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ default ] mo-message-forwarding-destination { gmsc-selected-from-imsi | smsc-supplied-by-subscriber }
> default
> Resets the SMS service configuration to the default message forwarding technique.
> gmsc-selected-from-imsi
> Entering this keyword enables SMS-MO messages to be forwarded on the basis of their IMSI prefix.
> smsc-supplied-by-subscriber
> Entering this keyword enables SMS-MO messages to be forwarded on the basis of the SMSC (SMS controller) address provided by the subscriber.
> Usage
> Use this command to define how the mobile originated SMS are to be routed.
> Example
> mo-message-forwarding-destination gmsc-selected-from-imsi
> smsc-routing
> This command configures the routing to the SMSC.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] smsc-routing { { any | imsi-starts-with | msisdn-starts-with } { isdn isdn_number | mobile-global-title mgt_number | point-code pt_code } }
> any
> Configures routing according to any IMSI prefix.
> imsi-starts-with IMSI_prefix
> Defines the IMSI prefix. Enter a string of up to 15 integers.
> msisdn-starts-with msisdn_prefix
> Defines the MSISDN prefix. Enter a string of up to 15 integers.
> isdn isdn_number
> Defines the ISDN E.164 number of the SMSC.
> mobile-global-title mgt_number
> Defines the mobile global title for conversion
> point-code pt_code
> Defines the point code for the SMSC. Enter a string of up to 11 digits in SS7 dotted decimal or decimal format
> Usage
> Use this command to define routing to the SMSC based on any point code.
> Example
> smsc-routing any point-code 1.222.1
> timeout
> This command defines the SMS service timers.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> timeout { tc1n-timer time | tr1n-timer time | tr2n timer time }
> default timeout { tc1n-timer | tr1n-timer | tr2n timer }
> default
> Resets the configuration to the default value for the specified timer.
> tc1n-timer time
> Configures the TC1N timer in seconds.
> time: Must an integer from 1 to 255. The default is 5 seconds.
> tr1n-timer time
> Configures the TR1N timer in seconds.
> time: Must an integer from 1 to 255. The default is 30 seconds.
> tr2n-timer time
> Configures the TR2N timer in seconds.
> time: Must an integer from 1 to 255. The default is 30 seconds.
> Usage
> Use this command to set SMS service timers. The command can be repeated to set all of the timers, one-at-a-time.
> Example
> tr1n-timer 25

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883