> RP Schema Statistics
> The RP schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> RP Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the PDSN service. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the PDSN service. This is an internal reference number. | Int32
> servname | Displays the name of the PDSN service for which the statistics are displayed. | String
> num-sessions | The current total number of RP sessions | Int32
> sess-cursetup | The total number of current sessions per service. | Int32
> sess-currevasetup | The total number of current EVDO-Rev A sessions per service. | Int32
> sess-ttlsetup | The total sessions setup per service. | Int32
> sess-ttlrevasetup | The total EVDO-Rev A sessions setup per service. | Int32
> sess-ttlrevareleased | The total EVDO-Rev A sessions released per service. | Int32
> sess-ttlrevadowngrade | The total EVDO-Rev A sessions that were downgraded per service. | Int32
> sess-ttlreleased | The total number of sessions released per service. | Int32
> svctype | Indicates the type of services running for this schema. It is collected at the per service level. | String
> a10-cursetup | The total number of current A10s per service. | Int32
> a10aux-cursetup | The total number of current aux A10s per service. | Int32
> a10main-cursetup | The total number of current main A10s per service. | Int32
> a10-ttlsetup | The total number of A10s setup per service. | Int32
> a10aux-ttlsetup | The total number of aux A10s setup per service. | Int32
> a10main-ttlsetup | The total number of main a10s setup per service. | Int32
> a10-ttlreleased | The total number of a10s released per service. | Int32
> a10aux-ttlreleased | The total number of aux A10s released per service. | Int32
> a10main-ttlreleased | The total number of main A10s released per service. | Int32
> sess-release-dereg | The total number of sessions de-registered per service. | Int32
> sess-release-expiry | The total number of sessions released due to lifetime expiry per service. | Int32
> sess-release-ppplayer | The total number of sessions released due to a PPP Layer command reported per service. | Int32
> sess-release-pcfmonfail | The total number of sessions released due to a PCF Monitor failure reported per service. | Int32
> sess-release-grekey | The total number of sessions released due to a GRE Key Mismatch reported per service. | Int32
> sess-release-purged | The total number of sessions released due to inconsistencies found during audits between the A11 Manager task and the Session Manager task. When an inconsistency is identified, the session is released and accounting stops are issued. | Int32
> sess-release-other | The total number of sessions released due to other reasons reported per service. | Int32
> recv-total | The total number of registration requests, renewals, and de-registrations received. | Int32
> accept-total | The total number of registration requests that have been accepted. | Int32
> denied-total | The total number of registration requests that have been rejected. | Int32
> reply -total | The total number of registration replies sent. | Int32
> discard-total | The total number of registration requests that have been discarded. | Int32
> accept-initial | The total number of initial registration requests received and accepted. | Int32
> recv-initial | The total number of initial registration requests received. | Int32
> accept-intrapdsn | The total number of registration requests received for sessions going through an intra-PDSN handoff. Important: This statistic is provided for compatibility only. Please use the accept-active-intrapdsn statistic. | Int32
> accept-active-intrapdsn | The total number of registration requests received with ACTIVE START for an intra-PDSN handoff. | Int32
> accept-dormant-intrapdsn | The total number of registration requests received with ACTIVE STOP for an intra-PDSN handoff. | Int32
> accept-interpdsn | The total number of registration requests received for sessions going through an inter-PDSN handoff. | Int32
> reva-rrq-recv | The total number of Rev-A RRQs received per service. | Int32
> reva-rrq-accept | The total number of Rev-A RRQs accepted per service. | Int32
> reva-rrq-denied | The total number of Rev-A RRQs denied per service. | Int32
> reva-rrq-reply | The total number of Rev-A RRQs per service that were replied to. | Int32
> denied-initial | The total number of initial registration requests received and rejected. | Int32
> discard-initial | The total number of Initial RRQ discarded. | Int32
> recv-initial-setupstart | The total number of Initial Setup/Start RRQ received. | Int32
> accept-initial-setupstart | The total number of Initial Setup/Start RRQ received and accepted. | Int32
> denied-initial-setupstart | The total number of Initial Setup/Start RRQ received and denied. | Int32
> discard-initial-setupstart | The total number of initial start or setup registration requests that have been received and discarded. | Int32
> accept-renew | The total number of registration request renewals received and accepted. | Int32
> denied-renew | The total number of registration request renewals received and rejected. | Int32
> recv-renew | The total number of registration request renewals received. | Int32
> discard-renew | The total number of registration request renewals received and discarded | Int32
> recv-renew-noairlink | The total number of registration request renewals received due to “No airlink”. | Int32
> accept-renew-noairlink | The total number of registration request renewals received due to “No airlink” and accepted. | Int32
> denied-renew-noairlink | The total number of registration request renewals received due to “No airlink” and denied. | Int32
> discard-renew-noairlink | The total number of registration request renewals received due to “No airlink” and discarded. | Int32
> active-start-renew | The total number of ACTIVE START registration request renewals received. Important: This statistic is provided for compatibility only. Please use the accept-renew-activestart statistic. | Int32
> recv-renew-activestart | The total number of RRQ renewals with an Active Start record received. | Int32
> accept-renew-activestart | The total number of RRQ renewals with an Active Start record received and accepted. | Int32
> denied-renew-activestart | The total number of RRQ renewals with an Active Start record received and denied. | Int32
> discard-renew-activestart | The total number of RRQ renewals with an Active Start record received and discarded. | Int32
> active-stop-renew | The total number of ACTIVE STOP registration request renewals received. Important: This statistic is provided for compatibility only. Please use the accept-renew-activestop statistic. | Int32
> recv-renew-activestop | The total number of RRQ renewals with an Active Stop record received. | Int32
> accept-renew-activestop | The total number of RRQ renewals with an Active Stop record received and accepted. | Int32
> denied-renew-activestop | The total number of RRQ renewals with an Active Stop record received and denied. | Int32
> discard-renew-activestop | The total number of RRQ renewals with an Active Stop record received and discarded. | Int32
> accept-dereg | The total number of de-registration requests received and accepted. | Int32
> denied-dereg | The total number of de-registration request renewals received and rejected. | Int32
> recv-dereg | The total number of de-registration request renewals received. | Int32
> discard-dereg | The the total number of de-registration requests received and discarded. | Int32
> recv-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received. | Int32
> accept-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received and accepted. | Int32
> denied-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received and denied | Int32
> discard-dereg-noactivestop | The total number of de-registration requests with a No Active Stop record received and discarded. | Int32
> active-stop-dereg | The total number of ACTIVE STOP de-registration request renewals received and accepted. Important: This statistic is provided for compatibility only. Please use the accept-dereg-activestop statistic. | Int32
> recv-dereg-activestop | The the total number of de-registration request with an Active Stop record received. | Int32
> accept-dereg-activestop | The the total number of de-registration request with an Active Stop record received and accepted. | Int32
> denied-dereg-activestop | The the total number of de-registration request with an Active Stop record received and denied. | Int32
> discard-dereg-activestop | The the total number of de-registration request with an Active Stop record received and discarded. | Int32
> recv-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active Access Network Identifier (ANID) received. | Int32
> accept-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active ANID received and accepted. | Int32
> denied-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active ANID received and denied. | Int32
> discard-intrapdsn-activeanidhandoff | The total number of intra PDSN handoff RRQs with active ANID received and discarded. | Int32
> recv-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received. | Int32
> accept-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received and accepted. | Int32
> denied-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received and denied. | Int32
> discard-intrapdsn-dormantanidhandoff | The total number of intra PDSN handoff RRQs with dormant ANID received and discarded. | Int32
> recv-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active Mobility Event Indicator (MEI) and ANID received. | Int32
> accept-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active MEI and ANID received and accepted. | Int32
> denied-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active MEI and ANID received and denied. | Int32
> discard-interpdsn-activemeianidhandoff | The total number of inter PDSN handoff RRQs with active MEI and ANID received and discarded. | Int32
> send-error | The total number of registration replies for which errors were experienced during transmission. | Int32
> hash-error | The total number of registration requests that had internal hash lookup errors. | Int32
> decode-error | The total number of registration requests that had decode errors. | Int32
> unhandled | The total number of registration requests that had unhandled errors. | Int32
> seqerror | The total number of registration requests that had sequence numbers that were not acceptable. | Int32
> deny-unspec | The total number of registration requests that were denied using reply code of 80H (Registration Denied - reason unspecified) | Int32
> deny-adminprohib | The total number of registration requests that were denied using reply code of 81H (Registration Denied - administratively prohibited). | Int32
> deny-noresource | The total number of registration requests that were denied using reply code of 82H (Registration Denied - insufficient resources). | Int32
> deny-auth | The total number of registration requests that were denied using reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
> deny-idmismatch | The total number of registration requests that were denied using reply code of 85H (Registration Denied - identification mismatch). | Int32
> deny-badrequest | The total number of registration requests that were denied using reply code of 86H (Registration Denied - poorly formed request). | Int32
> deny-unknownpdsn | The total number of registration requests that were denied using reply code of 88H (Registration Denied - unknown PDSN address) | Int32
> deny-revtununavail | The total number of registration requests that were denied using reply code of 89H (Registration Denied - requested reverse tunnel unavailable). | Int32
> deny-revtunreq | The total number of registration requests that were denied using reply code of 8AH (Registration Denied - reverse tunnel is mandatory and “T”-bit not set). | Int32
> deny-unrecogvend | The total number of registration requests that were denied using reply code of 8DH (Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE). | Int32
> deny-sessclosed | The total number of registration requests that were denied using an error code 0x8E for absent RP sessions. Refer to the session-already-closed keyword for the registration-deny command in the PDSN Configuration Mode chapter of the Command Line Interface Reference for additional information. | Int32
> deny-bsninfo | The total number of registration requests that were denied because BSN information was unavailable. | Int32
> deny-noresource-nosessmgr | The total number of RRQ denied due to Insufficient resource, no session manager reported per service. | Int32
> deny-noresource-nomem | The total number of RRQ denied due to Insufficient resource, no memory reported per service. | Int32
> deny-noresource-sessmgrretried | The total number of RRQ denied due to Insufficient resource, session managers retried reported per service. | Int32
> deny-noresource-inputq | The total number of RRQ denied due to Insufficient resource, input queue exceeded reported per service. | Int32
> deny-noresource-policy | The total number of RRQ denied due to Insufficient resource, policy rejected reported per service. | Int32
> deny-noresource-sessmgrrej | The total number of RRQ denied due to Insufficient resource, session manager rejected reported per service. | Int32
> deny-noresource-a11mgrrej | The total number of RRQ denied due to Insufficient resource, A11 manager rejected reported per service. | Int32
> deny-badrequest-alrdorm | The total number of RRQ denied due to poorly formed request, session already dormant reported per service. | Int32
> deny-badrequest-alractive | The total number of RRQ denied due to poorly formed request, already active reported per service. | Int32
> deny-badrequest-setupabsent | The total number of RRQ denied due to poorly formed request, airlink setup absent reported per service. | Int32
> deny-badrequest-miscoaaddr | The total number of RRQ denied due to poorly formed request, mismatched CoA/Source address reported per service. | Int32
> deny-badrequest-pkttooshort | The total number of RRQ denied due to poorly formed request, packet too short reported per service. | Int32
> deny-badrequest-pkttoolong | The total number of RRQ denied due to poorly formed request, packet too long reported per service. | Int32
> deny-badrequest-fieldlen | The total number of RRQ denied due to poorly formed request, invalid field length reported per service. | Int32
> deny-badrequest-flags | The total number of RRQ denied due to poorly formed request, invalid flags reported per service. | Int32
> deny-badrequest-hoanonzero | The total number of RRQ denied due to poorly formed request, HOA non-zero reported per service. | Int32
> deny-badrequest-sse | The total number of RRQ denied due to poorly formed request, invalid SSE reported per service. | Int32
> deny-badrequest-vse | The total number of RRQ denied due to poorly formed request, invalid VSE reported per service. | Int32
> deny-badrequest-authextn | The total number of RRQ denied due to poorly formed request, invalid authorization extension reported per service. | Int32
> deny-badrequest-unkextn | The total number of RRQ denied due to poorly formed request, invalid unknown extension reported per service. | Int32
> deny-badrequest-other | The total number of RRQ denied due to poorly formed request, other reason reported per service. | Int32
> deny-unspec-nullpkt | The total number of RRQ denied due to unspecified reason, null packet received reported per service. | Int32
> deny-unspec-lifezero | The total number of RRQ denied due to unspecified reason, lifetime zero in initial RRQ reported per service. | Int32
> deny-unspec-notready | The total number of RRQ denied due to unspecified reason, session manager not ready reported per service. | Int32
> deny-unspec-crphandoff | The total number of RRQ denied due to unspecified reason, Closed RP handoff in progress reported per service. | Int32
> deny-unspec-noairlink | The total number of RRQ denied due to unspecified reason, no airlink setup reported per service. | Int32
> deny-unspec-intrahandoff | The total number of RRQ Denied due to unspecified reason, intra PDSN handoff triggered reported per service. | Int32
> deny-cong-drop | The total number of denied registration replies discarded due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> deny-cong-adminprohib | The total number of denied registration replies that were sent with a reply code of 81H (Registration Denied - administratively prohibited) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> deny-cong-unknownpdsn | The total number of denied registration replies that were sent with a reply code of 88H (Registration Denied - unknown PDSN address) due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. | Int32
> upd-total | The total number of registration updates that were transmitted. | Int32
> upd-accept | The total number of registration updates that were accepted by the PCF. | Int32
> upd-denied | The total number of registration updates that were denied. | Int32
> upd-unack | The total number of registration updates that were not acknowledged. | Int32
> upd-trans | The total number of initial registration updates that were transmitted. | Int32
> upd-ttlnoretrans | The total number of registration updates that were not re-transmitted due to TTL expiration. | Int32
> upd-retrans | The total number of registration updates that were re-transmitted. | Int32
> upd-received | The total number of registration acknowledgements that were received. | Int32
> upd-ack-received | The total number of registration acknowledgements that were received. | Int32
> upd-discard | The total number of registration acknowledgements that were discarded. | Int32
> upd-senderror | The total number of registration updates for which errors were experienced during transmission. | Int32
> upd-upltrinit | The total number of registration updates that were initiated by upper processing layers. Important: This statistic is obsolete. | Int32
> upd-uplyrinit | The total number of registration updates that were initiated by upper processing layers. Important: This statistic is obsolete. | Int32
> upd-other | The total number of registration updates that were sent due to reasons other than those listed here. | Int32
> upd-handoff | The number of registration updates that were sent due to handoff releases. | Int32
> upd-lifetime | The total number of registration updates that the send reason was Lifetime Expiry reported per service. | Int32
> upd-smgrexit | The total number of registration updates that the send reason was that the session manager exited reported per service. | Int32
> upddeny-unspec | The total number of denied registration updates that were sent with a reply code of 80H (Registration Denied - reason unspecified). | Int32
> upddeny-adminprohib | The total number of denied registration updates that were sent with a reply code of 81H (Registration Denied - administratively prohibited). | Int32
> upddeny-auth | The total number of denied registration updates that were sent with a reply code of 83H (Registration Denied - mobile node failed authentication). | Int32
> upddeny-idmismatch | The total number of denied registration updates that were sent with a reply code of 85H (Registration Denied - identification mismatch). | Int32
> upddeny-badrequest | The total number of denied registration updates that were sent with a reply code of 86H (Registration Denied - poorly formed request). | Int32
> upd-discard-absent | The total number of registration acknowledgements that were discarded due to the session having been already ended because the acknowledgement was late. | Int32
> upd-discard-nomem | The total number of registration acknowledgements that were discarded due to insufficient memory. | Int32
> upd-discard-malform | The total number of registration acknowledgements that were discarded due to being poorly formed. | Int32
> upd-discard-authfail | The total number of registration acknowledgements that were discarded due to the mobile node failing authentication. | Int32
> upd-discard-bounce | The total number of internal communication messages between an A11 Manager task and a Session Manager task that bounced (were not successfully sent). | Int32
> upd-discard-inputq | The number of times that the queue in which incoming calls are kept prior to being processed exceeded its capacity. | Int32
> upd-discard-mismatchid | The total number of discarded registration acknowledgements due to reply code 85H (Registration Denied - identification mismatch). | Int32
> upd-discard-invpktlen | The total number of registration acknowledgements that were discarded due to having an invalid packet length. | Int32
> upd-discard-unkpcf | The total number of registration acknowledgements that were discarded due to Unknown PCF. | Int32
> upd-discard-unhpkt | The total number of registration acknowledgements that were discarded due to Unhandled Packet. | Int32
> upd-discard-misc | The number of registration acknowledgements that were discarded due to reasons other than those listed above. | Int32
> disc-absent | Important: This statistic has been renamed to upd-discard-absent. However, this statistic name is still provided for compatibility only. | Int32
> disc-nomem | Important: This statistic has been renamed to upd-discard-nomem. However, this statistic name is still provided for compatibility only. | Int32
> disc-malform | Important: This statistic has been renamed to upd-discard-malform. However, this statistic name is still provided for compatibility only. | Int32
> disc-authfail | Important: This statistic has been renamed to upd-discard-authfail. However, this statistic name is still provided for compatibility only. | Int32
> disc-bounce | Important: This statistic has been renamed to upd-discard-bounce. However, this statistic name is still provided for compatibility only. | Int32
> disc-inputq | Important: This statistic has been renamed to upd-discard-inputq. However, this statistic name is still provided for compatibility only. | Int32
> disc-mismatchid | Important: This statistic has been renamed to upd-discard-mismatchid. However, this statistic name is still provided for compatibility only. | Int32
> disc-invpktlen | Important: This statistic has been renamed to upd-discard-invpktlen. However, this statistic name is still provided for compatibility only. | Int32
> disc-misc | Important: This statistic has been renamed to upd-discard-misc. However, this statistic name is still provided for compatibility only. | Int32
> sec-violations | The total number of security violations that occurred. | Int32
> sec-badauth | The total number of security violations that occurred due to a mis-computed authentication field. | Int32
> sec-badid | The total number of security violations that occurred due to the receipt of a Security Parameter Index (SPI) that is not configured on the PDSN. | Int32
> sec-badspi | The total number of security violations that occurred due to the receipt of a Security Parameter Index (SPI) that was in the reserved range (0 through 255). | Int32
> sec-mnhaauth | The total number of security violations that occurred due to missing mobile node-home agent authentication extensions. | Int32
> sec-regupdate | The total number of security violations that occurred due to missing registration update authentication extensions | Int32
> rrqdiscard-nosessmgr | The total number of registration requests discarded due to no session manager, reported per service. | Int32
> rrqdiscard-nomem | The total number of registration requests discarded due to no memory, reported per service. | Int32
> rrqdiscard-authfail | The total number of registration requests discarded due to auth failure, reported per service. | Int32
> rrqdiscard-smgrdead | The total number of registration requests discarded due to session manager dead, reported per service. | Int32
> rrqdiscard-adminprohib | The total number of registration requests discarded due to admin prohibited, reported per service. | Int32
> rrqdiscard-smgrnotready | The total number of registration requests discarded due to session manager not ready, reported per service. | Int32
> rrqdiscard-unkpdsn | The total number of registration requests discarded due to unknown pdsn, reported per service. | Int32
> rrqdiscard-bounce | The total number of registration requests discarded due to internal bounce error, reported per service. | Int32
> rrqdiscard-inputq | The total number of registration requests discarded due to input queue exceeded, reported per service. | Int32
> rrqdiscard-maxsess | The total number of registration requests discarded due to max sessions reached, reported per service. | Int32
> rrqdiscard-invlen | The total number of registration requests discarded due to invalid packet length, reported per service. | Int32
> rrqdiscard-grekey | The total number of registration requests discarded due to GRE key changed, reported per service. | Int32
> rrqdiscard-overload | The total number of registration requests discarded due to overload/congestion, reported per service. | Int32
> rrqdiscard-misc | The total number of registration requests discarded due to miscellaneous errors reported per service. | Int32
> ttlprepaid | The total number of Prepaid calls facilitated by the service. | Int32
> curprepaid | The total number of Prepaid calls currently being facilitated by the service. | Int32
> ttlonlineauthsucc | The total number of successful Online Authentications for the service. | Int32
> ttlonlineauthfail | TThe total number of successful Online Authentications for the service. | Int32
> rx-pkt-xoff | The total number of packets Received with XOFF per service. | Int32
> rx-pkt-xon | The total number of packets Received with XON per Service. | Int32
> xontoxoff | The total number of XON->XOFF transitions per service. | Int32
> pkt-dropped-xoff | The total number of output packets dropped to XOFF per service. | Int32
> bytes-dropped-xoff | The total number of output bytes dropped on XOFF per Service. | Int32
> sess-num-transmitted | The total number of RP session update messages transmitted. | Int32
> sess-accepted | The total number of RP session update ack messages accepted. | Int32
> sess-denied | The total number of RP session update messages denied. | Int32
> sess-not-acknowledged | The total number of RP session update messages not acknowledged. | Int32
> sess-initial-update | The total number of RP session update messages initially transmitted. | Int32
> sess-update-retransmitted | The total number of RP session update messages re-transmitted. | Int32
> sess-update-ack-received | The total number of RP session update acknowledgement messages received. | Int32
> sess-update-ack-discarded | The total number of RP session update acknowledgement messages discarded. | Int32
> sess-update-send-error | The total number of RP session update send errors that occurred. | Int32
> sess-updreason-alwayson | The total number of session updates sent due to Always On, reported per service. This is a Rev-A specific statistic. | Int32
> sess-updreason-qosinfo | The total number of session updates sent due to QoS Info, reported per service. | Int32
> sess-updreason-qostftviol | The total number of session updates sent due to TFT Violation, reported per service. | Int32
> sess-updreason-qostrafviol | The total number of session updates sent due to Traffic Violation, reported per service. | Int32
> sess-updreason-qostrafpol | The total number of session updates sent due to Traffic Policing, reported per service. | Int32
> sess-updreason-qosoptrig | The total number of session updates sent due to Operator Triggered, reported per service. | Int32
> sess-always-on-indication | The total number of RP session updates supporting Always-on functionality. | Int32
> sess-reason-unspecified | The total number of RP session update messages denied with status code reason-unspecified. | Int32
> sess-PDSN-auth-fail | The total number of RP session update messages denied due to message authentication failure at the PCF. Important: This statistic is provided for compatibility only. Please use the sess-pdsn-auth-fail statistic. | Int32
> sess-pdsn-auth-fail | The total number of RP session update messages denied due to message authentication failure at the PCF. | Int32
> sess-ID-mismatch | The total number of RP session update messages denied due to having an ID mismatch at the PCF. Important: This statistic is provided for compatibility only. Please use the sess-id-mismatch statistic. | Int32
> sess-id-mismatch | The total number of RP session update messages denied due to having an ID mismatch at the PCF. | Int32
> sess-poorly-formed-update | The total number of session update messages denied by the PCF due to poorly formed message error. | Int32
> sess-para-not-update | The total number of update ack messages received with status code indicating that parameters were not updated. | Int32
> sess-upddenied-noresource | The total number of session updates sent due to Insufficient Resources, reported per service. | Int32
> sess-upddenied-adminprohib | The total number of session updates denied due to Admin Prohibited, reported per service. | Int32
> sess-upddenied-idnotsupp | The total number of session updates denied due to Profile ID Not Supported, reported per service. | Int32
> sess-upddenied-handoff | The total number of session updates denied due to handoffs in progress per service. | Int32
> sess-absent | The total number of update ack messages that were discarded by the PDSN due to no session being present at the PDSN. | Int32
> sess-no-memory | The total number of update ack messages that were discarded by the PDSN due to no memory available. | Int32
> sess-malformed | The total number of update ack messages that were discarded by the PDSN due to being malformed. | Int32
> sess-auth-fail | The total number of update ack messages that were discarded by the PDSN due to message authentication failure. | Int32
> sess-ID-bounce-error | The total number of update ack messages that were discarded by the PDSN due to internal communication error within the PDSN. | Int32
> sess-input-Q-exceeded | The total number of update ack messages that were discarded by the PDSN due to exceeding input pacing queues at the PDSN. | Int32
> sess-mismatched-ID | The total number of update ack messages that were discarded by the PDSN due to mismatched id in the message. | Int32
> sess-invalid-packet-length | The total number of update ack messages that were discarded by the PDSN due to bad packet length. | Int32
> sess-misc-reasons | The total number of update ack messages that were discarded by the PDSN due to other reasons. | Int32
> sess-updackdisc-sessdisc | Session Update Ack Discard Reasons – Session Disconnecting per service. | Int32
> sess-updackdisc-pktnothand | Session Update Ack Discard Reasons – Packet Not Handled per service. | Int32
> sess-gre-packet-sent-sdb | The total number of GRE packets transmitted in short data burst (SDB). | Int32
> sess-gre-byte-sent-sdb | The total number of GRE bytes transmitted in short data burst (SDB). | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883