> UDR Format Configuration Mode Commands
> The UDR Configuration Mode enables configuring User Detail Record (UDR) formats. UDR file formats are represented in Comma Separated Value (CSV).
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> attribute
> This command specifies the order of fields in the UDR.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> attribute attribute { [ format { MM/DD/YY-HH:MM:SS | MM/DD/YYYY-HH:MM:SS | YYYY/MM/DD-HH:MM:SS | YYYYMMDDHHMMSS | seconds } [ localtime ] | [ { bytes | pkts } { downlink | uplink } ] ] priority priority }
> no attribute attribute [ priority priority ]
> no
> Removes the specified attribute configuration.
> attribute
> Specifies the attribute.
> attribute must be one of the following:

> Attribute | Description
> diameter-session-id | Unique Diameter session identifier. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> radius-called-station-id | Called Station ID of the mobile handling the flow.
> radius-calling-station-id | Calling Station ID of the mobile handling the flow.
> radius-fa-nas-identifier | RADIUS NAS identifier of Foreign Agent (FA).
> radius-fa-nas-ip-address | RADIUS IP address of Foreign Agent (FA).
> radius-nas-identifier | RADIUS NAS identifier.
> radius-nas-ip-address | RADIUS NAS IP address. Note: This attribute is interchangeable with sn-st16-ip-addr for the user.
> radius-user-name | User name associated with the flow.
> sn-3gpp2-bsid | This option is obsolete. To configure this attribute see the rule-variable command.
> sn-3gpp2-carrier-id | This option is obsolete. To configure this attribute see the rule-variable command.
> sn-3gpp2-esn | This option is obsolete. To configure this attribute see the rule-variable command.
> sn-3gpp2-meid | This option is obsolete. To configure this attribute see the rule-variable command.
> sn-3gpp2-service-option | This option is obsolete. To configure this attribute see the rule-variable command.
> sn-acct-beginning-session | Session beginning information. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-acct-session-continue | Session continue information. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-acct-session-id | Indicator for the accounting session Identifier.
> sn-acct-session-time | Duration from acct-status-type:start to acct-status-type:stop. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-acct-status-type | Accounting status identifier. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-charging-type | Charging type:
> • | offline
> • | online
> Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-closure-reason | Includes reason for the termination of the flow/UDR:
> • | 0: normal, i.e., subscriber session ended
> • | 1: handoff control processing specified
> • | 2: subscriber session terminated
> • | 3: flow timeout
> sn-content-id | Unique identifier for the content-id.
> sn-content-label | Identifier for text label for content-id.
> sn-content-vol | Identifier for content volume.
> sn-correlation-id | RADIUS correlation identifier.
> sn-duration | Duration between the last and first packet for the record.
> sn-end-time [ format format] | Timestamp for last packet of flow in UTC.
> sn-fa-correlation-id | RADIUS Correlation Identifier of the Foreign Agent (FA).
> sn-filler-blank | Keeps attributes place blank and generates an empty UDR field.
> sn-filler-zero | Fills ‘0’ for this attribute place in the EDR/UDR.
> sn-format-name | Indicates the name of the UDR/EDR format used.
> sn-group-id | Indicates the sequence group identifier for the records.
> sn-ha-ip-address | Home Agent IP address. Important: This attribute is customer specific, and is only available in ‘ 8.3 and later releases.
> sn-local-seq-no | Unique local sequence number of UDR identifier per ACSMgr and linearly increasing in UDR file.
> sn-ocs-ip-address | Online Charging Server's IP address. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-rulebase | Indicates the name of the ACS rulebase used.
> sn-sequence-no | Unique sequence number (per sn-sequence -group and radius-nas-ip-address) of UDR identifier and linearly increasing in UDR file.
> sn-served-bsa-addr | Indicator for address of Base Station Area being served.
> sn-service-name | Indicator for ACS service name.
> sn-st16-ip-addr | IP address of the chassis handling this flow. Important: This attribute is interchangeable with radius-nas-ip-address for other systems.
> sn-start-time [ format format ] | Timestamp for first packet of flow in UTC.
> sn-stream-number | Unique UDR billing record identifier. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.
> sn-subscriber-id | Indicator for subscriber ID.
> sn-subscriber-nat-flow-ip | NAT IP address(es) of NAT-enabled subscriber.
> sn-timestamp | Timestamp when the UDR is actually generated. Important: This attribute is customer specific, and is only available in Release 8.3 and later releases.

> ‌
> format { MM/DD/YY-HH:MM:SS | MM/DD/YYYY-HH:MM:SS | YYYY/MM/DD-HH:MM:SS | YYYYMMDDHHMMSS | seconds }
> Specifies the timestamp format.
> localtime
> Specifies the local time. By default, timestamps are displayed in GMT.
> { bytes | pkts } { downlink | uplink }
> Specifies bytes/packets sent/received from/by mobile.
> priority priority
> Specifies the position priority of the value within the UDR. Lower numbered priorities (across all attribute, event-label, and rule-variable) occur first.
> priority must be an integer from 1 through 65535. Up to 50 position priorities (across all attribute, event-label, and rule-variable) can be configured.
> Usage
> Use this command to set the attributes and priority for UDR file format.
> A particular field in UDR format can be entered multiple times at different priorities. While removing the UDR field using the no attribute command either you can remove all occurrences of a particular field by specifying the field name or a single occurrence by additionally specifying the optional priority keyword.
> Example
> attribute radius-user-name priority 12
> end
> This command returns the CLI prompt to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to change to the Exec mode.
> event-label
> This command configures an optional event ID to use in generated billing records.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> event-label label priority priority
> no event-label
> no
> Removes the previously configured event label for UDR attribute.
> label
> Specifies event label for attribute to be used for UDR format.
> label must be an alpha and/or numeric string of 1 through 63 characters in length.
> priority priority
> Specifies the CSV position of event ID in UDR.
> priority must be an integer from 1 through 65535.
> Usage
> Use this command to set the event ID and its position in UDR file format.
> Example
> event-label radius_csv1 priority 23
> exit
> This command exits the UDR Format Configuration Mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> rule-variable
> This command specifies the order of fields in the UDR.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> rule-variable protocol rule priority priority
> no rule-variable [ priority priority ] protocol rule
> no
> Removes the rule-variable protocol configuration.
> protocol rule
> Specifies the rule variable for UDR format.
> protocol must be one of the following with specified rule:

> • | bearer 3gpp2: Bearer-related configuration:

> • | always-on

> • | bsid

> • | carrier-id

> • | esn

> • | ip-qos

> • | ip-technology

> • | meid

> • | release-indicator

> • | service-option

> • | session-begin

> • | session-continue

> Important: For more information on protocol-based rules see the Ruledef Configuration Mode Commands chapter.
> priority priority
> Specifies the CSV position of the value in the UDR.
> priority must be an integer from 1 through 65535.
> Usage
> Use this command to set the rule variables priority for UDR file format.
> A particular field in UDR format can be entered multiple times at different priorities. While removing the UDR field using the no rule-variable command either you can remove all occurrences of a particular field by specifying the field name or a single occurrence by additionally specifying the optional priority keyword.
> Example
> rule-variable bearer 3gpp2 bsid priority 36

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883