> MAG Schema Statistics
> This schema provides the following type of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise described.
> The following variables are supported:
> MAG Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the MAG service. | String / Static
> vpnid | The identification number of the context configured on the system that is currently facilitating the MAG service. This is an internal reference number. | Gauge / Int32
> servname | Displays the name of the MAG service for which the statistics are displayed. | String / Static
> servid | The identification number of the service configured on the system that is currently facilitating the MAG service. This is an internal reference number. | Gauge / Int32
> sess-cur | The total number of sessions currently established on this system. | Counter / Int32
> bindupd | The total number of all binding updates sent by this system. | Counter / Int32
> bindupd-init | The total number of initial request transmit binding updates sent by this system. | Counter / Int32
> bindupd-initretrans | The total number of initial request retransmit binding updates sent by this system. | Counter / Int32
> bindupd-renew | The total number of renew request transmit binding updates sent by this system. | Counter / Int32
> bindupd-renewretrans | The total number of renew request retransmit binding updates sent by this system. | Counter / Int32
> bindupd-dereg | The total number of deregistration request transmit binding updates sent by this system. | Counter / Int32
> bindupd-deregretrans | The total number of deregistration request retransmit binding updates sent by this system. | Counter / Int32
> bindack | The total number of all binding acknowledgements received by this system. | Counter / Int32
> bindack-error | The total number of all binding acknowledgements, with errors, received by this system. | Counter / Int32
> bindack-accept | The total number of all binding acknowledgements received, and accepted by this system or the specified service. | Counter / Int32
> bindack-denied | The total number of all binding acknowledgements received, but denied by this system or the specified service. | Counter / Int32
> bindack-init | The total number of all binding acknowledgements - initial reply received by this system. | Counter / Int32
> bindack-renew | The total number of all binding acknowledgements - renew reply received by this system. | Counter / Int32
> bindack-dereg | The total number of all binding acknowledgements - deregistration reply received by this system. | Counter / Int32
> deniedlma-noresource | The total number of binding updates sent by this system or the specified service but denied by the LMA due to insufficient resources. | Counter / Int32
> deniedlma-mismatchid | The total number of binding updates sent by this system or the specified service but denied by the LMA due to mismatched IDs. | Counter / Int32
> deniedlma-mnauthfail | The total number of binding updates sent by this system or the specified service but denied by the LMA due to mobile node authorization failures. | Counter / Int32
> deniedlma-adminproh | The total number of binding updates sent by this system or the specified service but denied by the LMA due to admin prohibited conditions. | Counter / Int32
> deniedlma-msgidrqd | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing message IDs. | Counter / Int32
> deniedlma-dadfailed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to DAD failures. | Counter / Int32
> deniedlma-homesubnet | The total number of binding updates sent by this system or the specified service but denied by the LMA due to incorrect home subnet. | Counter / Int32
> deniedlma-seqoow | The total number of binding updates sent by this system or the specified service but denied by the LMA due to sequence out of window conditions. | Counter / Int32
> deniedlma-typchgdis | The total number of binding updates sent by this system or the specified service but denied by the LMA due to registration type change disallowed. | Counter / Int32
> deniedlma-unspec | The total number of binding updates sent by this system or the specified service but denied by the LMA due to unspecified reasons. | Counter / Int32
> deniedlma-servauthfailed | The total number of binding updates sent by this system or the specified service but denied by the LMA due to failed service authorizations. | Counter / Int32
> deniedlma-proxyreg | The total number of binding updates sent by this system or the specified service but denied by the LMA due to proxy registration not being enabled. | Counter / Int32
> deniedlma-timestamp | The total number of binding updates sent by this system or the specified service but denied by the LMA due to timestamp mismatches. | Counter / Int32
> deniedlma-timestamplower | The total number of binding updates sent by this system or the specified service but denied by the LMA due to lower than expected timestamps. | Counter / Int32
> deniedlma-mismnid | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing mobile node ID options. | Counter / Int32
> deniedlma-mishnp | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing HNP options. | Counter / Int32
> deniedlma-misaccesstech | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing access technology options. | Counter / Int32
> deniedlma-mishandoffind | The total number of binding updates sent by this system or the specified service but denied by the LMA due to missing handoff indication options. | Counter / Int32
> deniedlma-notauthhnp | The total number of binding updates sent by this system or the specified service but denied by the LMA due to not being authorized for HNP. | Counter / Int32
> deniedlma-notlmamobile | The total number of binding updates sent by this system or the specified service but denied by the LMA due incorrect LMA for mobility. | Counter / Int32
> deniedlma-notauthproxyreg | The total number of binding updates sent by this system or the specified service but denied by the LMA due to not being authorized for proxy registration. | Counter / Int32
> deniedlma-bceprefix | The total number of binding updates sent by this system or the specified service but denied by the LMA due to BCE prefix mismatches. | Counter / Int32
> bindack-errormishnp | The total number of binding acknowledgements with missing HNP errors received by this system or the specified service. | Counter / Int32
> bindack-errornai | The total number of binding acknowledgements with missing NAI errors received by this system or the specified service. | Counter / Int32
> bindack-errorhomeaddconf | The total number of binding acknowledgements with home address conflict errors received by this system or the specified service. | Counter / Int32
> bindack-errormatchreq | The total number of binding acknowledgements with matching requests not found errors received by this system or the specified service. | Counter / Int32
> bindack-errorbadlyformed | The total number of binding acknowledgements with badly formed message errors received by this system or the specified service. | Counter / Int32
> bindack-errorchecksum | The total number of binding acknowledgements with checksum errors received by this system or the specified service. | Counter / Int32
> bindack-errorsessnotfound | The total number of binding acknowledgements with session not found errors received by this system or the specified service. | Counter / Int32
> bindrev-sent | The total number of binding revocations sent by this system or the specified service. | Counter / Int32
> bindrev-retriessent | The total number of binding revocation retries sent by this system or the specified service. | Counter / Int32
> bindrev-ackrcvd | The total number of binding revocation acknowledgements received by this system or the specified service. | Counter / Int32
> bindrev-notacked | The total number of binding revocations sent, but not acknowledged, by this system or the specified service. | Counter / Int32
> bindrev-rcvd | The total number of binding revocations received by this system or the specified service. | Counter / Int32
> bindrev-acksent | The total number of binding revocation acknowledgements sent by this system or the specified service. | Counter / Int32
> bindrev-discardtotal | The total number of binding revocation acknowledgements received and discarded by this system or the specified service. | Counter / Int32
> bindrev-discardsessnotfound | The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by this system or the specified service. | Counter / Int32
> bindrev-discardbadreq | The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by this system or the specified service. | Counter / Int32
> bindrev-discarddecode | The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by this system or the specified service. | Counter / Int32
> bindrev-discardchecksum | The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by this system or the specified service. | Counter / Int32
> bindrev-discardmsgtype | The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by this system or the specified service. | Counter / Int32
> bindrev-discardnomemory | The total number of binding revocation acknowledgements received and discarded, due to insufficient memory, by this system or the specified service. | Counter / Int32
> rxpackets | The total number of packets received by this system. | Counter / Int32
> rxpackets-6in6 | The total number of IPv6-in-IPv6 tunnel packets received by this system. | Counter / Int32
> rxpackets-4in6 | The total number of IPv4-in-IPv6 tunnel packets received by this system or the specified service. | Counter / Int32
> rxpackets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel packets received by this system or the specified service. | Counter / Int32
> rxpackets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel packets received by this system or the specified service. | Counter / Int32
> rxoctets | The total number of octets received by this system. | Counter / Int32
> rxoctets-6in6 | The total number of IPv6-in-IPv6 tunnel octets received by this system. | Counter / Int32
> rxoctets-4in6 | The total number of IPv4-in-IPv6 tunnel octets received by this system or the specified service. | Counter / Int32
> rxoctets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel octets received by this system or the specified service. | Counter / Int32
> rxoctets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel octets received by this system or the specified service. | Counter / Int32
> dataerror | The total number of data errors received by this system. | Counter / Int32
> dataerror-proto | The total number of protocol type data errors received by this system. | Counter / Int32
> dataerror-invpktlen | The total number of invalid packet length data errors received by this system. | Counter / Int32
> dataerror-nosess | The total number of no session found data errors received by this system. | Counter / Int32
> txpackets | The total number of packets sent by this system. | Counter / Int32
> txpackets-6in6 | The total number of IPv6-in-IPv6 tunnel packets sent by this system. | Counter / Int32
> txpackets-4in6 | The total number of IPv4-in-IPv6 tunnel packets sent by this system or the specified service. | Counter / Int32
> txpackets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel packets sent by this system or the specified service. | Counter / Int32
> txpackets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel packets sent by this system or the specified service. | Counter / Int32
> txoctets | The total number of octets sent by this system. | Counter / Int32
> txoctets-6in6 | The total number of IPv6-in-IPv6 tunnel octets sent by this system. | Counter / Int32
> txoctets-4in6 | The total number of IPv4-in-IPv6 tunnel octets sent by this system or the specified service. | Counter / Int32
> txoctets-ipv6greipv4 | The total number of IPv4-in-IPv6 GRE tunnel octets sent by this system or the specified service. | Counter / Int32
> txoctets-ipv6greipv6 | The total number of IPv6-in-IPv6 GRE tunnel octets sent by this system or the specified service. | Counter / Int32
> disc | The total number of disconnects initiated by this system. | Counter / Int32
> disclifetime | The total number of disconnects due to lifetime expiry initiated by this system. | Counter / Int32
> discaccessinit | The total number of disconnects due to de-registrations initiated by this system or the specified service. | Counter / Int32
> discadmin | The total number of disconnects due to admin drops initiated by this system. | Counter / Int32
> discother | The total number of disconnects due to “other reasons” initiated by this system. | Counter / Int32
> disclmarevoc | The total number of disconnects due to LMA revocations received by this system or the specified service. | Counter / Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883