> QCI - QoS Mapping Configuration Mode Commands
> The QoS Class Index (QCI) to QoS Mapping Configuration Mode is used to map QoS Class Indexes to enforceable QoS parameters. Mapping can occur between the RAN and the Serving Gateway (S-GW), the Mobility Management Entity (MME), and/or the PDN Gateway (P-GW) in an LTE network or between the RAN and the eHRPD Serving Gateway (HSGW) in an eHRPD network.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> qci
> Creates and maps QCI values to enforceable QoS parameters.
> Product
> HSGW, P-GW, S-GW
> Privilege
> Administrator
> Syntax
> qci num
> [ delay-class num precedence-class num reliability-class num
> [ downlink { encaps-header { copy-inner | dscp-marking hex } | user-datagram dscp-marking hex [ encaps-header { copy-inner | dscp-marking hex } ] } ]
> [ gbr ]
> [ max-packet-delay num max-error-rate num
> [ non-gbr ]
> [ uplink { encaps-header { copy-inner | dscp-marking hex } | user-datagram dscp-marking hex [ encaps-header { copy-inner | dscp-marking hex } ] } ]
> [ default | no ] qci num
> default
> Resets the default values for the select QCI value.
> no
> Disables the selected QCI value.
> num
> Specifies the QCI value to be enabled. num must be an integer value between 1 and 32.
> QCI values 1 through 9 are standard values. Only undefined values (10 through 32) can be defined.
> Important: QCI values 1 through 9 are defined in the 3GPP Specification TS 23.203 “Policy and charging control architecture”.
> delay-class num precedence-class num reliability-class num
> delay-class num: Pre-release 8 value for configuring packet delay. num must be an integer value between 1 and 32.
> precedence-class num: Pre-release 8 value for configuring packet precedence. num must be an integer value between 1 and 32.
> reliability-class num: Pre-release 8 value for configuring packet reliability. num must be an integer value between 1 and 32.
> downlink { encaps-header { copy-inner | dscp-marking hex } | user-datagram dscp-marking hex [ encaps-header { copy-inner | dscp-marking hex } ] }
> Configures parameters for downlink traffic.
> encaps-header: Specifies that the DSCP marking must be set on the encapsulation header for IP-in-IP, GRE, or GTP encapsulation.
> user-datagram dscp-marking hex: Specifies that the UDP DSCP marking is to be defined by this keyword. hex must expressed as a hexadecimal value from 0x00 through 0x3F.
> { copy-inner | dscp-marking hex }

> • | copy-inner: Specifies that the DSCP marking is to be acquired from the UDP headers within the encapsulation.

> • | dscp-marking hex: Specifies that the DSCP marking is to be defined by this keyword. hex must expressed as a hexadecimal value from 0x00 through 0x3F.

> gbr
> Specifies that this QCI type is Guaranteed Bit Rate (GBR).
> max-packet-delay num max-error-rate num
> max-packet-delay num: Specifies the maximum packet delay in milliseconds that can be applied to the data with the QCI. num must be an integer value from 10 through 1000. Default is 10ms for QCI values greater than 9.
> max-error-rate num: Specifies the maximum error loss rate of non-congestion related packet loss. num must be an integer value from 1 through 6 specifying 10-1 through 10-6. Default is 3 (or 10-3) for QCI values greater than 9.
> Important: Defaults for QCI values less than 9 are defined in the 3GPP Specification TS 23.203 “Policy and charging control architecture”.
> non-gbr
> Specifies that this QCI type is non-Guaranteed Bit Rate (non-GBR).
> uplink { encaps-header { copy-inner | dscp-marking hex } | user-datagram dscp-marking hex [ encaps-header { copy-inner | dscp-marking hex } ] }
> Configures parameters for uplink traffic.
> encaps-header: Specifies that the DSCP marking must be set on the encapsulation header for IP-in-IP, GRE, or GTP encapsulation.
> user-datagram dscp-marking hex: Specifies that the UDP DSCP marking is to be defined by this keyword. hex must expressed as a hexadecimal value from 0x00 through 0x3F.
> { copy-inner | dscp-marking hex }

> • | copy-inner: Specifies that the DSCP marking is to be acquired from the UDP headers within the encapsulation.

> • | dscp-marking hex: Specifies that the DSCP marking is to be defined by this keyword. hex must expressed as a hexadecimal value from 0x00 through 0x3F.

> Usage
> Use this command to create and map QCI values to enforceable QoS parameters.
> Example
> The following command creates a QCI value of 15 and defines the uplink encapsulation header as using the DSCP marking from the encapsulated UDP header:
> qci 15 uplink encaps-header copy-inner

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883