> EAP Mode Configuration Mode Commands
> The EAP Mode Configuration Mode is used to configure EAP authentication method supported by the system.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec Mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Returns to the previous mode.
> method
> Configures the EAP method used for authentication.
> Product
> PDIF, ASN GW
> Privilege
> Security Administrator, Administrator
> Syntax
> method { eap-aka | eap-gtc | eap-md5 } [ priority num ]
> eap-aka | eap-gtc | eap-md5
> eap-aka: Specifies that the EAP-AKA method is to be used for authentication.
> eap-gtc: Specifies that the EAP-GTC method is to be used for authentication.
> eap-md5: Specifies that the EAP-MD5 method is to be used for authentication.
> priority num
> Specifies a priority order for a specific EAP authentication method. num must be an integer fro 1 to 65535.
> Usage
> Use this command to specify the EAP authentication method(s) to use and to place multiple methods in priority order.
> Example
> The following command sets EAP-AKA as one of the EAP authentication methods and places it as priority of 3:
> method eap-aka priority 3

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883