> Accounting Management
> This section contains additions and changes made to the accounting-related parameters available in Release 8.0 unless specifically designated as being in Release 8.1.
> Bulk Statistic Enhancements in Release 8.0
> This section lists bulk statistic additions and changes in Release 8.0. Detailed information on bulk statistics is located in both the System Administration Guide and in the Statistics and Counters Reference.
> Bulk Statistic Additions
> Support for the following bulk statistics has been added:
> Context Schema
> The following are new for Release 8.0:

> l | sfw-total-dosattacks

> l | sfw-total-flows

> l | sfw-total-injectedbytes

> l | sfw-total-injectedpkts

> gprs schema
> The following are new for Release 8.0:

> l | sns-config-fail-rcv-prot-err-unspec

> l | sns-config-fail-sent-prot-err-unspec

> l | sns-config-fail-rcv-inval-essential-param

> l | sns-config-fail-sent-inval-essential-param

> l | sns-add-fail-rcv-prot-err-unspec

> l | sns-add-fail-sent-prot-err-unspec

> l | sns-add-fail-rcv-inval-essential-param

> l | sns-add-fail-sent-inval-essential-param

> l | num-sns-delete-rcvd

> l | sns-delete-fail-rcv-prot-err-unspec

> l | sns-delete-fail-sent-prot-err-unspec

> l | sns-delete-fail-rcv-inval-essential-param

> l | sns-delete-fail-sent-inval-essential-param

> l | num-sns-cw-rcvd

> l | sns-cw-fail-rcv-prot-err-unspec

> l | sns-cw-fail-sent-prot-err-unspec

> l | sns-cw-fail-rcv-inval-essential-param

> l | sns-cw-fail-sent-inval-essential-param

> l | bssgp-flush-llc-msg-sent

> l | bssgp-flush-llc-ack-msg-rcvd

> l | bssgp-cs-paging-msg-sent

> l | bssgp-ps-paging-msg-sent

> l | bssgp-pkt-drop-flow-ctrl-queue-full

> l | bssgp-downlink-pkt-drop

> l | bssgp-bvc-unknown-ms-status-msg-rcvd

> l | bssgp-bvc-unknown-ms-status-msg-sent

> l | sndcp-xid-req-ms-init

> l | sndcp-xid-ind-sgsn-init

> l | sndcp-npdus-ack-rcvd-ms

> l | sndcp-npdus-ack-sent-ms

> l | sndcp-npdus-uack-rcvd-ms

> l | sndcp-npdus-uack-sent-ms

> l | sndcp-bytes-ack-rcvd-ms

> l | sndcp-bytes-ack-sent-ms

> l | sndcp-bytes-uack-rcvd-ms

> l | llc-data-sent-ind-tx

> l | llc-frame-stats-ui-tx

> l | llc-frame-stats-ui-ciph-rx

> l | llc-frame-stats-ui-ciph-tx

> l | llc-frame-stats-octets-rcvd

> l | llc-frame-stats-octets-sent

> l | llc-frame-stats-unack-frames-rcvd

> l | llc-frame-stats-unack-frames-sent

> l | llc-frame-stats-xid-rcvd

> l | llc-frame-stats-xid-sent

> l | packets-sent-to-bsc

> l | packets-rcvd-from-bsc

> l | bytes-sent-to-bsc

> l | bytes-rcvd-from-bsc

> l | gprs-num-subs-gea0-capable

> l | gprs-num-subs-gea1-capable

> l | gprs-num-subs-gea2-capable

> l | gprs-num-subs-gea3-capable

> l | gprs-num-subs-gea0-negotiated

> l | gprs-num-subs-gea1-negotiated

> l | gprs-num-subs-gea2-negotiated

> l | gprs-num-subs-gea3-negotiated

> gtpc schema

> l | err-ind-rx-discard

> l | num-dt-recv-err-ind

> l | sri-req

> gtpp schema

> l | mgmt-int-close

> sccp schema

> l | sccp-reassem-err-timer

> l | sccp-reassem-err-sequence

> l | sccp-reassem-err-space

> l | sccp-err-msg-rcvd

> l | sccp-unequipped-user

> l | sccp-reason-unknown

> l | sccp-congested-msg-rcvd

> l | sccp-prohibit-msg-rcvd

> sgsn schema
> The following are new for Release 8.0:

> l | gprs_standby

> l | gprs_ready

> l | 2G-rau-accept-intra

> l | 3G-ret-rau-accept-periodic

> l | 2G-ret-rau-accept-periodic

> l | 3G-ms-init-detach

> l | 2G-ms-init-detach

> l | 3G-ms-init-imsi-detach

> l | 2G-ms-init-imsi-detach

> l | 3G-ms-init-comb-detach

> l | 3G-attached

> l | 2G-attached

> l | 3G-home-subscribers

> l | 2G-home-subscribers

> l | 3G-visiting-national

> l | 2G-visiting-national

> l | 3G-visiting-foreign

> l | 2G-visiting-foreign

> l | pmm-connected

> l | pmm-idle

> l | gprs-standby

> l | gprs-ready

> l | 3G-attached-with-pdp

> l | 2G-attached-with-pdp

> l | 3G-detached

> l | 3G-total-attach-req-all

> l | 3G-total-attach-req

> l | 3G-total-comb-attach-req

> l | 2G-total-attach-req-all

> l | 2G-total-attach-req

> l | 2G-total-comb-attach-req

> l | request-requesting-relayed

> l | request-renewing-relayed

> l | ack-rx

> l | ack-for-inform

> l | ack-renewing-rx

> l | ack-tx

> l | ack-renewing-tx

> l | ack-relayed

> l | ack-renewing-relayed

> l | 3G-local-ptmsi-Attch

> l | 3G-local-ptmsi-Attch-comb

> l | 3G-remote-ptmsi-Attch

> l | 3G-remote-ptmsi-Attch-comb

> l | 2G-local-ptmsi-Attch-comb

> l | 2G-remote-ptmsi-Attch-comb

> l | 3G-ret-imsi-attach

> l | 3G-ret-imsi-attach-comb

> l | 2G-ret-imsi-attach

> l | 2G-ret-imsi-attach-comb

> l | 3G-ret-local-ptmsi-attach

> l | 3G-ret-local-ptmsi-attach-comb

> l | 2G-ret-local-ptmsi-attach

> l | 2G-ret-local-ptmsi-attach-comb

> l | 3G-ret-remote-ptmsi-attach

> l | 3G-ret-remote-ptmsi-attach-comb

> l | 2G-ret-remote-ptmsi-attach

> l | 2G-ret-remote-ptmsi-attach-comb

> l | 3G-attach-accept

> l | 3G-comb-attach-accept

> l | 3G-ret-attach-accept

> l | 3G-ret-attach-accept-comb

> l | 2G-ret-attch-accept-comb

> l | 3G-attach-reject-all

> l | 3G-attach-reject

> l | 3G-attach-reject-comb

> l | 2G-attach-reject-all

> l | 2G-attach-reject

> l | 2G-attach-reject-comb

> l | 3G-comb-attach-rej-imsi-unknown-at-hlr

> l | 2G-comb-attach-rej-imsi-unknown-at-hlr

> l | 3G-comb-attach-rej-illegal-ms

> l | 2G-comb-attach-rej-illegal-ms

> l | 3G-comb-attach-rej-illegal-me

> l | 2G-comb-attach-rej-illegal-me

> l | 3G-comb-gprs-service-not-allowed

> l | 2G-comb-gprs-service-not-allowed

> l | 3G-comb-gprs-and-non-gprs-svc-not-allow

> l | 2G-comb-gprs-and-non-gprs-svc-not-allow

> l | 3G-comb-attach-rej-msid-not-derived-by-nwt

> l | 2G-comb-attach-rej-msid-not-derived-by-nwt

> l | 3G-comb-attach-rej-implicitly-detach

> l | 2G-comb-attach-rej-implicitly-detach

> l | 3G-comb-attach-rej-plmn-not-allowed

> l | 2G-comb-attach-rej-plmn-not-allowed

> l | 3G-comb-attach-rej-la-not-allowed

> l | 2G-comb-attach-rej-la-not-allowed

> l | 3G-comb-roam-not-allow-in-loc-area

> l | 2G-comb-roam-not-allow-in-loc-area

> l | 3G-comb-gprs-svc-not-allow-in-plmn

> l | 2G-comb-gprs-svc-not-allow-in-plmn

> l | 3G-comb-no-suitable-cells-in-loc-area

> l | 2G-comb-no-suitable-cells-in-loc-area

> l | 3G-comb-attach-rej-msc-not-reachable

> l | 2G-comb-attach-rej-msc-not-reachable

> l | 3G-comb-attach-rej-network-failure

> l | 2G-comb-attach-rej-network-failure

> l | 3G-comb-attach-rej-mac-failure

> l | 2G-comb-attach-rej-mac-failure

> l | 3G-comb-attach-rej-sync-failure

> l | 2G-comb-attach-rej-sync-failure

> l | 3G-comb-attach-rej-congestion

> l | 2G-comb-attach-rej-congestion

> l | 3G-comb-attach-rej-gsm-auth-unacceptable

> l | 2G-comb-attach-rej-gsm-auth-unacceptable

> l | 3G-comb-attach-rej-no-pdp-ctx-activated

> l | 2G-comb-attach-rej-no-pdp-ctx-activated

> l | 3G-comb-attach-rej-retry-from-new-cell

> l | 2G-comb-attach-rej-retry-from-new-cell

> l | 3G-comb-attach-rej-sem-wrong-msg

> l | 2G-comb-attach-rej-sem-wrong-msg

> l | 3G-comb-attach-rej-invalid-mand-info

> l | 2G-comb-attach-rej-invalid-mand-info

> l | 3G-comb-attach-rej-msg-type-not-exist

> l | 2G-comb-attach-rej-msg-type-not-exist

> l | 3G-comb-attach-rej-msg-type-not-comp-pstate

> l | 2G-comb-attach-rej-msg-type-not-comp-pstate

> l | 3G-comb-attach-rej-ie-non-existent

> l | 2G-comb-attach-rej-ie-non-existent

> l | 3G-comb-attach-rej-conditional-ie-err

> l | 2G-comb-attach-rej-conditional-ie-err

> l | 3G-comb-attach-rej-msg-not-comp-prot-state

> l | 2G-comb-attach-rej-msg-not-comp-prot-state

> l | 3G-comb-attach-rej-protocol-error

> l | 2G-comb-attach-rej-protocol-error

> l | 3G-comb-attach-rej-unknown-cause

> l | 2G-comb-attach-rej-unknown-cause

> l | 3G-total-attach-fail

> l | 3G-total-attach-fail-comb

> l | 2G-total-attach-fail

> l | 2G-total-attach-fail-comb

> l | 3G-attach-fail-Iu_release-comb

> l | 3G-attach-fail-ongoing-proc-comb

> l | 2G-attach-fail-ongoing-proc-comb

> l | 3G-comb-rau-reject

> l | 3G-comb-inter-rau-reject

> l | 2G-comb-rau-reject

> l | 2G-comb-inter-rau-reject

> l | 3G-comb-rau-rej-imsi-unknown-hlr

> l | 2G-comb-rau-rej-imsi-unknown-hlr

> l | 3G-comb-rau-rej-illegal-ms

> l | 2G-comb-rau-rej-illegal-ms

> l | 3G-comb-rau-rej-illegal-me

> l | 2G-comb-rau-rej-illegal-me

> l | 3G-comb-rau-rej-gprs-svc-not-allow

> l | 2G-comb-rau-rej-gprs-svc-not-allow

> l | 3G-comb-rau-rej-nongprs-svc-not-allow

> l | 2G-comb-rau-rej-nongprs-svc-not-allow

> l | 3G-comb-rau-rej-msid-not-derived-by-nw

> l | 2G-comb-rau-rej-msid-not-derived-by-nw

> l | 3G-comb-rau-rej-implicitly-detach

> l | 2G-comb-rau-rej-implicitly-detach

> l | 3G-comb-rau-rej-plmn-not-allowed

> l | 3G-comb-rau-rej-loc-area-not-allowed

> l | 2G-comb-rau-rej-loc-area-not-allowed

> l | 3G-comb-rau-rej-roam-not-allowed-larea

> l | 2G-comb-rau-rej-roam-not-allowed-larea

> l | 3G-comb-rau-rej-gprs-svc-not-allowed-plmn

> l | 2G-comb-rau-rej-gprs-svc-not-allowed-plmn

> l | 3G-comb-rau-rej-congestion

> l | 2G-comb-rau-rej-congestion

> l | 3G-comb-rau-rej-gsm-auth-unacceptable

> l | 2G-comb-rau-rej-gsm-auth-unacceptable

> l | 3G-comb-rau-rej-no-pdp-ctx-actv

> l | 2G-comb-rau-rej-no-pdp-ctx-actv

> l | 3G-comb-rau-rej-retry-from-new-cell

> l | 2G-comb-rau-rej-retry-from-new-cell

> l | 3G-comb-rau-rej-sem-wrong-msg

> l | 2G-comb-rau-rej-sem-wrong-msg

> l | 3G-comb-rau-rej-inval-mand-info

> l | 2G-comb-rau-rej-inval-mand-info

> l | 3G-comb-rau-rej-msg-type-non-exist

> l | 2G-comb-rau-rej-msg-type-non-exist

> l | 3G-comb-rau-rej-mtype-incompat-pstate

> l | 2G-comb-rau-rej-mtype-incompat-pstate

> l | 3G-comb-rau-rej-ie-non-existent

> l | 2G-comb-rau-rej-ie-non-existent

> l | 3G-comb-rau-rej-cond-ie-error

> l | 2G-comb-rau-rej-cond-ie-error

> l | 3G-comb-rau-rej-msg-incompat-pstate

> l | 2G-comb-rau-rej-msg-incompat-pstate

> l | 3G-comb-rau-rej-prot-error

> l | 2G-comb-rau-rej-prot-error

> l | 3G-comb-rau-rej-unknown-error

> l | 2G-comb-rau-rej-unknown-error

> l | 3G-comb-irau-rej-imsi-unknown-hlr

> l | 2G-comb-irau-rej-imsi-unknown-hlr

> l | 3G-comb-irau-rej-illegal-ms

> l | 2G-comb-irau-rej-illegal-ms

> l | 3G-comb-irau-rej-illegal-me

> l | 2G-comb-irau-rej-illegal-me

> l | 3G-comb-irau-rej-gprs-svc-not-allow

> l | 2G-comb-irau-rej-gprs-svc-not-allow

> l | 3G-comb-irau-rej-nongprs-svc-not-allow

> l | 2G-comb-irau-rej-nongprs-svc-not-allow

> l | 3G-comb-irau-rej-msid-not-derived-by-nw

> l | 2G-comb-irau-rej-msid-not-derived-by-nw

> l | 3G-comb-irau-rej-implicitly-detach

> l | 2G-comb-irau-rej-implicitly-detach

> l | 3G-comb-irau-rej-plmn-not-allowed

> l | 3G-comb-irau-rej-loc-area-not-allowed

> l | 2G-comb-irau-rej-loc-area-not-allowed

> l | 3G-comb-irau-rej-roam-not-allowed-larea

> l | 2G-comb-irau-rej-roam-not-allowed-larea

> l | 3G-comb-irau-rej-gprs-svc-not-allowed-plmn

> l | 2G-comb-irau-rej-gprs-svc-not-allowed-plmn

> l | 3G-comb-irau-rej-no-cells-in-location-area

> l | 2G-comb-irau-rej-no-cells-in-location-area

> l | 3G-comb-irau-rej-msc-not-reachable

> l | 2G-comb-irau-rej-msc-not-reachable

> l | 3G-comb-irau-rej-network-failure

> l | 2G-comb-irau-rej-network-failure

> l | 3G-comb-irau-rej-mac-failure

> l | 2G-comb-irau-rej-mac-failure

> l | 3G-comb-irau-rej-syn-failure

> l | 2G-comb-irau-rej-syn-failure

> l | 3G-comb-irau-rej-congestion

> l | 2G-comb-irau-rej-congestion

> l | 3G-comb-irau-rej-gsm-auth-unacceptable

> l | 2G-comb-irau-rej-gsm-auth-unacceptable

> l | 3G-comb-irau-rej-no-pdp-ctx-actv

> l | 2G-comb-irau-rej-no-pdp-ctx-actv

> l | 3G-comb-irau-rej-retry-from-new-cell

> l | 2G-comb-irau-rej-retry-from-new-cell

> l | 3G-comb-irau-rej-sem-wrong-msg

> l | 2G-comb-irau-rej-sem-wrong-msg

> l | 3G-comb-irau-rej-inval-mand-info

> l | 2G-comb-irau-rej-inval-mand-info

> l | 3G-comb-irau-rej-msg-type-non-exist

> l | 2G-comb-irau-rej-msg-type-non-exist

> l | 3G-comb-irau-rej-mtype-incompat-pstate

> l | 2G-comb-irau-rej-mtype-incompat-pstate

> l | 3G-comb-irau-rej-ie-non-existent

> l | 2G-comb-irau-rej-ie-non-existent

> l | 3G-comb-irau-rej-cond-ie-error

> l | 2G-comb-irau-rej-cond-ie-error

> l | 3G-comb-irau-rej-msg-not-compat-pstate

> l | 2G-comb-irau-rej-msg-not-compat-pstate

> l | 3G-comb-irau-rej-prot-error

> l | 2G-comb-irau-rej-prot-error

> l | 3G-comb-irau-rej-unknown-error

> l | 2G-comb-irau-rej-unknown-error

> l | 3G-total-intra-rau-failure-comb

> l | 2G-total-comb-inter-rau-failure

> l | 3G-paging-request

> l | 2G-paging-request

> l | 3G-ret-paging-request

> l | 2G-ret-pagin-request

> l | 3G-paging-success

> l | 3G-cs-page-request

> l | 2G-cs-page-request

> l | 3G-cs-page-response

> l | 2G-cs-page-response

> l | 3G-tmsi-identity-request

> l | 2G-tmsi-identity-request

> l | 3G-ret-tmsi-identity-request

> l | 2G-ret-tmsi-identity-request

> l | 3G-tmsi-identity-response

> l | 2G-tmsi-identity-response

> l | 2G-ready-timer-expiry

> l | 3G-total-num-actv-pdp

> l | 2G-total-num-actv-pdp

> l | 3G-total-actv-pdp-with-dir-tunnel

> l | 3G-actv-rej-service-not-subscribed

> l | 2G-actv-rej-service-not-subscribed

> l | 3G-sec-actv-rej-odb

> l | 2G-sec-actv-rej-odb

> l | 3G-sec-actv-rej-insufficient-resources

> l | 2G-sec-actv-rej-insufficient-resources

> l | 3G-sec-actv-rej-by-ggsn

> l | 2G-sec-actv-rej-by-ggsn

> l | 3G-sec-actv-rej-unspecified-error

> l | 2G-sec-actv-rej-unspecified-error

> l | 3G-sec-actv-rej-service-not-supported

> l | 2G-sec-actv-rej-service-not-supported

> l | 3G-sec-actv-rej-service-not-subscribed

> l | 2G-sec-actv-rej-service-not-subscribed

> l | 3G-sec-actv-rej-svc-opt-tmp-out-of-order

> l | 2G-sec-actv-rej-svc-opt-tmp-out-of-order

> l | 3G-sec-actv-rej-semantically-incorrect

> l | 2G-sec-actv-rej-semantically-incorrect

> l | 3G-sec-actv-rej-invalid-mandatory-info

> l | 2G-sec-actv-rej-invalid-mandatory-info

> l | 3G-sec-actv-rej-msg-type-non-existent

> l | 2G-sec-actv-rej-msg-type-non-existent

> l | 3G-sec-actv-rej-ie-non-existent

> l | 2G-sec-actv-rej-ie-non-existent

> l | 3G-sec-actv-rej-conditional-ie-err

> l | 2G-sec-actv-rej-conditional-ie-err

> l | 3G-sec-actv-rej-msg-not-compat-prot-state

> l | 2G-sec-actv-rej-msg-not-compat-prot-state

> l | 3G-sec-actv-rej-recovery-on-timer-expiry

> l | 2G-sec-actv-rej-recovery-on-timer-expiry

> l | 3G-sec-actv-rej-prot-err-unspecified

> l | 2G-sec-actv-rej-prot-err-unspecified

> l | 3G-sec-actv-rej-semantic-error-tft-operation

> l | 2G-sec-actv-rej-semantic-error-tft-operation

> l | 3G-sec-actv-rej-syntax-err-in-tft-operation

> l | 2G-sec-actv-rej-syntax-err-in-tft-operation

> l | 3G-sec-actv-rej-unknown-pdp-context

> l | 2G-sec-actv-rej-unknown-pdp-context

> l | 3G-sec-actv-rej-semantic-err-in-pkt-filter

> l | 2G-sec-actv-rej-semantic-err-in-pkt-filter

> l | 3G-sec-actv-rej-syntax-err-in-pkt-filter

> l | 2G-sec-actv-rej-syntax-err-in-pkt-filter

> l | 3G-sec-actv-rej-pdp-notft-actv

> l | 2G-sec-actv-rej-pdp-notft-actv

> l | 3G-ms-modify-rej-insufficient-resources

> l | 2G-ms-modify-rej-insufficient-resources

> l | 3G-ms-modify-rej-service-opt-not-supported

> l | 2G-ms-modify-rej-service-opt-not-supported

> l | 3G-ms-modify-rej-semantic-err-tft-operation

> l | 2G-ms-modify-rej-semantic-err-tft-operation

> l | 3G-ms-modify-rej-syntax-err-tft-operation

> l | 2G-ms-modify-rej-syntax-err-tft-operation

> l | 3G-ms-modify-rej-semnatic-err-pkt-filter

> l | 2G-ms-modify-rej-semnatic-err-pkt-filter

> l | 3G-ms-modify-rej-syntax-err-pkt-filter

> l | 2G-ms-modify-rej-syntax-err-pkt-filter

> l | 3G-ms-modify-rej-semnatic-incorrect-message

> l | 2G-ms-modify-rej-semnatic-incorrect-message

> l | 3G-ms-modify-rej-invalid-mand-info

> l | 2G-ms-modify-rej-invalid-mand-info

> l | 3G-ms-modify-rej-ie-non-existent

> l | 2G-ms-modify-rej-ie-non-existent

> l | 3G-ms-modify-rej-conditional-ie-err

> l | 2G-ms-modify-rej-conditional-ie-err

> l | 3G-ms-modify-rej-msg-not-compatible-prot-state

> l | 2G-ms-modify-rej-msg-not-compatible-prot-state

> l | 3G-ms-modify-rej-rcvry-on-tmr-expiry

> l | 2G-ms-modify-rej-rcvry-on-tmr-expiry

> l | 3G-ms-modify-rej-prot-err-unspec

> l | 2G-ms-modify-rej-prot-err-unspec

> l | srns-ctx-deny-no-response-from-rnc

> l | map-mo-fwd-req-sent

> l | map-mo-fwd-rsp-rcvd

> l | map-mo-fwd-rsp-failed

> l | map-mo-fwd-rsp-time-out

> l | map-mt-fwd-req-sent

> l | map-mt-fwd-rsp-rcvd

> l | map-mt-fwd-rsp-failed

> l | map-ready-for-sm-req

> l | map-ready-for-sm-rsp

> l | map-ready-for-sm-rsp-failed

> l | map-ready-for-sm-rsp-time-out

> l | tcap-total-active-trans

> l | tcap-total-active-invoks

> l | mo-sms-in-progress

> l | mt-sms-in-progress

> l | sms-memory-available-in-progress

> l | mo-sms-attempted

> l | mo-sms-successful

> l | mt-sms-attempted

> l | mt-sms-successful

> l | sms-memory-available-attempted

> l | sms-memory-available-successful

> l | conn-prot-data-tx

> l | conn-prot-data-rx

> l | conn-prot-ack-tx

> l | conn-prot-ack-rx

> l | conn-prot-error-tx

> l | conn-prot-error-rx

> l | conn-prot-error-nwt-fail-tx

> l | conn-prot-error-nwt-fail-rx

> l | conn-prot-error-congestion-tx

> l | conn-prot-error-congestion-rx

> l | conn-prot-error-invalid-tid-tx

> l | conn-prot-error-invalid-tid-rx

> l | conn-prot-error-invalid-semantic-tx

> l | conn-prot-error-invalid-semantic-rx

> l | conn-prot-error-invalid-mand-info-tx

> l | conn-prot-error-invalid-mand-info-rx

> l | conn-prot-error-invalid-msg-type-tx

> l | conn-prot-error-invalid-msg-type-rx

> l | conn-prot-error-invalid-prot-state-tx

> l | conn-prot-error-invalid-prot-state-rx

> l | conn-prot-error-invalid-ie-tx

> l | conn-prot-error-invalid-ie-rx

> l | conn-prot-error-protocol-error-tx

> l | conn-prot-error-protocol-error-rx

> l | conn-prot-error-undefined-cause-tx

> l | conn-prot-error-undefined-cause-rx

> l | conn-prot-data-dropped

> l | conn-prot-ack-dropped

> l | conn-prot-error-dropped

> l | conn-prot-inval-tid-rcvd

> l | relay-prot-data-tx

> l | relay-prot-data-rx

> l | relay-prot-ack-tx

> l | relay-prot-ack-rx

> l | relay-prot-err-tx

> l | relay-prot-err-rx

> l | relay-prot-err-unassigned-num

> l | relay-prot-err-opr-determ-barring

> l | relay-prot-err-call-barred

> l | relay-prot-err-reserved

> l | relay-prot-err-sm-transfer-rej

> l | relay-prot-err-dest-out-of-order

> l | relay-prot-err-unidentified-subs

> l | relay-prot-err-facility-rej

> l | relay-prot-err-unknown-subs

> l | relay-prot-err-netwk-out-of-order

> l | relay-prot-err-temp-fail

> l | relay-prot-err-congestion

> l | relay-prot-err-not-subscribed

> l | relay-prot-err-not-implemented

> l | relay-prot-err-interworking-err

> l | relay-prot-err-res-unavail

> l | relay-prot-err-mem-capacity-exceed

> l | relay-prot-err-inval-ref-num-tx

> l | relay-prot-err-inval-ref-num-rx

> l | relay-prot-err-inval-semantic-tx

> l | relay-prot-err-inval-semantic-rx

> l | relay-prot-err-inval-mand-info-tx

> l | relay-prot-err-inval-mand-info-rx

> l | relay-prot-err-inval-msg-type-tx

> l | relay-prot-err-inval-msg-type-rx

> l | relay-prot-err-inval-prot-state-tx

> l | relay-prot-err-inval-prot-state-rx

> l | relay-prot-err-inval-ie-tx

> l | relay-prot-err-inval-ie-rx

> l | relay-prot-err-protocol-error-tx

> l | relay-prot-err-unidentified-error-tx

> l | relay-prot-err-unidentified-error-rx

> l | relay-prot-data-dropped

> l | relay-prot-ack-dropped

> l | relay-prot-error-dropped

> l | relay-prot-decode-failure

> l | concat-mo-sms

> l | conn-prot-timer-expiry

> l | tr1n-timer-expiry

> l | tr2n-timer-expiry

> l | conn-prot-data-retrans

> l | relay-prot-msg-encode-fail

> l | conn-prot-data-tx-fail

> l | conn-prot-data-inval-tid

> l | conn-prot-max-retrans-reached

> l | mt-fail-no-db-rec

> l | mt-fail-conn-prot-data-no-ack-rcvd

> l | mt-fail-fwd-busy-subs

> l | mt-fail-fwd-detached-subs

> l | mt-fail-mt-queue-full

> l | 3G-comb-rau-rej-no-cells-in-loc-area

> l | 2G-comb-rau-rej-no-cells-in-loc-area

> l | 3G-comb-rau-rej-msc-not-reachable

> l | 2G-comb-rau-rej-msc-not-reachable

> l | 3G-comb-rau-rej-network-failure

> l | 2G-comb-rau-rej-network-failure

> l | 3G-comb-rau-rej-mac-failure

> l | 2G-comb-rau-rej-mac-failure

> l | 3G-comb-rau-rej-syn-failure

> l | 2G-comb-rau-rej-syn-failure

> l | 3G-actv-fail-iu-release-before-activate

> l | 3G-actv-fail-gaurd-timer-expiry 3

> l | G-actv-fail-duplicate-activation

> l | 3G-actv-fail-other-ongoing-procedure

> l | 3G-actv-fail-tunnel-deactivation

> l | 3G-actv-fail-handoff-before-activate-over

> l | 3G-actv-fail-detach-before-activate-over

> l | 3G-actv-fail-invalid-message-content

> l | 2G-actv-fail-gaurd-timer-expiry

> l | 2G-actv-fail-duplicate-activation

> l | 2G-actv-fail-other-ongoing-procedure

> l | 2G-actv-fail-tunnel-deactivation

> l | 2G-actv-fail-handoff-before-activate-over

> l | 2G-actv-fail-detach-before-activate-over

> l | 2G-actv-fail-invalid-msg-content

> l | inter-system-2G-to-3G-rau-requests

> l | inter-system-2G-to-3G-rau-accepts

> l | inter-system-2G-to-3G-comb-rau-requests inter-system-2G-to-3G-comb-rau-accepts

> l | inter-system-2G-to-3G-rau-rejects

> l | inter-system-2G-to-3G-comb-rau-rejects

> l | inter-system-2G-to-3G-attach-requests

> l | inter-system-2G-to-3G-attach-accepts

> l | inter-system-2G-to-3G-attach-rejects

> l | inter-system-2G-to-3G-comb-attach-requests

> l | inter-system-2G-to-3G-comb-attach-accepts

> l | inter-system-2G-to-3G-comb-attach-rejects

> l | inter-system-3G-to-2G-rau-requests

> l | inter-system-3G-to-2G-rau-accepts

> l | inter-system-3G-to-2G-comb-rau-requests

> l | inter-system-3G-to-2G-comb-rau-accepts

> l | inter-system-3G-to-2G-rau-rejects

> l | inter-system-3G-to-2G-comb-rau-rejects

> l | inter-system-3G-to-2G-attach-requests

> l | inter-system-3G-to-2G-attach-accepts

> l | inter-system-3G-to-2G-attach-rejects

> l | inter-system-3G-to-2G-comb-attach-requests

> l | inter-system-3G-to-2G-comb-attach-accepts

> l | inter-system-3G-to-2G-comb-attach-rejects

> l | 2G-intra-prau-rej-msc-not-reachable

> l | 3G-intra-prau-rej-network-failure

> l | 2G-intra-prau-rej-network-failure

> l | 3G-intra-prau-rej-mac-failure

> l | 2G-intra-prau-rej-mac-failure

> l | 3G-intra-prau-rej-syn-failure

> l | 2G-intra-prau-rej-syn-failure0

> l | 3G-comb-rau-rej-no-cells-in-loc-area

> l | 2G-comb-rau-rej-no-cells-in-loc-area

> l | 3G-comb-rau-rej-msc-not-reachable

> l | 2G-comb-rau-rej-msc-not-reachable

> l | 3G-comb-rau-rej-network-failure

> l | 2G-comb-rau-rej-network-failure

> l | 3G-comb-rau-rej-mac-failure

> l | 2G-comb-rau-rej-mac-failure

> l | 3G-comb-rau-rej-syn-failure

> l | 2G-comb-rau-rej-syn-failure

> l | intra-sgsn-inter-system-gsm-to-wcdma-success

> l | intra-sgsn-inter-system-gsm-to-wcdma-rej

> l | intra-sgsn-inter-system-gsm-to-wcdma-fail

> l | intra-sgsn-inter-system-wcdma-to-gsm-success

> l | intra-sgsn-inter-system-wcdma-to-gsm-rej

> l | intra-sgsn-inter-system-wcdma-to-gsm-fail

> l | ps-inter-rat-rau-total

> l | ps-inter-rat-rau-3g

> l | ps-inter-rat-rau-2g

> l | comb-inter-rat-rau-total

> l | comb-inter-rat-rau-3g

> l | comb-inter-rat-rau-2g

> l | ret-ps-inter-rat-rau-total

> l | ret-ps-inter-rat-rau-3g

> l | ret-ps-inter-rat-rau-2g

> l | ret-comb-inter-rat-rau-total

> l | ret-comb-inter-rat-rau-3g

> l | ret-comb-inter-rat-rau-2g

> l | ps-inter-service-rau-total

> l | ps-inter-service-rau-3g

> l | ps-inter-service-rau-2g

> l | comb-inter-service-rau-total

> l | comb-inter-service-rau-3g

> l | comb-inter-service-rau-2g

> l | ret-ps-inter-service-rau-total

> l | ret-ps-inter-service-rau-3g

> l | ret-ps-inter-service-rau-2g

> l | ret-comb-inter-service-rau-total

> l | ret-comb-inter-service-rau-3g

> l | ret-comb-inter-service-rau-2g

> l | ps-inter-rat-rau-acc-total

> l | ps-inter-rat-rau-acc-3g

> l | ps-inter-rat-rau-acc-2g

> l | comb-inter-rat-rau-acc-total

> l | comb-inter-rat-rau-acc-3g

> l | comb-inter-rat-rau-acc-2g

> l | ret-ps-inter-rat-rau-acc-total

> l | ret-ps-inter-rat-rau-acc-3g

> l | ret-ps-inter-rat-rau-acc-2g

> l | ret-comb-inter-rat-rau-acc-total

> l | ret-comb-inter-rat-rau-acc-3g

> l | ret-comb-inter-rat-rau-acc-2g

> l | ps-inter-service-rau-acc-total

> l | ps-inter-service-rau-acc-3g

> l | ps-inter-service-rau-acc-2g

> l | comb-inter-service-rau-acc-total

> l | comb-inter-service-rau-acc-3g

> l | comb-inter-service-rau-acc-2g

> l | ret-ps-inter-service-rau-acc-total

> l | ret-ps-inter-service-rau-acc-3g

> l | ret-ps-inter-service-rau-acc-2g

> l | ret-comb-inter-service-rau-acc-total

> l | ret-comb-inter-service-rau-acc-3g

> l | ret-comb-inter-service-rau-acc-2g

> l | ps-inter-rat-rau-rej-total

> l | ps-inter-rat-rau-rej-3g

> l | ps-inter-rat-rau-rej-2g

> l | comb-inter-rat-rau-rej-total

> l | comb-inter-rat-rau-rej-3g

> l | comb-inter-rat-rau-rej-2g

> l | ps-inter-service-rau-rej-total

> l | ps-inter-service-rau-rej-3g

> l | ps-inter-service-rau-rej-2g

> l | comb-inter-service-rau-rej-total

> l | comb-inter-service-rau-rej-3g

> l | comb-inter-service-rau-rej-2g

> l | 3G-isrv-ps-rej-imsi-unknown-hlr

> l | 2G-isrv-ps-rej-imsi-unknown-hlr

> l | 3G-isrv-ps-rej-illegal-ms

> l | 2G-isrv-ps-rej-illegal-ms

> l | 3G-isrv-ps-rej-illegal-me

> l | 2G-isrv-ps-rej-illegal-me

> l | 3G-isrv-ps-rej-gprs-svc-not-allow

> l | 2G-isrv-ps-rej-gprs-svc-not-allow

> l | 3G-isrv-ps-rej-nongprs-svc-not-allow

> l | 2G-isrv-ps-rej-nongprs-svc-not-allow

> l | 3G-isrv-ps-rej-msid-not-derived-by-nw

> l | 2G-isrv-ps-rej-msid-not-derived-by-nw

> l | 3G-isrv-ps-rej-implicitly-detach

> l | 2G-isrv-ps-rej-implicitly-detach

> l | 3G-isrv-ps-rej-plmn-not-allowed

> l | 2G-isrv-ps-rej-plmn-not-allowed

> l | 3G-isrv-ps-rej-loc-area-not-allowed

> l | 2G-isrv-ps-rej-loc-area-not-allowed

> l | 3G-isrv-ps-rej-roam-not-allowed-larea

> l | 2G-isrv-ps-rej-roam-not-allowed-larea

> l | 3G-isrv-ps-rej-gprs-svc-not-allowed-plmn

> l | 2G-isrv-ps-rej-gprs-svc-not-allowed-plmn

> l | 3G-isrv-ps-rej-no-cells-in-location-area

> l | 2G-isrv-ps-rej-no-cells-in-location-area

> l | 3G-isrv-ps-rej-msc-not-reachable

> l | 2G-isrv-ps-rej-msc-not-reachable

> l | 3G-isrv-ps-rej-network-failure

> l | 2G-isrv-ps-rej-network-failure

> l | 3G-isrv-ps-rej-mac-failure

> l | 2G-isrv-ps-rej-mac-failure

> l | 3G-isrv-ps-rej-syn-failure

> l | 2G-isrv-ps-rej-syn-failure

> l | 3G-isrv-ps-rej-congestion

> l | 2G-isrv-ps-rej-congestion

> l | 3G-isrv-ps-rej-gsm-auth-unacceptable

> l | 2G-isrv-ps-rej-gsm-auth-unacceptable

> l | 3G-isrv-ps-rej-no-pdp-ctx-actv

> l | 2G-isrv-ps-rej-no-pdp-ctx-actv

> l | 3G-isrv-ps-rej-retry-from-new-cell

> l | 2G-isrv-ps-rej-retry-from-new-cell

> l | 3G-isrv-ps-rej-sem-wrong-msg

> l | 2G-isrv-ps-rej-sem-wrong-msg

> l | 3G-isrv-ps-rej-inval-mand-info

> l | 2G-isrv-ps-rej-inval-mand-info

> l | 3G-isrv-ps-rej-msg-type-non-exist

> l | 2G-isrv-ps-rej-msg-type-non-exist

> l | 3G-isrv-ps-rej-mtype-incompat-pstate

> l | 2G-isrv-ps-rej-mtype-incompat-pstate

> l | 3G-isrv-ps-rej-ie-non-existent

> l | 2G-isrv-ps-rej-ie-non-existent

> l | 3G-isrv-ps-rej-cond-ie-error

> l | 2G-isrv-ps-rej-cond-ie-error

> l | 3G-isrv-ps-rej-msg-not-compat-pstate

> l | 2G-isrv-ps-rej-msg-not-compat-pstate

> l | 3G-isrv-ps-rej-prot-error

> l | 2G-isrv-ps-rej-prot-error

> l | 3G-isrv-ps-rej-unknown-error

> l | 2G-isrv-ps-rej-unknown-error

> l | 3G-isrv-comb-rej-imsi-unknown-hlr

> l | 2G-isrv-comb-rej-imsi-unknown-hlr

> l | 3G-isrv-comb-rej-illegal-ms

> l | 2G-isrv-comb-rej-illegal-ms

> l | 3G-isrv-comb-rej-illegal-me

> l | 2G-isrv-comb-rej-illegal-me

> l | 3G-isrv-comb-rej-gprs-svc-not-allow

> l | 2G-isrv-comb-rej-gprs-svc-not-allow

> l | 3G-isrv-comb-rej-nongprs-svc-not-allow

> l | 2G-isrv-comb-rej-nongprs-svc-not-allow

> l | 3G-isrv-comb-rej-msid-not-derived-by-nw

> l | 2G-isrv-comb-rej-msid-not-derived-by-nw

> l | 3G-isrv-comb-rej-implicitly-detach

> l | 2G-isrv-comb-rej-implicitly-detach

> l | 3G-isrv-comb-rej-plmn-not-allowed

> l | 2G-isrv-comb-rej-plmn-not-allowed

> l | 3G-isrv-comb-rej-loc-area-not-allowed

> l | 2G-isrv-comb-rej-loc-area-not-allowed

> l | 3G-isrv-comb-rej-roam-not-allowed-larea

> l | 2G-isrv-comb-rej-roam-not-allowed-larea

> l | 3G-isrv-comb-rej-gprs-svc-not-allowed-plmn

> l | 2G-isrv-comb-rej-gprs-svc-not-allowed-plmn

> l | 3G-isrv-comb-rej-no-cells-in-location-area

> l | 2G-isrv-comb-rej-no-cells-in-location-area

> l | 3G-isrv-comb-rej-msc-not-reachable

> l | 2G-isrv-comb-rej-msc-not-reachable

> l | 3G-isrv-comb-rej-network-failure

> l | 2G-isrv-comb-rej-network-failure

> l | 3G-isrv-comb-rej-mac-failure

> l | 2G-isrv-comb-rej-mac-failure

> l | 3G-isrv-comb-rej-syn-failure

> l | 2G-isrv-comb-rej-syn-failure

> l | 3G-isrv-comb-rej-congestion

> l | 2G-isrv-comb-rej-congestion

> l | 3G-isrv-comb-rej-gsm-auth-unacceptable

> l | 2G-isrv-comb-rej-gsm-auth-unacceptable

> l | 3G-isrv-comb-rej-no-pdp-ctx-actv

> l | 2G-isrv-comb-rej-no-pdp-ctx-actv

> l | 3G-isrv-comb-rej-retry-from-new-cell

> l | 2G-isrv-comb-rej-retry-from-new-cell

> l | 3G-isrv-comb-rej-sem-wrong-msg

> l | 2G-isrv-comb-rej-sem-wrong-msg

> l | 3G-isrv-comb-rej-inval-mand-info

> l | 2G-isrv-comb-rej-inval-mand-info

> l | 3G-isrv-comb-rej-msg-type-non-exist

> l | 2G-isrv-comb-rej-msg-type-non-exist

> l | 3G-isrv-comb-rej-mtype-incompat-pstate

> l | 2G-isrv-comb-rej-mtype-incompat-pstate

> l | 3G-isrv-comb-rej-ie-non-existent

> l | 2G-isrv-comb-rej-ie-non-existent

> l | 3G-isrv-comb-rej-cond-ie-error

> l | 2G-isrv-comb-rej-cond-ie-error

> l | 3G-isrv-comb-rej-msg-not-compat-pstate

> l | 2G-isrv-comb-rej-msg-not-compat-pstate

> l | 3G-isrv-comb-rej-prot-error

> l | 2G-isrv-comb-rej-prot-error

> l | 3G-isrv-comb-rej-unknown-error

> l | 2G-isrv-comb-rej-unknown-error

> l | 3G-irat-ps-rej-imsi-unknown-hlr

> l | 2G-irat-ps-rej-imsi-unknown-hlr

> l | 3G-irat-ps-rej-illegal-ms

> l | 2G-irat-ps-rej-illegal-ms

> l | 3G-irat-ps-rej-illegal-me

> l | 2G-irat-ps-rej-illegal-me

> l | 3G-irat-ps-rej-gprs-svc-not-allow

> l | 2G-irat-ps-rej-gprs-svc-not-allow

> l | 3G-irat-ps-rej-nongprs-svc-not-allow

> l | 2G-irat-ps-rej-nongprs-svc-not-allow

> l | 3G-irat-ps-rej-msid-not-derived-by-nw

> l | 2G-irat-ps-rej-msid-not-derived-by-nw

> l | 3G-irat-ps-rej-implicitly-detach

> l | 2G-irat-ps-rej-implicitly-detach

> l | 3G-irat-ps-rej-plmn-not-allowed

> l | 2G-irat-ps-rej-plmn-not-allowed

> l | 3G-irat-ps-rej-loc-area-not-allowed

> l | 2G-irat-ps-rej-loc-area-not-allowed

> l | 3G-irat-ps-rej-roam-not-allowed-larea

> l | 2G-irat-ps-rej-roam-not-allowed-larea

> l | 3G-irat-ps-rej-gprs-svc-not-allowed-plmn

> l | 2G-irat-ps-rej-gprs-svc-not-allowed-plmn

> l | 3G-irat-ps-rej-no-cells-in-location-area

> l | 2G-irat-ps-rej-no-cells-in-location-area

> l | 3G-irat-ps-rej-msc-not-reachable

> l | 2G-irat-ps-rej-msc-not-reachable

> l | 3G-irat-ps-rej-network-failure

> l | 2G-irat-ps-rej-network-failure

> l | 3G-irat-ps-rej-mac-failure

> l | 2G-irat-ps-rej-mac-failure

> l | 3G-irat-ps-rej-syn-failure

> l | 2G-irat-ps-rej-syn-failure

> l | 3G-irat-ps-rej-congestion

> l | 2G-irat-ps-rej-congestion

> l | 3G-irat-ps-rej-gsm-auth-unacceptable

> l | 2G-irat-ps-rej-gsm-auth-unacceptable

> l | 3G-irat-ps-rej-no-pdp-ctx-actv

> l | 2G-irat-ps-rej-no-pdp-ctx-actv

> l | 3G-irat-ps-rej-retry-from-new-cell

> l | 2G-irat-ps-rej-retry-from-new-cell

> l | 3G-irat-ps-rej-sem-wrong-msg

> l | 2G-irat-ps-rej-sem-wrong-msg

> l | 3G-irat-ps-rej-inval-mand-info

> l | 2G-irat-ps-rej-inval-mand-info

> l | 3G-irat-ps-rej-msg-type-non-exist

> l | 2G-irat-ps-rej-msg-type-non-exist

> l | 3G-irat-ps-rej-mtype-incompat-pstate

> l | 2G-irat-ps-rej-mtype-incompat-pstate

> l | 3G-irat-ps-rej-ie-non-existent

> l | 2G-irat-ps-rej-ie-non-existent

> l | 3G-irat-ps-rej-cond-ie-error

> l | 2G-irat-ps-rej-cond-ie-error

> l | 3G-irat-ps-rej-msg-not-compat-pstate

> l | 2G-irat-ps-rej-msg-not-compat-pstate

> l | 3G-irat-ps-rej-prot-error

> l | 2G-irat-ps-rej-prot-error

> l | 3G-irat-ps-rej-unknown-error

> l | 2G-irat-ps-rej-unknown-error

> l | 3G-irat-comb-rej-imsi-unknown-hlr

> l | 2G-irat-comb-rej-imsi-unknown-hlr

> l | 3G-irat-comb-rej-illegal-ms

> l | 2G-irat-comb-rej-illegal-ms

> l | 3G-irat-comb-rej-illegal-me

> l | 2G-irat-comb-rej-illegal-me

> l | 3G-irat-comb-rej-gprs-svc-not-allow

> l | 2G-irat-comb-rej-gprs-svc-not-allow

> l | 3G-irat-comb-rej-nongprs-svc-not-allow

> l | 2G-irat-comb-rej-nongprs-svc-not-allow

> l | 3G-irat-comb-rej-msid-not-derived-by-nw

> l | 2G-irat-comb-rej-msid-not-derived-by-nw

> l | 3G-irat-comb-rej-implicitly-detach

> l | 2G-irat-comb-rej-implicitly-detach

> l | 3G-irat-comb-rej-plmn-not-allowed

> l | 2G-irat-comb-rej-plmn-not-allowed

> l | 3G-irat-comb-rej-loc-area-not-allowed

> l | 2G-irat-comb-rej-loc-area-not-allowed

> l | 3G-irat-comb-rej-roam-not-allowed-larea

> l | 2G-irat-comb-rej-roam-not-allowed-larea

> l | 3G-irat-comb-rej-gprs-svc-not-allowed-plmn

> l | 2G-irat-comb-rej-gprs-svc-not-allowed-plmn

> l | 3G-irat-comb-rej-no-cells-in-location-area

> l | 2G-irat-comb-rej-no-cells-in-location-area

> l | 3G-irat-comb-rej-msc-not-reachable

> l | 2G-irat-comb-rej-msc-not-reachable

> l | 3G-irat-comb-rej-network-failure

> l | 2G-irat-comb-rej-network-failure

> l | 3G-irat-comb-rej-mac-failure

> l | 2G-irat-comb-rej-mac-failure

> l | 3G-irat-comb-rej-syn-failure

> l | 2G-irat-comb-rej-syn-failure

> l | 3G-irat-comb-rej-congestion

> l | 2G-irat-comb-rej-congestion

> l | 3G-irat-comb-rej-gsm-auth-unacceptable

> l | 2G-irat-comb-rej-gsm-auth-unacceptable

> l | 3G-irat-comb-rej-no-pdp-ctx-actv

> l | 2G-irat-comb-rej-no-pdp-ctx-actv

> l | 3G-irat-comb-rej-retry-from-new-cell

> l | 2G-irat-comb-rej-retry-from-new-cell

> l | 3G-irat-comb-rej-sem-wrong-msg

> l | 2G-irat-comb-rej-sem-wrong-msg

> l | 3G-irat-comb-rej-inval-mand-info

> l | 2G-irat-comb-rej-inval-mand-info

> l | 3G-irat-comb-rej-msg-type-non-exist

> l | 2G-irat-comb-rej-msg-type-non-exist

> l | 3G-irat-comb-rej-mtype-incompat-pstate

> l | 2G-irat-comb-rej-mtype-incompat-pstate

> l | 3G-irat-comb-rej-ie-non-existent

> l | 2G-irat-comb-rej-ie-non-existent

> l | 3G-irat-comb-rej-cond-ie-error

> l | 2G-irat-comb-rej-cond-ie-error

> l | 3G-irat-comb-rej-msg-not-compat-pstate

> l | 2G-irat-comb-rej-msg-not-compat-pstate

> l | 3G-irat-comb-rej-prot-error

> l | 2G-irat-comb-rej-prot-error

> l | 3G-irat-comb-rej-unknown-error

> l | 2G-irat-comb-rej-unknown-error

> l | 2G-sec-actv-rej-qos-not-acc -- This stat is not used and has been deprecated.

> l | 2G-actv-rej-qos-not-acc -- This stat is not used and has been deprecated.

> l | 2G-sec-actv-rej-llc-sndcp-fail -- This stat is not used and has been deprecated.

> l | 2G-actv-rej-llc-sndcp-fail -- This stat is not used and has been deprecated.

> sgtp schema

> l | sgtpc-upc-req-v0-tx

> l | sgtpc-upc-req-v1-rx

> l | sgtpc-upc-req-accept-v1-tx

> l | sgtpc-upc-req-accept-v1-rx

> l | sgtpc-upc-req-accept-v0-rx

> l | sgtpc-dpc-req-accept-v1-tx

> l | sgtpc-dpc-req-accept-v0-tx

> l | sgtpc-dpc-req-accept-v1-rx

> l | sgtpc-dpc-req-accept-v0-rx

> l | sgtpc-total-sri-req

> l | sgtpc-sri-req-v1

> l | sgtpc-sri-req-v0

> l | sgtpc-sri-req-v1-ret

> l | sgtpc-sri-req-v0-ret

> l | sgtpc-sri-req-denied

> l | sgtpc-total-fail-rpt-req

> l | sgtpc-fail-rpt-req-v1

> l | sgtpc-fail-rpt-req-v0

> l | sgtpc-fail-rpt-req-v1-ret

> l | sgtpc-fail-rpt-req-v0-ret

> l | sgtpc-fail-rpt-req-denied

> l | sgtpc-ident-req-accept-v1-tx

> l | sgtpc-ident-req-accept-v0-tx

> l | sgtpc-ident-req-accept-v1-rx

> l | sgtpc-ident-req-accept-v0-rx

> l | sgtpc-ident-req-denied-tx

> l | sgtpc-sgsn-ctxt-req-accept-v1-tx

> l | sgtpc-sgsn-ctxt-req-accept-v0-tx

> l | sgtpc-sgsn-ctxt-req-accept-v1-rx

> l | sgtpc-sgsn-ctxt-req-accept-v0-rx

> l | sgtpc-sgsn-ctxt-ack-accept-v1-tx

> l | sgtpc-sgsn-ctxt-ack-accept-v0-tx

> l | sgtpc-sgsn-ctxt-ack-accept-v1-rx

> l | sgtpc-sgsn-ctxt-ack-accept-v0-rx

> l | sgtpc-ret-v1-echo-req-rx

> l | sgtpc-ret-v0-echo-req-rx

> l | sgtpu-ggsn-pkt-drop-suspend-dealloc-st

> l | sgtpu-ggsn-byts-drop-suspend-dealloc-st

> l | sgtpu-rnc-byts-rau-in-active-reg-st

> l | sgtpu-rnc-pkt-drop-suspended-dealloc-st

> l | sgtpu-rnc-byts-drop-suspended-dealloc-st

> l | sgtpu-rnc-pkt-unknown-version

> l | sgtpu-v1-echo-req-tx

> l | sgtpu-v0-echo-req-tx

> l | sgtpu-v1-echo-req-rx

> l | sgtpu-v0-echo-req-rx

> l | sgtpu-v1-echo-rsp-tx

> l | sgtpu-v0-echo-rsp-tx

> l | sgtpu-v1-echo-rsp-rx

> l | sgtpu-v0-echo-rsp-rx

> l | sgtpu-v1-echo-req-retrans

> l | sgtpu-v0-echo-req-retrans

> l | sgtpu-sgsn-unsolicited-data-pkt

> l | sgtpu-sgsn-err-ind-for-unsolicited-pkt

> l | sgtpu-total-active-ggsn

> l | sgtpu-total-active-rnc

> l | sgtpu-ggsn-pkt-iu-release

> l | sgtpu-ggsn-byts-iu-release

> l | sgtpu-ggsn-pkt-t3-tmr-expiry

> l | sgtpu-ggsn-byts-t3-tmr-expiry

> l | sgtpu-ggsn-pkt-forwarded

> l | sgtpu-ggsn-byts-forwarded

> l | sgtpu-ggsn-pkt-bvc-block

> l | sgtpu-ggsn-byts-bvc-block

> l | sgtpc-upc-req-accept-tx

> l | sgtpc-upc-req-accept-rx

> l | sgtpc-dpc-req-accept-tx

> l | sgtpc-dpc-req-accept-rx

> l | sgtpc-ident-req-accept-tx

> l | sgtpc-ident-req-accept-rx

> l | sgtpc-sgsn-ctxt-req-accept-tx

> l | sgtpc-sgsn-ctxt-req-accept-rx

> l | sgtpc-sgsn-ctxt-ack-accept-tx

> l | sgtpc-sgsn-ctxt-ack-accept-rx

> l | sgtpu-echo-req-tx

> l | sgtpu-echo-req-rx

> l | sgtpu-echo-rsp-tx

> l | sgtpu-echo-rsp-rx

> ss7link schema
> The following are new for Release 8.0:

> l | ss7-link-qsaal-recovery-ack-tx

> The following are new for Release 8.1

> l | ss7-link-mtp3-inhibited-duration

> ss7rd schema

> l | ss7rd-sctp-init-ack-tx

> l | ss7rd-sctp-init-ack-rx

> l | ss7rd-sctp-shutdown-ack-tx

> l | ss7rd-sctp-heartbeat-ack-rx

> l | ss7rd-m3ua-scon-tx

> l | ss7rd-m3ua-deregrsp-tx

> l | ss7rd-m3ua-duna-rx

> l | ss7rd-m3ua-scon-rx

> l | ss7rd-m3ua-deregrsp-rx

> l | ss7rd-m3ua-psp-scon-tx

> l | ss7rd-m3ua-psp-deregrsp-tx

> l | ss7rd-m3ua-psp-duna-rx

> l | ss7rd-m3ua-psp-scon-rx

> l | ss7rd-m3ua-psp-deregrsp-rx

> l | ss7rd-m3ua-psp-congestion-level1

> system schema
> The following are new for Release 8.0:

> l | cf-cache-flushes

> l | cf-cache-has-path-hits

> l | cf-cache-hits

> l | cf-cache-misses

> l | cf-cat-abor-pkts-hit

> l | cf-cat-abor-pkts-block

> l | cf-cat-adult-pkts-hit

> l | cf-cat-adult-pkts-block

> l | cf-cat-adv-pkts-hit

> l | cf-cat-adv-pkts-block

> l | cf-cat-advert-pkts-hit

> l | cf-cat-advert-pkts-block

> l | cf-cat-anon-pkts-hit

> l | cf-cat-anon-pkts-block

> l | cf-cat-art-pkts-hit

> l | cf-cat-art-pkts-block

> l | cf-cat-auct-pkts-hit

> l | cf-cat-auct-pkts-block

> l | cf-cat-auto-pkts-hit

> l | cf-cat-auto-pkts-block

> l | cf-cat-black-pkts-hit

> l | cf-cat-black-pkts-block

> l | cf-cat-blog-pkts-hit

> l | cf-cat-blog-pkts-block

> l | cf-cat-busi-pkts-hit

> l | cf-cat-busi-pkts-block

> l | cf-cat-car-pkts-hit

> l | cf-cat-car-pkts-block

> l | cf-cat-chat-pkts-hit

> l | cf-cat-chat-pkts-block

> l | cf-cat-clean-pkts-hit

> l | cf-cat-clean-pkts-block

> l | cf-cat-cmc-pkts-hit

> l | cf-cat-cmc-pkts-block

> l | cf-cat-cporn-pkts-hit

> l | cf-cat-cporn-pkts-block

> l | cf-cat-crime-pkts-hit

> l | cf-cat-crime-pkts-block

> l | cf-cat-cult-pkts-hit

> l | cf-cat-cult-pkts-block

> l | cf-cat-drug-pkts-hit

> l | cf-cat-drug-pkts-block

> l | cf-cat-dynam-pkts-hit

> l | cf-cat-dynam-pkts-block

> l | cf-cat-edu-pkts-hit

> l | cf-cat-edu-pkts-block

> l | cf-cat-ent-pkts-hit

> l | cf-cat-ent-pkts-block

> l | cf-cat-esrb-pkts-hit

> l | cf-cat-esrb-pkts-block

> l | cf-cat-fin-pkts-hit

> l | cf-cat-fin-pkts-block

> l | cf-cat-forum-pkts-hit

> l | cf-cat-forum-pkts-block

> l | cf-cat-gamb-pkts-hit

> l | cf-cat-gamb-pkts-block

> l | cf-cat-game-pkts-hit

> l | cf-cat-game-pkts-block

> l | cf-cat-glam-pkts-hit

> l | cf-cat-glam-pkts-block

> l | cf-cat-govern-pkts-hit

> l | cf-cat-govern-pkts-block

> l | cf-cat-hack-pkts-hit

> l | cf-cat-hack-pkts-block

> l | cf-cat-hate-pkts-hit

> l | cf-cat-hate-pkts-block

> l | cf-cat-health-pkts-hit

> l | cf-cat-health-pkts-block

> l | cf-cat-hobby-pkts-hit

> l | cf-cat-hobby-pkts-block

> l | cf-cat-hosts-pkts-hit

> l | cf-cat-hosts-pkts-block

> l | cf-cat-kids-pkts-hit

> l | cf-cat-kids-pkts-block

> l | cf-cat-legal-pkts-hit

> l | cf-cat-legal-pkts-block

> l | cf-cat-lifes-pkts-hit

> l | cf-cat-lifes-pkts-block

> l | cf-cat-mail-pkts-hit

> l | cf-cat-mail-pkts-block

> l | cf-cat-mil-pkts-hit

> l | cf-cat-mil-pkts-block

> l | cf-cat-news-pkts-hit

> l | cf-cat-news-pkts-block

> l | cf-cat-occult-pkts-hit

> l | cf-cat-occult-pkts-block

> l | cf-cat-p2p-pkts-hit

> l | cf-cat-p2p-pkts-block

> l | cf-cat-peer-pkts-hit

> l | cf-cat-peer-pkts-block

> l | cf-cat-pers-pkts-hit

> l | cf-cat-pers-pkts-block

> l | cf-cat-phish-pkts-hit

> l | cf-cat-phish-pkts-block

> l | cf-cat-poltic-pkts-hit

> l | cf-cat-poltic-pkts-block

> l | cf-cat-porn-pkts-hit

> l | cf-cat-porn-pkts-block

> l | cf-cat-portal-pkts-hit

> l | cf-cat-portal-pkts-block

> l | cf-cat-proxy-pkts-hit

> l | cf-cat-proxy-pkts-block

> l | cf-cat-radio-pkts-hit

> l | cf-cat-radio-pkts-block

> l | cf-cat-ref-pkts-hit

> l | cf-cat-ref-pkts-block

> l | cf-cat-rel-pkts-hit

> l | cf-cat-rel-pkts-block

> l | cf-cat-sci-pkts-hit

> l | cf-cat-sci-pkts-block

> l | cf-cat-search-pkts-hit

> l | cf-cat-search-pkts-block

> l | cf-cat-sftwre-pkts-hit

> l | cf-cat-sftwre-pkts-block

> l | cf-cat-shop-pkts-hit

> l | cf-cat-shop-pkts-block

> l | cf-cat-sport-pkts-hit

> l | cf-cat-sport-pkts-block

> l | cf-cat-spywre-pkts-hit

> l | cf-cat-spywre-pkts-block

> l | cf-cat-suic-pkts-hit

> l | cf-cat-suic-pkts-block

> l | cf-cat-susp-pkts-hit

> l | cf-cat-susp-pkts-block

> l | cf-cat-sxed-pkts-hit

> l | cf-cat-sxed-pkts-block

> l | cf-cat-tech-pkts-hit

> l | cf-cat-tech-pkts-block

> l | cf-cat-trav-pkts-hit

> l | cf-cat-trav-pkts-block

> l | cf-cat-viol-pkts-hit

> l | cf-cat-viol-pkts-block

> l | cf-cat-weap-pkts-hit

> l | cf-cat-weap-pkts-block

> l | cf-cat-white-pkts-hit

> l | cf-cat-white-pkts-block

> l | cf-cat-unknow-pkts-hit

> l | cf-cat-unknow-pkts-block

> l | cf-cat-pkts-hit-summary

> l | cf-cat-pkts-block-summary

> l | disc-reason-291

> l | disc-reason-291

> l | disc-reason-292

> l | disc-reason-293

> l | disc-reason-294

> l | disc-reason-295

> l | disc-reason-296

> l | disc-reason-297

> l | disc-reason-298

> l | disc-reason-299

> l | disc-reason-300

> l | disc-reason-301

> l | disc-reason-302

> l | disc-reason-303

> l | disc-reason-304

> l | disc-reason-305

> l | disc-reason-306

> l | disc-reason-307

> l | disc-reason-308

> l | disc-reason-309

> l | disc-reason-310

> l | disc-reason-311

> l | disc-reason-312

> l | curr-proxy

> l | curr-relay-agent

> l | sess-total-setup

> l | setup-proxy

> l | setup-relay-agent

> l | total-released

> l | rel-proxy-admin-releases

> l | rel-proxy-bearer-call-term.

> l | rel-proxy-lease-exp-policy

> l | rel-proxy-lease-renew-failure

> l | rel-proxy-ip-mis-match

> l | rel-proxy-lease-time-mis-match

> l | rel-proxy-other-reasons

> l | rel-relay-admin-releases

> l | rel-relay-bearer-call-ter.

> l | rel-relay-lease-time-out

> l | rel-relay-other-reasons

> l | discover-tx

> l | discover-retransmitted

> l | discover-rx

> l | discover-retried-rx

> l | discover-relayed

> l | discoverd-retried-relayed

> l | offer-rx

> l | offer-discarded

> l | offer-tx

> l | offer-relayed

> l | request-tx

> l | request-retransmitted

> l | request-rx

> l | request-renewal-rx

> l | request-requesting-relayed

> l | request-renewing-relayed

> l | ack-rx

> l | ack-for-inform

> l | ack-renewing-rx

> l | ack-tx

> l | ack-renewing-tx

> l | ack-relayed

> l | ack-renewing-relayed

> l | nak-rx

> l | nak-for-inform

> l | nak-tx

> l | nak-relayed

> l | decline-tx

> l | decline-rx

> l | decline-relayed

> l | release-tx

> l | release-rx

> l | release-relayed

> l | release-for-relay-call

> l | inform-tx

> l | inform-retransmitted

> l | inform-rx

> l | inform-relayed

> l | offer-dis-parse-err

> l | offer-dis-lease-less-than-min

> l | offer-dis-lease-greater-than-max

> l | offer-dis-ip-val-failed

> l | offer-dis-xid-mismatch

> l | ack-dis-parse-err

> l | ack-dis-xid-mis-match

> l | decline-dis-ip-mis-match

> l | ip-lease-renewal

> l | failed-ip-lease-renew

> l | no-reply-from-server

> l | server-nak

> l | ip-addr-mis-match

> l | lease-mis-match

> Bulk Statistic Modifications
> The following modifications were made for Release 8.0:
> Obsoleted Bulk Statistics
> None for this release.
> gprs schema

> l | ns-num-bytes-rvcd

> l | ns-num-bytes-sent

> l | ns-num-nsvc-failed

> l | ns-num-nsvc-congest

> l | ns-num-unit-data-msg-rcvd

> l | ns-num-unit-data-msg-sent

> l | ns-num-alive-pdu-rcvd

> l | ns-num-alive-pdu-sent

> l | ns-num-alive-ack-pdu-rcvd

> l | ns-num-alive-ack-pdu-sent

> l | ns-num-block-pdu-rcvd

> l | ns-num-block-pdu-sent

> l | ns-num-block-ack-pdu-rcvd

> l | ns-num-block-ack-pdu-sent

> l | ns-num-unblock-pdu-rcvd

> l | ns-num-unblock-pdu-sent

> l | ns-num-unblock-ack-pdu-rcvd

> l | ns-num-unblock-ack-pdu-sent

> l | ns-num-reset-pdu-rcvd

> l | ns-num-reset-pdu-sent

> l | ns-num-reset-ack-pdu-rcvd

> l | ns-num-reset-ack-pdu-sent

> l | ns-num-status-pdu-rcvd

> l | ns-num-status-pdu-sent

> l | bssgp-radio-status-msg-sent

> sgsn schema

> l | 3G-attached-no-pdp

> l | 2G-attached-no-pdp

> l | 3G-rau-rej-imsi-unknown-hlr

> l | 2G-rau-rej-imsi-unknown-hlr

> l | 3G-rau-rej-illegal-ms

> l | 2G-rau-rej-illegal-ms

> l | 3G-rau-rej-illegal-me

> l | 2G-rau-rej-illegal-me

> l | 3G-rau-rej-gprs-svc-not-allow

> l | 2G-rau-rej-gprs-svc-not-allow

> l | 3G-rau-rej-gprs-and-nongprs-svc-not-allow

> l | 2G-rau-rej-gprs-and-nongprs-svc-not-allow

> l | 3G-rau-rej-msid-not-derived-by-nw

> l | 2G-rau-rej-msid-not-derived-by-nw

> l | 3G-rau-rej-implicitly-detach

> l | 2G-rau-rej-implicitly-detach

> l | 3G-rau-rej-plmn-not-allowed

> l | 2G-rau-rej-plmn-not-allowed

> l | 3G-rau-rej-location-area-not-allowed

> l | 2G-rau-rej-location-area-not-allowed

> l | 3G-rau-rej-roam-not-allowed-in-larea

> l | 2G-rau-rej-roam-not-allowed-in-larea

> l | 3G-rau-rej-gprs-svc-not-allowed-in-plmn

> l | 2G-rau-rej-gprs-svc-not-allowed-in-plmn

> l | 3G-rau-rej-no-cells-in-location-area

> l | 2G-rau-rej-no-cells-in-location-area

> l | 3G-rau-rej-msc-not-reachable

> l | 2G-rau-rej-msc-not-reachable

> l | 3G-rau-rej-network-failure

> l | 2G-rau-rej-network-failure

> l | 3G-rau-rej-mac-failure

> l | 2G-rau-rej-mac-failure

> l | 3G-rau-rej-syn-failure

> l | 2G-rau-rej-syn-failure

> l | 3G-rau-rej-congestion

> l | 2G-rau-rej-congestion

> l | 3G-rau-rej-gsm-auth-unacceptable

> l | 2G-rau-rej-gsm-auth-unacceptable

> l | 3G-rau-rej-no-pdp-ctx-actv

> l | 2G-rau-rej-no-pdp-ctx-actv

> l | 3G-rau-rej-retry-from-new-cell

> l | 2G-rau-rej-retry-from-new-cell

> l | 3G-rau-rej-sem-wrong-msg

> l | 2G-rau-rej-sem-wrong-msg

> l | 3G-rau-rej-inval-mand-info

> l | 2G-rau-rej-inval-mand-info

> l | 3G-rau-rej-msg-type-non-exist

> l | 2G-rau-rej-msg-type-non-exist

> l | 3G-rau-rej-mtype-not-compat-prot-state

> l | 2G-rau-rej-mtype-not-compat-prot-state

> l | 3G-rau-rej-ie-non-existent

> l | 2G-rau-rej-ie-non-existent

> l | 3G-rau-rej-cond-ie-error

> l | 2G-rau-rej-cond-ie-error

> l | 3G-rau-rej-msg-not-compat-prot-state

> l | 2G-rau-rej-msg-not-compat-prot-state

> l | 3G-rau-rej-prot-error

> l | 2G-rau-rej-prot-error

> l | 3G-rau-rej-unknown-error

> l | 2G-rau-rej-unknown-error

> l | 2G-signalling-service-request

> l | 2G-data-service-request

> l | 2G-service-response

> l | 2G-service-reject

> l | 2G-service-rej-netwk-fail

> l | 2G-service-rej-imsi-unknown-at-hlr

> l | 2G-service-rej-msid-not-derived-by-nwtk

> l | 2G-service-rej-implicity-detach

> l | 2G-service-rej-illegal-ms

> l | 2G-service-rej-msg-not-compat-prot-state

> l | 2G-service-rej-no-pdp-ctx-actv

> l | 2G-actv-rej-llc-sndcp-fail

> l | 2G-actv-rej-qos-not-acc

> l | 3G-actv-rej-semantic-error-tft-operation

> l | 2G-actv-rej-semantic-error-tft-operation

> l | 3G-actv-rej-syntax-err-in-tft-operation

> l | 2G-actv-rej-syntax-err-in-tft-operation

> l | 3G-actv-rej-unknown-pdp-context

> l | 2G-actv-rej-unknown-pdp-context

> l | 3G-actv-rej-semantic-err-in-pkt-filter

> l | 2G-actv-rej-semantic-err-in-pkt-filter

> l | 3G-actv-rej-syntax-err-in-pkt-filter

> l | 2G-actv-rej-syntax-err-in-pkt-filter

> l | 3G-actv-rej-pdp-notft-actv

> l | 2G-actv-rej-pdp-notft-actv

> l | 2G-sec-actv-rej-llc-sndcp-fail

> l | 2G-sec-actv-rej-qos-not-acc

> l | rab-assign-rej

> sgtp schema

> l | sgtpc-cpc-req-denied

> l | sgtpc-upc-req-v0-rx

> l | sgtpc-fwd-reloc-discard-tx

> l | sgtpc-fwd-srnsctxt-discard-rx

> Web Element Manager Path
> Click Accounting | Bulk Statistics Configuration.
> Bulk Statistic Enhancements in Release 8.1
> This section lists bulk statistic additions and changes in Release 8.1. Detailed information on bulk statistics is located in both the System Administration Guide and in the Statistics and Counters Reference.
> Bulk Statistic Additions
> Support for the following bulk statistics has been added:
> ECS Schema
> The following are new for Release 8.1

> l | p2p-irc-uplnk-bytes

> l | p2p-irc-dwlnk-bytes

> l | p2p-irc-uplnk-pkts

> l | p2p-irc-dwlnk-pkts

> l | p2p-steam-uplnk-bytes

> l | p2p-steam-dwlnk-bytes

> l | p2p-steam-uplnk-pkts

> l | p2p-steam-dwlnk-pkts

> l | p2p-ddlink-uplnk-bytes

> l | p2p-ddlink-dwlnk-bytes

> l | p2p-ddlink-uplnk-pkts

> l | p2p-ddlink-dwlnk-pkts

> l | p2p-halflife2-uplnk-bytes

> l | p2p-halflife2-dwlnk-bytes

> l | p2p-halflife2-uplnk-pkts

> l | p2p-halflife2-dwlnk-pkts

> l | p2p-hamachivpn-uplnk-bytes

> l | p2p-hamachivpn-dwlnk-bytes

> l | p2p-hamachivpn-uplnk-pkts

> l | p2p-hamachivpn-dwlnk-pkts

> l | p2p-tvants-uplnk-bytes

> l | p2p-tvants-dwlnk-bytes

> l | p2p-tvants-uplnk-pkts

> l | p2p-tvants-dwlnk-pkts

> l | p2p-tvuplayer-uplnk-bytes

> l | p2p-tvuplayer-dwlnk-bytes

> l | p2p-tvuplayer-uplnk-pkts

> l | p2p-tvuplayer-dwlnk-pkts

> l | p2p-uusee-uplnk-bytes

> l | p2p-uusee-dwlnk-bytes

> l | p2p-uusee-uplnk-pkts

> l | p2p-uusee-dwlnk-pkts

> l | p2p-vpnx-uplnk-bytes

> l | p2p-vpnx-dwlnk-bytes

> l | p2p-vpnx-uplnk-pkts

> l | p2p-vpnx-dwlnk-pkts

> l | p2p-vtun-uplnk-bytes

> l | p2p-vtun-dwlnk-bytes

> l | p2p-vtun-uplnk-pkts

> l | p2p-vtun-dwlnk-pkts

> l | p2p-winmx-uplnk-bytes

> l | p2p-winmx-dwlnk-bytes

> l | p2p-winmx-uplnk-pkts

> l | p2p-winmx-dwlnk-pkts

> l | p2p-wofwarcraft-uplnk-bytes

> l | p2p-wofwarcraft-dwlnk-bytes

> l | p2p-wofwarcraft-uplnk-pkts

> l | p2p-wofwarcraft-dwlnk-pkts

> l | p2p-xbox-uplnk-bytes

> l | p2p-xbox-dwlnk-bytes

> l | p2p-xbox-uplnk-pkts

> l | p2p-xbox-dwlnk-pkts

> Card Schema
> Added following for High Water Peak management counters:

> l | 15peak-cpubusy

> l | 5peak-cpubusy

> l | 15peak-memused

> l | 5peak-memused

> l | cpu0-15peak-cpubusy

> l | cpu0-5peak-cpubusy

> l | cpu0-15peak-memused

> l | cpu0-5peak-memused

> l | cpu1-15peak-cpubusy

> l | cpu1-5peak-cpubusy

> l | cpu1-15peak-memused

> l | cpu1-5peak-memused

> l | cpu2-15peak-cpubusy

> l | cpu2-5peak-cpubusy

> l | cpu2-15peak-memused

> l | cpu2-5peak-memused

> l | cpu3-15peak-cpubusy

> l | cpu3-5peak-cpubusy

> l | cpu3-15peak-memused

> l | cpu3-5peak-memused

> System Schema
> Added following for High Water Peak management counters:

> l | pdp-ctx-15peak-active

> l | pdp-ctx-5peak-active

> Also added following for bulk statistics enhancement:

> l | ggsn-ttlsgsnconn

> l | ggsn-cursgsnact

> l | sess-ttlcallop

> l | sess-curaaaacctpending

> l | sess-total-curr

> l | hamipv6-totalsubscriber

> l | curr-proxy

> l | curr-relay-agent

> l | dhcp-curservsess

> l | sess-total-setup

> l | setup-proxy

> l | setup-relay-agent

> l | dhcp-ttlservsess

> l | total-released

> l | proxy-bearer-call-term

> l | proxy-lease-exp-policy

> l | proxy-lease-renew-failure

> l | proxy-ip-mis-match

> l | proxy-lease-time-mis-match

> l | proxy-other-reasons

> l | relay-admin-releases

> l | relay-bearer-call-term

> l | relay-lease-time-out

> l | relay-other-reasons

> l | dhcp-servdisc-admin

> l | dhcp-servdisc-callterm

> l | dhcp-servdisc-leasetmo

> l | dhcp-servdisc-other

> l | dhcp-msg-discover-tx

> l | dhcp-msg-discover-retransmitted

> l | dhcp-msg-discover-rx

> l | dhcp-msg-discover-retried-rx

> l | dhcp-msg-discover-relayed

> l | dhcp-msg-discoverd-retried-relayed

> l | dhcp-msg-offer-rx

> l | dhcp-msg-offer-discarded

> l | dhcp-msg-offer-tx

> l | dhcp-msg-offer-relayed

> l | dhcp-msg-request-tx

> l | dhcp-msg-request-retransmitted

> l | dhcp-msg-request-rx

> l | dhcp-msg-request-renewal-rx

> l | dhcp-msg-request-requesting-relayed

> l | dhcp-msg-request-renewing-relayed

> l | dhcp-msg-ack-rx

> l | dhcp-msg-ack-for-inform

> l | dhcp-msg-ack-renewing-rx

> l | dhcp-msg-ack-tx

> l | dhcp-msg-ack-renewing-tx

> l | dhcp-msg-ack-relayed

> l | dhcp-msg-ack-renewing-relayed

> l | dhcp-msg-nak-rx

> l | dhcp-msg-nak-for-inform

> l | dhcp-msg-nak-tx

> l | dhcp-msg-nak-relayed

> l | dhcp-msg-decline-tx

> l | dhcp-msg-decline-rx

> l | dhcp-msg-decline-relayed

> l | dhcp-msg-release-tx

> l | dhcp-msg-release-rx

> l | dhcp-msg-release-relayed

> l | dhcp-msg-release-for-relay-call

> l | dhcp-msg-inform-tx

> l | dhcp-msg-inform-retransmitted

> l | dhcp-msg-inform-rx

> l | dhcp-msg-inform-relayed

> l | offer-dis-parse-err

> l | offer-dis-lease-less-than-min

> l | offer-dis-lease-greater-than-max

> l | offer-dis-ip-val-failed

> l | offer-dis-xid-mis-match

> l | ack-dis-parse-err

> l | ack-dis-xid-mis-match

> l | decline-dis-ip-mis-match

> l | ip-lease-renewal

> l | failed-ip-lease-renew

> l | no-reply-from-server

> l | server-nak

> l | ip-addr-mis-match

> l | lease-mis-match

> l | storage-name

> l | storage-curavail

> l | storage-ttlavail

> l | cf-cat-all-pkts-hit

> l | cf-cat-all-pkts-block

> l | cf-cat-timer-pkts-hit

> l | cf-cat-timer-pkts-block

> l | cf-cat-xcategory-pkts-hit

> l | cf-cat-xcategory-pkts-block

> l | cf-cursub

> l | cf-ttlsub

> l | url-blacklisting-hits

> l | url-blacklisting-misses

> Port Schema
> Added following for High Water Peak management counters:

> l | port-5peak-rx-util

> l | port-5peak-tx-util

> l | port-15peak-rx-util

> l | port-15peak-rx-util

> GPRS Schema

> l | packets-sent-to-bsc

> l | packets-rcvd-from-bsc

> l | bytes-sent-to-bsc

> l | bytes-rcvd-from-bsc

> l | gprs-num-subs-gea0-capable

> l | gprs-num-subs-gea1-capable

> l | gprs-num-subs-gea2-capable

> l | gprs-num-subs-gea3-capable

> l | gprs-num-subs-gea0-negotiated

> l | gprs-num-subs-gea1-negotiated

> l | gprs-num-subs-gea2-negotiated

> l | gprs-num-subs-gea3-negotiated

> GTPC Schema
> Added following for this schema:

> l | mbms-ses-start-tx- accept

> l | mbms-ses-start-tx-deny

> l | mbms-ses-stop-tx

> l | mbms-ses-stop-tx- accept

> l | sess-in-preservation-mode

> l | transition-to-preservation-mode

> l | transition-to-non-preservation-mode

> l | sess-in-focs

> l | cnt-of-release-due-to-other

> l | cnt-of-release-due-to-violation

> l | ipca-pdp-context-tx

> l | ipca-pdp-context-tx-accepted

> l | ipca-pdp-context-tx-denied

> l | ipca-reject-rx-no-resources

> l | ipca-reject-rx-no-mem-avail

> l | ipca-reject-rx-sys-failure

> l | ipca-reject-rx-non-existent

> l | ipca-reject-rx-unsupported-service

> l | ipca-reject-rx-invalid-msg-format

> l | ipca-reject-rx-semantic-err-in-tft

> l | ipca-reject-rx-syntactic-err-in-tft

> l | ipca-reject-rx-man-ie-incorrect

> l | ipca-reject-rx-semantic-err-in-pac-filter

> l | ipca-reject-rx-man-ie-missing

> l | ipca-reject-rx-optional-ie-incorrect

> l | ipca-reject-rx-syntactic-err-in-pac-filter

> l | ipca-reject-rx-ue-not-gprs-rsp

> l | ipca-reject-rx-ue-refuses

> l | ipca-reject-rx-invalid-correlation-id

> GTPC Schema
> Added following for this schema:

> l | total-gmbcdr-xmit

> l | total-gmbcdr-rexmit

> l | total-gmbcdr-accept

> l | total-gmscdr-fail

> System Schema
> Added following stats for system setup time counters:

> l | sess-setuptime-18sec

> l | sess-setuptime-over18sec

> SGSN Schema
> Added following stats:

> l | 3G-actv-fail-phase-2-offload

> l | 2G-actv-fail-phase-2-offload

> l | 3G-network-sharing-supp-ue

> l | 3G-network-sharing-non-supp-ue

> CSCF Schema
> Added the following stats for this schema:

> l | de-regs-fromue

> l | de-regs-fromnw

> l | reg-resp-4xxrx

> l | reg-resp-4xxtx

> l | reg-resp-5xxrx

> l | reg-resp-5xxtx

> l | reg-resp-6xxrx

> l | reg-resp-6xxtx

> l | rereg-resp-4xxrx

> l | rereg-resp-4xxtx

> l | rereg-resp-5xxrx

> l | rereg-resp-5xxtx

> l | rereg-resp-6xxrx

> l | rereg-resp-6xxtx

> l | dereg-resp-4xxrx

> l | dereg-resp-4xxtx

> l | dereg-resp-5xxrx

> l | dereg-resp-5xxtx

> l | dereg-resp-6xxrx

> l | dereg-resp-6xxtx

> l | msgsum-subs-resp-3xxrx

> l | msgsum-subs-resp-3xxtx

> l | msgsum-subs-resp-4xxrx

> l | msgsum-subs-resp-4xxtx

> l | msgsum-subs-resp-5xxrx

> l | msgsum-subs-resp-5xxtx

> l | msgsum-subs-resp-6xxrx

> l | msgsum-subs-resp-6xxtx

> l | msgsum-resubs-resp-3xxrx

> l | msgsum-resubs-resp-3xxtx

> l | msgsum-resubs-resp-4xxrx

> l | msgsum-resubs-resp-4xxtx

> l | msgsum-resubs-resp-5xxrx

> l | msgsum-resubs-resp-5xxtx

> l | msgsum-resubs-resp-6xxrx

> l | msgsum-resubs-resp-6xxtx

> l | msgsum-unsubs-resp-3xxrx

> l | msgsum-unsubs-resp-3xxtx

> l | msgsum-unsubs-resp-4xxrx

> l | msgsum-unsubs-resp-4xxtx

> l | msgsum-unsubs-resp-5xxrx

> l | msgsum-unsubs-resp-5xxtx

> l | msgsum-unsubs-resp-6xxrx

> l | msgsum-unsubs-resp-6xxtx

> l | msgsum-notify-attrx

> l | msgsum-notify-atttx

> l | msgsum-notify-succrx

> l | msgsum-notify-succtx

> l | msgsum-notify-failrx

> l | msgsum-notify-failtx

> l | msgsum-notify-resp-3xxrx

> l | msgsum-notify-resp-3xxtx

> l | msgsum-notify-resp-400rx

> l | msgsum-notify-resp-400tx

> l | msgsum-notify-resp-481rx

> l | msgsum-notify-resp-481tx

> l | msgsum-notify-resp-489rx

> l | msgsum-notify-resp-489tx

> l | msgsum-notify-resp-4xxrx

> l | msgsum-notify-resp-4xxtx

> l | msgsum-notify-resp-500rx

> l | msgsum-notify-resp-500tx

> l | msgsum-notify-resp-5xxrx

> l | msgsum-notify-resp-5xxtx

> l | msgsum-notify-resp-6xxrx

> l | msgsum-notify-resp-6xxtx

> l | msgsum-pub-attrx

> l | msgsum-pub-atttx

> l | msgsum-pub-succrx

> l | msgsum-pub-succtx

> l | msgsum-pub-failrx

> l | msgsum-pub-failtx

> l | msgsum-pub-resp-3xxrx

> l | msgsum-pub-resp-3xxtx

> l | msgsum-pub-resp-400rx

> l | msgsum-pub-resp-400tx

> l | msgsum-pub-resp-404rx

> l | msgsum-pub-resp-404tx

> l | msgsum-pub-resp-412rx

> l | msgsum-pub-resp-412tx

> l | msgsum-pub-resp-423rx

> l | msgsum-pub-resp-423tx

> l | msgsum-pub-resp-489rx

> l | msgsum-pub-resp-489tx

> l | msgsum-pub-resp-4xxrx

> l | msgsum-pub-resp-4xxtx

> l | msgsum-pub-resp-500rx

> l | msgsum-pub-resp-500tx

> l | msgsum-pub-resp-503rx

> l | msgsum-pub-resp-503tx

> l | msgsum-pub-resp-5xxrx

> l | msgsum-pub-resp-5xxtx

> l | msgsum-pub-resp-6xxrx

> l | msgsum-pub-resp-6xxtx

> l | msgsum-unpub-attrx

> l | msgsum-unpub-atttx

> l | msgsum-unpub-succrx

> l | msgsum-unpub-succtx

> l | msgsum-unpub-failrx

> l | msgsum-unpub-failtx

> l | msgsum-unpub-resp-3xxrx

> l | msgsum-unpub-resp-3xxtx

> l | msgsum-unpub-resp-400rx

> l | msgsum-unpub-resp-400tx

> l | msgsum-unpub-resp-404rx

> l | msgsum-unpub-resp-404tx

> l | msgsum-unpub-resp-412rx

> l | msgsum-unpub-resp-412tx

> l | msgsum-unpub-resp-423rx

> l | msgsum-unpub-resp-423tx

> l | msgsum-unpub-resp-489rx

> l | msgsum-unpub-resp-489tx

> l | msgsum-unpub-resp-4xxrx

> l | msgsum-unpub-resp-4xxtx

> l | msgsum-unpub-resp-500rx

> l | msgsum-unpub-resp-500tx

> l | msgsum-unpub-resp-503rx

> l | msgsum-unpub-resp-503tx

> l | msgsum-unpub-resp-5xxrx

> l | msgsum-unpub-resp-5xxtx

> l | msgsum-unpub-resp-6xxrx

> l | msgsum-unpub-resp-6xxtx

> l | pres-subs-resp-3xxrx

> l | pres-subs-resp-3xxtx

> l | pres-subs-resp-4xxrx

> l | pres-subs-resp-4xxtx

> l | pres-subs-resp-5xxrx

> l | pres-subs-resp-5xxtx

> l | pres-subs-resp-6xxrx

> l | pres-subs-resp-6xxtx

> l | pres-resubs-resp-3xxrx

> l | pres-resubs-resp-3xxtx

> l | pres-resubs-resp-4xxrx

> l | pres-resubs-resp-4xxtx

> l | pres-resubs-resp-5xxrx

> l | pres-resubs-resp-5xxtx

> l | pres-resubs-resp-6xxrx

> l | pres-resubs-resp-6xxtx

> l | pres-unsubs-resp-3xxrx

> l | pres-unsubs-resp-3xxtx

> l | pres-unsubs-resp-4xxrx

> l | pres-unsubs-resp-4xxtx

> l | pres-unsubs-resp-5xxrx

> l | pres-unsubs-resp-5xxtx

> l | pres-unsubs-resp-6xxrx

> l | pres-unsubs-resp-6xxtx

> l | pres-notify-attrx

> l | pres-notify-atttx

> l | pres-notify-succrx

> l | pres-notify-succtx

> l | pres-notify-failrx

> l | pres-notify-failtx

> l | pres-notify-resp-3xxrx

> l | pres-notify-resp-3xxtx

> l | pres-notify-resp-400rx

> l | pres-notify-resp-400tx

> l | pres-notify-resp-481rx

> l | pres-notify-resp-481tx

> l | pres-notify-resp-489rx

> l | pres-notify-resp-489tx

> l | pres-notify-resp-4xxrx

> l | pres-notify-resp-4xxtx

> l | pres-notify-resp-500rx

> l | pres-notify-resp-500tx

> l | pres-notify-resp-5xxrx

> l | pres-notify-resp-5xxtx

> l | pres-notify-resp-6xxrx

> l | pres-notify-resp-6xxtx

> l | pres-pub-attrx

> l | pres-pub-atttx

> l | pres-pub-succrx

> l | pres-pub-succtx

> l | pres-pub-failrx

> l | pres-pub-failtx

> l | pres-pub-resp-3xxrx

> l | pres-pub-resp-3xxtx

> l | pres-pub-resp-400rx

> l | pres-pub-resp-400tx

> l | pres-pub-resp-404rx

> l | pres-pub-resp-404tx

> l | pres-pub-resp-412rx

> l | pres-pub-resp-412tx

> l | pres-pub-resp-423rx

> l | pres-pub-resp-423tx

> l | pres-pub-resp-489rx

> l | pres-pub-resp-489tx

> l | pres-pub-resp-4xxrx

> l | pres-pub-resp-4xxtx

> l | pres-pub-resp-500rx

> l | pres-pub-resp-500tx

> l | pres-pub-resp-503rx

> l | pres-pub-resp-503tx

> l | pres-pub-resp-5xxrx

> l | pres-pub-resp-5xxtx

> l | pres-pub-resp-6xxrx

> l | pres-pub-resp-6xxtx

> l | pres-unpub-attrx

> l | pres-unpub-atttx

> l | pres-unpub-succrx

> l | pres-unpub-succtx

> l | pres-unpub-failrx

> l | pres-unpub-failtx

> l | pres-unpub-resp-3xxrx

> l | pres-unpub-resp-3xxtx

> l | pres-unpub-resp-400rx

> l | pres-unpub-resp-400tx

> l | pres-unpub-resp-404rx

> l | pres-unpub-resp-404tx

> l | pres-unpub-resp-412rx

> l | pres-unpub-resp-412tx

> l | pres-unpub-resp-423rx

> l | pres-unpub-resp-423tx

> l | pres-unpub-resp-489rx

> l | pres-unpub-resp-489tx

> l | pres-unpub-resp-4xxrx

> l | pres-unpub-resp-4xxtx

> l | pres-unpub-resp-500rx

> l | pres-unpub-resp-500tx

> l | pres-unpub-resp-503rx

> l | pres-unpub-resp-503tx

> l | pres-unpub-resp-5xxrx

> l | pres-unpub-resp-5xxtx

> l | pres-unpub-resp-6xxrx

> l | pres-unpub-resp-6xxtx

> l | reg-subs-resp-3xxrx

> l | reg-subs-resp-3xxtx

> l | reg-subs-resp-4xxrx

> l | reg-subs-resp-4xxtx

> l | reg-subs-resp-5xxrx

> l | reg-subs-resp-5xxtx

> l | reg-subs-resp-6xxrx

> l | reg-subs-resp-6xxtx

> l | reg-resubs-resp-3xxrx

> l | reg-resubs-resp-3xxtx

> l | reg-resubs-resp-4xxrx

> l | reg-resubs-resp-4xxtx

> l | reg-resubs-resp-5xxrx

> l | reg-resubs-resp-5xxtx

> l | reg-resubs-resp-6xxrx

> l | reg-resubs-resp-6xxtx

> l | reg-unsubs-resp-3xxrx

> l | reg-unsubs-resp-3xxtx

> l | reg-unsubs-resp-4xxrx

> l | reg-unsubs-resp-4xxtx

> l | reg-unsubs-resp-5xxrx

> l | reg-unsubs-resp-5xxtx

> l | reg-unsubs-resp-6xxrx

> l | reg-unsubs-resp-6xxtx

> l | reg-notify-attrx

> l | reg-notify-atttx

> l | reg-notify-succrx

> l | reg-notify-succtx

> l | reg-notify-failrx

> l | reg-notify-failtx

> l | reg-notify-resp-3xxrx

> l | reg-notify-resp-3xxtx

> l | reg-notify-resp-400rx

> l | reg-notify-resp-400tx

> l | reg-notify-resp-481rx

> l | reg-notify-resp-481tx

> l | reg-notify-resp-489rx

> l | reg-notify-resp-489tx

> l | reg-notify-resp-4xxrx

> l | reg-notify-resp-4xxtx

> l | reg-notify-resp-500rx

> l | reg-notify-resp-500tx

> l | reg-notify-resp-5xxrx

> l | reg-notify-resp-5xxtx

> l | reg-notify-resp-6xxrx

> l | reg-notify-resp-6xxtx

> l | reg-pub-attrx

> l | reg-pub-atttx

> l | reg-pub-succrx

> l | reg-pub-succtx

> l | reg-pub-failrx

> l | reg-pub-failtx

> l | reg-pub-resp-3xxrx

> l | reg-pub-resp-3xxtx

> l | reg-pub-resp-400rx

> l | reg-pub-resp-400tx

> l | reg-pub-resp-404rx

> l | reg-pub-resp-404tx

> l | reg-pub-resp-412rx

> l | reg-pub-resp-412tx

> l | reg-pub-resp-423rx

> l | reg-pub-resp-423tx

> l | reg-pub-resp-489rx

> l | reg-pub-resp-489tx

> l | reg-pub-resp-4xxrx

> l | reg-pub-resp-4xxtx

> l | reg-pub-resp-500rx

> l | reg-pub-resp-500tx

> l | reg-pub-resp-503rx

> l | reg-pub-resp-503tx

> l | reg-pub-resp-5xxrx

> l | reg-pub-resp-5xxtx

> l | reg-pub-resp-6xxrx

> l | reg-pub-resp-6xxtx

> l | reg-unpub-attrx

> l | reg-unpub-atttx

> l | reg-unpub-succrx

> l | reg-unpub-succtx

> l | reg-unpub-failrx

> l | reg-unpub-failtx

> l | reg-unpub-resp-3xxrx

> l | reg-unpub-resp-3xxtx

> l | reg-unpub-resp-400rx

> l | reg-unpub-resp-400tx

> l | reg-unpub-resp-404rx

> l | reg-unpub-resp-404tx

> l | reg-unpub-resp-412rx

> l | reg-unpub-resp-412tx

> l | reg-unpub-resp-423rx

> l | reg-unpub-resp-423tx

> l | reg-unpub-resp-489rx

> l | reg-unpub-resp-489tx

> l | reg-unpub-resp-4xxrx

> l | reg-unpub-resp-4xxtx

> l | reg-unpub-resp-500rx

> l | reg-unpub-resp-500tx

> l | reg-unpub-resp-503rx

> l | reg-unpub-resp-503tx

> l | reg-unpub-resp-5xxrx

> l | reg-unpub-resp-5xxtx

> l | reg-unpub-resp-6xxrx

> l | reg-unpub-resp-6xxtx

> l | winfo-subs-resp-3xxrx

> l | winfo-subs-resp-3xxtx

> l | winfo-subs-resp-4xxrx

> l | winfo-subs-resp-4xxtx

> l | winfo-subs-resp-5xxrx

> l | winfo-subs-resp-5xxtx

> l | winfo-subs-resp-6xxrx

> l | winfo-subs-resp-6xxtx

> l | winfo-resubs-resp-3xxrx

> l | winfo-resubs-resp-3xxtx

> l | winfo-resubs-resp-4xxrx

> l | winfo-resubs-resp-4xxtx

> l | winfo-resubs-resp-5xxrx

> l | winfo-resubs-resp-5xxtx

> l | winfo-resubs-resp-6xxrx

> l | winfo-resubs-resp-6xxtx

> l | winfo-unsubs-resp-3xxrx

> l | winfo-unsubs-resp-3xxtx

> l | winfo-unsubs-resp-4xxrx

> l | winfo-unsubs-resp-4xxtx

> l | winfo-unsubs-resp-5xxrx

> l | winfo-unsubs-resp-5xxtx

> l | winfo-unsubs-resp-6xxrx

> l | winfo-unsubs-resp-6xxtx

> l | winfo-notify-attrx

> l | winfo-notify-atttx

> l | winfo-notify-succrx

> l | winfo-notify-succtx

> l | winfo-notify-failrx

> l | winfo-notify-failtx

> l | winfo-notify-resp-3xxrx

> l | winfo-notify-resp-3xxtx

> l | winfo-notify-resp-400rx

> l | winfo-notify-resp-400tx

> l | winfo-notify-resp-481rx

> l | winfo-notify-resp-481tx

> l | winfo-notify-resp-489rx

> l | winfo-notify-resp-489tx

> l | winfo-notify-resp-4xxrx

> l | winfo-notify-resp-4xxtx

> l | winfo-notify-resp-500rx

> l | winfo-notify-resp-500tx

> l | winfo-notify-resp-5xxrx

> l | winfo-notify-resp-5xxtx

> l | winfo-notify-resp-6xxrx

> l | winfo-notify-resp-6xxtx

> l | winfo-pub-attrx

> l | winfo-pub-atttx

> l | winfo-pub-succrx

> l | winfo-pub-succtx

> l | winfo-pub-failrx

> l | winfo-pub-failtx

> l | winfo-pub-resp-3xxrx

> l | winfo-pub-resp-3xxtx

> l | winfo-pub-resp-400rx

> l | winfo-pub-resp-400tx

> l | winfo-pub-resp-404rx

> l | winfo-pub-resp-404tx

> l | winfo-pub-resp-412rx

> l | winfo-pub-resp-412tx

> l | winfo-pub-resp-423rx

> l | winfo-pub-resp-423tx

> l | winfo-pub-resp-489rx

> l | winfo-pub-resp-489tx

> l | winfo-pub-resp-4xxrx

> l | winfo-pub-resp-4xxtx

> l | winfo-pub-resp-500rx

> l | winfo-pub-resp-500tx

> l | winfo-pub-resp-503rx

> l | winfo-pub-resp-503tx

> l | winfo-pub-resp-5xxrx

> l | winfo-pub-resp-5xxtx

> l | winfo-pub-resp-6xxrx

> l | winfo-pub-resp-6xxtx

> l | winfo-unpub-attrx

> l | winfo-unpub-atttx

> l | winfo-unpub-succrx

> l | winfo-unpub-succtx

> l | winfo-unpub-failrx

> l | winfo-unpub-failtx

> l | winfo-unpub-resp-3xxrx

> l | winfo-unpub-resp-3xxtx

> l | winfo-unpub-resp-400rx

> l | winfo-unpub-resp-400tx

> l | winfo-unpub-resp-404rx

> l | winfo-unpub-resp-404tx

> l | winfo-unpub-resp-412rx

> l | winfo-unpub-resp-412tx

> l | winfo-unpub-resp-423rx

> l | winfo-unpub-resp-423tx

> l | winfo-unpub-resp-489rx

> l | winfo-unpub-resp-489tx

> l | winfo-unpub-resp-4xxrx

> l | winfo-unpub-resp-4xxtx

> l | winfo-unpub-resp-500rx

> l | winfo-unpub-resp-500tx

> l | winfo-unpub-resp-503rx

> l | winfo-unpub-resp-503tx

> l | winfo-unpub-resp-5xxrx

> l | winfo-unpub-resp-5xxtx

> l | winfo-unpub-resp-6xxrx

> l | winfo-unpub-resp-6xxtx

> l | callrel-from-ue

> l | callrel-from-nw

> l | callrel-from-radioloss

> l | callrel-from-local

> l | beerrrx

> l | beerrtx

> l | tot-sip-msgs-proc

> l | regreqretx

> l | invreqretx

> l | byereqretx

> l | cancreqretx

> l | req-retx

> l | resp-retx

> l | reqresp-retx

> l | subsetup<200ms

> l | subsetup200-400ms

> l | subsetup400-600ms

> l | subsetup600-800ms

> l | subsetup800-1000ms

> l | subsetup1000-1200ms

> l | subsetup1200-1400ms

> l | subsetup1400-1600ms

> l | subsetup1600-1800ms

> l | subsetup1800-2000ms

> l | subsetup2000-2200ms

> l | subsetup2200-2400ms

> l | subsetup2400-2600ms

> l | subsetup2600-2800ms

> l | subsetup2800-3000ms

> l | subsetup3-5sec

> l | subsetup5-7sec

> l | subsetup7-9sec

> l | subsetup9-11sec

> l | subsetup11-13sec

> l | subsetup13-15sec

> l | subsetup15-17sec

> l | subsetup17-19sec

> l | subsetup19-21sec

> l | subsetup>21sec

> l | subdur<1hr

> l | subdur1-2hr

> l | subdur2-3hr

> l | subdur3-4hr

> l | subdur4-5hr

> l | subdur5-6hr

> l | subdur6-7hr

> l | subdur7-8hr

> l | subdur8-9hr

> l | subdur9-10hr

> l | subdur>10hr

> l | curr-reg-subs

> l | active-reg-subs

> l | curr-sigcomp-subs

> l | active-sigcomp-subs

> l | curr-ipsec-subs

> l | active-ipsec-subs

> l | active-voip-subs

> l | curr-presence-subs

> l | active-presence-subs

> l | active-im-subs

> l | dpeca-curr-sessions

> l | dpeca-tot-sess-init

> l | dpeca-tot-sess-terminated

> l | dpeca-tot-sess-failovers

> l | dpeca-tot-sess-failover-err

> l | dpeca-tot-msg-received

> l | dpeca-tot-msg-sent

> l | dpeca-tot-aar-sent

> l | dpeca-tot-aaa-received

> l | dpeca-tot-uncorr-aaa

> l | dpeca-tot-uncorr-sta

> l | dpeca-tot-aari-sent

> l | dpeca-tot-aaai-received

> l | dpeca-tot-aaai-accepted

> l | dpeca-tot-aaai-rejected

> l | dpeca-tot-aaai-timeout

> l | dpeca-tot-aaru-sent

> l | dpeca-tot-aaau-received

> l | dpeca-tot-aaau-timeout

> l | dpeca-tot-str-sent

> l | dpeca-tot-sta-received

> l | dpeca-tot-sta-timeout

> l | dpeca-tot-asr-received

> l | dpeca-tot-asa-sent

> l | dpeca-tot-rar-received

> l | dpeca-tot-raa-sent

> l | dpeca-tot-protocol-err

> l | dpeca-tot-aaa-parse-err

> l | dpeca-tot-unk-sess-req

> l | dpeca-tot-unk-cmd-codes

> l | dpeca-tc-logout

> l | dpeca-tc-service-not-prov

> l | dpeca-tc-bad-ans

> l | dpeca-tc-administrative

> l | dpeca-tc-link-broken

> l | dpeca-tc-auth-expired

> l | dpeca-tc-user-moved

> l | dpeca-tc-session-timeout

> l | dpeca-auth-rejected

> l | dpeca-other-errors

> l | dpeca-exp-res-invalid-

> l | service-info

> l | dpeca-exp-res-filter-

> l | restrictions

> l | dpeca-exp-res-req-service-

> l | not-authorized

> l | dpeca-exp-res-duplicated-af-session

> l | dpeca-exp-res-ipcan-session-not-avail

> CSCFINTF Schema
> The CSCFINT schema was added to track CSCF interfaces.
> Added the following stats for this schema:

> l | sitserrrx

> l | sitserrtx

> Obsoleted Bulk Statistics
> GTPP Schema
> Following are obsolete now:

> l | total-gmbsccdr-xmit

> l | total-gmbsccdr-rexmit

> l | total-gmbsccdr-accept

> l | total-gmbscdr-fail

> System Schema
> Following are obsolete now:

> l | curr-proxy

> l | curr-relay-agent

> l | sess-total-setup

> l | setup-proxy

> l | setup-relay-agent

> l | total-released

> l | rel-proxy-admin-releases

> l | rel-proxy-bearer-call-term.

> l | rel-proxy-lease-exp-policy

> l | rel-proxy-lease-renew-failure

> l | rel-proxy-ip-mis-match

> l | rel-proxy-lease-time-mis-match

> l | rel-proxy-other-reasons

> l | rel-relay-admin-releases

> l | rel-relay-bearer-call-ter.

> l | rel-relay-lease-time-out

> l | rel-relay-other-reasons

> l | discover-tx

> l | discover-retransmitted

> l | discover-rx

> l | discover-retried-rx

> l | discover-relayed

> l | discoverd-retried-relayed

> l | offer-rx

> l | offer-discarded

> l | offer-tx

> l | offer-relayed

> l | request-tx

> l | request-retransmitted

> l | request-rx

> l | request-renewal-rx

> l | request-requesting-relayed

> l | request-renewing-relayed

> l | ack-rx

> l | ack-for-inform

> l | ack-renewing-rx

> l | ack-tx

> l | ack-renewing-tx

> l | ack-relayed

> l | ack-renewing-relayed

> l | nak-rx

> l | nak-for-inform

> l | nak-tx

> l | nak-relayed

> l | decline-tx

> l | decline-rx

> l | decline-relayed

> l | release-tx

> l | release-rx

> l | release-relayed

> l | release-for-relay-call

> l | inform-tx

> l | inform-retransmitted

> l | inform-rx

> l | inform-relayed

> l | offer-dis-parse-err

> l | offer-dis-lease-less-than-min

> l | offer-dis-lease-greater-than-max

> l | offer-dis-ip-val-failed

> l | offer-dis-xid-mismatch

> l | ack-dis-parse-err

> l | ack-dis-xid-mis-match

> l | decline-dis-ip-mis-match

> l | ip-lease-renewal

> l | failed-ip-lease-renew

> l | no-reply-from-server

> l | server-nak

> l | ip-addr-mis-match

> l | lease-mis-match

> l | cf-cat-adv-pkts-hit

> l | cf-cat-adv-pkts-block

> l | cf-cat-auct-pkts-hit

> l | cf-cat-auct-pkts-block

> l | cf-cat-clean-pkts-hit

> l | cf-cat-clean-pkts-block

> l | cf-cat-cporn-pkts-hit

> l | cf-cat-cporn-pkts-block

> l | cf-cat-esrb-pkts-hit

> l | cf-cat-esrb-pkts-block

> l | cf-cat-p2p-pkts-hit

> l | cf-cat-p2p-pkts-block

> l | cf-cat-phish-pkts-hit

> l | cf-cat-phish-pkts-block

> l | cf-cat-radio-pkts-hit

> l | cf-cat-radio-pkts-block

> l | cf-cat-sftwre-pkts-hit

> l | cf-cat-sftwre-pkts-block

> l | cf-cat-spywre-pkts-hit

> l | cf-cat-spywre-pkts-block

> l | cf-cat-susp-pkts-hit

> l | cf-cat-susp-pkts-block

> HAMIPv6 Schema
> The following are new for Release 8.1

> l | admprohreason_badreq

> l | insufresource_badreq

> l | bindacksent_senderror

> l | admprohreason_congcondenied

> l | ICMPv6_toobigdrop

> l | bindupddiscard_congdisc

> l | bindupddiscard_chkerror

> l | bindupddiscard_iniauthpend

> l | bindupddiscard_sessnotfound

> l | bindupddiscard_hamgrnotrea

> l | bindupddiscard_decfail

> l | bindupddiscard_invbuflen

> Obsoleted Bulk Statistics
> The following bulkstats are obsoleted for Release 8.1
> HAMIPv6 Schema

> l | icmpv6_toobiggenerate

> l | rrqdeny_admprohibit

> l | rrqdeny_unknownha

> l | denyreason_simbindexceed

> l | denyreason_senderror

> l | denyreason_badreq

> l | hamipv6-totalsubscriber

> Bulk Statistic Enhancements in Release 8.3
> This section lists bulk statistic additions and changes in Release 8.3. Detailed information on bulk statistics is located in both the System Administration Guide and in the Statistics and Counters Reference.
> Bulk Statistic Additions
> Support for the following bulk statistics has been added:
> nat-realm Schema
> The new schema nat-realm supports the following variables:

> l | vpnname

> l | realmname

> l | nat-bind-updates

> l | nat-rlm-bytes-tx

> l | nat-rlm-flows

> l | nat-rlm-ip-denied

> l | nat-rlm-port-denied

> l | nat-rlm-ttl-ips

> l | nat-rlm-ips-in-use

> l | nat-rlm-current-users

> l | nat-rlm-ttl-port-chunks

> l | nat-rlm-chunks-in-use

> system Schema
> The following statistics have been added to the system schema in Release 8.3:

> l | ikev2-ikesadel

> l | ikev2-ikesadelreq-sent

> l | ikev2-ikesadelreq-recv

> l | ikev2-ikesadelrep-sent

> l | ikev2-ikesadelrep-recv

> l | ikev2-curikev2sa

> l | ikev2-curhalfsa

> l | ikev2-curconnsa

> l | ikev2-curestsa

> l | ikev2-curchildsa

> l | ikev2-exp-retran

> l | ikev2-exp-setupnoxchg

> l | ikev2-exp-setup

> l | ikev2-exp-lifesoft

> l | ikev2-exp-lifehard

> l | ikev2-exp-childsetupnoxchg

> l | ikev2-exp-childlifesoft

> l | ikev2-exp-childlifehard

> l | ikev2-auth-p1succ

> l | ikev2-auth-p1fail

> l | ikev2-auth-p1req

> l | ikev2-auth-p1rsp

> l | ikev2-auth-p2succ

> l | ikev2-auth-p2fail

> l | ikev2-auth-p2req

> l | ikev2-auth-p2rsp

> l | ikev2-auth-p2succmd5

> l | ikev2-auth-p2failmd5

> l | ikev2-auth-p2succgtc

> l | ikev2-auth-p2failgtc

> l | ikev2-auth-failhash

> l | ikev2-auth-failsign

> l | ikev2-auth-failmskmiss

> l | ikev2-auth-failmissanother

> l | ikev2-xchg-droprspnoikesa

> l | ikev2-xchg-dropinvrsp

> l | ikev2-xchg-dropnoninitnoikesa

> l | ikev2-xchg-dropinvmsgid

> l | ikev2-xchg-dropinvmajver

> l | ikev2-xchg-dropikesaerr

> l | ikev2-xchg-dropunkcrit

> l | ikev2-xchg-dropretransdisc

> l | ikev2-notif-cooksent

> l | ikev2-notif-cookrecv

> l | ikev2-notif-cookmatch

> l | ikev2-notif-cooknomatch

> l | ikev2-notif-multauthsupp

> l | ikev2-notif-anothauth

> l | ikev2-rekey-ikesareqsent

> l | ikev2-rekey-ikesareqrcvd

> l | ikev2-rekey-ikesarspsent

> l | ikev2-rekey-ikesarsprcvd

> l | ikev2-rekey-ikesaignored

> l | ikev2-rekey-childsareqsent

> l | ikev2-rekey-childsareqrecv

> l | ikev2-rekey-childsarspsent

> l | ikev2-rekey-childsarsprecv

> l | ikev2-rekey-childsaignored

> l | ikev2-mobike-sent

> l | ikev2-mobike-recv

> l | ikev2-mobike-ignored

> l | ikev2-misc-ikesacrefail

> l | ikev2-misc-saflowopfail

> l | ikev2-notifpaysent-invke

> l | ikev2-notifpaysent-invmajver

> l | ikev2-notifpaysent-invmsgid

> l | ikev2-notifpaysent-invsyn

> l | ikev2-notifpaysent-noaddsa

> l | ikev2-notifpaysent-noprop

> l | ikev2-notifpaysent-tsunaccept

> l | ikev2-notifpaysent-unsuppcrit

> l | ikev2-notifpaysent-intfail

> l | ikev2-notifpayrecv-invke

> l | ikev2-notifpayrecv-nvmajver

> l | ikev2-notifpayrecv-invmsgid

> l | ikev2-notifpayrecv-invsyn

> l | ikev2-notifpayrecv-noaddsa

> l | ikev2-notifpayrecv-noprop

> l | ikev2-notifpayrecv-tsunaccept

> l | ikev2-notifpayrecv-unsuppcrit

> l | ikev2-decfail-pktfail

> l | ikev2-decfail-interr

> l | ikev2-decfail-iphdr

> l | ikev2-decfail-udphdr

> l | ikev2-decfail-ikehdr

> l | ikev2-decfail-ikehdrpay

> l | ikev2-decfail-ikehdrinitspi

> l | ikev2-decfail-ikehdrrspspi

> l | ikev2-decfail-ikehdrmajver

> l | ikev2-decfail-ikehdrminver

> l | ikev2-decfail-ikehdrxchgtyp

> l | ikev2-decfail-ikehdrrecvflag

> l | ikev2-decfail-ikehdrlen

> l | ikev2-decfail-syn

> l | ikev2-decfail-paysyn

> l | ikev2-decfail-paylen

> l | ikev2-decfail-unkcritpay

> l | ikev2-decfail-toomanypay

> l | ikev2-decfail-sapaylen

> l | ikev2-decfail-saprophdr

> l | ikev2-decfail-saprophdrrecv

> l | ikev2-decfail-toomanytrans

> l | ikev2-decfail-saprophdrlen

> l | ikev2-decfail-toomanyprop

> l | ikev2-decfail-1stsapropnum

> l | ikev2-decfail-saprotid

> l | ikev2-decfail-sapropnum

> l | ikev2-decfail-translen

> l | ikev2-decfail-transhdr

> l | ikev2-decfail-transhdrrecv

> l | ikev2-decfail-transtype

> l | ikev2-decfail-transid

> l | ikev2-decfail-kepaylen

> l | ikev2-decfail-kedhgrp

> l | ikev2-decfail-kedhgrplen

> l | ikev2-decfail-idpaylen

> l | ikev2-decfail-idpaytype

> l | ikev2-decfail-authpaylen

> l | ikev2-decfail-noncepaylen

> l | ikev2-decfail-notifpaylen

> l | ikev2-decfail-notifpayspilen

> l | ikev2-decfail-notifpaynat

> l | ikev2-decfail-notifpayprotid

> l | ikev2-decfail-eappaylen

> l | ikev2-decfail-notifpayrekey

> l | ikev2-decfail-cppaylen

> l | ikev2-decfail-notifpaycook

> l | ikev2-decfail-tspaylen

> l | ikev2-decfail-cppayattrlen

> l | ikev2-decfail-tspayrecv

> l | ikev2-decfail-encrpaylen

> l | ikev2-decfail-tspaytstype

> l | ikev2-decfail-unsuppcritpay

> l | ikev2-decfail-unsuppcertpay

> l | ikev2-decfail-unsuppnotifprotah

> l | ikev2-decfail-unsuppauthmeth

> l | ikev2-decfail-unsupppaycritvid

> l | ikev2-decfail-unsuppmeth

> l | ikev2-decfail-unkerr

> l | ikev2-decfail-unsuppsapayprotah

> l | ikev2-decfail-unsupptspaytsnum

> l | ikev2-decfail-unsupptspaytstype

> l | ikev2-decfail-unsupptspaytsprot

> l | ikev2-decfail-cppaynoipaddr

> l | ikev2-decfail-cppayunkattr

> l | ikev2-decryptfail

> l | ikev2-decryptfail-hmac

> l | ikev2-decryptfail-pad

> l | ikev2-xchg-badmsgid

> l | ikev2-xchg-badresp

> l | ikev2-xchg-stalemsgid

> l | ikev2-xchg-unkerr

> l | ikev2-xchg-statelookfail

> l | ikev2-notifrecv-unsuppcritpay

> l | ikev2-notifrecv-invikespi

> l | ikev2-notifrecv-invmajver

> l | ikev2-notifrecv-invsyn

> l | ikev2-notifrecv-invmsgid

> l | ikev2-notifrecv-invspi

> l | ikev2-notifrecv-nopropchosen

> l | ikev2-notifrecv-invkepay

> l | ikev2-notifrecv-authfail

> l | ikev2-notifrecv-singpairreq

> l | ikev2-notifrecv-noaddsa

> l | ikev2-notifrecv-intaddrfail

> l | ikev2-notifrecv-failcpreq

> l | ikev2-notifrecv-tsunaccept

> l | ikev2-notifrecv-invsel

> l | ikev2-notifrecv-unacceptaddr

> l | ikev2-notifrecv-multiauthsupp

> l | ikev2-notifrecv-anothauthfoll

> l | ikev2-notifrecv-unexpectnat

> l | ikev2-notifrecv-macauthfail

> l | ikev2-notifrecv-hsserrusrunk

> l | ikev2-notifrecv-initcont

> l | ikev2-notifrecv-windsiz

> l | ikev2-notifrecv-addtsposs

> l | ikev2-notifrecv-ipcompsupp

> l | ikev2-notifrecv-natdetsrcip

> l | ikev2-notifrecv-natdetdstip

> l | ikev2-notifrecv-cookie

> l | ikev2-notifrecv-usetransmode

> l | ikev2-notifrecv-httpcertsupp

> l | ikev2-notifrecv-rekeysa

> l | ikev2-notifrecv-nonfirstfragalso

> l | ikev2-notifrecv-mobikesupp

> l | ikev2-notifrecv-addip4addr

> l | ikev2-notifrecv-addip6addr

> l | ikev2-notifrecv-noaddaddr

> l | ikev2-notifrecv-updsaaddr

> l | ikev2-notifrecv-cookie2

> l | ikev2-notifrecv-nonatallow

> l | ikev2-notifrecv-other

> l | ikev2-notifrecv-sipfallbnotallow

> l | ikev2-notifrecv-esptfcpadnotsupp

> l | ikev2-notifrecv-congrejrecv

> l | ikev2-cert-reqsent

> l | ikev2-cert-reqrecv

> l | ikev2-cert-sent

> l | ikev2-cert-recv

> l | ike-udpflows

> l | ike-cookieflows

> l | ike-txpackets

> l | ike-rxpackets

> l | ike-reqrecv

> l | ike-udpflowpackets

> l | ike-cookieflowpackets

> l | crypto-txesppacket

> l | crypto-txespoctet

> l | crypto-txahpacket

> l | crypto-txahoctet

> l | crypto-rxesppacket

> l | crypto-rxespoctet

> l | crypto-rxahpacket

> l | crypto-rxahoctet

> l | crypto-errauthpacket

> l | crypto-errauthoctet

> l | crypto-errbadrecpacket

> l | crypto-errbadrecoctet

> l | crypto-errdiscpacket

> l | crypto-errdiscoctet

> l | crypto-errignpacket

> l | crypto-errignoctet

> l | crypto-errunderrunpacket

> l | crypto-errunderrunoctet

> l | crypto-errinvpacket

> l | crypto-errinvoctet

> l | crypto-errreplaypacket

> l | crypto-errreplayoctet

> PDIF schema
> The following statistics have been added to the PDIF schema in Release 8.3:

> l | sess-distysetuptimeout

> l | ipsec-violpacket

> CDR Enhancements
> This section lists new GTPP dictionaries and changes in Release 8.1. Refer to the AAA Interface Configuration and Reference for details.

> l | custom14: Custom dictionary, now with support for S-CDR

> l | custom21: Custom dictionary, with support for G-CDR

> l | custom22: Custom dictionary, with support for G-CDR

> l | custom23: Custom dictionary, with support for S-CDR

> Command Enhancements
> None for this release.
> New Commands
> None for this release.
> Diameter AVPs in Release 8.0
> This section lists additions and changes to Diameter AVPs in Release 8.0. Refer to the AAA Interface Configuration and Reference for details on the attribute value pairs supported by the system.
> New Attributes

> l | BCID

> l | Acct-Realtime-Required

> l | Additional-MBMS-Trace-Info

> l | Alternative-APN

> l | BM-Address

> l | BM-Cause-Code

> l | BM-Correlation-ID

> l | BM-Information

> l | BM-Type

> l | Carrier-ID

> l | Correlate-Reason

> l | Dialog-Id

> l | Digest-Algorithm

> l | Digest-Auth-Param

> l | Digest-Domain

> l | Digest-HA1

> l | Digest-QoP

> l | Digest-Realm

> l | Direction

> l | Direct-Message

> l | Element-ID

> l | Element-Type

> l | Event-Message-Type

> l | Experimental-Result-Code

> l | Expires

> l | FDR-Reason

> l | First-Packet-Direction

> l | GMT-Timezone-Offset

> l | Group-ID

> l | HBM-Address

> l | HOA-Session-ID

> l | IMS-Communication-Service-Identifier

> l | Initial-CellSector-ID

> l | IN-Service

> l | IPGW-Address

> l | Last-CellSector-ID

> l | Last-CellSector-Location

> l | LI-Information

> l | MBMS-2G-3G-Indicator

> l | MBMS-BMSC-SSM-IP-Address

> l | MBMS-BMSC-SSM-IPv6-Address

> l | MBMS-Counting-Information

> l | MBMS-Required-QoS

> l | MBMS-Service-Area

> l | MBMS-Service-Type

> l | MBMS-Session-Duration

> l | MBMS-Session-Identity

> l | MBMS-Session-Repetition-number

> l | MBMS-StartStop-Indication

> l | MBMS-Time-To-Data-Transfer

> l | MBMS-User-Data-Mode-Indication

> l | New-Dialog-Id

> l | Nortel-Data-Reference

> l | RAI

> l | Required-MBMS-Bearer-Capabilities

> l | SIP-Digest-Authenticate

> l | SIP-Message

> l | SN-Bandwidth-Control

> l | Start-Time

> l | Stop-Time

> l | Tap-Id

> l | TMGI

> l | Transport-Protocol

> l | VBM-Address

> l | VOA-Session-ID

> Modified Attributes

> l | 3GPP-RAT-Type-Enum

> l | Event-Trigger

> l | IP-CAN-Type

> l | Max-Requested-Bandwidth-DL

> l | Max-Requested-Bandwidth-UL

> l | QoS-Class-Identifier

> Removed Attributes
> No attributes were removed from Release 8.0.
> Diameter AVPs in Release 8.1
> IMPORTANT: This section lists additions and changes to Diameter AVPs in Release 8.1.
> Refer to the AAA Interface Administration and Reference for details on the attribute value pairs supported by the system.
> New Attributes

> l | Acceptable-Service-Info

> l | Binding-Information

> l | Binding-Input-List

> l | Binding-Output-List

> l | BSID

> l | Customer-Id

> l | DIR

> l | Home-Agent

> l | IP-Version-Authorized

> l | Latching-Indication

> l | MBMS-BMSC-SSM-IP-Address

> l | MBMS-BMSC-SSM-IPv6-Address

> l | MBMS-GGSN-Address

> l | MBMS-GGSN-IPv6-Address

> l | MBMS-User-Data-Mode-Indication

> l | Multiple-Auth-Profile

> l | Multiple-Auth-Support

> l | Paging-Group-Id

> l | Port-Number

> l | Reservation-Class

> l | Revalidation-Time

> l | Rule-Activation-Time

> l | Rule-Deactivation-Time

> l | Rule-Failure-Code

> l | Rule-Reason-Code

> l | SDP-Answer-Timestamp

> l | SDP-Offer-Timestamp

> l | SDP-TimeStamps

> l | Service-Class

> l | Service-Info-Status

> l | Session-Release-Cause

> l | SN-Bandwidth-Control

> l | SN-Firewall-Policy

> l | SN-Monitoring-Key

> l | SN-Service-Flow-Detection

> l | SN-Traffic-Policy

> l | SN-Transparent-Data

> l | SN-Usage-Monitoring

> l | SN-Usage-Monitoring-Control

> l | SN-Usage-Volume

> l | Transport-Class

> l | UAR-Flags

> l | V4-Transport-Address

> l | V6-Transport-Address

> Modified Attributes

> l | 3GPP-RAT-Type-Enum

> l | Bearer-Control-Mode

> l | Charging-Rule-Install

> l | Charging-Rule-Report

> l | Early-Media-Description

> l | Event-Trigger

> l | Experimental-Result-Code

> l | Flow-Status

> l | IP-Version-Authorized

> l | Max-Requested-Bandwidth-DL

> l | Max-Requested-Bandwidth-UL

> l | TFT-Packet-Filter-Information

> Removed Attributes
> No attributes were removed from Release 8.1.
> RADIUS Attributes in Release 8.0
> This section lists additions and changes to RADIUS attributes in Release 8.0. Refer to the AAA Interface Reference for details on the attributes supported by the system.
> New Attributes

> l | Access-Request-Response-Average-Round-Trip-Time

> l | Accounting-Response-Average-Round-Trip-Time

> l | 3GPP2-MIP6-Authenticator

> l | 3GPP2-MIP6-CoA

> l | 3GPP2-MIP6-HA

> l | 3GPP2-MIP6-HoA

> l | 3GPP2-MIP6-HoA-Not-Authorized

> l | 3GPP2-MIP6-Home-Address

> l | 3GPP2-MIP6-Home-Agent

> l | 3GPP2-MIP6-Home-Link-Prefix

> l | 3GPP2-MIP6-MAC-Mobility-Data

> l | 3GPP2-MIP6-Mesg-ID

> l | 3GPP2-MIP6-Session-Key

> l | DNS

> l | FA-RK-SPI

> l | PMIP-Authenticated-Nwk-Id

> l | SN1-DNS-Proxy-Use-Subscr-Addr

> l | SN1-Ecs-Data-Volume

> l | SN1-Firewall-Enabled

> l | SN1-MIP-Reg-Lifetime-Realm

> l | SN1-QoS-Traffic-Policy

> l | SN1-Tunnel-Gn

> l | SN-DNS-Proxy-Use-Subscr-Addr

> l | SN-Ecs-Data-Volume

> l | SN-Firewall-Enabled

> l | SN-MIP-Reg-Lifetime-Realm

> l | SN-QoS-Traffic-Policy

> l | SN-Sec-IP-Pool-Name

> l | SN-Tunnel-Gn

> Modified Attributes

> l | SN1-Disconnect-Reason

> l | SN1-PPP-Progress-Code

> l | SN1-QoS-Traffic-Policy

> l | SN1-Tp-Uplk-Violate-Action

> l | SN-Disconnect-Reason

> l | SN-PPP-Progress-Code

> l | SN-QoS-Tp-Dnlk

> l | SN-QoS-Tp-Uplk

> l | SN-QoS-Traffic-Policy

> l | SN-Tp-Uplk-Violate-Action

> Removed Attributes

> l | SN-Firewall-Policy

> l | SN1-Firewall-Policy

> RADIUS Attributes in Release 8.1
> IMPORTANT: This section lists additions and changes to RADIUS attributes in Release 8.1.
> Refer to the AAA Interface Administration and Reference for details.
> New Attributes

> l | SN1-NAT-IP-Address

> l | SN1-Transparent-Data

> l | SN-Acs-Credit-Control-Group

> l | SN-Bandwidth-Policy

> l | SN-CBB-Policy

> l | SN-Firewall-Policy

> l | SN-NAT-IP-Address

> l | SN-Sec-IP-Pool-Name

> l | SN-Transparent-Data

> l | UAR-Flags

> l | WiMAX-Packet-Flow-Descriptor-V2

> l | WiMAX-PPAC

> l | WiMAX-PPAQ

> l | WiMAX-Session-Term-Capability

> Modified Attributes

> l | 3GPP2-Remote-IPv4-Addr-Octets

> l | Session-Timeout

> l | SN1-Disconnect-Reason

> l | SN1-PPP-Progress-Code

> l | SN1-Prepaid

> l | SN1-QoS-Traffic-Policy

> l | SN1-Tp-Dnlk-Exceed-Action

> l | SN1-Tp-Dnlk-Violate-Action

> l | SN1-Tp-Uplk-Exceed-Action

> l | SN1-Tp-Uplk-Violate-Action

> l | SN-CSCF-Rf-SDP-Media-Components

> l | SN-Disconnect-Reason

> l | SN-PPP-Progress-Code

> l | SN-Prepaid

> l | SN-QoS-Traffic-Policy

> l | SN-Tp-Dnlk-Exceed-Action

> l | SN-Tp-Dnlk-Violate-Action

> l | SN-Tp-Uplk-Exceed-Action

> l | SN-Tp-Uplk-Violate-Action

> l | WiMAX-PPAQ

> l | WiMAX-Prepaid-Indicator

> l | WiMAX-QoS-Descriptor

> Removed Attributes
> No attributes were removed from Release 8.1.
> RADIUS Attributes in Release 8.3
> IMPORTANT: This section lists additions and changes to RADIUS attributes in Release 8.3.
> Refer to the AAA Interface Administration and Reference for details.
> New Attributes
> No new attributes for this release.
> Modified Attributes

> l | SN1-MIP-Send-Term-Verification

> l | SN-MIP-Send-Term-Verification

> Removed Attributes
> No attributes were removed from Release 8.3.
> Web Element Manager Enhancements
> None for this release.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883