> show gprs-service
> This chapter includes the show gprs-service command output tables.
> show gprs-service all
> show gprs-service all Command Output Descriptions

> Field | Description
> Service name | The GPRS service name that is running in this session.
> Context | Name of the VPN context in which specified GPRS service is running.
> Status | Status of the GPRS service for which statistics are displayed.
> Accounting Context Name | Name of the accounting context for this GPRS service to enable accounting parameters.
> Self PLMN | Name of the PLMN of this GPRS service.
> MAP Service | Name of the mobile application part (MAP) service configured in this GPRS service.
> SGTP Service | Name of the SGSN GTPP (SGTP) service configured in this GPRS service.
> GS Serviceq | Name of the Gs service configured in this GPRS service to provide Gs interface support between an SGSN and an MSC/VLR.
> SM-T3385 Timeout | The time-out duration in seconds for GPRS session management timer - T3385 on network side for PDP context activation.
> SM-T3386 Timeout | The time-out duration in seconds for GPRS session management timer - T3386 on network side for PDP context modification.
> SM-T3395 Timeout | The time-out duration in seconds for GPRS session management timer - T3395 on network side for PDP context deactivation.
> SM-Max Activate Retries | Total number of retries for PDP context activation from GPRS session manager.
> SM-Max Modify Retries | Total number of retries for PDP context modification from GPRS session manager.
> SM-Max Deactivate Retries | Total number of retries for PDP context deactivation from GPRS session manager.
> SM-Ignore PCO IE Decode Error | Indicates whether the decoding error ignored due to incorrect PCO IE length in SM messages is enabled/disabled.
> SM-Trim Trailing Spaces in APN | Indicates whether the removal of any trailing space(s) in requested APN by SGSN is enabled/disabled.
> SM-APN Partial match | Indicates whether the partial matching of requested APN during APN selection is enabled/disabled.
> SM-APN(R) from First Sub Record | Indicates (enabled) that the selection of the APN from the first subscription record is to be used as the requested APN.
> GMM-Mnr Timeout | The time-out duration in seconds for GPRS mobility management timer - Mobile Reachable on network side.
> GMM-Purge Timeout | The time-out duration in seconds for GPRS mobility management timer - Purge to hold the detach of MM context on network side.
> GMM-T3313 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3313 on network side for paging procedure initiation.
> GMM-T3312 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3313 on network side for RAU procedure initiation.
> GMM-T3370 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3370 on network side for identity request procedure.
> GMM-Max Identity Retries | Maximum number of retries for identity request procedure from GPRS mobility manager.
> GMM-T3360 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3360 on network side for Authentication and Cipher request procedure.
> GMM-Max Auth Retries | Maximum number of retries for authentication request procedure from GPRS mobility manager.
> GMM LLC Timeout | Configured timeout duration in seconds at the logical link control protocol message procedure from GPRS mobility manager.
> GMM LLC MAX Retries | Maximum number of retries at the logical link control protocol message procedure from GPRS mobility manager.
> GMM LLC PDU Life Time | Configured life time in seconds at the logical link control protocol message procedure from GPRS mobility manager.
> GMM-Perform-Identity-After-Auth | Specifies whether “perform identity after authentication” procedure is enabled or not.
> Ciphering Algorithm | This group provides the ciphering algorithm configuration in this GPRS service.
> Priority 1..3 | Specifies the priority for GPRS Encryption Algorithm (GEA) configured for ciphering in this GPRS service. Possible GPRS encryption algorithms are: gea0: GPRS Encryption Algorithm 0 (GEA0)gea1: GPRS Encryption Algorithm 1 (GEA1)gea2: GPRS Encryption Algorithm 2 (GEA2)gea3: GPRS Encryption Algorithm 3(GEA3)
> Accounting cdr-types | Specifies type of accounting CDRs configured in this GPRS service. Possible values are: mcdr: Mobility CDR (M-CDR)scdr: SGSN CDR (S-CDR)sms mo-cdr: SMS Mobile Originated CDR (S-MO-CDR)sms mt-cdr: SMS Mobile Terminated CDR (S-MT-CDR)
> Charging Characteristics(CC) Profiles | This group provides the charging characteristics (CC) profiles configured in this GPRS service
> Profile nn | Specifies the charging characteristic (CC) profile configured in this SGSN service. nn is the number of CC profiles configured in this GPRS service and possible values are 1 through 15.
> Buckets | Specifies the charging bucket configured for charging characteristic in this GPRS service
> paging-scheme | Specifies the paging scheme configuration information in this GPRS service
> max-page-retransmission | Specifies the maximum number of retries configured for paging in this GPRS service
> paging-area | Specifies the paging area information in this GPRS service.
> last-known-cell | Indicate the last known cell of the subscriber.
> last-known-ra | Indicate the last known routing area of the subscriber.
> last-known-la | Indicate the last known location area of the subscriber.
> last-known-bsc | Indicate the last known base station controller (BSC) of the subscriber.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883