> ASN Service Profile Configuration Mode Commands
> The ASN Service Profile Configuration Mode is used to create and manage the service profiles table for the ASN GW service subscribers within the current context.
> downlink-classifier
> This command specifies the classifier to match for traffic flow in downlink direction for subscribers in this service.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> [ no ] downlink-classifier class-map class_map_name
> no
> Removes/deletes the configured class map for this traffic flow in the ASN GW service.
> class-map class_map_name
> Specifies the configured Class-Map to this traffic flow.
> class_map_name is the name of an existing Class-Map configured in the destination context.
> Refer to the Class-Map Configuration Mode chapter of this reference for additional information to configure the class maps.
> Usage
> Use this command to configure classifier for downlink traffic with a configured Class-Map for the ASN GW service subscribers.
> A maximum of 4 class-maps can be configured in one ASN GW service profile.
> Class-Map Configuration Mode is accessible through Context Configuration Mode.
> Example
> The following command applies the Class-Map class_1 to this traffic:
> downlink-classifier class-map class_1
> downlink-qos-id
> This command specifies the QoS table identifier to traffic flow in downlink direction for subscribers in this service.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> downlink-qos-id qos_table_id
> [ no ] downlink-qos-id
> no
> Removes/deletes the configured class map for this traffic flow in the ASN GW service.
> qos_table_id
> Specifies the configured ASN QoS Descriptor Identifier to this traffic flow.
> qos_table_id is the identifier of an existing ASN QoS Descriptor Table configured in the source context.
> Refer to the ASN QoS Descriptor Configuration Mode chapter of this reference for additional information to configure QoS descriptor table identifier.
> Usage
> Use this command to apply a QoS identifier for downlink traffic with a configured ASN QoS Descriptor Table Identifier for the ASN GW service subscribers.
> Only one QoS identifier can be configured in one ASN GW service profile.
> ASN QoS Descriptor Configuration Mode is accessible through Context Configuration Mode.
> Example
> The following command applies the QoS table identifier 123 to this traffic:
> downlink-qos-id 123
> end
> This command exits the current mode and returns to the Executive Mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Executive mode.
> exit
> This command exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> uplink-classifier
> This command specifies the classifier to match for traffic flow in uplink direction for subscribers in this service.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> [ no ] uplink-classifier class-map class_map_name
> no
> Removes/deletes the configured class map for this traffic flow in the ASN GW service.
> class-map class_map_name
> Specifies the configured Class-Map to this traffic flow.
> class_map_name is the name of an existing Class-Map configured in the destination context.
> Refer to the Class-Map Configuration Mode chapter of this reference for additional information to configure class maps.
> Usage
> Use this command to configure classifier for uplink traffic with a configured Class-Map for the ASN GW service subscribers.
> A maximum of 4 class-maps can be configured in one ASN GW service profile.
> Class-Map Configuration Mode is accessible through Context Configuration Mode.
> Example
> The following command applies the Class-Map class_1 to this traffic:
> uplink-classifier class-map class_1
> uplink-qos-id
> This command specifies the QoS table identifier to traffic flow in uplink direction for subscribers in this service.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> uplink-qos-id qos_table_id
> [ no ] uplink-qos-id
> no
> Removes/deletes the configured class map for this traffic flow in the ASN GW service.
> qos_table_id
> Specifies the configured ASN QoS Descriptor Identifier to this traffic flow.
> qos_table_id is the identifier of an existing ASN QoS Descriptor Table configured in the source context.
> Refer to the ASN QoS Descriptor Configuration Mode chapter of this reference for additional information to configure QoS descriptor table identifier.
> Usage
> Use this command to apply a QoS identifier for uplink traffic with a configured ASN QoS Descriptor Table Identifier for the ASN GW service subscribers.
> Only one QoS identifier can be configured in one ASN GW service profile.
> ASN QoS Descriptor Configuration Mode is accessible through Context Configuration Mode.
> Example
> The following command applies the QoS table identifier 123 to this traffic:
> uplink-qos-id 123

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883